QA output created by 033
meta-data=DDEV isize=XXX agcount=N, agsize=XXX blks
data     = bsize=XXX blocks=XXX, imaxpct=PCT
         = sunit=XXX swidth=XXX, unwritten=X
naming   =VERN bsize=XXX
log      =LDEV bsize=XXX blocks=XXX
realtime =RDEV extsz=XXX blocks=XXX, rtextents=XXX
Corrupting root inode - setting bits to 0
Wrote X.XXKb (value 0x0)
Phase 1 - find and verify superblock...
Phase 2 - using <TYPEOF> log
        - zero log...
        - scan filesystem freespace and inode maps...
        - found root inode chunk
Phase 3 - for each AG...
        - scan and clear agi unlinked lists...
        - process known inodes and perform inode discovery...
bad magic number 0x0 on inode INO
bad version number 0x0 on inode INO
bad magic number 0x0 on inode INO, resetting magic number
bad version number 0x0 on inode INO, resetting version number
imap claims a free inode INO is in use, correcting imap and clearing inode
cleared root inode INO
        - process newly discovered inodes...
Phase 4 - check for duplicate blocks...
        - setting up duplicate extent list...
root inode lost
        - check for inodes claiming duplicate blocks...
Phase 5 - rebuild AG headers and trees...
        - reset superblock...
Phase 6 - check inode connectivity...
reinitializing root directory
        - resetting contents of realtime bitmap and summary inodes
        - traversing filesystem ...
        - traversal finished ...
        - moving disconnected inodes to lost+found ...
Phase 7 - verify and correct link counts...
resetting inode INO nlinks from 1 to 2
done
Corrupting rt bitmap inode - setting bits to 0
Wrote X.XXKb (value 0x0)
Phase 1 - find and verify superblock...
Phase 2 - using <TYPEOF> log
        - zero log...
        - scan filesystem freespace and inode maps...
        - found root inode chunk
Phase 3 - for each AG...
        - scan and clear agi unlinked lists...
        - process known inodes and perform inode discovery...
bad magic number 0x0 on inode INO
bad version number 0x0 on inode INO
bad magic number 0x0 on inode INO, resetting magic number
bad version number 0x0 on inode INO, resetting version number
imap claims a free inode INO is in use, correcting imap and clearing inode
cleared realtime bitmap inode INO
        - process newly discovered inodes...
Phase 4 - check for duplicate blocks...
        - setting up duplicate extent list...
        - check for inodes claiming duplicate blocks...
Phase 5 - rebuild AG headers and trees...
        - reset superblock...
Phase 6 - check inode connectivity...
reinitializing realtime bitmap inode
        - resetting contents of realtime bitmap and summary inodes
        - traversing filesystem ...
        - traversal finished ...
        - moving disconnected inodes to lost+found ...
Phase 7 - verify and correct link counts...
done
Corrupting rt summary inode - setting bits to 0
Wrote X.XXKb (value 0x0)
Phase 1 - find and verify superblock...
Phase 2 - using <TYPEOF> log
        - zero log...
        - scan filesystem freespace and inode maps...
        - found root inode chunk
Phase 3 - for each AG...
        - scan and clear agi unlinked lists...
        - process known inodes and perform inode discovery...
bad magic number 0x0 on inode INO
bad version number 0x0 on inode INO
bad magic number 0x0 on inode INO, resetting magic number
bad version number 0x0 on inode INO, resetting version number
imap claims a free inode INO is in use, correcting imap and clearing inode
cleared realtime summary inode INO
        - process newly discovered inodes...
Phase 4 - check for duplicate blocks...
        - setting up duplicate extent list...
        - check for inodes claiming duplicate blocks...
Phase 5 - rebuild AG headers and trees...
        - reset superblock...
Phase 6 - check inode connectivity...
reinitializing realtime summary inode
        - resetting contents of realtime bitmap and summary inodes
        - traversing filesystem ...
        - traversal finished ...
        - moving disconnected inodes to lost+found ...
Phase 7 - verify and correct link counts...
done
Corrupting root inode - setting bits to -1
Wrote X.XXKb (value 0xffffffff)
Phase 1 - find and verify superblock...
Phase 2 - using <TYPEOF> log
        - zero log...
        - scan filesystem freespace and inode maps...
        - found root inode chunk
Phase 3 - for each AG...
        - scan and clear agi unlinked lists...
        - process known inodes and perform inode discovery...
bad magic number 0xffff on inode INO
bad version number 0xffffffff on inode INO
bad (negative) size -1 on inode INO
bad magic number 0xffff on inode INO, resetting magic number
bad version number 0xffffffff on inode INO, resetting version number
bad (negative) size -1 on inode INO
cleared root inode INO
        - process newly discovered inodes...
Phase 4 - check for duplicate blocks...
        - setting up duplicate extent list...
root inode lost
        - check for inodes claiming duplicate blocks...
Phase 5 - rebuild AG headers and trees...
        - reset superblock...
Phase 6 - check inode connectivity...
reinitializing root directory
        - resetting contents of realtime bitmap and summary inodes
        - traversing filesystem ...
        - traversal finished ...
        - moving disconnected inodes to lost+found ...
Phase 7 - verify and correct link counts...
resetting inode INO nlinks from 1 to 2
done
Corrupting rt bitmap inode - setting bits to -1
Wrote X.XXKb (value 0xffffffff)
Phase 1 - find and verify superblock...
Phase 2 - using <TYPEOF> log
        - zero log...
        - scan filesystem freespace and inode maps...
        - found root inode chunk
Phase 3 - for each AG...
        - scan and clear agi unlinked lists...
        - process known inodes and perform inode discovery...
bad magic number 0xffff on inode INO
bad version number 0xffffffff on inode INO
bad (negative) size -1 on inode INO
bad magic number 0xffff on inode INO, resetting magic number
bad version number 0xffffffff on inode INO, resetting version number
bad (negative) size -1 on inode INO
cleared realtime bitmap inode INO
        - process newly discovered inodes...
Phase 4 - check for duplicate blocks...
        - setting up duplicate extent list...
        - check for inodes claiming duplicate blocks...
Phase 5 - rebuild AG headers and trees...
        - reset superblock...
Phase 6 - check inode connectivity...
reinitializing realtime bitmap inode
        - resetting contents of realtime bitmap and summary inodes
        - traversing filesystem ...
        - traversal finished ...
        - moving disconnected inodes to lost+found ...
Phase 7 - verify and correct link counts...
done
Corrupting rt summary inode - setting bits to -1
Wrote X.XXKb (value 0xffffffff)
Phase 1 - find and verify superblock...
Phase 2 - using <TYPEOF> log
        - zero log...
        - scan filesystem freespace and inode maps...
        - found root inode chunk
Phase 3 - for each AG...
        - scan and clear agi unlinked lists...
        - process known inodes and perform inode discovery...
bad magic number 0xffff on inode INO
bad version number 0xffffffff on inode INO
bad (negative) size -1 on inode INO
bad magic number 0xffff on inode INO, resetting magic number
bad version number 0xffffffff on inode INO, resetting version number
bad (negative) size -1 on inode INO
cleared realtime summary inode INO
        - process newly discovered inodes...
Phase 4 - check for duplicate blocks...
        - setting up duplicate extent list...
        - check for inodes claiming duplicate blocks...
Phase 5 - rebuild AG headers and trees...
        - reset superblock...
Phase 6 - check inode connectivity...
reinitializing realtime summary inode
        - resetting contents of realtime bitmap and summary inodes
        - traversing filesystem ...
        - traversal finished ...
        - moving disconnected inodes to lost+found ...
Phase 7 - verify and correct link counts...
done
