diff --git a/Documentation/devicetree/bindings/sound/adi,axi-spdif-tx.txt b/Documentation/devicetree/bindings/sound/adi,axi-spdif-tx.txt
index 46f344965313..4eb7997674a0 100644
--- a/Documentation/devicetree/bindings/sound/adi,axi-spdif-tx.txt
+++ b/Documentation/devicetree/bindings/sound/adi,axi-spdif-tx.txt
@@ -1,7 +1,7 @@
 ADI AXI-SPDIF controller
 
 Required properties:
- - compatible : Must be "adi,axi-spdif-1.00.a"
+ - compatible : Must be "adi,axi-spdif-tx-1.00.a"
  - reg : Must contain SPDIF core's registers location and length
  - clocks : Pairs of phandle and specifier referencing the controller's clocks.
    The controller expects two clocks, the clock used for the AXI interface and
diff --git a/Makefile b/Makefile
index 05279d4f44c9..b1746b486646 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 14
-SUBLEVEL = 18
+SUBLEVEL = 19
 EXTRAVERSION =
 NAME = Remembering Coco
 
diff --git a/arch/mips/cavium-octeon/setup.c b/arch/mips/cavium-octeon/setup.c
index 331b837cec57..270cb3c6c498 100644
--- a/arch/mips/cavium-octeon/setup.c
+++ b/arch/mips/cavium-octeon/setup.c
@@ -458,6 +458,18 @@ static void octeon_halt(void)
 	octeon_kill_core(NULL);
 }
 
+static char __read_mostly octeon_system_type[80];
+
+static int __init init_octeon_system_type(void)
+{
+	snprintf(octeon_system_type, sizeof(octeon_system_type), "%s (%s)",
+		cvmx_board_type_to_string(octeon_bootinfo->board_type),
+		octeon_model_get_string(read_c0_prid()));
+
+	return 0;
+}
+early_initcall(init_octeon_system_type);
+
 /**
  * Return a string representing the system type
  *
@@ -465,11 +477,7 @@ static void octeon_halt(void)
  */
 const char *octeon_board_type_string(void)
 {
-	static char name[80];
-	sprintf(name, "%s (%s)",
-		cvmx_board_type_to_string(octeon_bootinfo->board_type),
-		octeon_model_get_string(read_c0_prid()));
-	return name;
+	return octeon_system_type;
 }
 
 const char *get_system_type(void)
diff --git a/arch/mips/include/asm/ptrace.h b/arch/mips/include/asm/ptrace.h
index 7bba9da110af..6d019ca1bead 100644
--- a/arch/mips/include/asm/ptrace.h
+++ b/arch/mips/include/asm/ptrace.h
@@ -23,7 +23,7 @@
 struct pt_regs {
 #ifdef CONFIG_32BIT
 	/* Pad bytes for argument save space on the stack. */
-	unsigned long pad0[6];
+	unsigned long pad0[8];
 #endif
 
 	/* Saved main processor registers. */
diff --git a/arch/mips/include/asm/reg.h b/arch/mips/include/asm/reg.h
index 910e71a12466..b8343ccbc989 100644
--- a/arch/mips/include/asm/reg.h
+++ b/arch/mips/include/asm/reg.h
@@ -12,116 +12,194 @@
 #ifndef __ASM_MIPS_REG_H
 #define __ASM_MIPS_REG_H
 
-
-#if defined(CONFIG_32BIT) || defined(WANT_COMPAT_REG_H)
-
-#define EF_R0			6
-#define EF_R1			7
-#define EF_R2			8
-#define EF_R3			9
-#define EF_R4			10
-#define EF_R5			11
-#define EF_R6			12
-#define EF_R7			13
-#define EF_R8			14
-#define EF_R9			15
-#define EF_R10			16
-#define EF_R11			17
-#define EF_R12			18
-#define EF_R13			19
-#define EF_R14			20
-#define EF_R15			21
-#define EF_R16			22
-#define EF_R17			23
-#define EF_R18			24
-#define EF_R19			25
-#define EF_R20			26
-#define EF_R21			27
-#define EF_R22			28
-#define EF_R23			29
-#define EF_R24			30
-#define EF_R25			31
+#define MIPS32_EF_R0		6
+#define MIPS32_EF_R1		7
+#define MIPS32_EF_R2		8
+#define MIPS32_EF_R3		9
+#define MIPS32_EF_R4		10
+#define MIPS32_EF_R5		11
+#define MIPS32_EF_R6		12
+#define MIPS32_EF_R7		13
+#define MIPS32_EF_R8		14
+#define MIPS32_EF_R9		15
+#define MIPS32_EF_R10		16
+#define MIPS32_EF_R11		17
+#define MIPS32_EF_R12		18
+#define MIPS32_EF_R13		19
+#define MIPS32_EF_R14		20
+#define MIPS32_EF_R15		21
+#define MIPS32_EF_R16		22
+#define MIPS32_EF_R17		23
+#define MIPS32_EF_R18		24
+#define MIPS32_EF_R19		25
+#define MIPS32_EF_R20		26
+#define MIPS32_EF_R21		27
+#define MIPS32_EF_R22		28
+#define MIPS32_EF_R23		29
+#define MIPS32_EF_R24		30
+#define MIPS32_EF_R25		31
 
 /*
  * k0/k1 unsaved
  */
-#define EF_R26			32
-#define EF_R27			33
+#define MIPS32_EF_R26		32
+#define MIPS32_EF_R27		33
 
-#define EF_R28			34
-#define EF_R29			35
-#define EF_R30			36
-#define EF_R31			37
+#define MIPS32_EF_R28		34
+#define MIPS32_EF_R29		35
+#define MIPS32_EF_R30		36
+#define MIPS32_EF_R31		37
 
 /*
  * Saved special registers
  */
-#define EF_LO			38
-#define EF_HI			39
-
-#define EF_CP0_EPC		40
-#define EF_CP0_BADVADDR		41
-#define EF_CP0_STATUS		42
-#define EF_CP0_CAUSE		43
-#define EF_UNUSED0		44
-
-#define EF_SIZE			180
-
-#endif
-
-#if defined(CONFIG_64BIT) && !defined(WANT_COMPAT_REG_H)
-
-#define EF_R0			 0
-#define EF_R1			 1
-#define EF_R2			 2
-#define EF_R3			 3
-#define EF_R4			 4
-#define EF_R5			 5
-#define EF_R6			 6
-#define EF_R7			 7
-#define EF_R8			 8
-#define EF_R9			 9
-#define EF_R10			10
-#define EF_R11			11
-#define EF_R12			12
-#define EF_R13			13
-#define EF_R14			14
-#define EF_R15			15
-#define EF_R16			16
-#define EF_R17			17
-#define EF_R18			18
-#define EF_R19			19
-#define EF_R20			20
-#define EF_R21			21
-#define EF_R22			22
-#define EF_R23			23
-#define EF_R24			24
-#define EF_R25			25
+#define MIPS32_EF_LO		38
+#define MIPS32_EF_HI		39
+
+#define MIPS32_EF_CP0_EPC	40
+#define MIPS32_EF_CP0_BADVADDR	41
+#define MIPS32_EF_CP0_STATUS	42
+#define MIPS32_EF_CP0_CAUSE	43
+#define MIPS32_EF_UNUSED0	44
+
+#define MIPS32_EF_SIZE		180
+
+#define MIPS64_EF_R0		0
+#define MIPS64_EF_R1		1
+#define MIPS64_EF_R2		2
+#define MIPS64_EF_R3		3
+#define MIPS64_EF_R4		4
+#define MIPS64_EF_R5		5
+#define MIPS64_EF_R6		6
+#define MIPS64_EF_R7		7
+#define MIPS64_EF_R8		8
+#define MIPS64_EF_R9		9
+#define MIPS64_EF_R10		10
+#define MIPS64_EF_R11		11
+#define MIPS64_EF_R12		12
+#define MIPS64_EF_R13		13
+#define MIPS64_EF_R14		14
+#define MIPS64_EF_R15		15
+#define MIPS64_EF_R16		16
+#define MIPS64_EF_R17		17
+#define MIPS64_EF_R18		18
+#define MIPS64_EF_R19		19
+#define MIPS64_EF_R20		20
+#define MIPS64_EF_R21		21
+#define MIPS64_EF_R22		22
+#define MIPS64_EF_R23		23
+#define MIPS64_EF_R24		24
+#define MIPS64_EF_R25		25
 
 /*
  * k0/k1 unsaved
  */
-#define EF_R26			26
-#define EF_R27			27
+#define MIPS64_EF_R26		26
+#define MIPS64_EF_R27		27
 
 
-#define EF_R28			28
-#define EF_R29			29
-#define EF_R30			30
-#define EF_R31			31
+#define MIPS64_EF_R28		28
+#define MIPS64_EF_R29		29
+#define MIPS64_EF_R30		30
+#define MIPS64_EF_R31		31
 
 /*
  * Saved special registers
  */
-#define EF_LO			32
-#define EF_HI			33
-
-#define EF_CP0_EPC		34
-#define EF_CP0_BADVADDR		35
-#define EF_CP0_STATUS		36
-#define EF_CP0_CAUSE		37
-
-#define EF_SIZE			304	/* size in bytes */
+#define MIPS64_EF_LO		32
+#define MIPS64_EF_HI		33
+
+#define MIPS64_EF_CP0_EPC	34
+#define MIPS64_EF_CP0_BADVADDR	35
+#define MIPS64_EF_CP0_STATUS	36
+#define MIPS64_EF_CP0_CAUSE	37
+
+#define MIPS64_EF_SIZE		304	/* size in bytes */
+
+#if defined(CONFIG_32BIT)
+
+#define EF_R0			MIPS32_EF_R0
+#define EF_R1			MIPS32_EF_R1
+#define EF_R2			MIPS32_EF_R2
+#define EF_R3			MIPS32_EF_R3
+#define EF_R4			MIPS32_EF_R4
+#define EF_R5			MIPS32_EF_R5
+#define EF_R6			MIPS32_EF_R6
+#define EF_R7			MIPS32_EF_R7
+#define EF_R8			MIPS32_EF_R8
+#define EF_R9			MIPS32_EF_R9
+#define EF_R10			MIPS32_EF_R10
+#define EF_R11			MIPS32_EF_R11
+#define EF_R12			MIPS32_EF_R12
+#define EF_R13			MIPS32_EF_R13
+#define EF_R14			MIPS32_EF_R14
+#define EF_R15			MIPS32_EF_R15
+#define EF_R16			MIPS32_EF_R16
+#define EF_R17			MIPS32_EF_R17
+#define EF_R18			MIPS32_EF_R18
+#define EF_R19			MIPS32_EF_R19
+#define EF_R20			MIPS32_EF_R20
+#define EF_R21			MIPS32_EF_R21
+#define EF_R22			MIPS32_EF_R22
+#define EF_R23			MIPS32_EF_R23
+#define EF_R24			MIPS32_EF_R24
+#define EF_R25			MIPS32_EF_R25
+#define EF_R26			MIPS32_EF_R26
+#define EF_R27			MIPS32_EF_R27
+#define EF_R28			MIPS32_EF_R28
+#define EF_R29			MIPS32_EF_R29
+#define EF_R30			MIPS32_EF_R30
+#define EF_R31			MIPS32_EF_R31
+#define EF_LO			MIPS32_EF_LO
+#define EF_HI			MIPS32_EF_HI
+#define EF_CP0_EPC		MIPS32_EF_CP0_EPC
+#define EF_CP0_BADVADDR		MIPS32_EF_CP0_BADVADDR
+#define EF_CP0_STATUS		MIPS32_EF_CP0_STATUS
+#define EF_CP0_CAUSE		MIPS32_EF_CP0_CAUSE
+#define EF_UNUSED0		MIPS32_EF_UNUSED0
+#define EF_SIZE			MIPS32_EF_SIZE
+
+#elif defined(CONFIG_64BIT)
+
+#define EF_R0			MIPS64_EF_R0
+#define EF_R1			MIPS64_EF_R1
+#define EF_R2			MIPS64_EF_R2
+#define EF_R3			MIPS64_EF_R3
+#define EF_R4			MIPS64_EF_R4
+#define EF_R5			MIPS64_EF_R5
+#define EF_R6			MIPS64_EF_R6
+#define EF_R7			MIPS64_EF_R7
+#define EF_R8			MIPS64_EF_R8
+#define EF_R9			MIPS64_EF_R9
+#define EF_R10			MIPS64_EF_R10
+#define EF_R11			MIPS64_EF_R11
+#define EF_R12			MIPS64_EF_R12
+#define EF_R13			MIPS64_EF_R13
+#define EF_R14			MIPS64_EF_R14
+#define EF_R15			MIPS64_EF_R15
+#define EF_R16			MIPS64_EF_R16
+#define EF_R17			MIPS64_EF_R17
+#define EF_R18			MIPS64_EF_R18
+#define EF_R19			MIPS64_EF_R19
+#define EF_R20			MIPS64_EF_R20
+#define EF_R21			MIPS64_EF_R21
+#define EF_R22			MIPS64_EF_R22
+#define EF_R23			MIPS64_EF_R23
+#define EF_R24			MIPS64_EF_R24
+#define EF_R25			MIPS64_EF_R25
+#define EF_R26			MIPS64_EF_R26
+#define EF_R27			MIPS64_EF_R27
+#define EF_R28			MIPS64_EF_R28
+#define EF_R29			MIPS64_EF_R29
+#define EF_R30			MIPS64_EF_R30
+#define EF_R31			MIPS64_EF_R31
+#define EF_LO			MIPS64_EF_LO
+#define EF_HI			MIPS64_EF_HI
+#define EF_CP0_EPC		MIPS64_EF_CP0_EPC
+#define EF_CP0_BADVADDR		MIPS64_EF_CP0_BADVADDR
+#define EF_CP0_STATUS		MIPS64_EF_CP0_STATUS
+#define EF_CP0_CAUSE		MIPS64_EF_CP0_CAUSE
+#define EF_SIZE			MIPS64_EF_SIZE
 
 #endif /* CONFIG_64BIT */
 
diff --git a/arch/mips/kernel/binfmt_elfo32.c b/arch/mips/kernel/binfmt_elfo32.c
index 7faf5f2bee25..71df942fb77c 100644
--- a/arch/mips/kernel/binfmt_elfo32.c
+++ b/arch/mips/kernel/binfmt_elfo32.c
@@ -72,12 +72,6 @@ typedef elf_fpreg_t elf_fpregset_t[ELF_NFPREG];
 
 #include <asm/processor.h>
 
-/*
- * When this file is selected, we are definitely running a 64bit kernel.
- * So using the right regs define in asm/reg.h
- */
-#define WANT_COMPAT_REG_H
-
 /* These MUST be defined before elf.h gets included */
 extern void elf32_core_copy_regs(elf_gregset_t grp, struct pt_regs *regs);
 #define ELF_CORE_COPY_REGS(_dest, _regs) elf32_core_copy_regs(_dest, _regs);
@@ -149,21 +143,21 @@ void elf32_core_copy_regs(elf_gregset_t grp, struct pt_regs *regs)
 {
 	int i;
 
-	for (i = 0; i < EF_R0; i++)
+	for (i = 0; i < MIPS32_EF_R0; i++)
 		grp[i] = 0;
-	grp[EF_R0] = 0;
+	grp[MIPS32_EF_R0] = 0;
 	for (i = 1; i <= 31; i++)
-		grp[EF_R0 + i] = (elf_greg_t) regs->regs[i];
-	grp[EF_R26] = 0;
-	grp[EF_R27] = 0;
-	grp[EF_LO] = (elf_greg_t) regs->lo;
-	grp[EF_HI] = (elf_greg_t) regs->hi;
-	grp[EF_CP0_EPC] = (elf_greg_t) regs->cp0_epc;
-	grp[EF_CP0_BADVADDR] = (elf_greg_t) regs->cp0_badvaddr;
-	grp[EF_CP0_STATUS] = (elf_greg_t) regs->cp0_status;
-	grp[EF_CP0_CAUSE] = (elf_greg_t) regs->cp0_cause;
-#ifdef EF_UNUSED0
-	grp[EF_UNUSED0] = 0;
+		grp[MIPS32_EF_R0 + i] = (elf_greg_t) regs->regs[i];
+	grp[MIPS32_EF_R26] = 0;
+	grp[MIPS32_EF_R27] = 0;
+	grp[MIPS32_EF_LO] = (elf_greg_t) regs->lo;
+	grp[MIPS32_EF_HI] = (elf_greg_t) regs->hi;
+	grp[MIPS32_EF_CP0_EPC] = (elf_greg_t) regs->cp0_epc;
+	grp[MIPS32_EF_CP0_BADVADDR] = (elf_greg_t) regs->cp0_badvaddr;
+	grp[MIPS32_EF_CP0_STATUS] = (elf_greg_t) regs->cp0_status;
+	grp[MIPS32_EF_CP0_CAUSE] = (elf_greg_t) regs->cp0_cause;
+#ifdef MIPS32_EF_UNUSED0
+	grp[MIPS32_EF_UNUSED0] = 0;
 #endif
 }
 
diff --git a/arch/mips/kernel/irq-gic.c b/arch/mips/kernel/irq-gic.c
index 5b5ddb231f26..78f18436cdf2 100644
--- a/arch/mips/kernel/irq-gic.c
+++ b/arch/mips/kernel/irq-gic.c
@@ -255,11 +255,13 @@ static void __init gic_setup_intr(unsigned int intr, unsigned int cpu,
 
 	/* Setup Intr to Pin mapping */
 	if (pin & GIC_MAP_TO_NMI_MSK) {
+		int i;
+
 		GICWRITE(GIC_REG_ADDR(SHARED, GIC_SH_MAP_TO_PIN(intr)), pin);
 		/* FIXME: hack to route NMI to all cpu's */
-		for (cpu = 0; cpu < NR_CPUS; cpu += 32) {
+		for (i = 0; i < NR_CPUS; i += 32) {
 			GICWRITE(GIC_REG_ADDR(SHARED,
-					  GIC_SH_MAP_TO_VPE_REG_OFF(intr, cpu)),
+					  GIC_SH_MAP_TO_VPE_REG_OFF(intr, i)),
 				 0xffffffff);
 		}
 	} else {
diff --git a/arch/mips/kernel/ptrace.c b/arch/mips/kernel/ptrace.c
index 7da9b76db4d9..60f48febe762 100644
--- a/arch/mips/kernel/ptrace.c
+++ b/arch/mips/kernel/ptrace.c
@@ -170,6 +170,7 @@ int ptrace_setfpregs(struct task_struct *child, __u32 __user *data)
 		__get_user(fregs[i], i + (__u64 __user *) data);
 
 	__get_user(child->thread.fpu.fcr31, data + 64);
+	child->thread.fpu.fcr31 &= ~FPU_CSR_ALL_X;
 
 	/* FIR may not be written.  */
 
@@ -265,36 +266,160 @@ int ptrace_set_watch_regs(struct task_struct *child,
 
 /* regset get/set implementations */
 
-static int gpr_get(struct task_struct *target,
-		   const struct user_regset *regset,
-		   unsigned int pos, unsigned int count,
-		   void *kbuf, void __user *ubuf)
+#if defined(CONFIG_32BIT) || defined(CONFIG_MIPS32_O32)
+
+static int gpr32_get(struct task_struct *target,
+		     const struct user_regset *regset,
+		     unsigned int pos, unsigned int count,
+		     void *kbuf, void __user *ubuf)
 {
 	struct pt_regs *regs = task_pt_regs(target);
+	u32 uregs[ELF_NGREG] = {};
+	unsigned i;
 
-	return user_regset_copyout(&pos, &count, &kbuf, &ubuf,
-				   regs, 0, sizeof(*regs));
+	for (i = MIPS32_EF_R1; i <= MIPS32_EF_R31; i++) {
+		/* k0/k1 are copied as zero. */
+		if (i == MIPS32_EF_R26 || i == MIPS32_EF_R27)
+			continue;
+
+		uregs[i] = regs->regs[i - MIPS32_EF_R0];
+	}
+
+	uregs[MIPS32_EF_LO] = regs->lo;
+	uregs[MIPS32_EF_HI] = regs->hi;
+	uregs[MIPS32_EF_CP0_EPC] = regs->cp0_epc;
+	uregs[MIPS32_EF_CP0_BADVADDR] = regs->cp0_badvaddr;
+	uregs[MIPS32_EF_CP0_STATUS] = regs->cp0_status;
+	uregs[MIPS32_EF_CP0_CAUSE] = regs->cp0_cause;
+
+	return user_regset_copyout(&pos, &count, &kbuf, &ubuf, uregs, 0,
+				   sizeof(uregs));
 }
 
-static int gpr_set(struct task_struct *target,
-		   const struct user_regset *regset,
-		   unsigned int pos, unsigned int count,
-		   const void *kbuf, const void __user *ubuf)
+static int gpr32_set(struct task_struct *target,
+		     const struct user_regset *regset,
+		     unsigned int pos, unsigned int count,
+		     const void *kbuf, const void __user *ubuf)
 {
-	struct pt_regs newregs;
-	int ret;
+	struct pt_regs *regs = task_pt_regs(target);
+	u32 uregs[ELF_NGREG];
+	unsigned start, num_regs, i;
+	int err;
 
-	ret = user_regset_copyin(&pos, &count, &kbuf, &ubuf,
-				 &newregs,
-				 0, sizeof(newregs));
-	if (ret)
-		return ret;
+	start = pos / sizeof(u32);
+	num_regs = count / sizeof(u32);
 
-	*task_pt_regs(target) = newregs;
+	if (start + num_regs > ELF_NGREG)
+		return -EIO;
+
+	err = user_regset_copyin(&pos, &count, &kbuf, &ubuf, uregs, 0,
+				 sizeof(uregs));
+	if (err)
+		return err;
+
+	for (i = start; i < num_regs; i++) {
+		/*
+		 * Cast all values to signed here so that if this is a 64-bit
+		 * kernel, the supplied 32-bit values will be sign extended.
+		 */
+		switch (i) {
+		case MIPS32_EF_R1 ... MIPS32_EF_R25:
+			/* k0/k1 are ignored. */
+		case MIPS32_EF_R28 ... MIPS32_EF_R31:
+			regs->regs[i - MIPS32_EF_R0] = (s32)uregs[i];
+			break;
+		case MIPS32_EF_LO:
+			regs->lo = (s32)uregs[i];
+			break;
+		case MIPS32_EF_HI:
+			regs->hi = (s32)uregs[i];
+			break;
+		case MIPS32_EF_CP0_EPC:
+			regs->cp0_epc = (s32)uregs[i];
+			break;
+		}
+	}
 
 	return 0;
 }
 
+#endif /* CONFIG_32BIT || CONFIG_MIPS32_O32 */
+
+#ifdef CONFIG_64BIT
+
+static int gpr64_get(struct task_struct *target,
+		     const struct user_regset *regset,
+		     unsigned int pos, unsigned int count,
+		     void *kbuf, void __user *ubuf)
+{
+	struct pt_regs *regs = task_pt_regs(target);
+	u64 uregs[ELF_NGREG] = {};
+	unsigned i;
+
+	for (i = MIPS64_EF_R1; i <= MIPS64_EF_R31; i++) {
+		/* k0/k1 are copied as zero. */
+		if (i == MIPS64_EF_R26 || i == MIPS64_EF_R27)
+			continue;
+
+		uregs[i] = regs->regs[i - MIPS64_EF_R0];
+	}
+
+	uregs[MIPS64_EF_LO] = regs->lo;
+	uregs[MIPS64_EF_HI] = regs->hi;
+	uregs[MIPS64_EF_CP0_EPC] = regs->cp0_epc;
+	uregs[MIPS64_EF_CP0_BADVADDR] = regs->cp0_badvaddr;
+	uregs[MIPS64_EF_CP0_STATUS] = regs->cp0_status;
+	uregs[MIPS64_EF_CP0_CAUSE] = regs->cp0_cause;
+
+	return user_regset_copyout(&pos, &count, &kbuf, &ubuf, uregs, 0,
+				   sizeof(uregs));
+}
+
+static int gpr64_set(struct task_struct *target,
+		     const struct user_regset *regset,
+		     unsigned int pos, unsigned int count,
+		     const void *kbuf, const void __user *ubuf)
+{
+	struct pt_regs *regs = task_pt_regs(target);
+	u64 uregs[ELF_NGREG];
+	unsigned start, num_regs, i;
+	int err;
+
+	start = pos / sizeof(u64);
+	num_regs = count / sizeof(u64);
+
+	if (start + num_regs > ELF_NGREG)
+		return -EIO;
+
+	err = user_regset_copyin(&pos, &count, &kbuf, &ubuf, uregs, 0,
+				 sizeof(uregs));
+	if (err)
+		return err;
+
+	for (i = start; i < num_regs; i++) {
+		switch (i) {
+		case MIPS64_EF_R1 ... MIPS64_EF_R25:
+			/* k0/k1 are ignored. */
+		case MIPS64_EF_R28 ... MIPS64_EF_R31:
+			regs->regs[i - MIPS64_EF_R0] = uregs[i];
+			break;
+		case MIPS64_EF_LO:
+			regs->lo = uregs[i];
+			break;
+		case MIPS64_EF_HI:
+			regs->hi = uregs[i];
+			break;
+		case MIPS64_EF_CP0_EPC:
+			regs->cp0_epc = uregs[i];
+			break;
+		}
+	}
+
+	return 0;
+}
+
+#endif /* CONFIG_64BIT */
+
 static int fpr_get(struct task_struct *target,
 		   const struct user_regset *regset,
 		   unsigned int pos, unsigned int count,
@@ -322,14 +447,16 @@ enum mips_regset {
 	REGSET_FPR,
 };
 
+#if defined(CONFIG_32BIT) || defined(CONFIG_MIPS32_O32)
+
 static const struct user_regset mips_regsets[] = {
 	[REGSET_GPR] = {
 		.core_note_type	= NT_PRSTATUS,
 		.n		= ELF_NGREG,
 		.size		= sizeof(unsigned int),
 		.align		= sizeof(unsigned int),
-		.get		= gpr_get,
-		.set		= gpr_set,
+		.get		= gpr32_get,
+		.set		= gpr32_set,
 	},
 	[REGSET_FPR] = {
 		.core_note_type	= NT_PRFPREG,
@@ -349,14 +476,18 @@ static const struct user_regset_view user_mips_view = {
 	.n		= ARRAY_SIZE(mips_regsets),
 };
 
+#endif /* CONFIG_32BIT || CONFIG_MIPS32_O32 */
+
+#ifdef CONFIG_64BIT
+
 static const struct user_regset mips64_regsets[] = {
 	[REGSET_GPR] = {
 		.core_note_type	= NT_PRSTATUS,
 		.n		= ELF_NGREG,
 		.size		= sizeof(unsigned long),
 		.align		= sizeof(unsigned long),
-		.get		= gpr_get,
-		.set		= gpr_set,
+		.get		= gpr64_get,
+		.set		= gpr64_set,
 	},
 	[REGSET_FPR] = {
 		.core_note_type	= NT_PRFPREG,
@@ -369,25 +500,26 @@ static const struct user_regset mips64_regsets[] = {
 };
 
 static const struct user_regset_view user_mips64_view = {
-	.name		= "mips",
+	.name		= "mips64",
 	.e_machine	= ELF_ARCH,
 	.ei_osabi	= ELF_OSABI,
 	.regsets	= mips64_regsets,
-	.n		= ARRAY_SIZE(mips_regsets),
+	.n		= ARRAY_SIZE(mips64_regsets),
 };
 
+#endif /* CONFIG_64BIT */
+
 const struct user_regset_view *task_user_regset_view(struct task_struct *task)
 {
 #ifdef CONFIG_32BIT
 	return &user_mips_view;
-#endif
-
+#else
 #ifdef CONFIG_MIPS32_O32
-		if (test_thread_flag(TIF_32BIT_REGS))
-			return &user_mips_view;
+	if (test_tsk_thread_flag(task, TIF_32BIT_REGS))
+		return &user_mips_view;
 #endif
-
 	return &user_mips64_view;
+#endif
 }
 
 long arch_ptrace(struct task_struct *child, long request,
@@ -593,7 +725,7 @@ long arch_ptrace(struct task_struct *child, long request,
 			break;
 #endif
 		case FPC_CSR:
-			child->thread.fpu.fcr31 = data;
+			child->thread.fpu.fcr31 = data & ~FPU_CSR_ALL_X;
 			break;
 		case DSP_BASE ... DSP_BASE + 5: {
 			dspreg_t *dregs;
diff --git a/arch/mips/kernel/unaligned.c b/arch/mips/kernel/unaligned.c
index c369a5d35527..b897dde93e7a 100644
--- a/arch/mips/kernel/unaligned.c
+++ b/arch/mips/kernel/unaligned.c
@@ -605,7 +605,6 @@ static void emulate_load_store_insn(struct pt_regs *regs,
 	case sdc1_op:
 		die_if_kernel("Unaligned FP access in kernel code", regs);
 		BUG_ON(!used_math());
-		BUG_ON(!is_fpu_owner());
 
 		lose_fpu(1);	/* Save FPU state for the emulator. */
 		res = fpu_emulator_cop1Handler(regs, &current->thread.fpu, 1,
diff --git a/arch/mips/mm/tlbex.c b/arch/mips/mm/tlbex.c
index b234b1b5ccad..65d452aa1fda 100644
--- a/arch/mips/mm/tlbex.c
+++ b/arch/mips/mm/tlbex.c
@@ -1295,6 +1295,7 @@ static void build_r4000_tlb_refill_handler(void)
 	}
 #ifdef CONFIG_MIPS_HUGE_TLB_SUPPORT
 	uasm_l_tlb_huge_update(&l, p);
+	UASM_i_LW(&p, K0, 0, K1);
 	build_huge_update_entries(&p, htlb_info.huge_pte, K1);
 	build_huge_tlb_write_entry(&p, &l, &r, K0, tlb_random,
 				   htlb_info.restore_scratch);
diff --git a/arch/powerpc/include/asm/machdep.h b/arch/powerpc/include/asm/machdep.h
index ad3025d0880b..f20786825b8f 100644
--- a/arch/powerpc/include/asm/machdep.h
+++ b/arch/powerpc/include/asm/machdep.h
@@ -57,10 +57,10 @@ struct machdep_calls {
 	void            (*hpte_removebolted)(unsigned long ea,
 					     int psize, int ssize);
 	void		(*flush_hash_range)(unsigned long number, int local);
-	void		(*hugepage_invalidate)(struct mm_struct *mm,
+	void		(*hugepage_invalidate)(unsigned long vsid,
+					       unsigned long addr,
 					       unsigned char *hpte_slot_array,
-					       unsigned long addr, int psize);
-
+					       int psize, int ssize);
 	/* special for kexec, to be called in real mode, linear mapping is
 	 * destroyed as well */
 	void		(*hpte_clear_all)(void);
diff --git a/arch/powerpc/include/asm/pgtable-ppc64.h b/arch/powerpc/include/asm/pgtable-ppc64.h
index eb9261024f51..7b3d54fae46f 100644
--- a/arch/powerpc/include/asm/pgtable-ppc64.h
+++ b/arch/powerpc/include/asm/pgtable-ppc64.h
@@ -413,7 +413,7 @@ static inline char *get_hpte_slot_array(pmd_t *pmdp)
 }
 
 extern void hpte_do_hugepage_flush(struct mm_struct *mm, unsigned long addr,
-				   pmd_t *pmdp);
+				   pmd_t *pmdp, unsigned long old_pmd);
 #ifdef CONFIG_TRANSPARENT_HUGEPAGE
 extern pmd_t pfn_pmd(unsigned long pfn, pgprot_t pgprot);
 extern pmd_t mk_pmd(struct page *page, pgprot_t pgprot);
diff --git a/arch/powerpc/include/asm/pte-hash64-64k.h b/arch/powerpc/include/asm/pte-hash64-64k.h
index d836d945068d..9ecede1e124c 100644
--- a/arch/powerpc/include/asm/pte-hash64-64k.h
+++ b/arch/powerpc/include/asm/pte-hash64-64k.h
@@ -46,11 +46,31 @@
  * in order to deal with 64K made of 4K HW pages. Thus we override the
  * generic accessors and iterators here
  */
-#define __real_pte(e,p) 	((real_pte_t) { \
-			(e), (pte_val(e) & _PAGE_COMBO) ? \
-				(pte_val(*((p) + PTRS_PER_PTE))) : 0 })
-#define __rpte_to_hidx(r,index)	((pte_val((r).pte) & _PAGE_COMBO) ? \
-        (((r).hidx >> ((index)<<2)) & 0xf) : ((pte_val((r).pte) >> 12) & 0xf))
+#define __real_pte __real_pte
+static inline real_pte_t __real_pte(pte_t pte, pte_t *ptep)
+{
+	real_pte_t rpte;
+
+	rpte.pte = pte;
+	rpte.hidx = 0;
+	if (pte_val(pte) & _PAGE_COMBO) {
+		/*
+		 * Make sure we order the hidx load against the _PAGE_COMBO
+		 * check. The store side ordering is done in __hash_page_4K
+		 */
+		smp_rmb();
+		rpte.hidx = pte_val(*((ptep) + PTRS_PER_PTE));
+	}
+	return rpte;
+}
+
+static inline unsigned long __rpte_to_hidx(real_pte_t rpte, unsigned long index)
+{
+	if ((pte_val(rpte.pte) & _PAGE_COMBO))
+		return (rpte.hidx >> (index<<2)) & 0xf;
+	return (pte_val(rpte.pte) >> 12) & 0xf;
+}
+
 #define __rpte_to_pte(r)	((r).pte)
 #define __rpte_sub_valid(rpte, index) \
 	(pte_val(rpte.pte) & (_PAGE_HPTE_SUB0 >> (index)))
diff --git a/arch/powerpc/mm/hash_native_64.c b/arch/powerpc/mm/hash_native_64.c
index 3ea26c25590b..838de8e17dc5 100644
--- a/arch/powerpc/mm/hash_native_64.c
+++ b/arch/powerpc/mm/hash_native_64.c
@@ -418,18 +418,18 @@ static void native_hpte_invalidate(unsigned long slot, unsigned long vpn,
 	local_irq_restore(flags);
 }
 
-static void native_hugepage_invalidate(struct mm_struct *mm,
+static void native_hugepage_invalidate(unsigned long vsid,
+				       unsigned long addr,
 				       unsigned char *hpte_slot_array,
-				       unsigned long addr, int psize)
+				       int psize, int ssize)
 {
-	int ssize = 0, i;
-	int lock_tlbie;
+	int i;
 	struct hash_pte *hptep;
 	int actual_psize = MMU_PAGE_16M;
 	unsigned int max_hpte_count, valid;
 	unsigned long flags, s_addr = addr;
 	unsigned long hpte_v, want_v, shift;
-	unsigned long hidx, vpn = 0, vsid, hash, slot;
+	unsigned long hidx, vpn = 0, hash, slot;
 
 	shift = mmu_psize_defs[psize].shift;
 	max_hpte_count = 1U << (PMD_SHIFT - shift);
@@ -443,15 +443,6 @@ static void native_hugepage_invalidate(struct mm_struct *mm,
 
 		/* get the vpn */
 		addr = s_addr + (i * (1ul << shift));
-		if (!is_kernel_addr(addr)) {
-			ssize = user_segment_size(addr);
-			vsid = get_vsid(mm->context.id, addr, ssize);
-			WARN_ON(vsid == 0);
-		} else {
-			vsid = get_kernel_vsid(addr, mmu_kernel_ssize);
-			ssize = mmu_kernel_ssize;
-		}
-
 		vpn = hpt_vpn(addr, vsid, ssize);
 		hash = hpt_hash(vpn, shift, ssize);
 		if (hidx & _PTEIDX_SECONDARY)
@@ -471,22 +462,13 @@ static void native_hugepage_invalidate(struct mm_struct *mm,
 		else
 			/* Invalidate the hpte. NOTE: this also unlocks it */
 			hptep->v = 0;
+		/*
+		 * We need to do tlb invalidate for all the address, tlbie
+		 * instruction compares entry_VA in tlb with the VA specified
+		 * here
+		 */
+		tlbie(vpn, psize, actual_psize, ssize, 0);
 	}
-	/*
-	 * Since this is a hugepage, we just need a single tlbie.
-	 * use the last vpn.
-	 */
-	lock_tlbie = !mmu_has_feature(MMU_FTR_LOCKLESS_TLBIE);
-	if (lock_tlbie)
-		raw_spin_lock(&native_tlbie_lock);
-
-	asm volatile("ptesync":::"memory");
-	__tlbie(vpn, psize, actual_psize, ssize);
-	asm volatile("eieio; tlbsync; ptesync":::"memory");
-
-	if (lock_tlbie)
-		raw_spin_unlock(&native_tlbie_lock);
-
 	local_irq_restore(flags);
 }
 
diff --git a/arch/powerpc/mm/hugepage-hash64.c b/arch/powerpc/mm/hugepage-hash64.c
index 826893fcb3a7..5f5e6328c21c 100644
--- a/arch/powerpc/mm/hugepage-hash64.c
+++ b/arch/powerpc/mm/hugepage-hash64.c
@@ -18,6 +18,57 @@
 #include <linux/mm.h>
 #include <asm/machdep.h>
 
+static void invalidate_old_hpte(unsigned long vsid, unsigned long addr,
+				pmd_t *pmdp, unsigned int psize, int ssize)
+{
+	int i, max_hpte_count, valid;
+	unsigned long s_addr;
+	unsigned char *hpte_slot_array;
+	unsigned long hidx, shift, vpn, hash, slot;
+
+	s_addr = addr & HPAGE_PMD_MASK;
+	hpte_slot_array = get_hpte_slot_array(pmdp);
+	/*
+	 * IF we try to do a HUGE PTE update after a withdraw is done.
+	 * we will find the below NULL. This happens when we do
+	 * split_huge_page_pmd
+	 */
+	if (!hpte_slot_array)
+		return;
+
+	if (ppc_md.hugepage_invalidate)
+		return ppc_md.hugepage_invalidate(vsid, s_addr, hpte_slot_array,
+						  psize, ssize);
+	/*
+	 * No bluk hpte removal support, invalidate each entry
+	 */
+	shift = mmu_psize_defs[psize].shift;
+	max_hpte_count = HPAGE_PMD_SIZE >> shift;
+	for (i = 0; i < max_hpte_count; i++) {
+		/*
+		 * 8 bits per each hpte entries
+		 * 000| [ secondary group (one bit) | hidx (3 bits) | valid bit]
+		 */
+		valid = hpte_valid(hpte_slot_array, i);
+		if (!valid)
+			continue;
+		hidx =  hpte_hash_index(hpte_slot_array, i);
+
+		/* get the vpn */
+		addr = s_addr + (i * (1ul << shift));
+		vpn = hpt_vpn(addr, vsid, ssize);
+		hash = hpt_hash(vpn, shift, ssize);
+		if (hidx & _PTEIDX_SECONDARY)
+			hash = ~hash;
+
+		slot = (hash & htab_hash_mask) * HPTES_PER_GROUP;
+		slot += hidx & _PTEIDX_GROUP_IX;
+		ppc_md.hpte_invalidate(slot, vpn, psize,
+				       MMU_PAGE_16M, ssize, 0);
+	}
+}
+
+
 int __hash_page_thp(unsigned long ea, unsigned long access, unsigned long vsid,
 		    pmd_t *pmdp, unsigned long trap, int local, int ssize,
 		    unsigned int psize)
@@ -33,7 +84,9 @@ int __hash_page_thp(unsigned long ea, unsigned long access, unsigned long vsid,
 	 * atomically mark the linux large page PMD busy and dirty
 	 */
 	do {
-		old_pmd = pmd_val(*pmdp);
+		pmd_t pmd = ACCESS_ONCE(*pmdp);
+
+		old_pmd = pmd_val(pmd);
 		/* If PMD busy, retry the access */
 		if (unlikely(old_pmd & _PAGE_BUSY))
 			return 0;
@@ -85,6 +138,15 @@ int __hash_page_thp(unsigned long ea, unsigned long access, unsigned long vsid,
 	vpn = hpt_vpn(ea, vsid, ssize);
 	hash = hpt_hash(vpn, shift, ssize);
 	hpte_slot_array = get_hpte_slot_array(pmdp);
+	if (psize == MMU_PAGE_4K) {
+		/*
+		 * invalidate the old hpte entry if we have that mapped via 64K
+		 * base page size. This is because demote_segment won't flush
+		 * hash page table entries.
+		 */
+		if ((old_pmd & _PAGE_HASHPTE) && !(old_pmd & _PAGE_COMBO))
+			invalidate_old_hpte(vsid, ea, pmdp, MMU_PAGE_64K, ssize);
+	}
 
 	valid = hpte_valid(hpte_slot_array, index);
 	if (valid) {
@@ -107,11 +169,8 @@ int __hash_page_thp(unsigned long ea, unsigned long access, unsigned long vsid,
 			 * safely update this here.
 			 */
 			valid = 0;
-			new_pmd &= ~_PAGE_HPTEFLAGS;
 			hpte_slot_array[index] = 0;
-		} else
-			/* clear the busy bits and set the hash pte bits */
-			new_pmd = (new_pmd & ~_PAGE_HPTEFLAGS) | _PAGE_HASHPTE;
+		}
 	}
 
 	if (!valid) {
@@ -119,11 +178,7 @@ int __hash_page_thp(unsigned long ea, unsigned long access, unsigned long vsid,
 
 		/* insert new entry */
 		pa = pmd_pfn(__pmd(old_pmd)) << PAGE_SHIFT;
-repeat:
-		hpte_group = ((hash & htab_hash_mask) * HPTES_PER_GROUP) & ~0x7UL;
-
-		/* clear the busy bits and set the hash pte bits */
-		new_pmd = (new_pmd & ~_PAGE_HPTEFLAGS) | _PAGE_HASHPTE;
+		new_pmd |= _PAGE_HASHPTE;
 
 		/* Add in WIMG bits */
 		rflags |= (new_pmd & (_PAGE_WRITETHRU | _PAGE_NO_CACHE |
@@ -132,6 +187,8 @@ repeat:
 		 * enable the memory coherence always
 		 */
 		rflags |= HPTE_R_M;
+repeat:
+		hpte_group = ((hash & htab_hash_mask) * HPTES_PER_GROUP) & ~0x7UL;
 
 		/* Insert into the hash table, primary slot */
 		slot = ppc_md.hpte_insert(hpte_group, vpn, pa, rflags, 0,
@@ -172,8 +229,17 @@ repeat:
 		mark_hpte_slot_valid(hpte_slot_array, index, slot);
 	}
 	/*
-	 * No need to use ldarx/stdcx here
+	 * Mark the pte with _PAGE_COMBO, if we are trying to hash it with
+	 * base page size 4k.
+	 */
+	if (psize == MMU_PAGE_4K)
+		new_pmd |= _PAGE_COMBO;
+	/*
+	 * The hpte valid is stored in the pgtable whose address is in the
+	 * second half of the PMD. Order this against clearing of the busy bit in
+	 * huge pmd.
 	 */
+	smp_wmb();
 	*pmdp = __pmd(new_pmd & ~_PAGE_BUSY);
 	return 0;
 }
diff --git a/arch/powerpc/mm/numa.c b/arch/powerpc/mm/numa.c
index 30a42e24bf14..a5fff173be4f 100644
--- a/arch/powerpc/mm/numa.c
+++ b/arch/powerpc/mm/numa.c
@@ -610,8 +610,8 @@ static int cpu_numa_callback(struct notifier_block *nfb, unsigned long action,
 	case CPU_UP_CANCELED:
 	case CPU_UP_CANCELED_FROZEN:
 		unmap_cpu_from_node(lcpu);
-		break;
 		ret = NOTIFY_OK;
+		break;
 #endif
 	}
 	return ret;
diff --git a/arch/powerpc/mm/pgtable_64.c b/arch/powerpc/mm/pgtable_64.c
index 62bf5e8e78da..c64da56d7582 100644
--- a/arch/powerpc/mm/pgtable_64.c
+++ b/arch/powerpc/mm/pgtable_64.c
@@ -538,7 +538,7 @@ unsigned long pmd_hugepage_update(struct mm_struct *mm, unsigned long addr,
 	*pmdp = __pmd((old & ~clr) | set);
 #endif
 	if (old & _PAGE_HASHPTE)
-		hpte_do_hugepage_flush(mm, addr, pmdp);
+		hpte_do_hugepage_flush(mm, addr, pmdp, old);
 	return old;
 }
 
@@ -645,7 +645,7 @@ void pmdp_splitting_flush(struct vm_area_struct *vma,
 	if (!(old & _PAGE_SPLITTING)) {
 		/* We need to flush the hpte */
 		if (old & _PAGE_HASHPTE)
-			hpte_do_hugepage_flush(vma->vm_mm, address, pmdp);
+			hpte_do_hugepage_flush(vma->vm_mm, address, pmdp, old);
 	}
 }
 
@@ -718,7 +718,7 @@ void pmdp_invalidate(struct vm_area_struct *vma, unsigned long address,
  * neesd to be flushed.
  */
 void hpte_do_hugepage_flush(struct mm_struct *mm, unsigned long addr,
-			    pmd_t *pmdp)
+			    pmd_t *pmdp, unsigned long old_pmd)
 {
 	int ssize, i;
 	unsigned long s_addr;
@@ -740,12 +740,29 @@ void hpte_do_hugepage_flush(struct mm_struct *mm, unsigned long addr,
 	if (!hpte_slot_array)
 		return;
 
-	/* get the base page size */
+	/* get the base page size,vsid and segment size */
+#ifdef CONFIG_DEBUG_VM
 	psize = get_slice_psize(mm, s_addr);
+	BUG_ON(psize == MMU_PAGE_16M);
+#endif
+	if (old_pmd & _PAGE_COMBO)
+		psize = MMU_PAGE_4K;
+	else
+		psize = MMU_PAGE_64K;
+
+	if (!is_kernel_addr(s_addr)) {
+		ssize = user_segment_size(s_addr);
+		vsid = get_vsid(mm->context.id, s_addr, ssize);
+		WARN_ON(vsid == 0);
+	} else {
+		vsid = get_kernel_vsid(s_addr, mmu_kernel_ssize);
+		ssize = mmu_kernel_ssize;
+	}
 
 	if (ppc_md.hugepage_invalidate)
-		return ppc_md.hugepage_invalidate(mm, hpte_slot_array,
-						  s_addr, psize);
+		return ppc_md.hugepage_invalidate(vsid, s_addr,
+						  hpte_slot_array,
+						  psize, ssize);
 	/*
 	 * No bluk hpte removal support, invalidate each entry
 	 */
@@ -763,15 +780,6 @@ void hpte_do_hugepage_flush(struct mm_struct *mm, unsigned long addr,
 
 		/* get the vpn */
 		addr = s_addr + (i * (1ul << shift));
-		if (!is_kernel_addr(addr)) {
-			ssize = user_segment_size(addr);
-			vsid = get_vsid(mm->context.id, addr, ssize);
-			WARN_ON(vsid == 0);
-		} else {
-			vsid = get_kernel_vsid(addr, mmu_kernel_ssize);
-			ssize = mmu_kernel_ssize;
-		}
-
 		vpn = hpt_vpn(addr, vsid, ssize);
 		hash = hpt_hash(vpn, shift, ssize);
 		if (hidx & _PTEIDX_SECONDARY)
diff --git a/arch/powerpc/mm/tlb_hash64.c b/arch/powerpc/mm/tlb_hash64.c
index c99f6510a0b2..9adda5790463 100644
--- a/arch/powerpc/mm/tlb_hash64.c
+++ b/arch/powerpc/mm/tlb_hash64.c
@@ -216,7 +216,7 @@ void __flush_hash_table_range(struct mm_struct *mm, unsigned long start,
 		if (!(pte & _PAGE_HASHPTE))
 			continue;
 		if (unlikely(hugepage_shift && pmd_trans_huge(*(pmd_t *)pte)))
-			hpte_do_hugepage_flush(mm, start, (pmd_t *)pte);
+			hpte_do_hugepage_flush(mm, start, (pmd_t *)ptep, pte);
 		else
 			hpte_need_flush(mm, start, ptep, pte, 0);
 	}
diff --git a/arch/powerpc/platforms/pseries/hotplug-memory.c b/arch/powerpc/platforms/pseries/hotplug-memory.c
index 9590dbb756f2..b9a82042760f 100644
--- a/arch/powerpc/platforms/pseries/hotplug-memory.c
+++ b/arch/powerpc/platforms/pseries/hotplug-memory.c
@@ -160,7 +160,7 @@ static int pseries_remove_memory(struct device_node *np)
 static inline int pseries_remove_memblock(unsigned long base,
 					  unsigned int memblock_size)
 {
-	return -EOPNOTSUPP;
+	return 0;
 }
 static inline int pseries_remove_memory(struct device_node *np)
 {
diff --git a/arch/powerpc/platforms/pseries/iommu.c b/arch/powerpc/platforms/pseries/iommu.c
index 33b552ffbe57..4642d6a4d356 100644
--- a/arch/powerpc/platforms/pseries/iommu.c
+++ b/arch/powerpc/platforms/pseries/iommu.c
@@ -721,13 +721,13 @@ static int __init disable_ddw_setup(char *str)
 
 early_param("disable_ddw", disable_ddw_setup);
 
-static void remove_ddw(struct device_node *np)
+static void remove_ddw(struct device_node *np, bool remove_prop)
 {
 	struct dynamic_dma_window_prop *dwp;
 	struct property *win64;
 	const u32 *ddw_avail;
 	u64 liobn;
-	int len, ret;
+	int len, ret = 0;
 
 	ddw_avail = of_get_property(np, "ibm,ddw-applicable", &len);
 	win64 = of_find_property(np, DIRECT64_PROPNAME, NULL);
@@ -761,7 +761,8 @@ static void remove_ddw(struct device_node *np)
 			np->full_name, ret, ddw_avail[2], liobn);
 
 delprop:
-	ret = of_remove_property(np, win64);
+	if (remove_prop)
+		ret = of_remove_property(np, win64);
 	if (ret)
 		pr_warning("%s: failed to remove direct window property: %d\n",
 			np->full_name, ret);
@@ -805,7 +806,7 @@ static int find_existing_ddw_windows(void)
 		window = kzalloc(sizeof(*window), GFP_KERNEL);
 		if (!window || len < sizeof(struct dynamic_dma_window_prop)) {
 			kfree(window);
-			remove_ddw(pdn);
+			remove_ddw(pdn, true);
 			continue;
 		}
 
@@ -1045,7 +1046,7 @@ out_free_window:
 	kfree(window);
 
 out_clear_window:
-	remove_ddw(pdn);
+	remove_ddw(pdn, true);
 
 out_free_prop:
 	kfree(win64->name);
@@ -1255,7 +1256,14 @@ static int iommu_reconfig_notifier(struct notifier_block *nb, unsigned long acti
 
 	switch (action) {
 	case OF_RECONFIG_DETACH_NODE:
-		remove_ddw(np);
+		/*
+		 * Removing the property will invoke the reconfig
+		 * notifier again, which causes dead-lock on the
+		 * read-write semaphore of the notifier chain. So
+		 * we have to remove the property when releasing
+		 * the device node.
+		 */
+		remove_ddw(np, false);
 		if (pci && pci->iommu_table)
 			iommu_free_table(pci->iommu_table, np->full_name);
 
diff --git a/arch/powerpc/platforms/pseries/lpar.c b/arch/powerpc/platforms/pseries/lpar.c
index b02af9ef3ff6..ccf6f162f69c 100644
--- a/arch/powerpc/platforms/pseries/lpar.c
+++ b/arch/powerpc/platforms/pseries/lpar.c
@@ -430,16 +430,17 @@ static void __pSeries_lpar_hugepage_invalidate(unsigned long *slot,
 		spin_unlock_irqrestore(&pSeries_lpar_tlbie_lock, flags);
 }
 
-static void pSeries_lpar_hugepage_invalidate(struct mm_struct *mm,
-				       unsigned char *hpte_slot_array,
-				       unsigned long addr, int psize)
+static void pSeries_lpar_hugepage_invalidate(unsigned long vsid,
+					     unsigned long addr,
+					     unsigned char *hpte_slot_array,
+					     int psize, int ssize)
 {
-	int ssize = 0, i, index = 0;
+	int i, index = 0;
 	unsigned long s_addr = addr;
 	unsigned int max_hpte_count, valid;
 	unsigned long vpn_array[PPC64_HUGE_HPTE_BATCH];
 	unsigned long slot_array[PPC64_HUGE_HPTE_BATCH];
-	unsigned long shift, hidx, vpn = 0, vsid, hash, slot;
+	unsigned long shift, hidx, vpn = 0, hash, slot;
 
 	shift = mmu_psize_defs[psize].shift;
 	max_hpte_count = 1U << (PMD_SHIFT - shift);
@@ -452,15 +453,6 @@ static void pSeries_lpar_hugepage_invalidate(struct mm_struct *mm,
 
 		/* get the vpn */
 		addr = s_addr + (i * (1ul << shift));
-		if (!is_kernel_addr(addr)) {
-			ssize = user_segment_size(addr);
-			vsid = get_vsid(mm->context.id, addr, ssize);
-			WARN_ON(vsid == 0);
-		} else {
-			vsid = get_kernel_vsid(addr, mmu_kernel_ssize);
-			ssize = mmu_kernel_ssize;
-		}
-
 		vpn = hpt_vpn(addr, vsid, ssize);
 		hash = hpt_hash(vpn, shift, ssize);
 		if (hidx & _PTEIDX_SECONDARY)
diff --git a/arch/s390/Kconfig b/arch/s390/Kconfig
index bb74b21f007a..a0a3bed6e4dc 100644
--- a/arch/s390/Kconfig
+++ b/arch/s390/Kconfig
@@ -93,6 +93,7 @@ config S390
 	select ARCH_INLINE_WRITE_UNLOCK_IRQ
 	select ARCH_INLINE_WRITE_UNLOCK_IRQRESTORE
 	select ARCH_SAVE_PAGE_KEYS if HIBERNATION
+	select ARCH_SUPPORTS_ATOMIC_RMW
 	select ARCH_USE_CMPXCHG_LOCKREF
 	select ARCH_WANT_IPC_PARSE_VERSION
 	select BUILDTIME_EXTABLE_SORT
diff --git a/drivers/acpi/acpica/utcopy.c b/drivers/acpi/acpica/utcopy.c
index edff4e653d9a..c66bca17e736 100644
--- a/drivers/acpi/acpica/utcopy.c
+++ b/drivers/acpi/acpica/utcopy.c
@@ -1001,5 +1001,11 @@ acpi_ut_copy_iobject_to_iobject(union acpi_operand_object *source_desc,
 		status = acpi_ut_copy_simple_object(source_desc, *dest_desc);
 	}
 
+	/* Delete the allocated object if copy failed */
+
+	if (ACPI_FAILURE(status)) {
+		acpi_ut_remove_reference(*dest_desc);
+	}
+
 	return_ACPI_STATUS(status);
 }
diff --git a/drivers/acpi/processor_idle.c b/drivers/acpi/processor_idle.c
index 3dca36d4ad26..17f9ec501972 100644
--- a/drivers/acpi/processor_idle.c
+++ b/drivers/acpi/processor_idle.c
@@ -1071,9 +1071,9 @@ int acpi_processor_cst_has_changed(struct acpi_processor *pr)
 
 	if (pr->id == 0 && cpuidle_get_driver() == &acpi_idle_driver) {
 
-		cpuidle_pause_and_lock();
 		/* Protect against cpu-hotplug */
 		get_online_cpus();
+		cpuidle_pause_and_lock();
 
 		/* Disable all cpuidle devices */
 		for_each_online_cpu(cpu) {
@@ -1100,8 +1100,8 @@ int acpi_processor_cst_has_changed(struct acpi_processor *pr)
 				cpuidle_enable_device(dev);
 			}
 		}
-		put_online_cpus();
 		cpuidle_resume_and_unlock();
+		put_online_cpus();
 	}
 
 	return 0;
diff --git a/drivers/acpi/scan.c b/drivers/acpi/scan.c
index 57b053f424d1..92d5184e3654 100644
--- a/drivers/acpi/scan.c
+++ b/drivers/acpi/scan.c
@@ -329,7 +329,8 @@ static int acpi_scan_hot_remove(struct acpi_device *device)
 	unsigned long long sta;
 	acpi_status status;
 
-	if (device->handler->hotplug.demand_offline && !acpi_force_hot_remove) {
+	if (device->handler && device->handler->hotplug.demand_offline
+	    && !acpi_force_hot_remove) {
 		if (!acpi_scan_is_offline(device, true))
 			return -EBUSY;
 	} else {
@@ -660,8 +661,14 @@ static ssize_t
 acpi_device_sun_show(struct device *dev, struct device_attribute *attr,
 		     char *buf) {
 	struct acpi_device *acpi_dev = to_acpi_device(dev);
+	acpi_status status;
+	unsigned long long sun;
+
+	status = acpi_evaluate_integer(acpi_dev->handle, "_SUN", NULL, &sun);
+	if (ACPI_FAILURE(status))
+		return -ENODEV;
 
-	return sprintf(buf, "%lu\n", acpi_dev->pnp.sun);
+	return sprintf(buf, "%llu\n", sun);
 }
 static DEVICE_ATTR(sun, 0444, acpi_device_sun_show, NULL);
 
@@ -683,7 +690,6 @@ static int acpi_device_setup_files(struct acpi_device *dev)
 {
 	struct acpi_buffer buffer = {ACPI_ALLOCATE_BUFFER, NULL};
 	acpi_status status;
-	unsigned long long sun;
 	int result = 0;
 
 	/*
@@ -724,14 +730,10 @@ static int acpi_device_setup_files(struct acpi_device *dev)
 	if (dev->pnp.unique_id)
 		result = device_create_file(&dev->dev, &dev_attr_uid);
 
-	status = acpi_evaluate_integer(dev->handle, "_SUN", NULL, &sun);
-	if (ACPI_SUCCESS(status)) {
-		dev->pnp.sun = (unsigned long)sun;
+	if (acpi_has_method(dev->handle, "_SUN")) {
 		result = device_create_file(&dev->dev, &dev_attr_sun);
 		if (result)
 			goto end;
-	} else {
-		dev->pnp.sun = (unsigned long)-1;
 	}
 
 	if (acpi_has_method(dev->handle, "_STA")) {
@@ -915,12 +917,17 @@ static void acpi_device_notify(acpi_handle handle, u32 event, void *data)
 	device->driver->ops.notify(device, event);
 }
 
-static acpi_status acpi_device_notify_fixed(void *data)
+static void acpi_device_notify_fixed(void *data)
 {
 	struct acpi_device *device = data;
 
 	/* Fixed hardware devices have no handles */
 	acpi_device_notify(NULL, ACPI_FIXED_HARDWARE_EVENT, device);
+}
+
+static acpi_status acpi_device_fixed_event(void *data)
+{
+	acpi_os_execute(OSL_NOTIFY_HANDLER, acpi_device_notify_fixed, data);
 	return AE_OK;
 }
 
@@ -931,12 +938,12 @@ static int acpi_device_install_notify_handler(struct acpi_device *device)
 	if (device->device_type == ACPI_BUS_TYPE_POWER_BUTTON)
 		status =
 		    acpi_install_fixed_event_handler(ACPI_EVENT_POWER_BUTTON,
-						     acpi_device_notify_fixed,
+						     acpi_device_fixed_event,
 						     device);
 	else if (device->device_type == ACPI_BUS_TYPE_SLEEP_BUTTON)
 		status =
 		    acpi_install_fixed_event_handler(ACPI_EVENT_SLEEP_BUTTON,
-						     acpi_device_notify_fixed,
+						     acpi_device_fixed_event,
 						     device);
 	else
 		status = acpi_install_notify_handler(device->handle,
@@ -953,10 +960,10 @@ static void acpi_device_remove_notify_handler(struct acpi_device *device)
 {
 	if (device->device_type == ACPI_BUS_TYPE_POWER_BUTTON)
 		acpi_remove_fixed_event_handler(ACPI_EVENT_POWER_BUTTON,
-						acpi_device_notify_fixed);
+						acpi_device_fixed_event);
 	else if (device->device_type == ACPI_BUS_TYPE_SLEEP_BUTTON)
 		acpi_remove_fixed_event_handler(ACPI_EVENT_SLEEP_BUTTON,
-						acpi_device_notify_fixed);
+						acpi_device_fixed_event);
 	else
 		acpi_remove_notify_handler(device->handle, ACPI_DEVICE_NOTIFY,
 					   acpi_device_notify);
diff --git a/drivers/bluetooth/btmrvl_drv.h b/drivers/bluetooth/btmrvl_drv.h
index 7399303d7d99..9e81a3d01d2b 100644
--- a/drivers/bluetooth/btmrvl_drv.h
+++ b/drivers/bluetooth/btmrvl_drv.h
@@ -66,6 +66,7 @@ struct btmrvl_adapter {
 	u8 hs_state;
 	u8 wakeup_tries;
 	wait_queue_head_t cmd_wait_q;
+	wait_queue_head_t event_hs_wait_q;
 	u8 cmd_complete;
 	bool is_suspended;
 };
diff --git a/drivers/bluetooth/btmrvl_main.c b/drivers/bluetooth/btmrvl_main.c
index 1e0320af00c6..49d20989b45a 100644
--- a/drivers/bluetooth/btmrvl_main.c
+++ b/drivers/bluetooth/btmrvl_main.c
@@ -112,6 +112,7 @@ int btmrvl_process_event(struct btmrvl_private *priv, struct sk_buff *skb)
 			adapter->hs_state = HS_ACTIVATED;
 			if (adapter->psmode)
 				adapter->ps_state = PS_SLEEP;
+			wake_up_interruptible(&adapter->event_hs_wait_q);
 			BT_DBG("HS ACTIVATED!");
 		} else {
 			BT_DBG("HS Enable failed");
@@ -251,11 +252,31 @@ EXPORT_SYMBOL_GPL(btmrvl_enable_ps);
 
 int btmrvl_enable_hs(struct btmrvl_private *priv)
 {
+	struct btmrvl_adapter *adapter = priv->adapter;
 	int ret;
 
 	ret = btmrvl_send_sync_cmd(priv, BT_CMD_HOST_SLEEP_ENABLE, NULL, 0);
-	if (ret)
+	if (ret) {
 		BT_ERR("Host sleep enable command failed\n");
+		return ret;
+	}
+
+	ret = wait_event_interruptible_timeout(adapter->event_hs_wait_q,
+					       adapter->hs_state,
+			msecs_to_jiffies(WAIT_UNTIL_HS_STATE_CHANGED));
+	if (ret < 0) {
+		BT_ERR("event_hs_wait_q terminated (%d): %d,%d,%d",
+		       ret, adapter->hs_state, adapter->ps_state,
+		       adapter->wakeup_tries);
+	} else if (!ret) {
+		BT_ERR("hs_enable timeout: %d,%d,%d", adapter->hs_state,
+		       adapter->ps_state, adapter->wakeup_tries);
+		ret = -ETIMEDOUT;
+	} else {
+		BT_DBG("host sleep enabled: %d,%d,%d", adapter->hs_state,
+		       adapter->ps_state, adapter->wakeup_tries);
+		ret = 0;
+	}
 
 	return ret;
 }
@@ -341,6 +362,7 @@ static void btmrvl_init_adapter(struct btmrvl_private *priv)
 	priv->adapter->ps_state = PS_AWAKE;
 
 	init_waitqueue_head(&priv->adapter->cmd_wait_q);
+	init_waitqueue_head(&priv->adapter->event_hs_wait_q);
 }
 
 static void btmrvl_free_adapter(struct btmrvl_private *priv)
@@ -648,6 +670,7 @@ int btmrvl_remove_card(struct btmrvl_private *priv)
 	hdev = priv->btmrvl_dev.hcidev;
 
 	wake_up_interruptible(&priv->adapter->cmd_wait_q);
+	wake_up_interruptible(&priv->adapter->event_hs_wait_q);
 
 	kthread_stop(priv->main_thread.task);
 
diff --git a/drivers/char/tpm/tpm-interface.c b/drivers/char/tpm/tpm-interface.c
index 62e10fd1e1cb..6af17002a115 100644
--- a/drivers/char/tpm/tpm-interface.c
+++ b/drivers/char/tpm/tpm-interface.c
@@ -491,11 +491,10 @@ static int tpm_startup(struct tpm_chip *chip, __be16 startup_type)
 int tpm_get_timeouts(struct tpm_chip *chip)
 {
 	struct tpm_cmd_t tpm_cmd;
-	struct timeout_t *timeout_cap;
+	unsigned long new_timeout[4];
+	unsigned long old_timeout[4];
 	struct duration_t *duration_cap;
 	ssize_t rc;
-	u32 timeout;
-	unsigned int scale = 1;
 
 	tpm_cmd.header.in = tpm_getcap_header;
 	tpm_cmd.params.getcap_in.cap = TPM_CAP_PROP;
@@ -529,25 +528,46 @@ int tpm_get_timeouts(struct tpm_chip *chip)
 	    != sizeof(tpm_cmd.header.out) + sizeof(u32) + 4 * sizeof(u32))
 		return -EINVAL;
 
-	timeout_cap = &tpm_cmd.params.getcap_out.cap.timeout;
-	/* Don't overwrite default if value is 0 */
-	timeout = be32_to_cpu(timeout_cap->a);
-	if (timeout && timeout < 1000) {
-		/* timeouts in msec rather usec */
-		scale = 1000;
-		chip->vendor.timeout_adjusted = true;
+	old_timeout[0] = be32_to_cpu(tpm_cmd.params.getcap_out.cap.timeout.a);
+	old_timeout[1] = be32_to_cpu(tpm_cmd.params.getcap_out.cap.timeout.b);
+	old_timeout[2] = be32_to_cpu(tpm_cmd.params.getcap_out.cap.timeout.c);
+	old_timeout[3] = be32_to_cpu(tpm_cmd.params.getcap_out.cap.timeout.d);
+	memcpy(new_timeout, old_timeout, sizeof(new_timeout));
+
+	/*
+	 * Provide ability for vendor overrides of timeout values in case
+	 * of misreporting.
+	 */
+	if (chip->ops->update_timeouts != NULL)
+		chip->vendor.timeout_adjusted =
+			chip->ops->update_timeouts(chip, new_timeout);
+
+	if (!chip->vendor.timeout_adjusted) {
+		/* Don't overwrite default if value is 0 */
+		if (new_timeout[0] != 0 && new_timeout[0] < 1000) {
+			int i;
+
+			/* timeouts in msec rather usec */
+			for (i = 0; i != ARRAY_SIZE(new_timeout); i++)
+				new_timeout[i] *= 1000;
+			chip->vendor.timeout_adjusted = true;
+		}
+	}
+
+	/* Report adjusted timeouts */
+	if (chip->vendor.timeout_adjusted) {
+		dev_info(chip->dev,
+			 HW_ERR "Adjusting reported timeouts: A %lu->%luus B %lu->%luus C %lu->%luus D %lu->%luus\n",
+			 old_timeout[0], new_timeout[0],
+			 old_timeout[1], new_timeout[1],
+			 old_timeout[2], new_timeout[2],
+			 old_timeout[3], new_timeout[3]);
 	}
-	if (timeout)
-		chip->vendor.timeout_a = usecs_to_jiffies(timeout * scale);
-	timeout = be32_to_cpu(timeout_cap->b);
-	if (timeout)
-		chip->vendor.timeout_b = usecs_to_jiffies(timeout * scale);
-	timeout = be32_to_cpu(timeout_cap->c);
-	if (timeout)
-		chip->vendor.timeout_c = usecs_to_jiffies(timeout * scale);
-	timeout = be32_to_cpu(timeout_cap->d);
-	if (timeout)
-		chip->vendor.timeout_d = usecs_to_jiffies(timeout * scale);
+
+	chip->vendor.timeout_a = usecs_to_jiffies(new_timeout[0]);
+	chip->vendor.timeout_b = usecs_to_jiffies(new_timeout[1]);
+	chip->vendor.timeout_c = usecs_to_jiffies(new_timeout[2]);
+	chip->vendor.timeout_d = usecs_to_jiffies(new_timeout[3]);
 
 duration:
 	tpm_cmd.header.in = tpm_getcap_header;
@@ -991,13 +1011,13 @@ int tpm_get_random(u32 chip_num, u8 *out, size_t max)
 	int err, total = 0, retries = 5;
 	u8 *dest = out;
 
+	if (!out || !num_bytes || max > TPM_MAX_RNG_DATA)
+		return -EINVAL;
+
 	chip = tpm_chip_find_get(chip_num);
 	if (chip == NULL)
 		return -ENODEV;
 
-	if (!out || !num_bytes || max > TPM_MAX_RNG_DATA)
-		return -EINVAL;
-
 	do {
 		tpm_cmd.header.in = tpm_getrandom_header;
 		tpm_cmd.params.getrandom_in.num_bytes = cpu_to_be32(num_bytes);
@@ -1016,6 +1036,7 @@ int tpm_get_random(u32 chip_num, u8 *out, size_t max)
 		num_bytes -= recd;
 	} while (retries-- && total < max);
 
+	tpm_chip_put(chip);
 	return total ? total : -EIO;
 }
 EXPORT_SYMBOL_GPL(tpm_get_random);
@@ -1095,7 +1116,7 @@ struct tpm_chip *tpm_register_hardware(struct device *dev,
 		goto del_misc;
 
 	if (tpm_add_ppi(&dev->kobj))
-		goto del_misc;
+		goto del_sysfs;
 
 	chip->bios_dir = tpm_bios_log_setup(chip->devname);
 
@@ -1106,6 +1127,8 @@ struct tpm_chip *tpm_register_hardware(struct device *dev,
 
 	return chip;
 
+del_sysfs:
+	tpm_sysfs_del_device(chip);
 del_misc:
 	tpm_dev_del_device(chip);
 put_device:
diff --git a/drivers/char/tpm/tpm_tis.c b/drivers/char/tpm/tpm_tis.c
index a9ed2270c25d..2c46734b266d 100644
--- a/drivers/char/tpm/tpm_tis.c
+++ b/drivers/char/tpm/tpm_tis.c
@@ -373,6 +373,36 @@ out_err:
 	return rc;
 }
 
+struct tis_vendor_timeout_override {
+	u32 did_vid;
+	unsigned long timeout_us[4];
+};
+
+static const struct tis_vendor_timeout_override vendor_timeout_overrides[] = {
+	/* Atmel 3204 */
+	{ 0x32041114, { (TIS_SHORT_TIMEOUT*1000), (TIS_LONG_TIMEOUT*1000),
+			(TIS_SHORT_TIMEOUT*1000), (TIS_SHORT_TIMEOUT*1000) } },
+};
+
+static bool tpm_tis_update_timeouts(struct tpm_chip *chip,
+				    unsigned long *timeout_cap)
+{
+	int i;
+	u32 did_vid;
+
+	did_vid = ioread32(chip->vendor.iobase + TPM_DID_VID(0));
+
+	for (i = 0; i != ARRAY_SIZE(vendor_timeout_overrides); i++) {
+		if (vendor_timeout_overrides[i].did_vid != did_vid)
+			continue;
+		memcpy(timeout_cap, vendor_timeout_overrides[i].timeout_us,
+		       sizeof(vendor_timeout_overrides[i].timeout_us));
+		return true;
+	}
+
+	return false;
+}
+
 /*
  * Early probing for iTPM with STS_DATA_EXPECT flaw.
  * Try sending command without itpm flag set and if that
@@ -437,6 +467,7 @@ static const struct tpm_class_ops tpm_tis = {
 	.recv = tpm_tis_recv,
 	.send = tpm_tis_send,
 	.cancel = tpm_tis_ready,
+	.update_timeouts = tpm_tis_update_timeouts,
 	.req_complete_mask = TPM_STS_DATA_AVAIL | TPM_STS_VALID,
 	.req_complete_val = TPM_STS_DATA_AVAIL | TPM_STS_VALID,
 	.req_canceled = tpm_tis_req_canceled,
diff --git a/drivers/firmware/efi/vars.c b/drivers/firmware/efi/vars.c
index b22659cccca4..e6125522860a 100644
--- a/drivers/firmware/efi/vars.c
+++ b/drivers/firmware/efi/vars.c
@@ -481,7 +481,7 @@ EXPORT_SYMBOL_GPL(efivar_entry_remove);
  */
 static void efivar_entry_list_del_unlock(struct efivar_entry *entry)
 {
-	WARN_ON(!spin_is_locked(&__efivars->lock));
+	lockdep_assert_held(&__efivars->lock);
 
 	list_del(&entry->list);
 	spin_unlock_irq(&__efivars->lock);
@@ -507,7 +507,7 @@ int __efivar_entry_delete(struct efivar_entry *entry)
 	const struct efivar_operations *ops = __efivars->ops;
 	efi_status_t status;
 
-	WARN_ON(!spin_is_locked(&__efivars->lock));
+	lockdep_assert_held(&__efivars->lock);
 
 	status = ops->set_variable(entry->var.VariableName,
 				   &entry->var.VendorGuid,
@@ -667,7 +667,7 @@ struct efivar_entry *efivar_entry_find(efi_char16_t *name, efi_guid_t guid,
 	int strsize1, strsize2;
 	bool found = false;
 
-	WARN_ON(!spin_is_locked(&__efivars->lock));
+	lockdep_assert_held(&__efivars->lock);
 
 	list_for_each_entry_safe(entry, n, head, list) {
 		strsize1 = ucs2_strsize(name, 1024);
@@ -739,7 +739,7 @@ int __efivar_entry_get(struct efivar_entry *entry, u32 *attributes,
 	const struct efivar_operations *ops = __efivars->ops;
 	efi_status_t status;
 
-	WARN_ON(!spin_is_locked(&__efivars->lock));
+	lockdep_assert_held(&__efivars->lock);
 
 	status = ops->get_variable(entry->var.VariableName,
 				   &entry->var.VendorGuid,
diff --git a/drivers/gpu/drm/nouveau/nouveau_drm.h b/drivers/gpu/drm/nouveau/nouveau_drm.h
index 23ca7a517246..74ed08a750f4 100644
--- a/drivers/gpu/drm/nouveau/nouveau_drm.h
+++ b/drivers/gpu/drm/nouveau/nouveau_drm.h
@@ -10,7 +10,7 @@
 
 #define DRIVER_MAJOR		1
 #define DRIVER_MINOR		1
-#define DRIVER_PATCHLEVEL	1
+#define DRIVER_PATCHLEVEL	2
 
 /*
  * 1.1.1:
@@ -21,6 +21,8 @@
  *        to control registers on the MPs to enable performance counters,
  *        and to control the warp error enable mask (OpenGL requires out of
  *        bounds access to local memory to be silently ignored / return 0).
+ * 1.1.2:
+ *      - fixes multiple bugs in flip completion events and timestamping
  */
 
 #include <core/client.h>
diff --git a/drivers/gpu/drm/radeon/cik.c b/drivers/gpu/drm/radeon/cik.c
index bc9e56eb4e9c..7b3537c55c77 100644
--- a/drivers/gpu/drm/radeon/cik.c
+++ b/drivers/gpu/drm/radeon/cik.c
@@ -7779,6 +7779,7 @@ restart_ih:
 static int cik_startup(struct radeon_device *rdev)
 {
 	struct radeon_ring *ring;
+	u32 nop;
 	int r;
 
 	/* enable pcie gen2/3 link */
@@ -7896,9 +7897,15 @@ static int cik_startup(struct radeon_device *rdev)
 	}
 	cik_irq_set(rdev);
 
+	if (rdev->family == CHIP_HAWAII) {
+		nop = RADEON_CP_PACKET2;
+	} else {
+		nop = PACKET3(PACKET3_NOP, 0x3FFF);
+	}
+
 	ring = &rdev->ring[RADEON_RING_TYPE_GFX_INDEX];
 	r = radeon_ring_init(rdev, ring, ring->ring_size, RADEON_WB_CP_RPTR_OFFSET,
-			     PACKET3(PACKET3_NOP, 0x3FFF));
+			     nop);
 	if (r)
 		return r;
 
@@ -7906,7 +7913,7 @@ static int cik_startup(struct radeon_device *rdev)
 	/* type-2 packets are deprecated on MEC, use type-3 instead */
 	ring = &rdev->ring[CAYMAN_RING_TYPE_CP1_INDEX];
 	r = radeon_ring_init(rdev, ring, ring->ring_size, RADEON_WB_CP1_RPTR_OFFSET,
-			     PACKET3(PACKET3_NOP, 0x3FFF));
+			     nop);
 	if (r)
 		return r;
 	ring->me = 1; /* first MEC */
@@ -7917,7 +7924,7 @@ static int cik_startup(struct radeon_device *rdev)
 	/* type-2 packets are deprecated on MEC, use type-3 instead */
 	ring = &rdev->ring[CAYMAN_RING_TYPE_CP2_INDEX];
 	r = radeon_ring_init(rdev, ring, ring->ring_size, RADEON_WB_CP2_RPTR_OFFSET,
-			     PACKET3(PACKET3_NOP, 0x3FFF));
+			     nop);
 	if (r)
 		return r;
 	/* dGPU only have 1 MEC */
diff --git a/drivers/infiniband/core/iwcm.c b/drivers/infiniband/core/iwcm.c
index 3d2e489ab732..ff9163dc1596 100644
--- a/drivers/infiniband/core/iwcm.c
+++ b/drivers/infiniband/core/iwcm.c
@@ -46,6 +46,7 @@
 #include <linux/completion.h>
 #include <linux/slab.h>
 #include <linux/module.h>
+#include <linux/sysctl.h>
 
 #include <rdma/iw_cm.h>
 #include <rdma/ib_addr.h>
@@ -65,6 +66,20 @@ struct iwcm_work {
 	struct list_head free_list;
 };
 
+static unsigned int default_backlog = 256;
+
+static struct ctl_table_header *iwcm_ctl_table_hdr;
+static struct ctl_table iwcm_ctl_table[] = {
+	{
+		.procname	= "default_backlog",
+		.data		= &default_backlog,
+		.maxlen		= sizeof(default_backlog),
+		.mode		= 0644,
+		.proc_handler	= proc_dointvec,
+	},
+	{ }
+};
+
 /*
  * The following services provide a mechanism for pre-allocating iwcm_work
  * elements.  The design pre-allocates them  based on the cm_id type:
@@ -425,6 +440,9 @@ int iw_cm_listen(struct iw_cm_id *cm_id, int backlog)
 
 	cm_id_priv = container_of(cm_id, struct iwcm_id_private, id);
 
+	if (!backlog)
+		backlog = default_backlog;
+
 	ret = alloc_work_entries(cm_id_priv, backlog);
 	if (ret)
 		return ret;
@@ -1030,11 +1048,20 @@ static int __init iw_cm_init(void)
 	if (!iwcm_wq)
 		return -ENOMEM;
 
+	iwcm_ctl_table_hdr = register_net_sysctl(&init_net, "net/iw_cm",
+						 iwcm_ctl_table);
+	if (!iwcm_ctl_table_hdr) {
+		pr_err("iw_cm: couldn't register sysctl paths\n");
+		destroy_workqueue(iwcm_wq);
+		return -ENOMEM;
+	}
+
 	return 0;
 }
 
 static void __exit iw_cm_cleanup(void)
 {
+	unregister_net_sysctl_table(iwcm_ctl_table_hdr);
 	destroy_workqueue(iwcm_wq);
 }
 
diff --git a/drivers/infiniband/ulp/srp/ib_srp.c b/drivers/infiniband/ulp/srp/ib_srp.c
index e96c07ee6756..ca0bc6c67abe 100644
--- a/drivers/infiniband/ulp/srp/ib_srp.c
+++ b/drivers/infiniband/ulp/srp/ib_srp.c
@@ -120,6 +120,7 @@ static void srp_send_completion(struct ib_cq *cq, void *target_ptr);
 static int srp_cm_handler(struct ib_cm_id *cm_id, struct ib_cm_event *event);
 
 static struct scsi_transport_template *ib_srp_transport_template;
+static struct workqueue_struct *srp_remove_wq;
 
 static struct ib_client srp_client = {
 	.name   = "srp",
@@ -539,7 +540,7 @@ static bool srp_queue_remove_work(struct srp_target_port *target)
 	spin_unlock_irq(&target->lock);
 
 	if (changed)
-		queue_work(system_long_wq, &target->remove_work);
+		queue_work(srp_remove_wq, &target->remove_work);
 
 	return changed;
 }
@@ -2886,9 +2887,10 @@ static void srp_remove_one(struct ib_device *device)
 		spin_unlock(&host->target_lock);
 
 		/*
-		 * Wait for target port removal tasks.
+		 * Wait for tl_err and target port removal tasks.
 		 */
 		flush_workqueue(system_long_wq);
+		flush_workqueue(srp_remove_wq);
 
 		kfree(host);
 	}
@@ -2940,16 +2942,22 @@ static int __init srp_init_module(void)
 		indirect_sg_entries = cmd_sg_entries;
 	}
 
+	srp_remove_wq = create_workqueue("srp_remove");
+	if (IS_ERR(srp_remove_wq)) {
+		ret = PTR_ERR(srp_remove_wq);
+		goto out;
+	}
+
+	ret = -ENOMEM;
 	ib_srp_transport_template =
 		srp_attach_transport(&ib_srp_transport_functions);
 	if (!ib_srp_transport_template)
-		return -ENOMEM;
+		goto destroy_wq;
 
 	ret = class_register(&srp_class);
 	if (ret) {
 		pr_err("couldn't register class infiniband_srp\n");
-		srp_release_transport(ib_srp_transport_template);
-		return ret;
+		goto release_tr;
 	}
 
 	ib_sa_register_client(&srp_sa_client);
@@ -2957,13 +2965,22 @@ static int __init srp_init_module(void)
 	ret = ib_register_client(&srp_client);
 	if (ret) {
 		pr_err("couldn't register IB client\n");
-		srp_release_transport(ib_srp_transport_template);
-		ib_sa_unregister_client(&srp_sa_client);
-		class_unregister(&srp_class);
-		return ret;
+		goto unreg_sa;
 	}
 
-	return 0;
+out:
+	return ret;
+
+unreg_sa:
+	ib_sa_unregister_client(&srp_sa_client);
+	class_unregister(&srp_class);
+
+release_tr:
+	srp_release_transport(ib_srp_transport_template);
+
+destroy_wq:
+	destroy_workqueue(srp_remove_wq);
+	goto out;
 }
 
 static void __exit srp_cleanup_module(void)
@@ -2972,6 +2989,7 @@ static void __exit srp_cleanup_module(void)
 	ib_sa_unregister_client(&srp_sa_client);
 	class_unregister(&srp_class);
 	srp_release_transport(ib_srp_transport_template);
+	destroy_workqueue(srp_remove_wq);
 }
 
 module_init(srp_init_module);
diff --git a/drivers/iommu/amd_iommu.c b/drivers/iommu/amd_iommu.c
index 71776ff5aedc..9cbef59d404a 100644
--- a/drivers/iommu/amd_iommu.c
+++ b/drivers/iommu/amd_iommu.c
@@ -3227,14 +3227,16 @@ free_domains:
 
 static void cleanup_domain(struct protection_domain *domain)
 {
-	struct iommu_dev_data *dev_data, *next;
+	struct iommu_dev_data *entry;
 	unsigned long flags;
 
 	write_lock_irqsave(&amd_iommu_devtable_lock, flags);
 
-	list_for_each_entry_safe(dev_data, next, &domain->dev_list, list) {
-		__detach_device(dev_data);
-		atomic_set(&dev_data->bind, 0);
+	while (!list_empty(&domain->dev_list)) {
+		entry = list_first_entry(&domain->dev_list,
+					 struct iommu_dev_data, list);
+		__detach_device(entry);
+		atomic_set(&entry->bind, 0);
 	}
 
 	write_unlock_irqrestore(&amd_iommu_devtable_lock, flags);
diff --git a/drivers/md/raid1.c b/drivers/md/raid1.c
index 56e24c072b62..d7690f86fdb9 100644
--- a/drivers/md/raid1.c
+++ b/drivers/md/raid1.c
@@ -1501,12 +1501,12 @@ static void error(struct mddev *mddev, struct md_rdev *rdev)
 		mddev->degraded++;
 		set_bit(Faulty, &rdev->flags);
 		spin_unlock_irqrestore(&conf->device_lock, flags);
-		/*
-		 * if recovery is running, make sure it aborts.
-		 */
-		set_bit(MD_RECOVERY_INTR, &mddev->recovery);
 	} else
 		set_bit(Faulty, &rdev->flags);
+	/*
+	 * if recovery is running, make sure it aborts.
+	 */
+	set_bit(MD_RECOVERY_INTR, &mddev->recovery);
 	set_bit(MD_CHANGE_DEVS, &mddev->flags);
 	printk(KERN_ALERT
 	       "md/raid1:%s: Disk failure on %s, disabling device.\n"
diff --git a/drivers/md/raid10.c b/drivers/md/raid10.c
index cb882aae9e20..a46124ecafc7 100644
--- a/drivers/md/raid10.c
+++ b/drivers/md/raid10.c
@@ -1684,13 +1684,12 @@ static void error(struct mddev *mddev, struct md_rdev *rdev)
 		spin_unlock_irqrestore(&conf->device_lock, flags);
 		return;
 	}
-	if (test_and_clear_bit(In_sync, &rdev->flags)) {
+	if (test_and_clear_bit(In_sync, &rdev->flags))
 		mddev->degraded++;
-			/*
-		 * if recovery is running, make sure it aborts.
-		 */
-		set_bit(MD_RECOVERY_INTR, &mddev->recovery);
-	}
+	/*
+	 * If recovery is running, make sure it aborts.
+	 */
+	set_bit(MD_RECOVERY_INTR, &mddev->recovery);
 	set_bit(Blocked, &rdev->flags);
 	set_bit(Faulty, &rdev->flags);
 	set_bit(MD_CHANGE_DEVS, &mddev->flags);
@@ -2954,6 +2953,7 @@ static sector_t sync_request(struct mddev *mddev, sector_t sector_nr,
 		 */
 		if (test_bit(MD_RECOVERY_RESHAPE, &mddev->recovery)) {
 			end_reshape(conf);
+			close_sync(conf);
 			return 0;
 		}
 
@@ -4411,7 +4411,7 @@ read_more:
 	read_bio->bi_private = r10_bio;
 	read_bio->bi_end_io = end_sync_read;
 	read_bio->bi_rw = READ;
-	read_bio->bi_flags &= ~(BIO_POOL_MASK - 1);
+	read_bio->bi_flags &= (~0UL << BIO_RESET_BITS);
 	read_bio->bi_flags |= 1 << BIO_UPTODATE;
 	read_bio->bi_vcnt = 0;
 	read_bio->bi_iter.bi_size = 0;
diff --git a/drivers/md/raid5.c b/drivers/md/raid5.c
index 16f5c21963db..18cda77b4f79 100644
--- a/drivers/md/raid5.c
+++ b/drivers/md/raid5.c
@@ -3779,6 +3779,8 @@ static void handle_stripe(struct stripe_head *sh)
 				set_bit(R5_Wantwrite, &dev->flags);
 				if (prexor)
 					continue;
+				if (s.failed > 1)
+					continue;
 				if (!test_bit(R5_Insync, &dev->flags) ||
 				    ((i == sh->pd_idx || i == sh->qd_idx)  &&
 				     s.failed == 0))
diff --git a/drivers/media/common/siano/Kconfig b/drivers/media/common/siano/Kconfig
index f953d33ee151..4bfbd5f463d1 100644
--- a/drivers/media/common/siano/Kconfig
+++ b/drivers/media/common/siano/Kconfig
@@ -22,8 +22,7 @@ config SMS_SIANO_DEBUGFS
 	bool "Enable debugfs for smsdvb"
 	depends on SMS_SIANO_MDTV
 	depends on DEBUG_FS
-	depends on SMS_USB_DRV
-	depends on CONFIG_SMS_USB_DRV = CONFIG_SMS_SDIO_DRV
+	depends on SMS_USB_DRV = SMS_SDIO_DRV
 
 	---help---
 	  Choose Y to enable visualizing a dump of the frontend
diff --git a/drivers/media/i2c/mt9v032.c b/drivers/media/i2c/mt9v032.c
index 36c504b78f2c..008ac87a9031 100644
--- a/drivers/media/i2c/mt9v032.c
+++ b/drivers/media/i2c/mt9v032.c
@@ -305,8 +305,8 @@ mt9v032_update_hblank(struct mt9v032 *mt9v032)
 
 	if (mt9v032->version->version == MT9V034_CHIP_ID_REV1)
 		min_hblank += (mt9v032->hratio - 1) * 10;
-	min_hblank = max_t(unsigned int, (int)mt9v032->model->data->min_row_time - crop->width,
-			   (int)min_hblank);
+	min_hblank = max_t(int, mt9v032->model->data->min_row_time - crop->width,
+			   min_hblank);
 	hblank = max_t(unsigned int, mt9v032->hblank, min_hblank);
 
 	return mt9v032_write(client, MT9V032_HORIZONTAL_BLANKING, hblank);
diff --git a/drivers/media/media-device.c b/drivers/media/media-device.c
index 703560fa5e73..88c1606fd555 100644
--- a/drivers/media/media-device.c
+++ b/drivers/media/media-device.c
@@ -106,8 +106,6 @@ static long media_device_enum_entities(struct media_device *mdev,
 	if (ent->name) {
 		strncpy(u_ent.name, ent->name, sizeof(u_ent.name));
 		u_ent.name[sizeof(u_ent.name) - 1] = '\0';
-	} else {
-		memset(u_ent.name, 0, sizeof(u_ent.name));
 	}
 	u_ent.type = ent->type;
 	u_ent.revision = ent->revision;
diff --git a/drivers/media/platform/vsp1/vsp1_video.c b/drivers/media/platform/vsp1/vsp1_video.c
index b4687a834f85..7245cca89257 100644
--- a/drivers/media/platform/vsp1/vsp1_video.c
+++ b/drivers/media/platform/vsp1/vsp1_video.c
@@ -635,8 +635,6 @@ static int vsp1_video_buffer_prepare(struct vb2_buffer *vb)
 	if (vb->num_planes < format->num_planes)
 		return -EINVAL;
 
-	buf->video = video;
-
 	for (i = 0; i < vb->num_planes; ++i) {
 		buf->addr[i] = vb2_dma_contig_plane_dma_addr(vb, i);
 		buf->length[i] = vb2_plane_size(vb, i);
diff --git a/drivers/media/platform/vsp1/vsp1_video.h b/drivers/media/platform/vsp1/vsp1_video.h
index d8612a378345..47b7a8ab5e2f 100644
--- a/drivers/media/platform/vsp1/vsp1_video.h
+++ b/drivers/media/platform/vsp1/vsp1_video.h
@@ -89,7 +89,6 @@ static inline struct vsp1_pipeline *to_vsp1_pipeline(struct media_entity *e)
 }
 
 struct vsp1_video_buffer {
-	struct vsp1_video *video;
 	struct vb2_buffer buf;
 	struct list_head queue;
 
diff --git a/drivers/media/tuners/xc4000.c b/drivers/media/tuners/xc4000.c
index 2018befabb5a..e71decbfd0af 100644
--- a/drivers/media/tuners/xc4000.c
+++ b/drivers/media/tuners/xc4000.c
@@ -93,7 +93,7 @@ struct xc4000_priv {
 	struct firmware_description *firm;
 	int	firm_size;
 	u32	if_khz;
-	u32	freq_hz;
+	u32	freq_hz, freq_offset;
 	u32	bandwidth;
 	u8	video_standard;
 	u8	rf_mode;
@@ -1157,14 +1157,14 @@ static int xc4000_set_params(struct dvb_frontend *fe)
 	case SYS_ATSC:
 		dprintk(1, "%s() VSB modulation\n", __func__);
 		priv->rf_mode = XC_RF_MODE_AIR;
-		priv->freq_hz = c->frequency - 1750000;
+		priv->freq_offset = 1750000;
 		priv->video_standard = XC4000_DTV6;
 		type = DTV6;
 		break;
 	case SYS_DVBC_ANNEX_B:
 		dprintk(1, "%s() QAM modulation\n", __func__);
 		priv->rf_mode = XC_RF_MODE_CABLE;
-		priv->freq_hz = c->frequency - 1750000;
+		priv->freq_offset = 1750000;
 		priv->video_standard = XC4000_DTV6;
 		type = DTV6;
 		break;
@@ -1173,23 +1173,23 @@ static int xc4000_set_params(struct dvb_frontend *fe)
 		dprintk(1, "%s() OFDM\n", __func__);
 		if (bw == 0) {
 			if (c->frequency < 400000000) {
-				priv->freq_hz = c->frequency - 2250000;
+				priv->freq_offset = 2250000;
 			} else {
-				priv->freq_hz = c->frequency - 2750000;
+				priv->freq_offset = 2750000;
 			}
 			priv->video_standard = XC4000_DTV7_8;
 			type = DTV78;
 		} else if (bw <= 6000000) {
 			priv->video_standard = XC4000_DTV6;
-			priv->freq_hz = c->frequency - 1750000;
+			priv->freq_offset = 1750000;
 			type = DTV6;
 		} else if (bw <= 7000000) {
 			priv->video_standard = XC4000_DTV7;
-			priv->freq_hz = c->frequency - 2250000;
+			priv->freq_offset = 2250000;
 			type = DTV7;
 		} else {
 			priv->video_standard = XC4000_DTV8;
-			priv->freq_hz = c->frequency - 2750000;
+			priv->freq_offset = 2750000;
 			type = DTV8;
 		}
 		priv->rf_mode = XC_RF_MODE_AIR;
@@ -1200,6 +1200,8 @@ static int xc4000_set_params(struct dvb_frontend *fe)
 		goto fail;
 	}
 
+	priv->freq_hz = c->frequency - priv->freq_offset;
+
 	dprintk(1, "%s() frequency=%d (compensated)\n",
 		__func__, priv->freq_hz);
 
@@ -1520,7 +1522,7 @@ static int xc4000_get_frequency(struct dvb_frontend *fe, u32 *freq)
 {
 	struct xc4000_priv *priv = fe->tuner_priv;
 
-	*freq = priv->freq_hz;
+	*freq = priv->freq_hz + priv->freq_offset;
 
 	if (debug) {
 		mutex_lock(&priv->lock);
diff --git a/drivers/media/tuners/xc5000.c b/drivers/media/tuners/xc5000.c
index 5cd09a681b6a..b2d9e9cb97f7 100644
--- a/drivers/media/tuners/xc5000.c
+++ b/drivers/media/tuners/xc5000.c
@@ -55,7 +55,7 @@ struct xc5000_priv {
 
 	u32 if_khz;
 	u16 xtal_khz;
-	u32 freq_hz;
+	u32 freq_hz, freq_offset;
 	u32 bandwidth;
 	u8  video_standard;
 	u8  rf_mode;
@@ -755,13 +755,13 @@ static int xc5000_set_params(struct dvb_frontend *fe)
 	case SYS_ATSC:
 		dprintk(1, "%s() VSB modulation\n", __func__);
 		priv->rf_mode = XC_RF_MODE_AIR;
-		priv->freq_hz = freq - 1750000;
+		priv->freq_offset = 1750000;
 		priv->video_standard = DTV6;
 		break;
 	case SYS_DVBC_ANNEX_B:
 		dprintk(1, "%s() QAM modulation\n", __func__);
 		priv->rf_mode = XC_RF_MODE_CABLE;
-		priv->freq_hz = freq - 1750000;
+		priv->freq_offset = 1750000;
 		priv->video_standard = DTV6;
 		break;
 	case SYS_ISDBT:
@@ -776,15 +776,15 @@ static int xc5000_set_params(struct dvb_frontend *fe)
 		switch (bw) {
 		case 6000000:
 			priv->video_standard = DTV6;
-			priv->freq_hz = freq - 1750000;
+			priv->freq_offset = 1750000;
 			break;
 		case 7000000:
 			priv->video_standard = DTV7;
-			priv->freq_hz = freq - 2250000;
+			priv->freq_offset = 2250000;
 			break;
 		case 8000000:
 			priv->video_standard = DTV8;
-			priv->freq_hz = freq - 2750000;
+			priv->freq_offset = 2750000;
 			break;
 		default:
 			printk(KERN_ERR "xc5000 bandwidth not set!\n");
@@ -798,15 +798,15 @@ static int xc5000_set_params(struct dvb_frontend *fe)
 		priv->rf_mode = XC_RF_MODE_CABLE;
 		if (bw <= 6000000) {
 			priv->video_standard = DTV6;
-			priv->freq_hz = freq - 1750000;
+			priv->freq_offset = 1750000;
 			b = 6;
 		} else if (bw <= 7000000) {
 			priv->video_standard = DTV7;
-			priv->freq_hz = freq - 2250000;
+			priv->freq_offset = 2250000;
 			b = 7;
 		} else {
 			priv->video_standard = DTV7_8;
-			priv->freq_hz = freq - 2750000;
+			priv->freq_offset = 2750000;
 			b = 8;
 		}
 		dprintk(1, "%s() Bandwidth %dMHz (%d)\n", __func__,
@@ -817,6 +817,8 @@ static int xc5000_set_params(struct dvb_frontend *fe)
 		return -EINVAL;
 	}
 
+	priv->freq_hz = freq - priv->freq_offset;
+
 	dprintk(1, "%s() frequency=%d (compensated to %d)\n",
 		__func__, freq, priv->freq_hz);
 
@@ -1067,7 +1069,7 @@ static int xc5000_get_frequency(struct dvb_frontend *fe, u32 *freq)
 {
 	struct xc5000_priv *priv = fe->tuner_priv;
 	dprintk(1, "%s()\n", __func__);
-	*freq = priv->freq_hz;
+	*freq = priv->freq_hz + priv->freq_offset;
 	return 0;
 }
 
diff --git a/drivers/media/usb/au0828/au0828-video.c b/drivers/media/usb/au0828/au0828-video.c
index f6154546b5c0..7ed75efa1c36 100644
--- a/drivers/media/usb/au0828/au0828-video.c
+++ b/drivers/media/usb/au0828/au0828-video.c
@@ -787,11 +787,27 @@ static int au0828_i2s_init(struct au0828_dev *dev)
 
 /*
  * Auvitek au0828 analog stream enable
- * Please set interface0 to AS5 before enable the stream
  */
 static int au0828_analog_stream_enable(struct au0828_dev *d)
 {
+	struct usb_interface *iface;
+	int ret;
+
 	dprintk(1, "au0828_analog_stream_enable called\n");
+
+	iface = usb_ifnum_to_if(d->usbdev, 0);
+	if (iface && iface->cur_altsetting->desc.bAlternateSetting != 5) {
+		dprintk(1, "Changing intf#0 to alt 5\n");
+		/* set au0828 interface0 to AS5 here again */
+		ret = usb_set_interface(d->usbdev, 0, 5);
+		if (ret < 0) {
+			printk(KERN_INFO "Au0828 can't set alt setting to 5!\n");
+			return -EBUSY;
+		}
+	}
+
+	/* FIXME: size should be calculated using d->width, d->height */
+
 	au0828_writereg(d, AU0828_SENSORCTRL_VBI_103, 0x00);
 	au0828_writereg(d, 0x106, 0x00);
 	/* set x position */
@@ -1002,15 +1018,6 @@ static int au0828_v4l2_open(struct file *filp)
 		return -ERESTARTSYS;
 	}
 	if (dev->users == 0) {
-		/* set au0828 interface0 to AS5 here again */
-		ret = usb_set_interface(dev->usbdev, 0, 5);
-		if (ret < 0) {
-			mutex_unlock(&dev->lock);
-			printk(KERN_INFO "Au0828 can't set alternate to 5!\n");
-			kfree(fh);
-			return -EBUSY;
-		}
-
 		au0828_analog_stream_enable(dev);
 		au0828_analog_stream_reset(dev);
 
@@ -1252,13 +1259,6 @@ static int au0828_set_format(struct au0828_dev *dev, unsigned int cmd,
 		}
 	}
 
-	/* set au0828 interface0 to AS5 here again */
-	ret = usb_set_interface(dev->usbdev, 0, 5);
-	if (ret < 0) {
-		printk(KERN_INFO "Au0828 can't set alt setting to 5!\n");
-		return -EBUSY;
-	}
-
 	au0828_analog_stream_enable(dev);
 
 	return 0;
diff --git a/drivers/mfd/omap-usb-host.c b/drivers/mfd/omap-usb-host.c
index 90b630ccc8bc..0aefe501fd3c 100644
--- a/drivers/mfd/omap-usb-host.c
+++ b/drivers/mfd/omap-usb-host.c
@@ -445,7 +445,7 @@ static unsigned omap_usbhs_rev1_hostconfig(struct usbhs_hcd_omap *omap,
 
 		for (i = 0; i < omap->nports; i++) {
 			if (is_ehci_phy_mode(pdata->port_mode[i])) {
-				reg &= OMAP_UHH_HOSTCONFIG_ULPI_BYPASS;
+				reg &= ~OMAP_UHH_HOSTCONFIG_ULPI_BYPASS;
 				break;
 			}
 		}
diff --git a/drivers/mtd/ftl.c b/drivers/mtd/ftl.c
index 19d637266fcd..71e4f6ccae2f 100644
--- a/drivers/mtd/ftl.c
+++ b/drivers/mtd/ftl.c
@@ -1075,7 +1075,6 @@ static void ftl_add_mtd(struct mtd_blktrans_ops *tr, struct mtd_info *mtd)
 			return;
 	}
 
-	ftl_freepart(partition);
 	kfree(partition);
 }
 
diff --git a/drivers/mtd/nand/omap2.c b/drivers/mtd/nand/omap2.c
index 6f55d92dc233..64d8e32b6ca0 100644
--- a/drivers/mtd/nand/omap2.c
+++ b/drivers/mtd/nand/omap2.c
@@ -933,7 +933,7 @@ static int omap_calculate_ecc(struct mtd_info *mtd, const u_char *dat,
 	u32 val;
 
 	val = readl(info->reg.gpmc_ecc_config);
-	if (((val >> ECC_CONFIG_CS_SHIFT)  & ~CS_MASK) != info->gpmc_cs)
+	if (((val >> ECC_CONFIG_CS_SHIFT) & CS_MASK) != info->gpmc_cs)
 		return -EINVAL;
 
 	/* read ecc result */
diff --git a/drivers/power/bq2415x_charger.c b/drivers/power/bq2415x_charger.c
index 79a37f6d3307..e384844a1ae1 100644
--- a/drivers/power/bq2415x_charger.c
+++ b/drivers/power/bq2415x_charger.c
@@ -840,8 +840,7 @@ static int bq2415x_notifier_call(struct notifier_block *nb,
 	if (bq->automode < 1)
 		return NOTIFY_OK;
 
-	sysfs_notify(&bq->charger.dev->kobj, NULL, "reported_mode");
-	bq2415x_set_mode(bq, bq->reported_mode);
+	schedule_delayed_work(&bq->work, 0);
 
 	return NOTIFY_OK;
 }
@@ -892,6 +891,11 @@ static void bq2415x_timer_work(struct work_struct *work)
 	int error;
 	int boost;
 
+	if (bq->automode > 0 && (bq->reported_mode != bq->mode)) {
+		sysfs_notify(&bq->charger.dev->kobj, NULL, "reported_mode");
+		bq2415x_set_mode(bq, bq->reported_mode);
+	}
+
 	if (!bq->autotimer)
 		return;
 
diff --git a/drivers/regulator/arizona-ldo1.c b/drivers/regulator/arizona-ldo1.c
index f0ea4fdfde87..8b963a757883 100644
--- a/drivers/regulator/arizona-ldo1.c
+++ b/drivers/regulator/arizona-ldo1.c
@@ -141,8 +141,6 @@ static struct regulator_ops arizona_ldo1_ops = {
 	.map_voltage = regulator_map_voltage_linear,
 	.get_voltage_sel = regulator_get_voltage_sel_regmap,
 	.set_voltage_sel = regulator_set_voltage_sel_regmap,
-	.get_bypass = regulator_get_bypass_regmap,
-	.set_bypass = regulator_set_bypass_regmap,
 };
 
 static const struct regulator_desc arizona_ldo1 = {
diff --git a/drivers/scsi/bfa/bfa_ioc.h b/drivers/scsi/bfa/bfa_ioc.h
index 2e28392c2fb6..a38aafa030b3 100644
--- a/drivers/scsi/bfa/bfa_ioc.h
+++ b/drivers/scsi/bfa/bfa_ioc.h
@@ -72,7 +72,7 @@ struct bfa_sge_s {
 } while (0)
 
 #define bfa_swap_words(_x)  (	\
-	((_x) << 32) | ((_x) >> 32))
+	((u64)(_x) << 32) | ((u64)(_x) >> 32))
 
 #ifdef __BIG_ENDIAN
 #define bfa_sge_to_be(_x)
diff --git a/drivers/scsi/scsi_devinfo.c b/drivers/scsi/scsi_devinfo.c
index f969aca0b54e..49014a143c6a 100644
--- a/drivers/scsi/scsi_devinfo.c
+++ b/drivers/scsi/scsi_devinfo.c
@@ -222,6 +222,7 @@ static struct {
 	{"PIONEER", "CD-ROM DRM-602X", NULL, BLIST_FORCELUN | BLIST_SINGLELUN},
 	{"PIONEER", "CD-ROM DRM-604X", NULL, BLIST_FORCELUN | BLIST_SINGLELUN},
 	{"PIONEER", "CD-ROM DRM-624X", NULL, BLIST_FORCELUN | BLIST_SINGLELUN},
+	{"Promise", "VTrak E610f", NULL, BLIST_SPARSELUN | BLIST_NO_RSOC},
 	{"Promise", "", NULL, BLIST_SPARSELUN},
 	{"QUANTUM", "XP34301", "1071", BLIST_NOTQ},
 	{"REGAL", "CDC-4X", NULL, BLIST_MAX5LUN | BLIST_SINGLELUN},
diff --git a/drivers/scsi/scsi_scan.c b/drivers/scsi/scsi_scan.c
index 4109530e92a0..054ec2c412a4 100644
--- a/drivers/scsi/scsi_scan.c
+++ b/drivers/scsi/scsi_scan.c
@@ -922,6 +922,12 @@ static int scsi_add_lun(struct scsi_device *sdev, unsigned char *inq_result,
 	if (*bflags & BLIST_USE_10_BYTE_MS)
 		sdev->use_10_for_ms = 1;
 
+	/* some devices don't like REPORT SUPPORTED OPERATION CODES
+	 * and will simply timeout causing sd_mod init to take a very
+	 * very long time */
+	if (*bflags & BLIST_NO_RSOC)
+		sdev->no_report_opcodes = 1;
+
 	/* set the device running here so that slave configure
 	 * may do I/O */
 	ret = scsi_device_set_state(sdev, SDEV_RUNNING);
@@ -950,7 +956,9 @@ static int scsi_add_lun(struct scsi_device *sdev, unsigned char *inq_result,
 
 	sdev->eh_timeout = SCSI_DEFAULT_EH_TIMEOUT;
 
-	if (*bflags & BLIST_SKIP_VPD_PAGES)
+	if (*bflags & BLIST_TRY_VPD_PAGES)
+		sdev->try_vpd_pages = 1;
+	else if (*bflags & BLIST_SKIP_VPD_PAGES)
 		sdev->skip_vpd_pages = 1;
 
 	transport_configure_device(&sdev->sdev_gendev);
@@ -1236,6 +1244,12 @@ static void scsi_sequential_lun_scan(struct scsi_target *starget,
 		max_dev_lun = min(8U, max_dev_lun);
 
 	/*
+	 * Stop scanning at 255 unless BLIST_SCSI3LUN
+	 */
+	if (!(bflags & BLIST_SCSI3LUN))
+		max_dev_lun = min(256U, max_dev_lun);
+
+	/*
 	 * We have already scanned LUN 0, so start at LUN 1. Keep scanning
 	 * until we reach the max, or no LUN is found and we are not
 	 * sparse_lun.
diff --git a/drivers/scsi/scsi_transport_srp.c b/drivers/scsi/scsi_transport_srp.c
index d47ffc8d3e43..e3e794ee7ddd 100644
--- a/drivers/scsi/scsi_transport_srp.c
+++ b/drivers/scsi/scsi_transport_srp.c
@@ -473,7 +473,8 @@ static void __srp_start_tl_fail_timers(struct srp_rport *rport)
 	if (delay > 0)
 		queue_delayed_work(system_long_wq, &rport->reconnect_work,
 				   1UL * delay * HZ);
-	if (srp_rport_set_state(rport, SRP_RPORT_BLOCKED) == 0) {
+	if ((fast_io_fail_tmo >= 0 || dev_loss_tmo >= 0) &&
+	    srp_rport_set_state(rport, SRP_RPORT_BLOCKED) == 0) {
 		pr_debug("%s new state: %d\n", dev_name(&shost->shost_gendev),
 			 rport->state);
 		scsi_target_block(&shost->shost_gendev);
diff --git a/drivers/scsi/sd.c b/drivers/scsi/sd.c
index 36d1a23f14be..e8abb731c7ec 100644
--- a/drivers/scsi/sd.c
+++ b/drivers/scsi/sd.c
@@ -2686,6 +2686,11 @@ static void sd_read_write_same(struct scsi_disk *sdkp, unsigned char *buffer)
 
 static int sd_try_extended_inquiry(struct scsi_device *sdp)
 {
+	/* Attempt VPD inquiry if the device blacklist explicitly calls
+	 * for it.
+	 */
+	if (sdp->try_vpd_pages)
+		return 1;
 	/*
 	 * Although VPD inquiries can go to SCSI-2 type devices,
 	 * some USB ones crash on receiving them, and the pages
diff --git a/drivers/scsi/storvsc_drv.c b/drivers/scsi/storvsc_drv.c
index 9969fa1ef7c4..ed0f899e8aa5 100644
--- a/drivers/scsi/storvsc_drv.c
+++ b/drivers/scsi/storvsc_drv.c
@@ -33,6 +33,7 @@
 #include <linux/device.h>
 #include <linux/hyperv.h>
 #include <linux/mempool.h>
+#include <linux/blkdev.h>
 #include <scsi/scsi.h>
 #include <scsi/scsi_cmnd.h>
 #include <scsi/scsi_host.h>
@@ -330,17 +331,17 @@ static int storvsc_timeout = 180;
 
 static void storvsc_on_channel_callback(void *context);
 
-/*
- * In Hyper-V, each port/path/target maps to 1 scsi host adapter.  In
- * reality, the path/target is not used (ie always set to 0) so our
- * scsi host adapter essentially has 1 bus with 1 target that contains
- * up to 256 luns.
- */
-#define STORVSC_MAX_LUNS_PER_TARGET			64
-#define STORVSC_MAX_TARGETS				1
-#define STORVSC_MAX_CHANNELS				1
+#define STORVSC_MAX_LUNS_PER_TARGET			255
+#define STORVSC_MAX_TARGETS				2
+#define STORVSC_MAX_CHANNELS				8
 
+#define STORVSC_FC_MAX_LUNS_PER_TARGET			255
+#define STORVSC_FC_MAX_TARGETS				128
+#define STORVSC_FC_MAX_CHANNELS				8
 
+#define STORVSC_IDE_MAX_LUNS_PER_TARGET			64
+#define STORVSC_IDE_MAX_TARGETS				1
+#define STORVSC_IDE_MAX_CHANNELS			1
 
 struct storvsc_cmd_request {
 	struct list_head entry;
@@ -1017,6 +1018,13 @@ static void storvsc_handle_error(struct vmscsi_request *vm_srb,
 		case ATA_12:
 			set_host_byte(scmnd, DID_PASSTHROUGH);
 			break;
+		/*
+		 * On Some Windows hosts TEST_UNIT_READY command can return
+		 * SRB_STATUS_ERROR, let the upper level code deal with it
+		 * based on the sense information.
+		 */
+		case TEST_UNIT_READY:
+			break;
 		default:
 			set_host_byte(scmnd, DID_TARGET_FAILURE);
 		}
@@ -1518,6 +1526,16 @@ static int storvsc_host_reset_handler(struct scsi_cmnd *scmnd)
 	return SUCCESS;
 }
 
+/*
+ * The host guarantees to respond to each command, although I/O latencies might
+ * be unbounded on Azure.  Reset the timer unconditionally to give the host a
+ * chance to perform EH.
+ */
+static enum blk_eh_timer_return storvsc_eh_timed_out(struct scsi_cmnd *scmnd)
+{
+	return BLK_EH_RESET_TIMER;
+}
+
 static bool storvsc_scsi_cmd_ok(struct scsi_cmnd *scmnd)
 {
 	bool allowed = true;
@@ -1553,9 +1571,19 @@ static int storvsc_queuecommand(struct Scsi_Host *host, struct scsi_cmnd *scmnd)
 	struct vmscsi_request *vm_srb;
 	struct stor_mem_pools *memp = scmnd->device->hostdata;
 
-	if (!storvsc_scsi_cmd_ok(scmnd)) {
-		scmnd->scsi_done(scmnd);
-		return 0;
+	if (vmstor_current_major <= VMSTOR_WIN8_MAJOR) {
+		/*
+		 * On legacy hosts filter unimplemented commands.
+		 * Future hosts are expected to correctly handle
+		 * unsupported commands. Furthermore, it is
+		 * possible that some of the currently
+		 * unsupported commands maybe supported in
+		 * future versions of the host.
+		 */
+		if (!storvsc_scsi_cmd_ok(scmnd)) {
+			scmnd->scsi_done(scmnd);
+			return 0;
+		}
 	}
 
 	request_size = sizeof(struct storvsc_cmd_request);
@@ -1580,26 +1608,24 @@ static int storvsc_queuecommand(struct Scsi_Host *host, struct scsi_cmnd *scmnd)
 	vm_srb = &cmd_request->vstor_packet.vm_srb;
 	vm_srb->win8_extension.time_out_value = 60;
 
+	vm_srb->win8_extension.srb_flags |=
+		(SRB_FLAGS_QUEUE_ACTION_ENABLE |
+		SRB_FLAGS_DISABLE_SYNCH_TRANSFER);
 
 	/* Build the SRB */
 	switch (scmnd->sc_data_direction) {
 	case DMA_TO_DEVICE:
 		vm_srb->data_in = WRITE_TYPE;
 		vm_srb->win8_extension.srb_flags |= SRB_FLAGS_DATA_OUT;
-		vm_srb->win8_extension.srb_flags |=
-			(SRB_FLAGS_QUEUE_ACTION_ENABLE |
-			SRB_FLAGS_DISABLE_SYNCH_TRANSFER);
 		break;
 	case DMA_FROM_DEVICE:
 		vm_srb->data_in = READ_TYPE;
 		vm_srb->win8_extension.srb_flags |= SRB_FLAGS_DATA_IN;
-		vm_srb->win8_extension.srb_flags |=
-			(SRB_FLAGS_QUEUE_ACTION_ENABLE |
-			SRB_FLAGS_DISABLE_SYNCH_TRANSFER);
 		break;
 	default:
 		vm_srb->data_in = UNKNOWN_TYPE;
-		vm_srb->win8_extension.srb_flags = 0;
+		vm_srb->win8_extension.srb_flags |= (SRB_FLAGS_DATA_IN |
+						     SRB_FLAGS_DATA_OUT);
 		break;
 	}
 
@@ -1687,11 +1713,11 @@ static struct scsi_host_template scsi_driver = {
 	.bios_param =		storvsc_get_chs,
 	.queuecommand =		storvsc_queuecommand,
 	.eh_host_reset_handler =	storvsc_host_reset_handler,
+	.eh_timed_out =		storvsc_eh_timed_out,
 	.slave_alloc =		storvsc_device_alloc,
 	.slave_destroy =	storvsc_device_destroy,
 	.slave_configure =	storvsc_device_configure,
-	.cmd_per_lun =		1,
-	/* 64 max_queue * 1 target */
+	.cmd_per_lun =		255,
 	.can_queue =		STORVSC_MAX_IO_REQUESTS*STORVSC_MAX_TARGETS,
 	.this_id =		-1,
 	/* no use setting to 0 since ll_blk_rw reset it to 1 */
@@ -1743,19 +1769,25 @@ static int storvsc_probe(struct hv_device *device,
 	 * set state to properly communicate with the host.
 	 */
 
-	if (vmbus_proto_version == VERSION_WIN8) {
-		sense_buffer_size = POST_WIN7_STORVSC_SENSE_BUFFER_SIZE;
-		vmscsi_size_delta = 0;
-		vmstor_current_major = VMSTOR_WIN8_MAJOR;
-		vmstor_current_minor = VMSTOR_WIN8_MINOR;
-	} else {
+	switch (vmbus_proto_version) {
+	case VERSION_WS2008:
+	case VERSION_WIN7:
 		sense_buffer_size = PRE_WIN8_STORVSC_SENSE_BUFFER_SIZE;
 		vmscsi_size_delta = sizeof(struct vmscsi_win8_extension);
 		vmstor_current_major = VMSTOR_WIN7_MAJOR;
 		vmstor_current_minor = VMSTOR_WIN7_MINOR;
+		break;
+	default:
+		sense_buffer_size = POST_WIN7_STORVSC_SENSE_BUFFER_SIZE;
+		vmscsi_size_delta = 0;
+		vmstor_current_major = VMSTOR_WIN8_MAJOR;
+		vmstor_current_minor = VMSTOR_WIN8_MINOR;
+		break;
 	}
 
-
+	if (dev_id->driver_data == SFC_GUID)
+		scsi_driver.can_queue = (STORVSC_MAX_IO_REQUESTS *
+					 STORVSC_FC_MAX_TARGETS);
 	host = scsi_host_alloc(&scsi_driver,
 			       sizeof(struct hv_host_device));
 	if (!host)
@@ -1789,12 +1821,25 @@ static int storvsc_probe(struct hv_device *device,
 	host_dev->path = stor_device->path_id;
 	host_dev->target = stor_device->target_id;
 
-	/* max # of devices per target */
-	host->max_lun = STORVSC_MAX_LUNS_PER_TARGET;
-	/* max # of targets per channel */
-	host->max_id = STORVSC_MAX_TARGETS;
-	/* max # of channels */
-	host->max_channel = STORVSC_MAX_CHANNELS - 1;
+	switch (dev_id->driver_data) {
+	case SFC_GUID:
+		host->max_lun = STORVSC_FC_MAX_LUNS_PER_TARGET;
+		host->max_id = STORVSC_FC_MAX_TARGETS;
+		host->max_channel = STORVSC_FC_MAX_CHANNELS - 1;
+		break;
+
+	case SCSI_GUID:
+		host->max_lun = STORVSC_MAX_LUNS_PER_TARGET;
+		host->max_id = STORVSC_MAX_TARGETS;
+		host->max_channel = STORVSC_MAX_CHANNELS - 1;
+		break;
+
+	default:
+		host->max_lun = STORVSC_IDE_MAX_LUNS_PER_TARGET;
+		host->max_id = STORVSC_IDE_MAX_TARGETS;
+		host->max_channel = STORVSC_IDE_MAX_CHANNELS - 1;
+		break;
+	}
 	/* max cmd length */
 	host->max_cmd_len = STORVSC_MAX_CMD_LEN;
 
diff --git a/drivers/spi/spi-omap2-mcspi.c b/drivers/spi/spi-omap2-mcspi.c
index a72127f08e39..a64f1557c156 100644
--- a/drivers/spi/spi-omap2-mcspi.c
+++ b/drivers/spi/spi-omap2-mcspi.c
@@ -147,6 +147,7 @@ struct omap2_mcspi_cs {
 	void __iomem		*base;
 	unsigned long		phys;
 	int			word_len;
+	u16			mode;
 	struct list_head	node;
 	/* Context save and restore shadow register */
 	u32			chconf0;
@@ -899,6 +900,8 @@ static int omap2_mcspi_setup_transfer(struct spi_device *spi,
 
 	mcspi_write_chconf0(spi, l);
 
+	cs->mode = spi->mode;
+
 	dev_dbg(&spi->dev, "setup: speed %d, sample %s edge, clk %s\n",
 			OMAP2_MCSPI_MAX_FREQ >> div,
 			(spi->mode & SPI_CPHA) ? "trailing" : "leading",
@@ -971,6 +974,7 @@ static int omap2_mcspi_setup(struct spi_device *spi)
 			return -ENOMEM;
 		cs->base = mcspi->base + spi->chip_select * 0x14;
 		cs->phys = mcspi->phys + spi->chip_select * 0x14;
+		cs->mode = 0;
 		cs->chconf0 = 0;
 		spi->controller_state = cs;
 		/* Link this to context save list */
@@ -1051,6 +1055,16 @@ static void omap2_mcspi_work(struct omap2_mcspi *mcspi, struct spi_message *m)
 	cs = spi->controller_state;
 	cd = spi->controller_data;
 
+	/*
+	 * The slave driver could have changed spi->mode in which case
+	 * it will be different from cs->mode (the current hardware setup).
+	 * If so, set par_override (even though its not a parity issue) so
+	 * omap2_mcspi_setup_transfer will be called to configure the hardware
+	 * with the correct mode on the first iteration of the loop below.
+	 */
+	if (spi->mode != cs->mode)
+		par_override = 1;
+
 	omap2_mcspi_set_enable(spi, 0);
 	list_for_each_entry(t, &m->transfers, transfer_list) {
 		if (t->tx_buf == NULL && t->rx_buf == NULL && t->len) {
diff --git a/drivers/spi/spi-orion.c b/drivers/spi/spi-orion.c
index 7f2121fe2622..977b0619bb78 100644
--- a/drivers/spi/spi-orion.c
+++ b/drivers/spi/spi-orion.c
@@ -404,8 +404,6 @@ static int orion_spi_probe(struct platform_device *pdev)
 	struct resource *r;
 	unsigned long tclk_hz;
 	int status = 0;
-	const u32 *iprop;
-	int size;
 
 	master = spi_alloc_master(&pdev->dev, sizeof(*spi));
 	if (master == NULL) {
@@ -416,10 +414,10 @@ static int orion_spi_probe(struct platform_device *pdev)
 	if (pdev->id != -1)
 		master->bus_num = pdev->id;
 	if (pdev->dev.of_node) {
-		iprop = of_get_property(pdev->dev.of_node, "cell-index",
-					&size);
-		if (iprop && size == sizeof(*iprop))
-			master->bus_num = *iprop;
+		u32 cell_index;
+		if (!of_property_read_u32(pdev->dev.of_node, "cell-index",
+					  &cell_index))
+			master->bus_num = cell_index;
 	}
 
 	/* we support only mode 0, and no options */
diff --git a/drivers/spi/spi-pxa2xx.c b/drivers/spi/spi-pxa2xx.c
index c702fc536a77..ced9ecffa163 100644
--- a/drivers/spi/spi-pxa2xx.c
+++ b/drivers/spi/spi-pxa2xx.c
@@ -1078,6 +1078,7 @@ static struct acpi_device_id pxa2xx_spi_acpi_match[] = {
 	{ "INT3430", 0 },
 	{ "INT3431", 0 },
 	{ "80860F0E", 0 },
+	{ "8086228E", 0 },
 	{ },
 };
 MODULE_DEVICE_TABLE(acpi, pxa2xx_spi_acpi_match);
diff --git a/drivers/xen/events/events_fifo.c b/drivers/xen/events/events_fifo.c
index 172a8bc27abd..ef7d446e07ee 100644
--- a/drivers/xen/events/events_fifo.c
+++ b/drivers/xen/events/events_fifo.c
@@ -99,6 +99,25 @@ static unsigned evtchn_fifo_nr_channels(void)
 	return event_array_pages * EVENT_WORDS_PER_PAGE;
 }
 
+static int init_control_block(int cpu,
+                              struct evtchn_fifo_control_block *control_block)
+{
+	struct evtchn_fifo_queue *q = &per_cpu(cpu_queue, cpu);
+	struct evtchn_init_control init_control;
+	unsigned int i;
+
+	/* Reset the control block and the local HEADs. */
+	clear_page(control_block);
+	for (i = 0; i < EVTCHN_FIFO_MAX_QUEUES; i++)
+		q->head[i] = 0;
+
+	init_control.control_gfn = virt_to_mfn(control_block);
+	init_control.offset      = 0;
+	init_control.vcpu        = cpu;
+
+	return HYPERVISOR_event_channel_op(EVTCHNOP_init_control, &init_control);
+}
+
 static void free_unused_array_pages(void)
 {
 	unsigned i;
@@ -327,7 +346,6 @@ static void evtchn_fifo_resume(void)
 
 	for_each_possible_cpu(cpu) {
 		void *control_block = per_cpu(cpu_control_block, cpu);
-		struct evtchn_init_control init_control;
 		int ret;
 
 		if (!control_block)
@@ -344,12 +362,7 @@ static void evtchn_fifo_resume(void)
 			continue;
 		}
 
-		init_control.control_gfn = virt_to_mfn(control_block);
-		init_control.offset = 0;
-		init_control.vcpu = cpu;
-
-		ret = HYPERVISOR_event_channel_op(EVTCHNOP_init_control,
-						  &init_control);
+		ret = init_control_block(cpu, control_block);
 		if (ret < 0)
 			BUG();
 	}
@@ -377,30 +390,25 @@ static const struct evtchn_ops evtchn_ops_fifo = {
 	.resume            = evtchn_fifo_resume,
 };
 
-static int evtchn_fifo_init_control_block(unsigned cpu)
+static int evtchn_fifo_alloc_control_block(unsigned cpu)
 {
-	struct page *control_block = NULL;
-	struct evtchn_init_control init_control;
+	void *control_block = NULL;
 	int ret = -ENOMEM;
 
-	control_block = alloc_page(GFP_KERNEL|__GFP_ZERO);
+	control_block = (void *)__get_free_page(GFP_KERNEL);
 	if (control_block == NULL)
 		goto error;
 
-	init_control.control_gfn = virt_to_mfn(page_address(control_block));
-	init_control.offset      = 0;
-	init_control.vcpu        = cpu;
-
-	ret = HYPERVISOR_event_channel_op(EVTCHNOP_init_control, &init_control);
+	ret = init_control_block(cpu, control_block);
 	if (ret < 0)
 		goto error;
 
-	per_cpu(cpu_control_block, cpu) = page_address(control_block);
+	per_cpu(cpu_control_block, cpu) = control_block;
 
 	return 0;
 
   error:
-	__free_page(control_block);
+	free_page((unsigned long)control_block);
 	return ret;
 }
 
@@ -414,7 +422,7 @@ static int evtchn_fifo_cpu_notification(struct notifier_block *self,
 	switch (action) {
 	case CPU_UP_PREPARE:
 		if (!per_cpu(cpu_control_block, cpu))
-			ret = evtchn_fifo_init_control_block(cpu);
+			ret = evtchn_fifo_alloc_control_block(cpu);
 		break;
 	default:
 		break;
@@ -431,7 +439,7 @@ int __init xen_evtchn_fifo_init(void)
 	int cpu = get_cpu();
 	int ret;
 
-	ret = evtchn_fifo_init_control_block(cpu);
+	ret = evtchn_fifo_alloc_control_block(cpu);
 	if (ret < 0)
 		goto out;
 
diff --git a/fs/cifs/cifsglob.h b/fs/cifs/cifsglob.h
index 30f6e9251a4a..f15d4353f30f 100644
--- a/fs/cifs/cifsglob.h
+++ b/fs/cifs/cifsglob.h
@@ -70,11 +70,6 @@
 #define SERVER_NAME_LENGTH 40
 #define SERVER_NAME_LEN_WITH_NULL     (SERVER_NAME_LENGTH + 1)
 
-/* used to define string lengths for reversing unicode strings */
-/*         (256+1)*2 = 514                                     */
-/*           (max path length + 1 for null) * 2 for unicode    */
-#define MAX_NAME 514
-
 /* SMB echo "timeout" -- FIXME: tunable? */
 #define SMB_ECHO_INTERVAL (60 * HZ)
 
diff --git a/fs/cifs/file.c b/fs/cifs/file.c
index 87c4dd072cde..8175b18df819 100644
--- a/fs/cifs/file.c
+++ b/fs/cifs/file.c
@@ -2844,7 +2844,7 @@ cifs_uncached_read_into_pages(struct TCP_Server_Info *server,
 		total_read += result;
 	}
 
-	return total_read > 0 ? total_read : result;
+	return total_read > 0 && result != -EAGAIN ? total_read : result;
 }
 
 static ssize_t
@@ -3267,7 +3267,7 @@ cifs_readpages_read_into_pages(struct TCP_Server_Info *server,
 		total_read += result;
 	}
 
-	return total_read > 0 ? total_read : result;
+	return total_read > 0 && result != -EAGAIN ? total_read : result;
 }
 
 static int cifs_readpages(struct file *file, struct address_space *mapping,
diff --git a/fs/cifs/inode.c b/fs/cifs/inode.c
index aadc2b68678b..f2ddcf7ac9c3 100644
--- a/fs/cifs/inode.c
+++ b/fs/cifs/inode.c
@@ -1706,13 +1706,22 @@ cifs_rename(struct inode *source_dir, struct dentry *source_dentry,
 unlink_target:
 	/* Try unlinking the target dentry if it's not negative */
 	if (target_dentry->d_inode && (rc == -EACCES || rc == -EEXIST)) {
-		tmprc = cifs_unlink(target_dir, target_dentry);
+		if (d_is_dir(target_dentry))
+			tmprc = cifs_rmdir(target_dir, target_dentry);
+		else
+			tmprc = cifs_unlink(target_dir, target_dentry);
 		if (tmprc)
 			goto cifs_rename_exit;
 		rc = cifs_do_rename(xid, source_dentry, from_name,
 				    target_dentry, to_name);
 	}
 
+	/* force revalidate to go get info when needed */
+	CIFS_I(source_dir)->time = CIFS_I(target_dir)->time = 0;
+
+	source_dir->i_ctime = source_dir->i_mtime = target_dir->i_ctime =
+		target_dir->i_mtime = current_fs_time(source_dir->i_sb);
+
 cifs_rename_exit:
 	kfree(info_buf_source);
 	kfree(from_name);
diff --git a/fs/cifs/readdir.c b/fs/cifs/readdir.c
index b15862e0f68c..2bbf11b09214 100644
--- a/fs/cifs/readdir.c
+++ b/fs/cifs/readdir.c
@@ -596,8 +596,8 @@ find_cifs_entry(const unsigned int xid, struct cifs_tcon *tcon, loff_t pos,
 		if (!cfile->srch_inf.endOfSearch && !cfile->invalidHandle) {
 			cfile->invalidHandle = true;
 			spin_unlock(&cifs_file_list_lock);
-			if (server->ops->close)
-				server->ops->close(xid, tcon, &cfile->fid);
+			if (server->ops->close_dir)
+				server->ops->close_dir(xid, tcon, &cfile->fid);
 		} else
 			spin_unlock(&cifs_file_list_lock);
 		if (cfile->srch_inf.ntwrk_buf_start) {
diff --git a/fs/cifs/smb2file.c b/fs/cifs/smb2file.c
index 3f17b4550831..45992944e238 100644
--- a/fs/cifs/smb2file.c
+++ b/fs/cifs/smb2file.c
@@ -50,7 +50,7 @@ smb2_open_file(const unsigned int xid, struct cifs_open_parms *oparms,
 		goto out;
 	}
 
-	smb2_data = kzalloc(sizeof(struct smb2_file_all_info) + MAX_NAME * 2,
+	smb2_data = kzalloc(sizeof(struct smb2_file_all_info) + PATH_MAX * 2,
 			    GFP_KERNEL);
 	if (smb2_data == NULL) {
 		rc = -ENOMEM;
diff --git a/fs/cifs/smb2inode.c b/fs/cifs/smb2inode.c
index 84c012a6aba0..215f8d3e3e53 100644
--- a/fs/cifs/smb2inode.c
+++ b/fs/cifs/smb2inode.c
@@ -131,7 +131,7 @@ smb2_query_path_info(const unsigned int xid, struct cifs_tcon *tcon,
 	*adjust_tz = false;
 	*symlink = false;
 
-	smb2_data = kzalloc(sizeof(struct smb2_file_all_info) + MAX_NAME * 2,
+	smb2_data = kzalloc(sizeof(struct smb2_file_all_info) + PATH_MAX * 2,
 			    GFP_KERNEL);
 	if (smb2_data == NULL)
 		return -ENOMEM;
diff --git a/fs/cifs/smb2maperror.c b/fs/cifs/smb2maperror.c
index 94bd4fbb13d3..e31a9dfdcd39 100644
--- a/fs/cifs/smb2maperror.c
+++ b/fs/cifs/smb2maperror.c
@@ -605,7 +605,7 @@ static const struct status_to_posix_error smb2_error_map_table[] = {
 	{STATUS_MAPPED_FILE_SIZE_ZERO, -EIO, "STATUS_MAPPED_FILE_SIZE_ZERO"},
 	{STATUS_TOO_MANY_OPENED_FILES, -EMFILE, "STATUS_TOO_MANY_OPENED_FILES"},
 	{STATUS_CANCELLED, -EIO, "STATUS_CANCELLED"},
-	{STATUS_CANNOT_DELETE, -EIO, "STATUS_CANNOT_DELETE"},
+	{STATUS_CANNOT_DELETE, -EACCES, "STATUS_CANNOT_DELETE"},
 	{STATUS_INVALID_COMPUTER_NAME, -EIO, "STATUS_INVALID_COMPUTER_NAME"},
 	{STATUS_FILE_DELETED, -EIO, "STATUS_FILE_DELETED"},
 	{STATUS_SPECIAL_ACCOUNT, -EIO, "STATUS_SPECIAL_ACCOUNT"},
diff --git a/fs/cifs/smb2ops.c b/fs/cifs/smb2ops.c
index 35ddc3ed119d..f8977b2d9187 100644
--- a/fs/cifs/smb2ops.c
+++ b/fs/cifs/smb2ops.c
@@ -339,7 +339,7 @@ smb2_query_file_info(const unsigned int xid, struct cifs_tcon *tcon,
 	int rc;
 	struct smb2_file_all_info *smb2_data;
 
-	smb2_data = kzalloc(sizeof(struct smb2_file_all_info) + MAX_NAME * 2,
+	smb2_data = kzalloc(sizeof(struct smb2_file_all_info) + PATH_MAX * 2,
 			    GFP_KERNEL);
 	if (smb2_data == NULL)
 		return -ENOMEM;
diff --git a/fs/cifs/smb2pdu.c b/fs/cifs/smb2pdu.c
index 049a3f2693ba..9aab8fe0e508 100644
--- a/fs/cifs/smb2pdu.c
+++ b/fs/cifs/smb2pdu.c
@@ -916,7 +916,8 @@ tcon_exit:
 tcon_error_exit:
 	if (rsp->hdr.Status == STATUS_BAD_NETWORK_NAME) {
 		cifs_dbg(VFS, "BAD_NETWORK_NAME: %s\n", tree);
-		tcon->bad_network_name = true;
+		if (tcon)
+			tcon->bad_network_name = true;
 	}
 	goto tcon_exit;
 }
@@ -1539,7 +1540,7 @@ SMB2_query_info(const unsigned int xid, struct cifs_tcon *tcon,
 {
 	return query_info(xid, tcon, persistent_fid, volatile_fid,
 			  FILE_ALL_INFORMATION,
-			  sizeof(struct smb2_file_all_info) + MAX_NAME * 2,
+			  sizeof(struct smb2_file_all_info) + PATH_MAX * 2,
 			  sizeof(struct smb2_file_all_info), data);
 }
 
diff --git a/fs/dcache.c b/fs/dcache.c
index 7f3b4004c6c3..58d57da91d2a 100644
--- a/fs/dcache.c
+++ b/fs/dcache.c
@@ -106,8 +106,7 @@ static inline struct hlist_bl_head *d_hash(const struct dentry *parent,
 					unsigned int hash)
 {
 	hash += (unsigned long) parent / L1_CACHE_BYTES;
-	hash = hash + (hash >> d_hash_shift);
-	return dentry_hashtable + (hash & d_hash_mask);
+	return dentry_hashtable + hash_32(hash, d_hash_shift);
 }
 
 /* Statistics gathering. */
diff --git a/fs/namei.c b/fs/namei.c
index bdea10963aa5..d5a4faeb39a5 100644
--- a/fs/namei.c
+++ b/fs/namei.c
@@ -34,6 +34,7 @@
 #include <linux/device_cgroup.h>
 #include <linux/fs_struct.h>
 #include <linux/posix_acl.h>
+#include <linux/hash.h>
 #include <asm/uaccess.h>
 
 #include "internal.h"
@@ -1624,8 +1625,7 @@ static inline int nested_symlink(struct path *path, struct nameidata *nd)
 
 static inline unsigned int fold_hash(unsigned long hash)
 {
-	hash += hash >> (8*sizeof(int));
-	return hash;
+	return hash_64(hash, 32);
 }
 
 #else	/* 32-bit case */
@@ -1797,7 +1797,7 @@ static int link_path_walk(const char *name, struct nameidata *nd)
 			if (err)
 				return err;
 		}
-		if (!d_is_directory(nd->path.dentry)) {
+		if (!d_can_lookup(nd->path.dentry)) {
 			err = -ENOTDIR; 
 			break;
 		}
@@ -1818,7 +1818,7 @@ static int path_init(int dfd, const char *name, unsigned int flags,
 		struct dentry *root = nd->root.dentry;
 		struct inode *inode = root->d_inode;
 		if (*name) {
-			if (!d_is_directory(root))
+			if (!d_can_lookup(root))
 				return -ENOTDIR;
 			retval = inode_permission(inode, MAY_EXEC);
 			if (retval)
@@ -1874,7 +1874,7 @@ static int path_init(int dfd, const char *name, unsigned int flags,
 		dentry = f.file->f_path.dentry;
 
 		if (*name) {
-			if (!d_is_directory(dentry)) {
+			if (!d_can_lookup(dentry)) {
 				fdput(f);
 				return -ENOTDIR;
 			}
@@ -1956,7 +1956,7 @@ static int path_lookupat(int dfd, const char *name,
 		err = complete_walk(nd);
 
 	if (!err && nd->flags & LOOKUP_DIRECTORY) {
-		if (!d_is_directory(nd->path.dentry)) {
+		if (!d_can_lookup(nd->path.dentry)) {
 			path_put(&nd->path);
 			err = -ENOTDIR;
 		}
@@ -2416,11 +2416,11 @@ static int may_delete(struct inode *dir, struct dentry *victim, bool isdir)
 	    IS_IMMUTABLE(inode) || IS_SWAPFILE(inode))
 		return -EPERM;
 	if (isdir) {
-		if (!d_is_directory(victim) && !d_is_autodir(victim))
+		if (!d_is_dir(victim))
 			return -ENOTDIR;
 		if (IS_ROOT(victim))
 			return -EBUSY;
-	} else if (d_is_directory(victim) || d_is_autodir(victim))
+	} else if (d_is_dir(victim))
 		return -EISDIR;
 	if (IS_DEADDIR(dir))
 		return -ENOENT;
@@ -3018,11 +3018,10 @@ finish_open:
 	}
 	audit_inode(name, nd->path.dentry, 0);
 	error = -EISDIR;
-	if ((open_flag & O_CREAT) &&
-	    (d_is_directory(nd->path.dentry) || d_is_autodir(nd->path.dentry)))
+	if ((open_flag & O_CREAT) && d_is_dir(nd->path.dentry))
 		goto out;
 	error = -ENOTDIR;
-	if ((nd->flags & LOOKUP_DIRECTORY) && !d_is_directory(nd->path.dentry))
+	if ((nd->flags & LOOKUP_DIRECTORY) && !d_can_lookup(nd->path.dentry))
 		goto out;
 	if (!S_ISREG(nd->inode->i_mode))
 		will_truncate = false;
@@ -3746,7 +3745,7 @@ exit1:
 slashes:
 	if (d_is_negative(dentry))
 		error = -ENOENT;
-	else if (d_is_directory(dentry) || d_is_autodir(dentry))
+	else if (d_is_dir(dentry))
 		error = -EISDIR;
 	else
 		error = -ENOTDIR;
@@ -4125,7 +4124,7 @@ int vfs_rename(struct inode *old_dir, struct dentry *old_dentry,
 	       struct inode **delegated_inode)
 {
 	int error;
-	int is_dir = d_is_directory(old_dentry) || d_is_autodir(old_dentry);
+	int is_dir = d_is_dir(old_dentry);
 	const unsigned char *old_name;
 
 	if (old_dentry->d_inode == new_dentry->d_inode)
@@ -4218,7 +4217,7 @@ retry_deleg:
 	if (d_is_negative(old_dentry))
 		goto exit4;
 	/* unless the source is a directory trailing slashes give -ENOTDIR */
-	if (!d_is_directory(old_dentry) && !d_is_autodir(old_dentry)) {
+	if (!d_is_dir(old_dentry)) {
 		error = -ENOTDIR;
 		if (oldnd.last.name[oldnd.last.len])
 			goto exit4;
diff --git a/fs/namespace.c b/fs/namespace.c
index 65233a5f390a..75536db4b69b 100644
--- a/fs/namespace.c
+++ b/fs/namespace.c
@@ -777,6 +777,20 @@ static void attach_mnt(struct mount *mnt,
 	list_add_tail(&mnt->mnt_child, &parent->mnt_mounts);
 }
 
+static void attach_shadowed(struct mount *mnt,
+			struct mount *parent,
+			struct mount *shadows)
+{
+	if (shadows) {
+		hlist_add_after_rcu(&shadows->mnt_hash, &mnt->mnt_hash);
+		list_add(&mnt->mnt_child, &shadows->mnt_child);
+	} else {
+		hlist_add_head_rcu(&mnt->mnt_hash,
+				m_hash(&parent->mnt, mnt->mnt_mountpoint));
+		list_add_tail(&mnt->mnt_child, &parent->mnt_mounts);
+	}
+}
+
 /*
  * vfsmount lock must be held for write
  */
@@ -795,12 +809,7 @@ static void commit_tree(struct mount *mnt, struct mount *shadows)
 
 	list_splice(&head, n->list.prev);
 
-	if (shadows)
-		hlist_add_after_rcu(&shadows->mnt_hash, &mnt->mnt_hash);
-	else
-		hlist_add_head_rcu(&mnt->mnt_hash,
-				m_hash(&parent->mnt, mnt->mnt_mountpoint));
-	list_add_tail(&mnt->mnt_child, &parent->mnt_mounts);
+	attach_shadowed(mnt, parent, shadows);
 	touch_mnt_namespace(n);
 }
 
@@ -887,8 +896,21 @@ static struct mount *clone_mnt(struct mount *old, struct dentry *root,
 
 	mnt->mnt.mnt_flags = old->mnt.mnt_flags & ~(MNT_WRITE_HOLD|MNT_MARKED);
 	/* Don't allow unprivileged users to change mount flags */
-	if ((flag & CL_UNPRIVILEGED) && (mnt->mnt.mnt_flags & MNT_READONLY))
-		mnt->mnt.mnt_flags |= MNT_LOCK_READONLY;
+	if (flag & CL_UNPRIVILEGED) {
+		mnt->mnt.mnt_flags |= MNT_LOCK_ATIME;
+
+		if (mnt->mnt.mnt_flags & MNT_READONLY)
+			mnt->mnt.mnt_flags |= MNT_LOCK_READONLY;
+
+		if (mnt->mnt.mnt_flags & MNT_NODEV)
+			mnt->mnt.mnt_flags |= MNT_LOCK_NODEV;
+
+		if (mnt->mnt.mnt_flags & MNT_NOSUID)
+			mnt->mnt.mnt_flags |= MNT_LOCK_NOSUID;
+
+		if (mnt->mnt.mnt_flags & MNT_NOEXEC)
+			mnt->mnt.mnt_flags |= MNT_LOCK_NOEXEC;
+	}
 
 	/* Don't allow unprivileged users to reveal what is under a mount */
 	if ((flag & CL_UNPRIVILEGED) && list_empty(&old->mnt_expire))
@@ -1204,6 +1226,11 @@ static void namespace_unlock(void)
 	head.first->pprev = &head.first;
 	INIT_HLIST_HEAD(&unmounted);
 
+	/* undo decrements we'd done in umount_tree() */
+	hlist_for_each_entry(mnt, &head, mnt_hash)
+		if (mnt->mnt_ex_mountpoint.mnt)
+			mntget(mnt->mnt_ex_mountpoint.mnt);
+
 	up_write(&namespace_sem);
 
 	synchronize_rcu();
@@ -1240,6 +1267,9 @@ void umount_tree(struct mount *mnt, int how)
 		hlist_add_head(&p->mnt_hash, &tmp_list);
 	}
 
+	hlist_for_each_entry(p, &tmp_list, mnt_hash)
+		list_del_init(&p->mnt_child);
+
 	if (how)
 		propagate_umount(&tmp_list);
 
@@ -1250,9 +1280,9 @@ void umount_tree(struct mount *mnt, int how)
 		p->mnt_ns = NULL;
 		if (how < 2)
 			p->mnt.mnt_flags |= MNT_SYNC_UMOUNT;
-		list_del_init(&p->mnt_child);
 		if (mnt_has_parent(p)) {
 			put_mountpoint(p->mnt_mp);
+			mnt_add_count(p->mnt_parent, -1);
 			/* move the reference to mountpoint into ->mnt_ex_mountpoint */
 			p->mnt_ex_mountpoint.dentry = p->mnt_mountpoint;
 			p->mnt_ex_mountpoint.mnt = &p->mnt_parent->mnt;
@@ -1483,6 +1513,7 @@ struct mount *copy_tree(struct mount *mnt, struct dentry *dentry,
 			continue;
 
 		for (s = r; s; s = next_mnt(s, r)) {
+			struct mount *t = NULL;
 			if (!(flag & CL_COPY_UNBINDABLE) &&
 			    IS_MNT_UNBINDABLE(s)) {
 				s = skip_mnt_tree(s);
@@ -1504,7 +1535,14 @@ struct mount *copy_tree(struct mount *mnt, struct dentry *dentry,
 				goto out;
 			lock_mount_hash();
 			list_add_tail(&q->mnt_list, &res->mnt_list);
-			attach_mnt(q, parent, p->mnt_mp);
+			mnt_set_mountpoint(parent, p->mnt_mp, q);
+			if (!list_empty(&parent->mnt_mounts)) {
+				t = list_last_entry(&parent->mnt_mounts,
+					struct mount, mnt_child);
+				if (t->mnt_mp != p->mnt_mp)
+					t = NULL;
+			}
+			attach_shadowed(q, parent, t);
 			unlock_mount_hash();
 		}
 	}
@@ -1887,9 +1925,6 @@ static int change_mount_flags(struct vfsmount *mnt, int ms_flags)
 	if (readonly_request == __mnt_is_readonly(mnt))
 		return 0;
 
-	if (mnt->mnt_flags & MNT_LOCK_READONLY)
-		return -EPERM;
-
 	if (readonly_request)
 		error = mnt_make_readonly(real_mount(mnt));
 	else
@@ -1915,6 +1950,33 @@ static int do_remount(struct path *path, int flags, int mnt_flags,
 	if (path->dentry != path->mnt->mnt_root)
 		return -EINVAL;
 
+	/* Don't allow changing of locked mnt flags.
+	 *
+	 * No locks need to be held here while testing the various
+	 * MNT_LOCK flags because those flags can never be cleared
+	 * once they are set.
+	 */
+	if ((mnt->mnt.mnt_flags & MNT_LOCK_READONLY) &&
+	    !(mnt_flags & MNT_READONLY)) {
+		return -EPERM;
+	}
+	if ((mnt->mnt.mnt_flags & MNT_LOCK_NODEV) &&
+	    !(mnt_flags & MNT_NODEV)) {
+		return -EPERM;
+	}
+	if ((mnt->mnt.mnt_flags & MNT_LOCK_NOSUID) &&
+	    !(mnt_flags & MNT_NOSUID)) {
+		return -EPERM;
+	}
+	if ((mnt->mnt.mnt_flags & MNT_LOCK_NOEXEC) &&
+	    !(mnt_flags & MNT_NOEXEC)) {
+		return -EPERM;
+	}
+	if ((mnt->mnt.mnt_flags & MNT_LOCK_ATIME) &&
+	    ((mnt->mnt.mnt_flags & MNT_ATIME_MASK) != (mnt_flags & MNT_ATIME_MASK))) {
+		return -EPERM;
+	}
+
 	err = security_sb_remount(sb, data);
 	if (err)
 		return err;
@@ -1928,7 +1990,7 @@ static int do_remount(struct path *path, int flags, int mnt_flags,
 		err = do_remount_sb(sb, flags, data, 0);
 	if (!err) {
 		lock_mount_hash();
-		mnt_flags |= mnt->mnt.mnt_flags & MNT_PROPAGATION_MASK;
+		mnt_flags |= mnt->mnt.mnt_flags & ~MNT_USER_SETTABLE_MASK;
 		mnt->mnt.mnt_flags = mnt_flags;
 		touch_mnt_namespace(mnt->mnt_ns);
 		unlock_mount_hash();
@@ -2113,7 +2175,7 @@ static int do_new_mount(struct path *path, const char *fstype, int flags,
 		 */
 		if (!(type->fs_flags & FS_USERNS_DEV_MOUNT)) {
 			flags |= MS_NODEV;
-			mnt_flags |= MNT_NODEV;
+			mnt_flags |= MNT_NODEV | MNT_LOCK_NODEV;
 		}
 	}
 
@@ -2427,6 +2489,14 @@ long do_mount(const char *dev_name, const char *dir_name,
 	if (flags & MS_RDONLY)
 		mnt_flags |= MNT_READONLY;
 
+	/* The default atime for remount is preservation */
+	if ((flags & MS_REMOUNT) &&
+	    ((flags & (MS_NOATIME | MS_NODIRATIME | MS_RELATIME |
+		       MS_STRICTATIME)) == 0)) {
+		mnt_flags &= ~MNT_ATIME_MASK;
+		mnt_flags |= path.mnt->mnt_flags & MNT_ATIME_MASK;
+	}
+
 	flags &= ~(MS_NOSUID | MS_NOEXEC | MS_NODEV | MS_ACTIVE | MS_BORN |
 		   MS_NOATIME | MS_NODIRATIME | MS_RELATIME| MS_KERNMOUNT |
 		   MS_STRICTATIME);
diff --git a/fs/pnode.c b/fs/pnode.c
index a364a704333b..b7f831089500 100644
--- a/fs/pnode.c
+++ b/fs/pnode.c
@@ -381,6 +381,7 @@ static void __propagate_umount(struct mount *mnt)
 		 * other children
 		 */
 		if (child && list_empty(&child->mnt_mounts)) {
+			list_del_init(&child->mnt_child);
 			hlist_del_init_rcu(&child->mnt_hash);
 			hlist_add_before_rcu(&child->mnt_hash, &mnt->mnt_hash);
 		}
diff --git a/fs/proc/array.c b/fs/proc/array.c
index 656e401794de..baf3464bbce0 100644
--- a/fs/proc/array.c
+++ b/fs/proc/array.c
@@ -297,15 +297,11 @@ static void render_cap_t(struct seq_file *m, const char *header,
 	seq_puts(m, header);
 	CAP_FOR_EACH_U32(__capi) {
 		seq_printf(m, "%08x",
-			   a->cap[(_KERNEL_CAPABILITY_U32S-1) - __capi]);
+			   a->cap[CAP_LAST_U32 - __capi]);
 	}
 	seq_putc(m, '\n');
 }
 
-/* Remove non-existent capabilities */
-#define NORM_CAPS(v) (v.cap[CAP_TO_INDEX(CAP_LAST_CAP)] &= \
-				CAP_TO_MASK(CAP_LAST_CAP + 1) - 1)
-
 static inline void task_cap(struct seq_file *m, struct task_struct *p)
 {
 	const struct cred *cred;
@@ -319,11 +315,6 @@ static inline void task_cap(struct seq_file *m, struct task_struct *p)
 	cap_bset	= cred->cap_bset;
 	rcu_read_unlock();
 
-	NORM_CAPS(cap_inheritable);
-	NORM_CAPS(cap_permitted);
-	NORM_CAPS(cap_effective);
-	NORM_CAPS(cap_bset);
-
 	render_cap_t(m, "CapInh:\t", &cap_inheritable);
 	render_cap_t(m, "CapPrm:\t", &cap_permitted);
 	render_cap_t(m, "CapEff:\t", &cap_effective);
diff --git a/fs/xfs/xfs_aops.c b/fs/xfs/xfs_aops.c
index db2cfb067d0b..5d2518b24cea 100644
--- a/fs/xfs/xfs_aops.c
+++ b/fs/xfs/xfs_aops.c
@@ -1660,11 +1660,72 @@ xfs_vm_readpages(
 	return mpage_readpages(mapping, pages, nr_pages, xfs_get_blocks);
 }
 
+/*
+ * This is basically a copy of __set_page_dirty_buffers() with one
+ * small tweak: buffers beyond EOF do not get marked dirty. If we mark them
+ * dirty, we'll never be able to clean them because we don't write buffers
+ * beyond EOF, and that means we can't invalidate pages that span EOF
+ * that have been marked dirty. Further, the dirty state can leak into
+ * the file interior if the file is extended, resulting in all sorts of
+ * bad things happening as the state does not match the underlying data.
+ *
+ * XXX: this really indicates that bufferheads in XFS need to die. Warts like
+ * this only exist because of bufferheads and how the generic code manages them.
+ */
+STATIC int
+xfs_vm_set_page_dirty(
+	struct page		*page)
+{
+	struct address_space	*mapping = page->mapping;
+	struct inode		*inode = mapping->host;
+	loff_t			end_offset;
+	loff_t			offset;
+	int			newly_dirty;
+
+	if (unlikely(!mapping))
+		return !TestSetPageDirty(page);
+
+	end_offset = i_size_read(inode);
+	offset = page_offset(page);
+
+	spin_lock(&mapping->private_lock);
+	if (page_has_buffers(page)) {
+		struct buffer_head *head = page_buffers(page);
+		struct buffer_head *bh = head;
+
+		do {
+			if (offset < end_offset)
+				set_buffer_dirty(bh);
+			bh = bh->b_this_page;
+			offset += 1 << inode->i_blkbits;
+		} while (bh != head);
+	}
+	newly_dirty = !TestSetPageDirty(page);
+	spin_unlock(&mapping->private_lock);
+
+	if (newly_dirty) {
+		/* sigh - __set_page_dirty() is static, so copy it here, too */
+		unsigned long flags;
+
+		spin_lock_irqsave(&mapping->tree_lock, flags);
+		if (page->mapping) {	/* Race with truncate? */
+			WARN_ON_ONCE(!PageUptodate(page));
+			account_page_dirtied(page, mapping);
+			radix_tree_tag_set(&mapping->page_tree,
+					page_index(page), PAGECACHE_TAG_DIRTY);
+		}
+		spin_unlock_irqrestore(&mapping->tree_lock, flags);
+		__mark_inode_dirty(mapping->host, I_DIRTY_PAGES);
+	}
+	return newly_dirty;
+}
+
 const struct address_space_operations xfs_address_space_operations = {
 	.readpage		= xfs_vm_readpage,
 	.readpages		= xfs_vm_readpages,
 	.writepage		= xfs_vm_writepage,
 	.writepages		= xfs_vm_writepages,
+	.set_page_dirty		= xfs_vm_set_page_dirty,
 	.releasepage		= xfs_vm_releasepage,
 	.invalidatepage		= xfs_vm_invalidatepage,
 	.write_begin		= xfs_vm_write_begin,
diff --git a/fs/xfs/xfs_dquot.c b/fs/xfs/xfs_dquot.c
index 7aeb4c895b32..95f94483c3d7 100644
--- a/fs/xfs/xfs_dquot.c
+++ b/fs/xfs/xfs_dquot.c
@@ -1011,7 +1011,8 @@ xfs_qm_dqflush(
 	 * Get the buffer containing the on-disk dquot
 	 */
 	error = xfs_trans_read_buf(mp, NULL, mp->m_ddev_targp, dqp->q_blkno,
-				   mp->m_quotainfo->qi_dqchunklen, 0, &bp, NULL);
+				   mp->m_quotainfo->qi_dqchunklen, 0, &bp,
+				   &xfs_dquot_buf_ops);
 	if (error)
 		goto out_unlock;
 
diff --git a/fs/xfs/xfs_file.c b/fs/xfs/xfs_file.c
index 64b48eade91d..f50def6018a9 100644
--- a/fs/xfs/xfs_file.c
+++ b/fs/xfs/xfs_file.c
@@ -302,7 +302,16 @@ xfs_file_aio_read(
 				xfs_rw_iunlock(ip, XFS_IOLOCK_EXCL);
 				return ret;
 			}
-			truncate_pagecache_range(VFS_I(ip), pos, -1);
+
+			/*
+			 * Invalidate whole pages. This can return an error if
+			 * we fail to invalidate a page, but this should never
+			 * happen on XFS. Warn if it does fail.
+			 */
+			ret = invalidate_inode_pages2_range(VFS_I(ip)->i_mapping,
+						pos >> PAGE_CACHE_SHIFT, -1);
+			WARN_ON_ONCE(ret);
+			ret = 0;
 		}
 		xfs_rw_ilock_demote(ip, XFS_IOLOCK_EXCL);
 	}
@@ -683,7 +692,15 @@ xfs_file_dio_aio_write(
 						    pos, -1);
 		if (ret)
 			goto out;
-		truncate_pagecache_range(VFS_I(ip), pos, -1);
+		/*
+		 * Invalidate whole pages. This can return an error if
+		 * we fail to invalidate a page, but this should never
+		 * happen on XFS. Warn if it does fail.
+		 */
+		ret = invalidate_inode_pages2_range(VFS_I(ip)->i_mapping,
+						pos >> PAGE_CACHE_SHIFT, -1);
+		WARN_ON_ONCE(ret);
+		ret = 0;
 	}
 
 	/*
diff --git a/fs/xfs/xfs_log_recover.c b/fs/xfs/xfs_log_recover.c
index bce53ac81096..eb26418814fe 100644
--- a/fs/xfs/xfs_log_recover.c
+++ b/fs/xfs/xfs_log_recover.c
@@ -2125,6 +2125,17 @@ xlog_recover_validate_buf_type(
 	__uint16_t		magic16;
 	__uint16_t		magicda;
 
+	/*
+	 * We can only do post recovery validation on items on CRC enabled
+	 * fielsystems as we need to know when the buffer was written to be able
+	 * to determine if we should have replayed the item. If we replay old
+	 * metadata over a newer buffer, then it will enter a temporarily
+	 * inconsistent state resulting in verification failures. Hence for now
+	 * just avoid the verification stage for non-crc filesystems
+	 */
+	if (!xfs_sb_version_hascrc(&mp->m_sb))
+		return;
+
 	magic32 = be32_to_cpu(*(__be32 *)bp->b_addr);
 	magic16 = be16_to_cpu(*(__be16*)bp->b_addr);
 	magicda = be16_to_cpu(info->magic);
@@ -2160,8 +2171,6 @@ xlog_recover_validate_buf_type(
 		bp->b_ops = &xfs_agf_buf_ops;
 		break;
 	case XFS_BLFT_AGFL_BUF:
-		if (!xfs_sb_version_hascrc(&mp->m_sb))
-			break;
 		if (magic32 != XFS_AGFL_MAGIC) {
 			xfs_warn(mp, "Bad AGFL block magic!");
 			ASSERT(0);
@@ -2194,10 +2203,6 @@ xlog_recover_validate_buf_type(
 #endif
 		break;
 	case XFS_BLFT_DINO_BUF:
-		/*
-		 * we get here with inode allocation buffers, not buffers that
-		 * track unlinked list changes.
-		 */
 		if (magic16 != XFS_DINODE_MAGIC) {
 			xfs_warn(mp, "Bad INODE block magic!");
 			ASSERT(0);
@@ -2277,8 +2282,6 @@ xlog_recover_validate_buf_type(
 		bp->b_ops = &xfs_attr3_leaf_buf_ops;
 		break;
 	case XFS_BLFT_ATTR_RMT_BUF:
-		if (!xfs_sb_version_hascrc(&mp->m_sb))
-			break;
 		if (magic32 != XFS_ATTR3_RMT_MAGIC) {
 			xfs_warn(mp, "Bad attr remote magic!");
 			ASSERT(0);
@@ -2385,16 +2388,7 @@ xlog_recover_do_reg_buffer(
 	/* Shouldn't be any more regions */
 	ASSERT(i == item->ri_total);
 
-	/*
-	 * We can only do post recovery validation on items on CRC enabled
-	 * fielsystems as we need to know when the buffer was written to be able
-	 * to determine if we should have replayed the item. If we replay old
-	 * metadata over a newer buffer, then it will enter a temporarily
-	 * inconsistent state resulting in verification failures. Hence for now
-	 * just avoid the verification stage for non-crc filesystems
-	 */
-	if (xfs_sb_version_hascrc(&mp->m_sb))
-		xlog_recover_validate_buf_type(mp, bp, buf_f);
+	xlog_recover_validate_buf_type(mp, bp, buf_f);
 }
 
 /*
@@ -2502,12 +2496,29 @@ xlog_recover_buffer_pass2(
 	}
 
 	/*
-	 * recover the buffer only if we get an LSN from it and it's less than
+	 * Recover the buffer only if we get an LSN from it and it's less than
 	 * the lsn of the transaction we are replaying.
+	 *
+	 * Note that we have to be extremely careful of readahead here.
+	 * Readahead does not attach verfiers to the buffers so if we don't
+	 * actually do any replay after readahead because of the LSN we found
+	 * in the buffer if more recent than that current transaction then we
+	 * need to attach the verifier directly. Failure to do so can lead to
+	 * future recovery actions (e.g. EFI and unlinked list recovery) can
+	 * operate on the buffers and they won't get the verifier attached. This
+	 * can lead to blocks on disk having the correct content but a stale
+	 * CRC.
+	 *
+	 * It is safe to assume these clean buffers are currently up to date.
+	 * If the buffer is dirtied by a later transaction being replayed, then
+	 * the verifier will be reset to match whatever recover turns that
+	 * buffer into.
 	 */
 	lsn = xlog_recover_get_buf_lsn(mp, bp);
-	if (lsn && lsn != -1 && XFS_LSN_CMP(lsn, current_lsn) >= 0)
+	if (lsn && lsn != -1 && XFS_LSN_CMP(lsn, current_lsn) >= 0) {
+		xlog_recover_validate_buf_type(mp, bp, buf_f);
 		goto out_release;
+	}
 
 	if (buf_f->blf_flags & XFS_BLF_INODE_BUF) {
 		error = xlog_recover_do_inode_buffer(mp, item, bp, buf_f);
diff --git a/fs/xfs/xfs_qm.c b/fs/xfs/xfs_qm.c
index 348e4d2ed6e6..6d7d1de13403 100644
--- a/fs/xfs/xfs_qm.c
+++ b/fs/xfs/xfs_qm.c
@@ -1176,6 +1176,12 @@ xfs_qm_dqiter_bufs(
 		if (error)
 			break;
 
+		/*
+		 * A corrupt buffer might not have a verifier attached, so
+		 * make sure we have the correct one attached before writeback
+		 * occurs.
+		 */
+		bp->b_ops = &xfs_dquot_buf_ops;
 		xfs_qm_reset_dqcounts(mp, bp, firstid, type);
 		xfs_buf_delwri_queue(bp, buffer_list);
 		xfs_buf_relse(bp);
@@ -1261,7 +1267,7 @@ xfs_qm_dqiterate(
 					xfs_buf_readahead(mp->m_ddev_targp,
 					       XFS_FSB_TO_DADDR(mp, rablkno),
 					       mp->m_quotainfo->qi_dqchunklen,
-					       NULL);
+					       &xfs_dquot_buf_ops);
 					rablkno++;
 				}
 			}
diff --git a/include/acpi/acpi_bus.h b/include/acpi/acpi_bus.h
index 8256eb4ad057..e9c4f190ffae 100644
--- a/include/acpi/acpi_bus.h
+++ b/include/acpi/acpi_bus.h
@@ -228,7 +228,6 @@ struct acpi_device_pnp {
 	acpi_device_name device_name;	/* Driver-determined */
 	acpi_device_class device_class;	/*        "          */
 	union acpi_object *str_obj;	/* unicode string for _STR method */
-	unsigned long sun;		/* _SUN */
 };
 
 #define acpi_device_bid(d)	((d)->pnp.bus_id)
diff --git a/include/linux/capability.h b/include/linux/capability.h
index 84b13ad67c1c..aa93e5ef594c 100644
--- a/include/linux/capability.h
+++ b/include/linux/capability.h
@@ -78,8 +78,11 @@ extern const kernel_cap_t __cap_init_eff_set;
 # error Fix up hand-coded capability macro initializers
 #else /* HAND-CODED capability initializers */
 
+#define CAP_LAST_U32			((_KERNEL_CAPABILITY_U32S) - 1)
+#define CAP_LAST_U32_VALID_MASK		(CAP_TO_MASK(CAP_LAST_CAP + 1) -1)
+
 # define CAP_EMPTY_SET    ((kernel_cap_t){{ 0, 0 }})
-# define CAP_FULL_SET     ((kernel_cap_t){{ ~0, ~0 }})
+# define CAP_FULL_SET     ((kernel_cap_t){{ ~0, CAP_LAST_U32_VALID_MASK }})
 # define CAP_FS_SET       ((kernel_cap_t){{ CAP_FS_MASK_B0 \
 				    | CAP_TO_MASK(CAP_LINUX_IMMUTABLE), \
 				    CAP_FS_MASK_B1 } })
diff --git a/include/linux/dcache.h b/include/linux/dcache.h
index bf72e9ac6de0..3b50cac7ccb3 100644
--- a/include/linux/dcache.h
+++ b/include/linux/dcache.h
@@ -429,7 +429,7 @@ static inline unsigned __d_entry_type(const struct dentry *dentry)
 	return dentry->d_flags & DCACHE_ENTRY_TYPE;
 }
 
-static inline bool d_is_directory(const struct dentry *dentry)
+static inline bool d_can_lookup(const struct dentry *dentry)
 {
 	return __d_entry_type(dentry) == DCACHE_DIRECTORY_TYPE;
 }
@@ -439,6 +439,11 @@ static inline bool d_is_autodir(const struct dentry *dentry)
 	return __d_entry_type(dentry) == DCACHE_AUTODIR_TYPE;
 }
 
+static inline bool d_is_dir(const struct dentry *dentry)
+{
+	return d_can_lookup(dentry) || d_is_autodir(dentry);
+}
+
 static inline bool d_is_symlink(const struct dentry *dentry)
 {
 	return __d_entry_type(dentry) == DCACHE_SYMLINK_TYPE;
diff --git a/include/linux/mount.h b/include/linux/mount.h
index 839bac270904..b0c1e6574e7f 100644
--- a/include/linux/mount.h
+++ b/include/linux/mount.h
@@ -42,13 +42,20 @@ struct mnt_namespace;
  * flag, consider how it interacts with shared mounts.
  */
 #define MNT_SHARED_MASK	(MNT_UNBINDABLE)
-#define MNT_PROPAGATION_MASK	(MNT_SHARED | MNT_UNBINDABLE)
+#define MNT_USER_SETTABLE_MASK  (MNT_NOSUID | MNT_NODEV | MNT_NOEXEC \
+				 | MNT_NOATIME | MNT_NODIRATIME | MNT_RELATIME \
+				 | MNT_READONLY)
+#define MNT_ATIME_MASK (MNT_NOATIME | MNT_NODIRATIME | MNT_RELATIME )
 
 #define MNT_INTERNAL_FLAGS (MNT_SHARED | MNT_WRITE_HOLD | MNT_INTERNAL | \
 			    MNT_DOOMED | MNT_SYNC_UMOUNT | MNT_MARKED)
 
 #define MNT_INTERNAL	0x4000
 
+#define MNT_LOCK_ATIME		0x040000
+#define MNT_LOCK_NOEXEC		0x080000
+#define MNT_LOCK_NOSUID		0x100000
+#define MNT_LOCK_NODEV		0x200000
 #define MNT_LOCK_READONLY	0x400000
 #define MNT_LOCKED		0x800000
 #define MNT_DOOMED		0x1000000
diff --git a/include/linux/tpm.h b/include/linux/tpm.h
index fff1d0976f80..8350c538b486 100644
--- a/include/linux/tpm.h
+++ b/include/linux/tpm.h
@@ -39,6 +39,9 @@ struct tpm_class_ops {
 	int (*send) (struct tpm_chip *chip, u8 *buf, size_t len);
 	void (*cancel) (struct tpm_chip *chip);
 	u8 (*status) (struct tpm_chip *chip);
+	bool (*update_timeouts)(struct tpm_chip *chip,
+				unsigned long *timeout_cap);
+
 };
 
 #if defined(CONFIG_TCG_TPM) || defined(CONFIG_TCG_TPM_MODULE)
diff --git a/include/scsi/scsi_device.h b/include/scsi/scsi_device.h
index b4f1effc9216..409fafb63f63 100644
--- a/include/scsi/scsi_device.h
+++ b/include/scsi/scsi_device.h
@@ -149,6 +149,7 @@ struct scsi_device {
 	unsigned skip_ms_page_8:1;	/* do not use MODE SENSE page 0x08 */
 	unsigned skip_ms_page_3f:1;	/* do not use MODE SENSE page 0x3f */
 	unsigned skip_vpd_pages:1;	/* do not read VPD pages */
+	unsigned try_vpd_pages:1;	/* attempt to read VPD pages */
 	unsigned use_192_bytes_for_3f:1; /* ask for 192 bytes from page 0x3f */
 	unsigned no_start_on_add:1;	/* do not issue start on add */
 	unsigned allow_restart:1; /* issue START_UNIT in error handler */
diff --git a/include/scsi/scsi_devinfo.h b/include/scsi/scsi_devinfo.h
index 447d2d7466fc..183eaab7c380 100644
--- a/include/scsi/scsi_devinfo.h
+++ b/include/scsi/scsi_devinfo.h
@@ -32,4 +32,9 @@
 #define BLIST_ATTACH_PQ3	0x1000000 /* Scan: Attach to PQ3 devices */
 #define BLIST_NO_DIF		0x2000000 /* Disable T10 PI (DIF) */
 #define BLIST_SKIP_VPD_PAGES	0x4000000 /* Ignore SBC-3 VPD pages */
+#define BLIST_SCSI3LUN		0x8000000 /* Scan more than 256 LUNs
+					     for sequential scan */
+#define BLIST_TRY_VPD_PAGES	0x10000000 /* Attempt to read VPD pages */
+#define BLIST_NO_RSOC		0x20000000 /* don't try to issue RSOC */
+
 #endif
diff --git a/include/uapi/rdma/rdma_user_cm.h b/include/uapi/rdma/rdma_user_cm.h
index 99b80abf360a..3066718eb120 100644
--- a/include/uapi/rdma/rdma_user_cm.h
+++ b/include/uapi/rdma/rdma_user_cm.h
@@ -34,6 +34,7 @@
 #define RDMA_USER_CM_H
 
 #include <linux/types.h>
+#include <linux/socket.h>
 #include <linux/in6.h>
 #include <rdma/ib_user_verbs.h>
 #include <rdma/ib_user_sa.h>
diff --git a/kernel/audit.c b/kernel/audit.c
index 0c9dc860cc15..2c0ecd1753de 100644
--- a/kernel/audit.c
+++ b/kernel/audit.c
@@ -1628,7 +1628,7 @@ void audit_log_cap(struct audit_buffer *ab, char *prefix, kernel_cap_t *cap)
 	audit_log_format(ab, " %s=", prefix);
 	CAP_FOR_EACH_U32(i) {
 		audit_log_format(ab, "%08x",
-				 cap->cap[(_KERNEL_CAPABILITY_U32S-1) - i]);
+				 cap->cap[CAP_LAST_U32 - i]);
 	}
 }
 
diff --git a/kernel/capability.c b/kernel/capability.c
index 1191a44786df..00adb2193d01 100644
--- a/kernel/capability.c
+++ b/kernel/capability.c
@@ -268,6 +268,10 @@ SYSCALL_DEFINE2(capset, cap_user_header_t, header, const cap_user_data_t, data)
 		i++;
 	}
 
+	effective.cap[CAP_LAST_U32] &= CAP_LAST_U32_VALID_MASK;
+	permitted.cap[CAP_LAST_U32] &= CAP_LAST_U32_VALID_MASK;
+	inheritable.cap[CAP_LAST_U32] &= CAP_LAST_U32_VALID_MASK;
+
 	new = prepare_creds();
 	if (!new)
 		return -ENOMEM;
diff --git a/kernel/smp.c b/kernel/smp.c
index ffee35bef179..ff87d4479558 100644
--- a/kernel/smp.c
+++ b/kernel/smp.c
@@ -617,7 +617,7 @@ void on_each_cpu_cond(bool (*cond_func)(int cpu, void *info),
 			if (cond_func(cpu, info)) {
 				ret = smp_call_function_single(cpu, func,
 								info, wait);
-				WARN_ON_ONCE(!ret);
+				WARN_ON_ONCE(ret);
 			}
 		preempt_enable();
 	}
diff --git a/kernel/trace/ring_buffer.c b/kernel/trace/ring_buffer.c
index 0954450df7dc..a53f1bbc546b 100644
--- a/kernel/trace/ring_buffer.c
+++ b/kernel/trace/ring_buffer.c
@@ -1981,7 +1981,7 @@ rb_add_time_stamp(struct ring_buffer_event *event, u64 delta)
 
 /**
  * rb_update_event - update event type and data
- * @event: the even to update
+ * @event: the event to update
  * @type: the type of event
  * @length: the size of the event field in the ring buffer
  *
@@ -3354,21 +3354,16 @@ static void rb_iter_reset(struct ring_buffer_iter *iter)
 	struct ring_buffer_per_cpu *cpu_buffer = iter->cpu_buffer;
 
 	/* Iterator usage is expected to have record disabled */
-	if (list_empty(&cpu_buffer->reader_page->list)) {
-		iter->head_page = rb_set_head_page(cpu_buffer);
-		if (unlikely(!iter->head_page))
-			return;
-		iter->head = iter->head_page->read;
-	} else {
-		iter->head_page = cpu_buffer->reader_page;
-		iter->head = cpu_buffer->reader_page->read;
-	}
+	iter->head_page = cpu_buffer->reader_page;
+	iter->head = cpu_buffer->reader_page->read;
+
+	iter->cache_reader_page = iter->head_page;
+	iter->cache_read = iter->head;
+
 	if (iter->head)
 		iter->read_stamp = cpu_buffer->read_stamp;
 	else
 		iter->read_stamp = iter->head_page->page->time_stamp;
-	iter->cache_reader_page = cpu_buffer->reader_page;
-	iter->cache_read = cpu_buffer->read;
 }
 
 /**
@@ -3761,12 +3756,14 @@ rb_iter_peek(struct ring_buffer_iter *iter, u64 *ts)
 		return NULL;
 
 	/*
-	 * We repeat when a time extend is encountered.
-	 * Since the time extend is always attached to a data event,
-	 * we should never loop more than once.
-	 * (We never hit the following condition more than twice).
+	 * We repeat when a time extend is encountered or we hit
+	 * the end of the page. Since the time extend is always attached
+	 * to a data event, we should never loop more than three times.
+	 * Once for going to next page, once on time extend, and
+	 * finally once to get the event.
+	 * (We never hit the following condition more than thrice).
 	 */
-	if (RB_WARN_ON(cpu_buffer, ++nr_loops > 2))
+	if (RB_WARN_ON(cpu_buffer, ++nr_loops > 3))
 		return NULL;
 
 	if (rb_per_cpu_empty(cpu_buffer))
diff --git a/lib/assoc_array.c b/lib/assoc_array.c
index c0b1007011e1..2404d03e251a 100644
--- a/lib/assoc_array.c
+++ b/lib/assoc_array.c
@@ -1723,11 +1723,13 @@ ascend_old_tree:
 		shortcut = assoc_array_ptr_to_shortcut(ptr);
 		slot = shortcut->parent_slot;
 		cursor = shortcut->back_pointer;
+		if (!cursor)
+			goto gc_complete;
 	} else {
 		slot = node->parent_slot;
 		cursor = ptr;
 	}
-	BUG_ON(!ptr);
+	BUG_ON(!cursor);
 	node = assoc_array_ptr_to_node(cursor);
 	slot++;
 	goto continue_node;
@@ -1735,7 +1737,7 @@ ascend_old_tree:
 gc_complete:
 	edit->set[0].to = new_root;
 	assoc_array_apply_edit(edit);
-	edit->array->nr_leaves_on_tree = nr_leaves_on_tree;
+	array->nr_leaves_on_tree = nr_leaves_on_tree;
 	return 0;
 
 enomem:
diff --git a/net/bluetooth/l2cap_sock.c b/net/bluetooth/l2cap_sock.c
index 27ae84154586..06a7a769737f 100644
--- a/net/bluetooth/l2cap_sock.c
+++ b/net/bluetooth/l2cap_sock.c
@@ -1112,7 +1112,8 @@ static int l2cap_sock_shutdown(struct socket *sock, int how)
 		l2cap_chan_close(chan, 0);
 		lock_sock(sk);
 
-		if (sock_flag(sk, SOCK_LINGER) && sk->sk_lingertime)
+		if (sock_flag(sk, SOCK_LINGER) && sk->sk_lingertime &&
+		    !(current->flags & PF_EXITING))
 			err = bt_sock_wait_state(sk, BT_CLOSED,
 						 sk->sk_lingertime);
 	}
diff --git a/net/bluetooth/rfcomm/core.c b/net/bluetooth/rfcomm/core.c
index facd8a79c038..b08865111024 100644
--- a/net/bluetooth/rfcomm/core.c
+++ b/net/bluetooth/rfcomm/core.c
@@ -1859,10 +1859,13 @@ static struct rfcomm_session *rfcomm_process_rx(struct rfcomm_session *s)
 	/* Get data directly from socket receive queue without copying it. */
 	while ((skb = skb_dequeue(&sk->sk_receive_queue))) {
 		skb_orphan(skb);
-		if (!skb_linearize(skb))
+		if (!skb_linearize(skb)) {
 			s = rfcomm_recv_frame(s, skb);
-		else
+			if (!s)
+				break;
+		} else {
 			kfree_skb(skb);
+		}
 	}
 
 	if (s && (sk->sk_state == BT_CLOSED))
diff --git a/net/bluetooth/rfcomm/sock.c b/net/bluetooth/rfcomm/sock.c
index 3c2d3e4aa2f5..a0050de6f1f1 100644
--- a/net/bluetooth/rfcomm/sock.c
+++ b/net/bluetooth/rfcomm/sock.c
@@ -898,7 +898,8 @@ static int rfcomm_sock_shutdown(struct socket *sock, int how)
 		sk->sk_shutdown = SHUTDOWN_MASK;
 		__rfcomm_sock_close(sk);
 
-		if (sock_flag(sk, SOCK_LINGER) && sk->sk_lingertime)
+		if (sock_flag(sk, SOCK_LINGER) && sk->sk_lingertime &&
+		    !(current->flags & PF_EXITING))
 			err = bt_sock_wait_state(sk, BT_CLOSED, sk->sk_lingertime);
 	}
 	release_sock(sk);
diff --git a/net/bluetooth/sco.c b/net/bluetooth/sco.c
index 24fa3964b3c8..316dd4e0af39 100644
--- a/net/bluetooth/sco.c
+++ b/net/bluetooth/sco.c
@@ -909,7 +909,8 @@ static int sco_sock_shutdown(struct socket *sock, int how)
 		sco_sock_clear_timer(sk);
 		__sco_sock_close(sk);
 
-		if (sock_flag(sk, SOCK_LINGER) && sk->sk_lingertime)
+		if (sock_flag(sk, SOCK_LINGER) && sk->sk_lingertime &&
+		    !(current->flags & PF_EXITING))
 			err = bt_sock_wait_state(sk, BT_CLOSED,
 						 sk->sk_lingertime);
 	}
@@ -929,7 +930,8 @@ static int sco_sock_release(struct socket *sock)
 
 	sco_sock_close(sk);
 
-	if (sock_flag(sk, SOCK_LINGER) && sk->sk_lingertime) {
+	if (sock_flag(sk, SOCK_LINGER) && sk->sk_lingertime &&
+	    !(current->flags & PF_EXITING)) {
 		lock_sock(sk);
 		err = bt_sock_wait_state(sk, BT_CLOSED, sk->sk_lingertime);
 		release_sock(sk);
diff --git a/net/ceph/auth_x.c b/net/ceph/auth_x.c
index 96238ba95f2b..de6662b14e1f 100644
--- a/net/ceph/auth_x.c
+++ b/net/ceph/auth_x.c
@@ -13,8 +13,6 @@
 #include "auth_x.h"
 #include "auth_x_protocol.h"
 
-#define TEMP_TICKET_BUF_LEN	256
-
 static void ceph_x_validate_tickets(struct ceph_auth_client *ac, int *pneed);
 
 static int ceph_x_is_authenticated(struct ceph_auth_client *ac)
@@ -64,7 +62,7 @@ static int ceph_x_encrypt(struct ceph_crypto_key *secret,
 }
 
 static int ceph_x_decrypt(struct ceph_crypto_key *secret,
-			  void **p, void *end, void *obuf, size_t olen)
+			  void **p, void *end, void **obuf, size_t olen)
 {
 	struct ceph_x_encrypt_header head;
 	size_t head_len = sizeof(head);
@@ -75,8 +73,14 @@ static int ceph_x_decrypt(struct ceph_crypto_key *secret,
 		return -EINVAL;
 
 	dout("ceph_x_decrypt len %d\n", len);
-	ret = ceph_decrypt2(secret, &head, &head_len, obuf, &olen,
-			    *p, len);
+	if (*obuf == NULL) {
+		*obuf = kmalloc(len, GFP_NOFS);
+		if (!*obuf)
+			return -ENOMEM;
+		olen = len;
+	}
+
+	ret = ceph_decrypt2(secret, &head, &head_len, *obuf, &olen, *p, len);
 	if (ret)
 		return ret;
 	if (head.struct_v != 1 || le64_to_cpu(head.magic) != CEPHX_ENC_MAGIC)
@@ -129,139 +133,120 @@ static void remove_ticket_handler(struct ceph_auth_client *ac,
 	kfree(th);
 }
 
-static int ceph_x_proc_ticket_reply(struct ceph_auth_client *ac,
-				    struct ceph_crypto_key *secret,
-				    void *buf, void *end)
+static int process_one_ticket(struct ceph_auth_client *ac,
+			      struct ceph_crypto_key *secret,
+			      void **p, void *end)
 {
 	struct ceph_x_info *xi = ac->private;
-	int num;
-	void *p = buf;
+	int type;
+	u8 tkt_struct_v, blob_struct_v;
+	struct ceph_x_ticket_handler *th;
+	void *dbuf = NULL;
+	void *dp, *dend;
+	int dlen;
+	char is_enc;
+	struct timespec validity;
+	struct ceph_crypto_key old_key;
+	void *ticket_buf = NULL;
+	void *tp, *tpend;
+	struct ceph_timespec new_validity;
+	struct ceph_crypto_key new_session_key;
+	struct ceph_buffer *new_ticket_blob;
+	unsigned long new_expires, new_renew_after;
+	u64 new_secret_id;
 	int ret;
-	char *dbuf;
-	char *ticket_buf;
-	u8 reply_struct_v;
 
-	dbuf = kmalloc(TEMP_TICKET_BUF_LEN, GFP_NOFS);
-	if (!dbuf)
-		return -ENOMEM;
+	ceph_decode_need(p, end, sizeof(u32) + 1, bad);
 
-	ret = -ENOMEM;
-	ticket_buf = kmalloc(TEMP_TICKET_BUF_LEN, GFP_NOFS);
-	if (!ticket_buf)
-		goto out_dbuf;
+	type = ceph_decode_32(p);
+	dout(" ticket type %d %s\n", type, ceph_entity_type_name(type));
 
-	ceph_decode_need(&p, end, 1 + sizeof(u32), bad);
-	reply_struct_v = ceph_decode_8(&p);
-	if (reply_struct_v != 1)
+	tkt_struct_v = ceph_decode_8(p);
+	if (tkt_struct_v != 1)
 		goto bad;
-	num = ceph_decode_32(&p);
-	dout("%d tickets\n", num);
-	while (num--) {
-		int type;
-		u8 tkt_struct_v, blob_struct_v;
-		struct ceph_x_ticket_handler *th;
-		void *dp, *dend;
-		int dlen;
-		char is_enc;
-		struct timespec validity;
-		struct ceph_crypto_key old_key;
-		void *tp, *tpend;
-		struct ceph_timespec new_validity;
-		struct ceph_crypto_key new_session_key;
-		struct ceph_buffer *new_ticket_blob;
-		unsigned long new_expires, new_renew_after;
-		u64 new_secret_id;
-
-		ceph_decode_need(&p, end, sizeof(u32) + 1, bad);
-
-		type = ceph_decode_32(&p);
-		dout(" ticket type %d %s\n", type, ceph_entity_type_name(type));
-
-		tkt_struct_v = ceph_decode_8(&p);
-		if (tkt_struct_v != 1)
-			goto bad;
-
-		th = get_ticket_handler(ac, type);
-		if (IS_ERR(th)) {
-			ret = PTR_ERR(th);
-			goto out;
-		}
 
-		/* blob for me */
-		dlen = ceph_x_decrypt(secret, &p, end, dbuf,
-				      TEMP_TICKET_BUF_LEN);
-		if (dlen <= 0) {
-			ret = dlen;
-			goto out;
-		}
-		dout(" decrypted %d bytes\n", dlen);
-		dend = dbuf + dlen;
-		dp = dbuf;
+	th = get_ticket_handler(ac, type);
+	if (IS_ERR(th)) {
+		ret = PTR_ERR(th);
+		goto out;
+	}
 
-		tkt_struct_v = ceph_decode_8(&dp);
-		if (tkt_struct_v != 1)
-			goto bad;
+	/* blob for me */
+	dlen = ceph_x_decrypt(secret, p, end, &dbuf, 0);
+	if (dlen <= 0) {
+		ret = dlen;
+		goto out;
+	}
+	dout(" decrypted %d bytes\n", dlen);
+	dp = dbuf;
+	dend = dp + dlen;
 
-		memcpy(&old_key, &th->session_key, sizeof(old_key));
-		ret = ceph_crypto_key_decode(&new_session_key, &dp, dend);
-		if (ret)
-			goto out;
+	tkt_struct_v = ceph_decode_8(&dp);
+	if (tkt_struct_v != 1)
+		goto bad;
 
-		ceph_decode_copy(&dp, &new_validity, sizeof(new_validity));
-		ceph_decode_timespec(&validity, &new_validity);
-		new_expires = get_seconds() + validity.tv_sec;
-		new_renew_after = new_expires - (validity.tv_sec / 4);
-		dout(" expires=%lu renew_after=%lu\n", new_expires,
-		     new_renew_after);
+	memcpy(&old_key, &th->session_key, sizeof(old_key));
+	ret = ceph_crypto_key_decode(&new_session_key, &dp, dend);
+	if (ret)
+		goto out;
 
-		/* ticket blob for service */
-		ceph_decode_8_safe(&p, end, is_enc, bad);
-		tp = ticket_buf;
-		if (is_enc) {
-			/* encrypted */
-			dout(" encrypted ticket\n");
-			dlen = ceph_x_decrypt(&old_key, &p, end, ticket_buf,
-					      TEMP_TICKET_BUF_LEN);
-			if (dlen < 0) {
-				ret = dlen;
-				goto out;
-			}
-			dlen = ceph_decode_32(&tp);
-		} else {
-			/* unencrypted */
-			ceph_decode_32_safe(&p, end, dlen, bad);
-			ceph_decode_need(&p, end, dlen, bad);
-			ceph_decode_copy(&p, ticket_buf, dlen);
+	ceph_decode_copy(&dp, &new_validity, sizeof(new_validity));
+	ceph_decode_timespec(&validity, &new_validity);
+	new_expires = get_seconds() + validity.tv_sec;
+	new_renew_after = new_expires - (validity.tv_sec / 4);
+	dout(" expires=%lu renew_after=%lu\n", new_expires,
+	     new_renew_after);
+
+	/* ticket blob for service */
+	ceph_decode_8_safe(p, end, is_enc, bad);
+	if (is_enc) {
+		/* encrypted */
+		dout(" encrypted ticket\n");
+		dlen = ceph_x_decrypt(&old_key, p, end, &ticket_buf, 0);
+		if (dlen < 0) {
+			ret = dlen;
+			goto out;
 		}
-		tpend = tp + dlen;
-		dout(" ticket blob is %d bytes\n", dlen);
-		ceph_decode_need(&tp, tpend, 1 + sizeof(u64), bad);
-		blob_struct_v = ceph_decode_8(&tp);
-		new_secret_id = ceph_decode_64(&tp);
-		ret = ceph_decode_buffer(&new_ticket_blob, &tp, tpend);
-		if (ret)
+		tp = ticket_buf;
+		dlen = ceph_decode_32(&tp);
+	} else {
+		/* unencrypted */
+		ceph_decode_32_safe(p, end, dlen, bad);
+		ticket_buf = kmalloc(dlen, GFP_NOFS);
+		if (!ticket_buf) {
+			ret = -ENOMEM;
 			goto out;
-
-		/* all is well, update our ticket */
-		ceph_crypto_key_destroy(&th->session_key);
-		if (th->ticket_blob)
-			ceph_buffer_put(th->ticket_blob);
-		th->session_key = new_session_key;
-		th->ticket_blob = new_ticket_blob;
-		th->validity = new_validity;
-		th->secret_id = new_secret_id;
-		th->expires = new_expires;
-		th->renew_after = new_renew_after;
-		dout(" got ticket service %d (%s) secret_id %lld len %d\n",
-		     type, ceph_entity_type_name(type), th->secret_id,
-		     (int)th->ticket_blob->vec.iov_len);
-		xi->have_keys |= th->service;
+		}
+		tp = ticket_buf;
+		ceph_decode_need(p, end, dlen, bad);
+		ceph_decode_copy(p, ticket_buf, dlen);
 	}
+	tpend = tp + dlen;
+	dout(" ticket blob is %d bytes\n", dlen);
+	ceph_decode_need(&tp, tpend, 1 + sizeof(u64), bad);
+	blob_struct_v = ceph_decode_8(&tp);
+	new_secret_id = ceph_decode_64(&tp);
+	ret = ceph_decode_buffer(&new_ticket_blob, &tp, tpend);
+	if (ret)
+		goto out;
+
+	/* all is well, update our ticket */
+	ceph_crypto_key_destroy(&th->session_key);
+	if (th->ticket_blob)
+		ceph_buffer_put(th->ticket_blob);
+	th->session_key = new_session_key;
+	th->ticket_blob = new_ticket_blob;
+	th->validity = new_validity;
+	th->secret_id = new_secret_id;
+	th->expires = new_expires;
+	th->renew_after = new_renew_after;
+	dout(" got ticket service %d (%s) secret_id %lld len %d\n",
+	     type, ceph_entity_type_name(type), th->secret_id,
+	     (int)th->ticket_blob->vec.iov_len);
+	xi->have_keys |= th->service;
 
-	ret = 0;
 out:
 	kfree(ticket_buf);
-out_dbuf:
 	kfree(dbuf);
 	return ret;
 
@@ -270,6 +255,34 @@ bad:
 	goto out;
 }
 
+static int ceph_x_proc_ticket_reply(struct ceph_auth_client *ac,
+				    struct ceph_crypto_key *secret,
+				    void *buf, void *end)
+{
+	void *p = buf;
+	u8 reply_struct_v;
+	u32 num;
+	int ret;
+
+	ceph_decode_8_safe(&p, end, reply_struct_v, bad);
+	if (reply_struct_v != 1)
+		return -EINVAL;
+
+	ceph_decode_32_safe(&p, end, num, bad);
+	dout("%d tickets\n", num);
+
+	while (num--) {
+		ret = process_one_ticket(ac, secret, &p, end);
+		if (ret)
+			return ret;
+	}
+
+	return 0;
+
+bad:
+	return -EINVAL;
+}
+
 static int ceph_x_build_authorizer(struct ceph_auth_client *ac,
 				   struct ceph_x_ticket_handler *th,
 				   struct ceph_x_authorizer *au)
@@ -583,13 +596,14 @@ static int ceph_x_verify_authorizer_reply(struct ceph_auth_client *ac,
 	struct ceph_x_ticket_handler *th;
 	int ret = 0;
 	struct ceph_x_authorize_reply reply;
+	void *preply = &reply;
 	void *p = au->reply_buf;
 	void *end = p + sizeof(au->reply_buf);
 
 	th = get_ticket_handler(ac, au->service);
 	if (IS_ERR(th))
 		return PTR_ERR(th);
-	ret = ceph_x_decrypt(&th->session_key, &p, end, &reply, sizeof(reply));
+	ret = ceph_x_decrypt(&th->session_key, &p, end, &preply, sizeof(reply));
 	if (ret < 0)
 		return ret;
 	if (ret != sizeof(reply))
diff --git a/net/ceph/messenger.c b/net/ceph/messenger.c
index 988721a629eb..0a31298737ac 100644
--- a/net/ceph/messenger.c
+++ b/net/ceph/messenger.c
@@ -900,7 +900,7 @@ static void ceph_msg_data_pages_cursor_init(struct ceph_msg_data_cursor *cursor,
 	BUG_ON(page_count > (int)USHRT_MAX);
 	cursor->page_count = (unsigned short)page_count;
 	BUG_ON(length > SIZE_MAX - cursor->page_offset);
-	cursor->last_piece = (size_t)cursor->page_offset + length <= PAGE_SIZE;
+	cursor->last_piece = cursor->page_offset + cursor->resid <= PAGE_SIZE;
 }
 
 static struct page *
diff --git a/net/ceph/mon_client.c b/net/ceph/mon_client.c
index 2ac9ef35110b..dbcbf5a4707f 100644
--- a/net/ceph/mon_client.c
+++ b/net/ceph/mon_client.c
@@ -1041,7 +1041,15 @@ static struct ceph_msg *mon_alloc_msg(struct ceph_connection *con,
 	if (!m) {
 		pr_info("alloc_msg unknown type %d\n", type);
 		*skip = 1;
+	} else if (front_len > m->front_alloc_len) {
+		pr_warning("mon_alloc_msg front %d > prealloc %d (%u#%llu)\n",
+			   front_len, m->front_alloc_len,
+			   (unsigned int)con->peer_name.type,
+			   le64_to_cpu(con->peer_name.num));
+		ceph_msg_put(m);
+		m = ceph_msg_new(type, front_len, GFP_NOFS, false);
 	}
+
 	return m;
 }
 
diff --git a/security/commoncap.c b/security/commoncap.c
index b9d613e0ef14..963dc5981661 100644
--- a/security/commoncap.c
+++ b/security/commoncap.c
@@ -421,6 +421,9 @@ int get_vfs_caps_from_disk(const struct dentry *dentry, struct cpu_vfs_cap_data
 		cpu_caps->inheritable.cap[i] = le32_to_cpu(caps.data[i].inheritable);
 	}
 
+	cpu_caps->permitted.cap[CAP_LAST_U32] &= CAP_LAST_U32_VALID_MASK;
+	cpu_caps->inheritable.cap[CAP_LAST_U32] &= CAP_LAST_U32_VALID_MASK;
+
 	return 0;
 }
 
diff --git a/sound/soc/blackfin/bf5xx-i2s-pcm.c b/sound/soc/blackfin/bf5xx-i2s-pcm.c
index a3881c4381c9..bcf591373a7a 100644
--- a/sound/soc/blackfin/bf5xx-i2s-pcm.c
+++ b/sound/soc/blackfin/bf5xx-i2s-pcm.c
@@ -290,19 +290,19 @@ static int bf5xx_pcm_silence(struct snd_pcm_substream *substream,
 	unsigned int sample_size = runtime->sample_bits / 8;
 	void *buf = runtime->dma_area;
 	struct bf5xx_i2s_pcm_data *dma_data;
-	unsigned int offset, size;
+	unsigned int offset, samples;
 
 	dma_data = snd_soc_dai_get_dma_data(rtd->cpu_dai, substream);
 
 	if (dma_data->tdm_mode) {
 		offset = pos * 8 * sample_size;
-		size = count * 8 * sample_size;
+		samples = count * 8;
 	} else {
 		offset = frames_to_bytes(runtime, pos);
-		size = frames_to_bytes(runtime, count);
+		samples = count * runtime->channels;
 	}
 
-	snd_pcm_format_set_silence(runtime->format, buf + offset, size);
+	snd_pcm_format_set_silence(runtime->format, buf + offset, samples);
 
 	return 0;
 }
diff --git a/sound/soc/codecs/adau1701.c b/sound/soc/codecs/adau1701.c
index d71c59cf7bdd..370b742117ef 100644
--- a/sound/soc/codecs/adau1701.c
+++ b/sound/soc/codecs/adau1701.c
@@ -230,8 +230,10 @@ static int adau1701_reg_read(void *context, unsigned int reg,
 
 	*value = 0;
 
-	for (i = 0; i < size; i++)
-		*value |= recv_buf[i] << (i * 8);
+	for (i = 0; i < size; i++) {
+		*value <<= 8;
+		*value |= recv_buf[i];
+	}
 
 	return 0;
 }
diff --git a/sound/soc/codecs/max98090.c b/sound/soc/codecs/max98090.c
index b3f7c9026a29..ddfb0fddd030 100644
--- a/sound/soc/codecs/max98090.c
+++ b/sound/soc/codecs/max98090.c
@@ -2250,7 +2250,7 @@ static int max98090_probe(struct snd_soc_codec *codec)
 	/* Register for interrupts */
 	dev_dbg(codec->dev, "irq = %d\n", max98090->irq);
 
-	ret = request_threaded_irq(max98090->irq, NULL,
+	ret = devm_request_threaded_irq(codec->dev, max98090->irq, NULL,
 		max98090_interrupt, IRQF_TRIGGER_FALLING | IRQF_ONESHOT,
 		"max98090_interrupt", codec);
 	if (ret < 0) {
diff --git a/sound/soc/codecs/rt5640.c b/sound/soc/codecs/rt5640.c
index 886924934aa5..5cb515b08a32 100644
--- a/sound/soc/codecs/rt5640.c
+++ b/sound/soc/codecs/rt5640.c
@@ -2071,6 +2071,7 @@ static struct snd_soc_codec_driver soc_codec_dev_rt5640 = {
 static const struct regmap_config rt5640_regmap = {
 	.reg_bits = 8,
 	.val_bits = 16,
+	.use_single_rw = true,
 
 	.max_register = RT5640_VENDOR_ID2 + 1 + (ARRAY_SIZE(rt5640_ranges) *
 					       RT5640_PR_SPACING),
diff --git a/sound/soc/codecs/wm8994.c b/sound/soc/codecs/wm8994.c
index adb72063d44e..d98e52f647d2 100644
--- a/sound/soc/codecs/wm8994.c
+++ b/sound/soc/codecs/wm8994.c
@@ -3497,6 +3497,7 @@ static irqreturn_t wm8994_mic_irq(int irq, void *data)
 	return IRQ_HANDLED;
 }
 
+/* Should be called with accdet_lock held */
 static void wm1811_micd_stop(struct snd_soc_codec *codec)
 {
 	struct wm8994_priv *wm8994 = snd_soc_codec_get_drvdata(codec);
@@ -3504,14 +3505,10 @@ static void wm1811_micd_stop(struct snd_soc_codec *codec)
 	if (!wm8994->jackdet)
 		return;
 
-	mutex_lock(&wm8994->accdet_lock);
-
 	snd_soc_update_bits(codec, WM8958_MIC_DETECT_1, WM8958_MICD_ENA, 0);
 
 	wm1811_jackdet_set_mode(codec, WM1811_JACKDET_MODE_JACK);
 
-	mutex_unlock(&wm8994->accdet_lock);
-
 	if (wm8994->wm8994->pdata.jd_ext_cap)
 		snd_soc_dapm_disable_pin(&codec->dapm,
 					 "MICBIAS2");
@@ -3552,10 +3549,10 @@ static void wm8958_open_circuit_work(struct work_struct *work)
 						  open_circuit_work.work);
 	struct device *dev = wm8994->wm8994->dev;
 
-	wm1811_micd_stop(wm8994->hubs.codec);
-
 	mutex_lock(&wm8994->accdet_lock);
 
+	wm1811_micd_stop(wm8994->hubs.codec);
+
 	dev_dbg(dev, "Reporting open circuit\n");
 
 	wm8994->jack_mic = false;
diff --git a/sound/soc/codecs/wm_adsp.c b/sound/soc/codecs/wm_adsp.c
index 444626fcab40..53c03aff762e 100644
--- a/sound/soc/codecs/wm_adsp.c
+++ b/sound/soc/codecs/wm_adsp.c
@@ -1745,3 +1745,5 @@ int wm_adsp2_init(struct wm_adsp *adsp, bool dvfs)
 	return 0;
 }
 EXPORT_SYMBOL_GPL(wm_adsp2_init);
+
+MODULE_LICENSE("GPL v2");
diff --git a/sound/soc/pxa/pxa-ssp.c b/sound/soc/pxa/pxa-ssp.c
index a3119a00d8fa..6c6b35e471c8 100644
--- a/sound/soc/pxa/pxa-ssp.c
+++ b/sound/soc/pxa/pxa-ssp.c
@@ -725,7 +725,8 @@ static int pxa_ssp_probe(struct snd_soc_dai *dai)
 		ssp_handle = of_parse_phandle(dev->of_node, "port", 0);
 		if (!ssp_handle) {
 			dev_err(dev, "unable to get 'port' phandle\n");
-			return -ENODEV;
+			ret = -ENODEV;
+			goto err_priv;
 		}
 
 		priv->ssp = pxa_ssp_request_of(ssp_handle, "SoC audio");
@@ -766,9 +767,7 @@ static int pxa_ssp_remove(struct snd_soc_dai *dai)
 			  SNDRV_PCM_RATE_48000 | SNDRV_PCM_RATE_64000 |	\
 			  SNDRV_PCM_RATE_88200 | SNDRV_PCM_RATE_96000)
 
-#define PXA_SSP_FORMATS (SNDRV_PCM_FMTBIT_S16_LE |\
-			    SNDRV_PCM_FMTBIT_S24_LE |	\
-			    SNDRV_PCM_FMTBIT_S32_LE)
+#define PXA_SSP_FORMATS (SNDRV_PCM_FMTBIT_S16_LE | SNDRV_PCM_FMTBIT_S32_LE)
 
 static const struct snd_soc_dai_ops pxa_ssp_dai_ops = {
 	.startup	= pxa_ssp_startup,
diff --git a/sound/soc/samsung/i2s.c b/sound/soc/samsung/i2s.c
index 0a9b44c940ce..5dae66002a11 100644
--- a/sound/soc/samsung/i2s.c
+++ b/sound/soc/samsung/i2s.c
@@ -915,11 +915,9 @@ static int i2s_suspend(struct snd_soc_dai *dai)
 {
 	struct i2s_dai *i2s = to_info(dai);
 
-	if (dai->active) {
-		i2s->suspend_i2smod = readl(i2s->addr + I2SMOD);
-		i2s->suspend_i2scon = readl(i2s->addr + I2SCON);
-		i2s->suspend_i2spsr = readl(i2s->addr + I2SPSR);
-	}
+	i2s->suspend_i2smod = readl(i2s->addr + I2SMOD);
+	i2s->suspend_i2scon = readl(i2s->addr + I2SCON);
+	i2s->suspend_i2spsr = readl(i2s->addr + I2SPSR);
 
 	return 0;
 }
@@ -928,11 +926,9 @@ static int i2s_resume(struct snd_soc_dai *dai)
 {
 	struct i2s_dai *i2s = to_info(dai);
 
-	if (dai->active) {
-		writel(i2s->suspend_i2scon, i2s->addr + I2SCON);
-		writel(i2s->suspend_i2smod, i2s->addr + I2SMOD);
-		writel(i2s->suspend_i2spsr, i2s->addr + I2SPSR);
-	}
+	writel(i2s->suspend_i2scon, i2s->addr + I2SCON);
+	writel(i2s->suspend_i2smod, i2s->addr + I2SMOD);
+	writel(i2s->suspend_i2spsr, i2s->addr + I2SPSR);
 
 	return 0;
 }
diff --git a/sound/soc/soc-pcm.c b/sound/soc/soc-pcm.c
index 47e1ce771e65..02733ded2cb1 100644
--- a/sound/soc/soc-pcm.c
+++ b/sound/soc/soc-pcm.c
@@ -2011,6 +2011,7 @@ int soc_dpcm_runtime_update(struct snd_soc_card *card)
 			dpcm_be_disconnect(fe, SNDRV_PCM_STREAM_PLAYBACK);
 		}
 
+		dpcm_path_put(&list);
 capture:
 		/* skip if FE doesn't have capture capability */
 		if (!fe->cpu_dai->driver->capture.channels_min)
diff --git a/tools/testing/selftests/Makefile b/tools/testing/selftests/Makefile
index 32487ed18354..3d5979b23e50 100644
--- a/tools/testing/selftests/Makefile
+++ b/tools/testing/selftests/Makefile
@@ -4,6 +4,7 @@ TARGETS += efivarfs
 TARGETS += kcmp
 TARGETS += memory-hotplug
 TARGETS += mqueue
+TARGETS += mount
 TARGETS += net
 TARGETS += ptrace
 TARGETS += timers
diff --git a/tools/testing/selftests/mount/Makefile b/tools/testing/selftests/mount/Makefile
new file mode 100644
index 000000000000..337d853c2b72
--- /dev/null
+++ b/tools/testing/selftests/mount/Makefile
@@ -0,0 +1,17 @@
+# Makefile for mount selftests.
+
+all: unprivileged-remount-test
+
+unprivileged-remount-test: unprivileged-remount-test.c
+	gcc -Wall -O2 unprivileged-remount-test.c -o unprivileged-remount-test
+
+# Allow specific tests to be selected.
+test_unprivileged_remount: unprivileged-remount-test
+	@if [ -f /proc/self/uid_map ] ; then ./unprivileged-remount-test ; fi
+
+run_tests: all test_unprivileged_remount
+
+clean:
+	rm -f unprivileged-remount-test
+
+.PHONY: all test_unprivileged_remount
diff --git a/tools/testing/selftests/mount/unprivileged-remount-test.c b/tools/testing/selftests/mount/unprivileged-remount-test.c
new file mode 100644
index 000000000000..1b3ff2fda4d0
--- /dev/null
+++ b/tools/testing/selftests/mount/unprivileged-remount-test.c
@@ -0,0 +1,242 @@
+#define _GNU_SOURCE
+#include <sched.h>
+#include <stdio.h>
+#include <errno.h>
+#include <string.h>
+#include <sys/types.h>
+#include <sys/mount.h>
+#include <sys/wait.h>
+#include <stdlib.h>
+#include <unistd.h>
+#include <fcntl.h>
+#include <grp.h>
+#include <stdbool.h>
+#include <stdarg.h>
+
+#ifndef CLONE_NEWNS
+# define CLONE_NEWNS 0x00020000
+#endif
+#ifndef CLONE_NEWUTS
+# define CLONE_NEWUTS 0x04000000
+#endif
+#ifndef CLONE_NEWIPC
+# define CLONE_NEWIPC 0x08000000
+#endif
+#ifndef CLONE_NEWNET
+# define CLONE_NEWNET 0x40000000
+#endif
+#ifndef CLONE_NEWUSER
+# define CLONE_NEWUSER 0x10000000
+#endif
+#ifndef CLONE_NEWPID
+# define CLONE_NEWPID 0x20000000
+#endif
+
+#ifndef MS_RELATIME
+#define MS_RELATIME (1 << 21)
+#endif
+#ifndef MS_STRICTATIME
+#define MS_STRICTATIME (1 << 24)
+#endif
+
+static void die(char *fmt, ...)
+{
+	va_list ap;
+	va_start(ap, fmt);
+	vfprintf(stderr, fmt, ap);
+	va_end(ap);
+	exit(EXIT_FAILURE);
+}
+
+static void write_file(char *filename, char *fmt, ...)
+{
+	char buf[4096];
+	int fd;
+	ssize_t written;
+	int buf_len;
+	va_list ap;
+
+	va_start(ap, fmt);
+	buf_len = vsnprintf(buf, sizeof(buf), fmt, ap);
+	va_end(ap);
+	if (buf_len < 0) {
+		die("vsnprintf failed: %s\n",
+		    strerror(errno));
+	}
+	if (buf_len >= sizeof(buf)) {
+		die("vsnprintf output truncated\n");
+	}
+
+	fd = open(filename, O_WRONLY);
+	if (fd < 0) {
+		die("open of %s failed: %s\n",
+		    filename, strerror(errno));
+	}
+	written = write(fd, buf, buf_len);
+	if (written != buf_len) {
+		if (written >= 0) {
+			die("short write to %s\n", filename);
+		} else {
+			die("write to %s failed: %s\n",
+				filename, strerror(errno));
+		}
+	}
+	if (close(fd) != 0) {
+		die("close of %s failed: %s\n",
+			filename, strerror(errno));
+	}
+}
+
+static void create_and_enter_userns(void)
+{
+	uid_t uid;
+	gid_t gid;
+
+	uid = getuid();
+	gid = getgid();
+
+	if (unshare(CLONE_NEWUSER) !=0) {
+		die("unshare(CLONE_NEWUSER) failed: %s\n",
+			strerror(errno));
+	}
+
+	write_file("/proc/self/uid_map", "0 %d 1", uid);
+	write_file("/proc/self/gid_map", "0 %d 1", gid);
+
+	if (setgroups(0, NULL) != 0) {
+		die("setgroups failed: %s\n",
+			strerror(errno));
+	}
+	if (setgid(0) != 0) {
+		die ("setgid(0) failed %s\n",
+			strerror(errno));
+	}
+	if (setuid(0) != 0) {
+		die("setuid(0) failed %s\n",
+			strerror(errno));
+	}
+}
+
+static
+bool test_unpriv_remount(int mount_flags, int remount_flags, int invalid_flags)
+{
+	pid_t child;
+
+	child = fork();
+	if (child == -1) {
+		die("fork failed: %s\n",
+			strerror(errno));
+	}
+	if (child != 0) { /* parent */
+		pid_t pid;
+		int status;
+		pid = waitpid(child, &status, 0);
+		if (pid == -1) {
+			die("waitpid failed: %s\n",
+				strerror(errno));
+		}
+		if (pid != child) {
+			die("waited for %d got %d\n",
+				child, pid);
+		}
+		if (!WIFEXITED(status)) {
+			die("child did not terminate cleanly\n");
+		}
+		return WEXITSTATUS(status) == EXIT_SUCCESS ? true : false;
+	}
+
+	create_and_enter_userns();
+	if (unshare(CLONE_NEWNS) != 0) {
+		die("unshare(CLONE_NEWNS) failed: %s\n",
+			strerror(errno));
+	}
+
+	if (mount("testing", "/tmp", "ramfs", mount_flags, NULL) != 0) {
+		die("mount of /tmp failed: %s\n",
+			strerror(errno));
+	}
+
+	create_and_enter_userns();
+
+	if (unshare(CLONE_NEWNS) != 0) {
+		die("unshare(CLONE_NEWNS) failed: %s\n",
+			strerror(errno));
+	}
+
+	if (mount("/tmp", "/tmp", "none",
+		  MS_REMOUNT | MS_BIND | remount_flags, NULL) != 0) {
+		/* system("cat /proc/self/mounts"); */
+		die("remount of /tmp failed: %s\n",
+		    strerror(errno));
+	}
+
+	if (mount("/tmp", "/tmp", "none",
+		  MS_REMOUNT | MS_BIND | invalid_flags, NULL) == 0) {
+		/* system("cat /proc/self/mounts"); */
+		die("remount of /tmp with invalid flags "
+		    "succeeded unexpectedly\n");
+	}
+	exit(EXIT_SUCCESS);
+}
+
+static bool test_unpriv_remount_simple(int mount_flags)
+{
+	return test_unpriv_remount(mount_flags, mount_flags, 0);
+}
+
+static bool test_unpriv_remount_atime(int mount_flags, int invalid_flags)
+{
+	return test_unpriv_remount(mount_flags, mount_flags, invalid_flags);
+}
+
+int main(int argc, char **argv)
+{
+	if (!test_unpriv_remount_simple(MS_RDONLY|MS_NODEV)) {
+		die("MS_RDONLY malfunctions\n");
+	}
+	if (!test_unpriv_remount_simple(MS_NODEV)) {
+		die("MS_NODEV malfunctions\n");
+	}
+	if (!test_unpriv_remount_simple(MS_NOSUID|MS_NODEV)) {
+		die("MS_NOSUID malfunctions\n");
+	}
+	if (!test_unpriv_remount_simple(MS_NOEXEC|MS_NODEV)) {
+		die("MS_NOEXEC malfunctions\n");
+	}
+	if (!test_unpriv_remount_atime(MS_RELATIME|MS_NODEV,
+				       MS_NOATIME|MS_NODEV))
+	{
+		die("MS_RELATIME malfunctions\n");
+	}
+	if (!test_unpriv_remount_atime(MS_STRICTATIME|MS_NODEV,
+				       MS_NOATIME|MS_NODEV))
+	{
+		die("MS_STRICTATIME malfunctions\n");
+	}
+	if (!test_unpriv_remount_atime(MS_NOATIME|MS_NODEV,
+				       MS_STRICTATIME|MS_NODEV))
+	{
+		die("MS_RELATIME malfunctions\n");
+	}
+	if (!test_unpriv_remount_atime(MS_RELATIME|MS_NODIRATIME|MS_NODEV,
+				       MS_NOATIME|MS_NODEV))
+	{
+		die("MS_RELATIME malfunctions\n");
+	}
+	if (!test_unpriv_remount_atime(MS_STRICTATIME|MS_NODIRATIME|MS_NODEV,
+				       MS_NOATIME|MS_NODEV))
+	{
+		die("MS_RELATIME malfunctions\n");
+	}
+	if (!test_unpriv_remount_atime(MS_NOATIME|MS_NODIRATIME|MS_NODEV,
+				       MS_STRICTATIME|MS_NODEV))
+	{
+		die("MS_RELATIME malfunctions\n");
+	}
+	if (!test_unpriv_remount(MS_STRICTATIME|MS_NODEV, MS_NODEV,
+				 MS_NOATIME|MS_NODEV))
+	{
+		die("Default atime malfunctions\n");
+	}
+	return EXIT_SUCCESS;
+}
