#!/bin/sh

# SPDX-License-Identifier: GPL-2.0-or-later
# Copyright (C) 2009-2014 Stephan Raue (stephan@openelec.tv)
# Copyright (C) 2018-present Team LibreELEC (https://libreelec.tv)

TEMP=0

if [ $(basename "$0") = "gputemp" -o "$1" = "gpu" ]; then

  if [ -x /usr/bin/nvidia-smi ]; then
    TEMP="$(/usr/bin/nvidia-smi -q -x | grep '<gpu_temp>' | awk '{ print $1 }' | sed 's,<gpu_temp>,,g')"
  fi

  if [ "$TEMP" = "0" ]; then
    for hwmon in /sys/class/hwmon/*; do
      if [ -f "${hwmon}/name" ]; then
        case $(cat ${hwmon}/name) in
          nouveau | radeon | amdgpu)
            [[ -f "${hwmon}/temp1_input" ]] && TEMP="$(cat ${hwmon}/temp1_input)" && break
            [[ -f "${hwmon}/temp2_input" ]] && TEMP="$(cat ${hwmon}/temp2_input)" && break
            ;;
            # intel gpu is supported by cpu coretemp below
        esac
      fi
    done

    TEMP="$(($TEMP / 1000))"
  fi
fi

if [ "$1" = "cpu" -o "$TEMP" = "0" ]; then

  for hwmon in /sys/class/hwmon/*; do
    if [ -f "${hwmon}/name" ]; then
      case $(cat ${hwmon}/name) in
        coretemp | k10temp | scpi_sensors)
          [[ -f "${hwmon}/temp1_input" ]] && TEMP="$(cat ${hwmon}/temp1_input)" && break
          [[ -f "${hwmon}/temp2_input" ]] && TEMP="$(cat ${hwmon}/temp2_input)" && break
          ;;
      esac
    fi
  done

  if [ "$TEMP" = "0" -a -f /sys/class/hwmon/hwmon0/device/temp1_input ]; then
    TEMP="$(cat /sys/class/hwmon/hwmon0/device/temp1_input)"
  fi

  TEMP="$(($TEMP / 1000))"
fi

echo "${TEMP} C"
