From 7145fe3d6a802243bcc43b305fe66347ed392a94 Mon Sep 17 00:00:00 2001
From: Christian Hewitt <christianshewitt@gmail.com>
Date: Wed, 1 Jan 2025 07:16:49 +0000
Subject: [PATCH 15/50] FROMGIT(6.16): arm64: dts: amlogic: gxlx-s905l-p271:
 add saradc compatible

Add the saradac node using the meson-gxlx-saradc compatible to ensure
MPLL clocks are poked and audio output is enabled on the p271 (S905L)
board.

Signed-off-by: Christian Hewitt <christianshewitt@gmail.com>
---
 arch/arm64/boot/dts/amlogic/meson-gxlx-s905l-p271.dts | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm64/boot/dts/amlogic/meson-gxlx-s905l-p271.dts b/arch/arm64/boot/dts/amlogic/meson-gxlx-s905l-p271.dts
index 942df754a0ed..1221f4545130 100644
--- a/arch/arm64/boot/dts/amlogic/meson-gxlx-s905l-p271.dts
+++ b/arch/arm64/boot/dts/amlogic/meson-gxlx-s905l-p271.dts
@@ -38,6 +38,10 @@ mali: gpu@c0000 {
 	};
 };
 
+&saradc {
+	compatible = "amlogic,meson-gxlx-saradc", "amlogic,meson-saradc";
+};
+
 &usb {
 	dr_mode = "host";
 };
-- 
2.34.1

