From ec86a3c23aca699c28875cb91179f312c23b3ced Mon Sep 17 00:00:00 2001
From: Christian Hewitt <christianshewitt@gmail.com>
Date: Tue, 18 Jan 2022 15:18:32 +0000
Subject: [PATCH 43/50] WIP: arm64: dts: meson: remove SDIO node from Khadas
 VIM1

Now that SDIO 100MHz max-frequency is inherited from the p212 dtsi we
can drop the node from the board dts.

Signed-off-by: Christian Hewitt <christianshewitt@gmail.com>
---
 arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts | 4 ----
 1 file changed, 4 deletions(-)

diff --git a/arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts b/arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts
index e137ebd48c5e..563e6e909363 100644
--- a/arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts
+++ b/arch/arm64/boot/dts/amlogic/meson-gxl-s905x-khadas-vim.dts
@@ -219,10 +219,6 @@ &pwm_ef {
 	pinctrl-0 = <&pwm_e_pins>, <&pwm_f_clk_pins>;
 };
 
-&sd_emmc_a {
-	max-frequency = <100000000>;
-};
-
 /* This is brought out on the Linux_RX (18) and Linux_TX (19) pins: */
 &uart_AO {
 	status = "okay";
-- 
2.34.1

