From fd223a84d313fc4161628cee55ba630d2f0c136f Mon Sep 17 00:00:00 2001
From: Christian Hewitt <christianshewitt@gmail.com>
Date: Sat, 6 Nov 2021 13:01:08 +0000
Subject: [PATCH 07/50] LOCAL: arm64: dts: meson: add rtc/vrtc aliases to
 Khadas VIM2

Add aliases to ensure the vrtc time (which normally proves first) is /dev/rtc1
while the onboard rtc chip claims /dev/rtc0.

Signed-off-by: Christian Hewitt <christianshewitt@gmail.com>
---
 arch/arm64/boot/dts/amlogic/meson-gxm-khadas-vim2.dts | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm64/boot/dts/amlogic/meson-gxm-khadas-vim2.dts b/arch/arm64/boot/dts/amlogic/meson-gxm-khadas-vim2.dts
index 2a09b3d550e2..8a89940869b0 100644
--- a/arch/arm64/boot/dts/amlogic/meson-gxm-khadas-vim2.dts
+++ b/arch/arm64/boot/dts/amlogic/meson-gxm-khadas-vim2.dts
@@ -18,6 +18,8 @@ / {
 	aliases {
 		serial0 = &uart_AO;
 		serial2 = &uart_AO_B;
+		rtc0 = &rtc;
+		rtc1 = &vrtc;
 	};
 
 	chosen {
-- 
2.34.1

