#!/bin/sh

# SPDX-License-Identifier: GPL-2.0
# Copyright (C) 2020-present Team LibreELEC (https://libreelec.tv)

# XU4 has 5x sensors so read them all and report the highest value
TEMP=$(cat /sys/devices/virtual/thermal/thermal_zone*/temp | sort -n | tail -1)
TEMP="$(($TEMP / 1000))"
echo "${TEMP} C"
