From c009b3b707bbde30fa6ff49ca3075160524ea7b9 Mon Sep 17 00:00:00 2001
From: Jernej Skrabec <jernej.skrabec@siol.net>
Date: Tue, 26 May 2020 20:08:27 +0200
Subject: [PATCH 41/44] arm64: dts: h6 deinterlace

Signed-off-by: Jernej Skrabec <jernej.skrabec@siol.net>
---
 arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi | 11 +++++++++++
 1 file changed, 11 insertions(+)

--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -160,6 +160,18 @@
 			};
 		};

+		deinterlace: deinterlace@1420000 {
+			compatible = "allwinner,sun50i-h6-deinterlace";
+			reg = <0x01420000 0x2000>;
+			clocks = <&ccu CLK_BUS_DEINTERLACE>,
+				 <&ccu CLK_DEINTERLACE>,
+				 <&ccu CLK_MBUS_DEINTERLACE>;
+			clock-names = "bus", "mod", "ram";
+			resets = <&ccu RST_BUS_DEINTERLACE>;
+			interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
+			iommus = <&iommu 2>;
+		};
+
 		video-codec@1c0e000 {
 			compatible = "allwinner,sun50i-h6-video-engine";
 			reg = <0x01c0e000 0x2000>;
