diff --git a/Documentation/kernel-parameters.txt b/Documentation/kernel-parameters.txt
index 7116fda..5d91ba1 100644
--- a/Documentation/kernel-parameters.txt
+++ b/Documentation/kernel-parameters.txt
@@ -1172,6 +1172,7 @@ bytes respectively. Such letter suffixes can also be entirely omitted.
 	i8042.notimeout	[HW] Ignore timeout condition signalled by controller
 	i8042.reset	[HW] Reset the controller during init and cleanup
 	i8042.unlock	[HW] Unlock (ignore) the keylock
+	i8042.kbdreset  [HW] Reset device connected to KBD port
 
 	i810=		[HW,DRM]
 
diff --git a/Makefile b/Makefile
index 7aff64e..5b94752 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 14
-SUBLEVEL = 29
+SUBLEVEL = 30
 EXTRAVERSION =
 NAME = Remembering Coco
 
diff --git a/arch/arc/boot/dts/nsimosci.dts b/arch/arc/boot/dts/nsimosci.dts
index 398064c..4c169d8 100644
--- a/arch/arc/boot/dts/nsimosci.dts
+++ b/arch/arc/boot/dts/nsimosci.dts
@@ -20,7 +20,7 @@
 		/* this is for console on PGU */
 		/* bootargs = "console=tty0 consoleblank=0"; */
 		/* this is for console on serial */
-		bootargs = "earlycon=uart8250,mmio32,0xc0000000,115200n8 console=tty0 console=ttyS0,115200n8 consoleblank=0 debug";
+		bootargs = "earlycon=uart8250,mmio32,0xf0000000,115200n8 console=tty0 console=ttyS0,115200n8 consoleblank=0 debug";
 	};
 
 	aliases {
@@ -46,9 +46,9 @@
 			#interrupt-cells = <1>;
 		};
 
-		uart0: serial@c0000000 {
+		uart0: serial@f0000000 {
 			compatible = "ns8250";
-			reg = <0xc0000000 0x2000>;
+			reg = <0xf0000000 0x2000>;
 			interrupts = <11>;
 			clock-frequency = <3686400>;
 			baud = <115200>;
@@ -57,21 +57,21 @@
 			no-loopback-test = <1>;
 		};
 
-		pgu0: pgu@c9000000 {
+		pgu0: pgu@f9000000 {
 			compatible = "snps,arcpgufb";
-			reg = <0xc9000000 0x400>;
+			reg = <0xf9000000 0x400>;
 		};
 
-		ps2: ps2@c9001000 {
+		ps2: ps2@f9001000 {
 			compatible = "snps,arc_ps2";
-			reg = <0xc9000400 0x14>;
+			reg = <0xf9000400 0x14>;
 			interrupts = <13>;
 			interrupt-names = "arc_ps2_irq";
 		};
 
-		eth0: ethernet@c0003000 {
+		eth0: ethernet@f0003000 {
 			compatible = "snps,oscilan";
-			reg = <0xc0003000 0x44>;
+			reg = <0xf0003000 0x44>;
 			interrupts = <7>, <8>;
 			interrupt-names = "rx", "tx";
 		};
diff --git a/arch/arc/include/asm/linkage.h b/arch/arc/include/asm/linkage.h
index 66ee552..5faad17 100644
--- a/arch/arc/include/asm/linkage.h
+++ b/arch/arc/include/asm/linkage.h
@@ -13,20 +13,6 @@
 
 #define ASM_NL		 `	/* use '`' to mark new line in macro */
 
-/* Can't use the ENTRY macro in linux/linkage.h
- * gas considers ';' as comment vs. newline
- */
-.macro ARC_ENTRY name
-	.global \name
-	.align 4
-	\name:
-.endm
-
-.macro ARC_EXIT name
-#define ASM_PREV_SYM_ADDR(name)  .-##name
-	.size \ name, ASM_PREV_SYM_ADDR(\name)
-.endm
-
 /* annotation for data we want in DCCM - if enabled in .config */
 .macro ARCFP_DATA nm
 #ifdef CONFIG_ARC_HAS_DCCM
diff --git a/arch/arc/kernel/ctx_sw_asm.S b/arch/arc/kernel/ctx_sw_asm.S
index 65690e7..2ff0347 100644
--- a/arch/arc/kernel/ctx_sw_asm.S
+++ b/arch/arc/kernel/ctx_sw_asm.S
@@ -62,4 +62,4 @@ __switch_to:
 	ld.ab   blink, [sp, 4]
 	j       [blink]
 
-ARC_EXIT __switch_to
+END(__switch_to)
diff --git a/arch/arc/kernel/entry.S b/arch/arc/kernel/entry.S
index 6e8f83a..29b82ad 100644
--- a/arch/arc/kernel/entry.S
+++ b/arch/arc/kernel/entry.S
@@ -141,7 +141,7 @@ VECTOR   EV_Extension            ; 0x130, Extn Intruction Excp  (0x26)
 VECTOR   reserved                ; Reserved Exceptions
 .endr
 
-#include <linux/linkage.h>   /* ARC_{EXTRY,EXIT} */
+#include <linux/linkage.h>   /* {EXTRY,EXIT} */
 #include <asm/entry.h>       /* SAVE_ALL_{INT1,INT2,SYS...} */
 #include <asm/errno.h>
 #include <asm/arcregs.h>
@@ -184,7 +184,7 @@ reserved:		; processor restart
 ; ---------------------------------------------
 ;  Level 2 ISR: Can interrupt a Level 1 ISR
 ; ---------------------------------------------
-ARC_ENTRY handle_interrupt_level2
+ENTRY(handle_interrupt_level2)
 
 	; TODO-vineetg for SMP this wont work
 	; free up r9 as scratchpad
@@ -225,14 +225,14 @@ ARC_ENTRY handle_interrupt_level2
 
 	b   ret_from_exception
 
-ARC_EXIT handle_interrupt_level2
+END(handle_interrupt_level2)
 
 #endif
 
 ; ---------------------------------------------
 ;  Level 1 ISR
 ; ---------------------------------------------
-ARC_ENTRY handle_interrupt_level1
+ENTRY(handle_interrupt_level1)
 
 	/* free up r9 as scratchpad */
 #ifdef CONFIG_SMP
@@ -265,7 +265,7 @@ ARC_ENTRY handle_interrupt_level1
 	sr r8, [AUX_IRQ_LV12]       ; clear bit in Sticky Status Reg
 
 	b   ret_from_exception
-ARC_EXIT handle_interrupt_level1
+END(handle_interrupt_level1)
 
 ;################### Non TLB Exception Handling #############################
 
@@ -273,7 +273,7 @@ ARC_EXIT handle_interrupt_level1
 ; Instruction Error Exception Handler
 ; ---------------------------------------------
 
-ARC_ENTRY instr_service
+ENTRY(instr_service)
 
 	EXCEPTION_PROLOGUE
 
@@ -284,13 +284,13 @@ ARC_ENTRY instr_service
 
 	bl  do_insterror_or_kprobe
 	b   ret_from_exception
-ARC_EXIT instr_service
+END(instr_service)
 
 ; ---------------------------------------------
 ; Memory Error Exception Handler
 ; ---------------------------------------------
 
-ARC_ENTRY mem_service
+ENTRY(mem_service)
 
 	EXCEPTION_PROLOGUE
 
@@ -301,13 +301,13 @@ ARC_ENTRY mem_service
 
 	bl  do_memory_error
 	b   ret_from_exception
-ARC_EXIT mem_service
+END(mem_service)
 
 ; ---------------------------------------------
 ; Machine Check Exception Handler
 ; ---------------------------------------------
 
-ARC_ENTRY EV_MachineCheck
+ENTRY(EV_MachineCheck)
 
 	EXCEPTION_PROLOGUE
 
@@ -331,13 +331,13 @@ ARC_ENTRY EV_MachineCheck
 
 	j  do_machine_check_fault
 
-ARC_EXIT EV_MachineCheck
+END(EV_MachineCheck)
 
 ; ---------------------------------------------
 ; Protection Violation Exception Handler
 ; ---------------------------------------------
 
-ARC_ENTRY EV_TLBProtV
+ENTRY(EV_TLBProtV)
 
 	EXCEPTION_PROLOGUE
 
@@ -385,12 +385,12 @@ ARC_ENTRY EV_TLBProtV
 
 	b   ret_from_exception
 
-ARC_EXIT EV_TLBProtV
+END(EV_TLBProtV)
 
 ; ---------------------------------------------
 ; Privilege Violation Exception Handler
 ; ---------------------------------------------
-ARC_ENTRY EV_PrivilegeV
+ENTRY(EV_PrivilegeV)
 
 	EXCEPTION_PROLOGUE
 
@@ -401,12 +401,12 @@ ARC_ENTRY EV_PrivilegeV
 
 	bl  do_privilege_fault
 	b   ret_from_exception
-ARC_EXIT EV_PrivilegeV
+END(EV_PrivilegeV)
 
 ; ---------------------------------------------
 ; Extension Instruction Exception Handler
 ; ---------------------------------------------
-ARC_ENTRY EV_Extension
+ENTRY(EV_Extension)
 
 	EXCEPTION_PROLOGUE
 
@@ -417,7 +417,7 @@ ARC_ENTRY EV_Extension
 
 	bl  do_extension_fault
 	b   ret_from_exception
-ARC_EXIT EV_Extension
+END(EV_Extension)
 
 ;######################### System Call Tracing #########################
 
@@ -504,7 +504,7 @@ trap_with_param:
 ;   (2) Break Points
 ;------------------------------------------------------------------
 
-ARC_ENTRY EV_Trap
+ENTRY(EV_Trap)
 
 	EXCEPTION_PROLOGUE
 
@@ -534,9 +534,9 @@ ARC_ENTRY EV_Trap
 	jl      [r9]        ; Entry into Sys Call Handler
 
 	; fall through to ret_from_system_call
-ARC_EXIT EV_Trap
+END(EV_Trap)
 
-ARC_ENTRY ret_from_system_call
+ENTRY(ret_from_system_call)
 
 	st  r0, [sp, PT_r0]     ; sys call return value in pt_regs
 
@@ -546,7 +546,7 @@ ARC_ENTRY ret_from_system_call
 ;
 ; If ret to user mode do we need to handle signals, schedule() et al.
 
-ARC_ENTRY ret_from_exception
+ENTRY(ret_from_exception)
 
 	; Pre-{IRQ,Trap,Exception} K/U mode from pt_regs->status32
 	ld  r8, [sp, PT_status32]   ; returning to User/Kernel Mode
@@ -728,9 +728,9 @@ not_level1_interrupt:
 debug_marker_syscall:
 	rtie
 
-ARC_EXIT ret_from_exception
+END(ret_from_exception)
 
-ARC_ENTRY ret_from_fork
+ENTRY(ret_from_fork)
 	; when the forked child comes here from the __switch_to function
 	; r0 has the last task pointer.
 	; put last task in scheduler queue
@@ -747,11 +747,11 @@ ARC_ENTRY ret_from_fork
 	; special case of kernel_thread entry point returning back due to
 	; kernel_execve() - pretend return from syscall to ret to userland
 	b    ret_from_exception
-ARC_EXIT ret_from_fork
+END(ret_from_fork)
 
 ;################### Special Sys Call Wrappers ##########################
 
-ARC_ENTRY sys_clone_wrapper
+ENTRY(sys_clone_wrapper)
 	SAVE_CALLEE_SAVED_USER
 	bl  @sys_clone
 	DISCARD_CALLEE_SAVED_USER
@@ -761,7 +761,7 @@ ARC_ENTRY sys_clone_wrapper
 	bnz  tracesys_exit
 
 	b ret_from_system_call
-ARC_EXIT sys_clone_wrapper
+END(sys_clone_wrapper)
 
 #ifdef CONFIG_ARC_DW2_UNWIND
 ; Workaround for bug 94179 (STAR ):
diff --git a/arch/arc/lib/memcmp.S b/arch/arc/lib/memcmp.S
index bc813d5..978bf83 100644
--- a/arch/arc/lib/memcmp.S
+++ b/arch/arc/lib/memcmp.S
@@ -6,7 +6,7 @@
  * published by the Free Software Foundation.
  */
 
-#include <asm/linkage.h>
+#include <linux/linkage.h>
 
 #ifdef __LITTLE_ENDIAN__
 #define WORD2 r2
@@ -16,7 +16,7 @@
 #define SHIFT r2
 #endif
 
-ARC_ENTRY memcmp
+ENTRY(memcmp)
 	or	r12,r0,r1
 	asl_s	r12,r12,30
 	sub	r3,r2,1
@@ -121,4 +121,4 @@ ARC_ENTRY memcmp
 .Lnil:
 	j_s.d	[blink]
 	mov	r0,0
-ARC_EXIT memcmp
+END(memcmp)
diff --git a/arch/arc/lib/memcpy-700.S b/arch/arc/lib/memcpy-700.S
index b64cc10..3222573 100644
--- a/arch/arc/lib/memcpy-700.S
+++ b/arch/arc/lib/memcpy-700.S
@@ -6,9 +6,9 @@
  * published by the Free Software Foundation.
  */
 
-#include <asm/linkage.h>
+#include <linux/linkage.h>
 
-ARC_ENTRY memcpy
+ENTRY(memcpy)
 	or	r3,r0,r1
 	asl_s	r3,r3,30
 	mov_s	r5,r0
@@ -63,4 +63,4 @@ ARC_ENTRY memcpy
 .Lendbloop:
 	j_s.d	[blink]
 	stb	r12,[r5,0]
-ARC_EXIT memcpy
+END(memcpy)
diff --git a/arch/arc/lib/memset.S b/arch/arc/lib/memset.S
index 9b2d88d..d36bd43 100644
--- a/arch/arc/lib/memset.S
+++ b/arch/arc/lib/memset.S
@@ -6,11 +6,11 @@
  * published by the Free Software Foundation.
  */
 
-#include <asm/linkage.h>
+#include <linux/linkage.h>
 
 #define SMALL	7 /* Must be at least 6 to deal with alignment/loop issues.  */
 
-ARC_ENTRY memset
+ENTRY(memset)
 	mov_s	r4,r0
 	or	r12,r0,r2
 	bmsk.f	r12,r12,1
@@ -46,14 +46,14 @@ ARC_ENTRY memset
 	stb.ab	r1,[r4,1]
 .Ltiny_end:
 	j_s	[blink]
-ARC_EXIT memset
+END(memset)
 
 ; memzero: @r0 = mem, @r1 = size_t
 ; memset:  @r0 = mem, @r1 = char, @r2 = size_t
 
-ARC_ENTRY memzero
+ENTRY(memzero)
     ; adjust bzero args to memset args
     mov r2, r1
     mov r1, 0
     b  memset    ;tail call so need to tinker with blink
-ARC_EXIT memzero
+END(memzero)
diff --git a/arch/arc/lib/strchr-700.S b/arch/arc/lib/strchr-700.S
index 9c548c7..b725d58 100644
--- a/arch/arc/lib/strchr-700.S
+++ b/arch/arc/lib/strchr-700.S
@@ -11,9 +11,9 @@
    presence of the norm instruction makes it easier to operate on whole
    words branch-free.  */
 
-#include <asm/linkage.h>
+#include <linux/linkage.h>
 
-ARC_ENTRY strchr
+ENTRY(strchr)
 	extb_s	r1,r1
 	asl	r5,r1,8
 	bmsk	r2,r0,1
@@ -130,4 +130,4 @@ ARC_ENTRY strchr
 	j_s.d	[blink]
 	mov.mi	r0,0
 #endif /* ENDIAN */
-ARC_EXIT strchr
+END(strchr)
diff --git a/arch/arc/lib/strcmp.S b/arch/arc/lib/strcmp.S
index 5dc802b..3544600 100644
--- a/arch/arc/lib/strcmp.S
+++ b/arch/arc/lib/strcmp.S
@@ -13,9 +13,9 @@
    source 1; however, that would increase the overhead for loop setup / finish,
    and strcmp might often terminate early.  */
 
-#include <asm/linkage.h>
+#include <linux/linkage.h>
 
-ARC_ENTRY strcmp
+ENTRY(strcmp)
 	or	r2,r0,r1
 	bmsk_s	r2,r2,1
 	brne	r2,0,.Lcharloop
@@ -93,4 +93,4 @@ ARC_ENTRY strcmp
 .Lcmpend:
 	j_s.d	[blink]
 	sub	r0,r2,r3
-ARC_EXIT strcmp
+END(strcmp)
diff --git a/arch/arc/lib/strcpy-700.S b/arch/arc/lib/strcpy-700.S
index b7ca4ae..8422f38 100644
--- a/arch/arc/lib/strcpy-700.S
+++ b/arch/arc/lib/strcpy-700.S
@@ -16,9 +16,9 @@
    there, but the it is not likely to be taken often, and it
    would also be likey to cost an unaligned mispredict at the next call.  */
 
-#include <asm/linkage.h>
+#include <linux/linkage.h>
 
-ARC_ENTRY strcpy
+ENTRY(strcpy)
 	or	r2,r0,r1
 	bmsk_s	r2,r2,1
 	brne.d	r2,0,charloop
@@ -67,4 +67,4 @@ charloop:
 	brne.d	r3,0,charloop
 	stb.ab	r3,[r10,1]
 	j	[blink]
-ARC_EXIT strcpy
+END(strcpy)
diff --git a/arch/arc/lib/strlen.S b/arch/arc/lib/strlen.S
index 39759e0..53cfd56 100644
--- a/arch/arc/lib/strlen.S
+++ b/arch/arc/lib/strlen.S
@@ -6,9 +6,9 @@
  * published by the Free Software Foundation.
  */
 
-#include <asm/linkage.h>
+#include <linux/linkage.h>
 
-ARC_ENTRY strlen
+ENTRY(strlen)
 	or	r3,r0,7
 	ld	r2,[r3,-7]
 	ld.a	r6,[r3,-3]
@@ -80,4 +80,4 @@ ARC_ENTRY strlen
 .Learly_end:
 	b.d	.Lend
 	sub_s.ne r1,r1,r1
-ARC_EXIT strlen
+END(strlen)
diff --git a/arch/arc/mm/tlbex.S b/arch/arc/mm/tlbex.S
index 3fcfdb3..79bfc81 100644
--- a/arch/arc/mm/tlbex.S
+++ b/arch/arc/mm/tlbex.S
@@ -260,7 +260,7 @@ ARCFP_CODE	;Fast Path Code, candidate for ICCM
 ; I-TLB Miss Exception Handler
 ;-----------------------------------------------------------------------------
 
-ARC_ENTRY EV_TLBMissI
+ENTRY(EV_TLBMissI)
 
 	TLBMISS_FREEUP_REGS
 
@@ -293,13 +293,13 @@ ARC_ENTRY EV_TLBMissI
 	TLBMISS_RESTORE_REGS
 	rtie
 
-ARC_EXIT EV_TLBMissI
+END(EV_TLBMissI)
 
 ;-----------------------------------------------------------------------------
 ; D-TLB Miss Exception Handler
 ;-----------------------------------------------------------------------------
 
-ARC_ENTRY EV_TLBMissD
+ENTRY(EV_TLBMissD)
 
 	TLBMISS_FREEUP_REGS
 
@@ -381,6 +381,4 @@ do_slow_path_pf:
 	bl  do_page_fault
 	b   ret_from_exception
 
-ARC_EXIT EV_TLBMissD
-
-ARC_ENTRY EV_TLBMissB   ; Bogus entry to measure sz of DTLBMiss hdlr
+END(EV_TLBMissD)
diff --git a/arch/arm/boot/dts/imx25.dtsi b/arch/arm/boot/dts/imx25.dtsi
index de16119..6a26e79 100644
--- a/arch/arm/boot/dts/imx25.dtsi
+++ b/arch/arm/boot/dts/imx25.dtsi
@@ -158,7 +158,7 @@
 				#size-cells = <0>;
 				compatible = "fsl,imx25-cspi", "fsl,imx35-cspi";
 				reg = <0x43fa4000 0x4000>;
-				clocks = <&clks 62>, <&clks 62>;
+				clocks = <&clks 78>, <&clks 78>;
 				clock-names = "ipg", "per";
 				interrupts = <14>;
 				status = "disabled";
diff --git a/arch/arm/mach-imx/clk-imx6q.c b/arch/arm/mach-imx/clk-imx6q.c
index 4d677f4..01a5765 100644
--- a/arch/arm/mach-imx/clk-imx6q.c
+++ b/arch/arm/mach-imx/clk-imx6q.c
@@ -161,8 +161,8 @@ static void __init imx6q_clocks_init(struct device_node *ccm_node)
 		post_div_table[1].div = 1;
 		post_div_table[2].div = 1;
 		video_div_table[1].div = 1;
-		video_div_table[2].div = 1;
-	};
+		video_div_table[3].div = 1;
+	}
 
 	/*                   type                               name         parent_name  base     div_mask */
 	clk[pll1_sys]      = imx_clk_pllv3(IMX_PLLV3_SYS,	"pll1_sys",	"osc", base,        0x7f);
diff --git a/arch/arm/mach-omap2/timer.c b/arch/arm/mach-omap2/timer.c
index 74044aa..73d80b8 100644
--- a/arch/arm/mach-omap2/timer.c
+++ b/arch/arm/mach-omap2/timer.c
@@ -513,11 +513,11 @@ static void __init realtime_counter_init(void)
 	rate = clk_get_rate(sys_clk);
 	/* Numerator/denumerator values refer TRM Realtime Counter section */
 	switch (rate) {
-	case 1200000:
+	case 12000000:
 		num = 64;
 		den = 125;
 		break;
-	case 1300000:
+	case 13000000:
 		num = 768;
 		den = 1625;
 		break;
@@ -529,11 +529,11 @@ static void __init realtime_counter_init(void)
 		num = 192;
 		den = 625;
 		break;
-	case 2600000:
+	case 26000000:
 		num = 384;
 		den = 1625;
 		break;
-	case 2700000:
+	case 27000000:
 		num = 256;
 		den = 1125;
 		break;
diff --git a/arch/arm/mach-shmobile/setup-sh73a0.c b/arch/arm/mach-shmobile/setup-sh73a0.c
index f74ab53..2b73c8a 100644
--- a/arch/arm/mach-shmobile/setup-sh73a0.c
+++ b/arch/arm/mach-shmobile/setup-sh73a0.c
@@ -617,6 +617,7 @@ static struct platform_device ipmmu_device = {
 
 static struct renesas_intc_irqpin_config irqpin0_platform_data = {
 	.irq_base = irq_pin(0), /* IRQ0 -> IRQ7 */
+	.control_parent = true,
 };
 
 static struct resource irqpin0_resources[] = {
@@ -678,6 +679,7 @@ static struct platform_device irqpin1_device = {
 
 static struct renesas_intc_irqpin_config irqpin2_platform_data = {
 	.irq_base = irq_pin(16), /* IRQ16 -> IRQ23 */
+	.control_parent = true,
 };
 
 static struct resource irqpin2_resources[] = {
@@ -708,6 +710,7 @@ static struct platform_device irqpin2_device = {
 
 static struct renesas_intc_irqpin_config irqpin3_platform_data = {
 	.irq_base = irq_pin(24), /* IRQ24 -> IRQ31 */
+	.control_parent = true,
 };
 
 static struct resource irqpin3_resources[] = {
diff --git a/arch/parisc/include/asm/ldcw.h b/arch/parisc/include/asm/ldcw.h
index d2d11b7..8121aa6 100644
--- a/arch/parisc/include/asm/ldcw.h
+++ b/arch/parisc/include/asm/ldcw.h
@@ -33,11 +33,18 @@
 
 #endif /*!CONFIG_PA20*/
 
-/* LDCW, the only atomic read-write operation PA-RISC has. *sigh*.  */
+/* LDCW, the only atomic read-write operation PA-RISC has. *sigh*.
+   We don't explicitly expose that "*a" may be written as reload
+   fails to find a register in class R1_REGS when "a" needs to be
+   reloaded when generating 64-bit PIC code.  Instead, we clobber
+   memory to indicate to the compiler that the assembly code reads
+   or writes to items other than those listed in the input and output
+   operands.  This may pessimize the code somewhat but __ldcw is
+   usually used within code blocks surrounded by memory barriors.  */
 #define __ldcw(a) ({						\
 	unsigned __ret;						\
-	__asm__ __volatile__(__LDCW " 0(%2),%0"			\
-		: "=r" (__ret), "+m" (*(a)) : "r" (a));		\
+	__asm__ __volatile__(__LDCW " 0(%1),%0"			\
+		: "=r" (__ret) : "r" (a) : "memory");		\
 	__ret;							\
 })
 
diff --git a/arch/um/Kconfig.common b/arch/um/Kconfig.common
index 21ca44c..1f0ea55 100644
--- a/arch/um/Kconfig.common
+++ b/arch/um/Kconfig.common
@@ -2,6 +2,7 @@ config UML
 	bool
 	default y
 	select HAVE_UID16
+	select HAVE_FUTEX_CMPXCHG if FUTEX
 	select GENERIC_IRQ_SHOW
 	select GENERIC_CPU_DEVICES
 	select GENERIC_IO
diff --git a/arch/x86/kernel/kprobes/core.c b/arch/x86/kernel/kprobes/core.c
index 79a3f96..a1f5b18 100644
--- a/arch/x86/kernel/kprobes/core.c
+++ b/arch/x86/kernel/kprobes/core.c
@@ -1017,6 +1017,15 @@ int __kprobes setjmp_pre_handler(struct kprobe *p, struct pt_regs *regs)
 	regs->flags &= ~X86_EFLAGS_IF;
 	trace_hardirqs_off();
 	regs->ip = (unsigned long)(jp->entry);
+
+	/*
+	 * jprobes use jprobe_return() which skips the normal return
+	 * path of the function, and this messes up the accounting of the
+	 * function graph tracer to get messed up.
+	 *
+	 * Pause function graph tracing while performing the jprobe function.
+	 */
+	pause_graph_tracing();
 	return 1;
 }
 
@@ -1042,24 +1051,25 @@ int __kprobes longjmp_break_handler(struct kprobe *p, struct pt_regs *regs)
 	struct kprobe_ctlblk *kcb = get_kprobe_ctlblk();
 	u8 *addr = (u8 *) (regs->ip - 1);
 	struct jprobe *jp = container_of(p, struct jprobe, kp);
+	void *saved_sp = kcb->jprobe_saved_sp;
 
 	if ((addr > (u8 *) jprobe_return) &&
 	    (addr < (u8 *) jprobe_return_end)) {
-		if (stack_addr(regs) != kcb->jprobe_saved_sp) {
+		if (stack_addr(regs) != saved_sp) {
 			struct pt_regs *saved_regs = &kcb->jprobe_saved_regs;
 			printk(KERN_ERR
 			       "current sp %p does not match saved sp %p\n",
-			       stack_addr(regs), kcb->jprobe_saved_sp);
+			       stack_addr(regs), saved_sp);
 			printk(KERN_ERR "Saved registers for jprobe %p\n", jp);
 			show_regs(saved_regs);
 			printk(KERN_ERR "Current registers\n");
 			show_regs(regs);
 			BUG();
 		}
+		/* It's OK to start function graph tracing again */
+		unpause_graph_tracing();
 		*regs = kcb->jprobe_saved_regs;
-		memcpy((kprobe_opcode_t *)(kcb->jprobe_saved_sp),
-		       kcb->jprobes_stack,
-		       MIN_STACK_SIZE(kcb->jprobe_saved_sp));
+		memcpy(saved_sp, kcb->jprobes_stack, MIN_STACK_SIZE(saved_sp));
 		preempt_enable_no_resched();
 		return 1;
 	}
diff --git a/arch/x86/kvm/vmx.c b/arch/x86/kvm/vmx.c
index 0c90f4b..de42688 100644
--- a/arch/x86/kvm/vmx.c
+++ b/arch/x86/kvm/vmx.c
@@ -2320,12 +2320,12 @@ static __init void nested_vmx_setup_ctls_msrs(void)
 	nested_vmx_secondary_ctls_low = 0;
 	nested_vmx_secondary_ctls_high &=
 		SECONDARY_EXEC_VIRTUALIZE_APIC_ACCESSES |
-		SECONDARY_EXEC_UNRESTRICTED_GUEST |
 		SECONDARY_EXEC_WBINVD_EXITING;
 
 	if (enable_ept) {
 		/* nested EPT: emulate EPT also to L1 */
-		nested_vmx_secondary_ctls_high |= SECONDARY_EXEC_ENABLE_EPT;
+		nested_vmx_secondary_ctls_high |= SECONDARY_EXEC_ENABLE_EPT |
+			SECONDARY_EXEC_UNRESTRICTED_GUEST;
 		nested_vmx_ept_caps = VMX_EPT_PAGE_WALK_4_BIT |
 			 VMX_EPTP_WB_BIT | VMX_EPT_2MB_PAGE_BIT |
 			 VMX_EPT_INVEPT_BIT;
diff --git a/arch/x86/um/sys_call_table_32.c b/arch/x86/um/sys_call_table_32.c
index 531d426..bd16d6c 100644
--- a/arch/x86/um/sys_call_table_32.c
+++ b/arch/x86/um/sys_call_table_32.c
@@ -34,7 +34,7 @@ typedef asmlinkage void (*sys_call_ptr_t)(void);
 
 extern asmlinkage void sys_ni_syscall(void);
 
-const sys_call_ptr_t sys_call_table[] __cacheline_aligned = {
+const sys_call_ptr_t sys_call_table[] ____cacheline_aligned = {
 	/*
 	 * Smells like a compiler bug -- it doesn't work
 	 * when the & below is removed.
diff --git a/arch/x86/um/sys_call_table_64.c b/arch/x86/um/sys_call_table_64.c
index f2f0723..9578308 100644
--- a/arch/x86/um/sys_call_table_64.c
+++ b/arch/x86/um/sys_call_table_64.c
@@ -46,7 +46,7 @@ typedef void (*sys_call_ptr_t)(void);
 
 extern void sys_ni_syscall(void);
 
-const sys_call_ptr_t sys_call_table[] __cacheline_aligned = {
+const sys_call_ptr_t sys_call_table[] ____cacheline_aligned = {
 	/*
 	 * Smells like a compiler bug -- it doesn't work
 	 * when the & below is removed.
diff --git a/drivers/clk/clk.c b/drivers/clk/clk.c
index f9c4632..7145f6d 100644
--- a/drivers/clk/clk.c
+++ b/drivers/clk/clk.c
@@ -2232,14 +2232,17 @@ int __clk_get(struct clk *clk)
 
 void __clk_put(struct clk *clk)
 {
+	struct module *owner;
+
 	if (!clk || WARN_ON_ONCE(IS_ERR(clk)))
 		return;
 
 	clk_prepare_lock();
+	owner = clk->owner;
 	kref_put(&clk->ref, __clk_release);
 	clk_prepare_unlock();
 
-	module_put(clk->owner);
+	module_put(owner);
 }
 
 /***        clk rate change notifiers        ***/
diff --git a/drivers/clk/samsung/clk-exynos-audss.c b/drivers/clk/samsung/clk-exynos-audss.c
index 884187f..7f30b94 100644
--- a/drivers/clk/samsung/clk-exynos-audss.c
+++ b/drivers/clk/samsung/clk-exynos-audss.c
@@ -210,6 +210,10 @@ static int exynos_audss_clk_remove(struct platform_device *pdev)
 {
 	int i;
 
+#ifdef CONFIG_PM_SLEEP
+	unregister_syscore_ops(&exynos_audss_clk_syscore_ops);
+#endif
+
 	of_clk_del_provider(pdev->dev.of_node);
 
 	for (i = 0; i < clk_data.clk_num; i++) {
diff --git a/drivers/gpio/gpiolib-of.c b/drivers/gpio/gpiolib-of.c
index e0a98f5..74ed17d 100644
--- a/drivers/gpio/gpiolib-of.c
+++ b/drivers/gpio/gpiolib-of.c
@@ -44,8 +44,14 @@ static int of_gpiochip_find_and_xlate(struct gpio_chip *gc, void *data)
 		return false;
 
 	ret = gc->of_xlate(gc, &gg_data->gpiospec, gg_data->flags);
-	if (ret < 0)
-		return false;
+	if (ret < 0) {
+		/* We've found the gpio chip, but the translation failed.
+		 * Return true to stop looking and return the translation
+		 * error via out_gpio
+		 */
+		gg_data->out_gpio = ERR_PTR(ret);
+		return true;
+	 }
 
 	gg_data->out_gpio = gpio_to_desc(ret + gc->base);
 	return true;
diff --git a/drivers/gpio/gpiolib.c b/drivers/gpio/gpiolib.c
index 50c4922..5b88c83 100644
--- a/drivers/gpio/gpiolib.c
+++ b/drivers/gpio/gpiolib.c
@@ -1222,6 +1222,9 @@ int gpiochip_add(struct gpio_chip *chip)
 
 	spin_unlock_irqrestore(&gpio_lock, flags);
 
+	if (status)
+		goto fail;
+
 #ifdef CONFIG_PINCTRL
 	INIT_LIST_HEAD(&chip->pin_ranges);
 #endif
@@ -1229,12 +1232,12 @@ int gpiochip_add(struct gpio_chip *chip)
 	of_gpiochip_add(chip);
 	acpi_gpiochip_add(chip);
 
-	if (status)
-		goto fail;
-
 	status = gpiochip_export(chip);
-	if (status)
+	if (status) {
+		acpi_gpiochip_remove(chip);
+		of_gpiochip_remove(chip);
 		goto fail;
+	}
 
 	pr_debug("%s: registered GPIOs %d to %d on device: %s\n", __func__,
 		chip->base, chip->base + chip->ngpio - 1,
diff --git a/drivers/gpu/drm/i915/i915_gem_stolen.c b/drivers/gpu/drm/i915/i915_gem_stolen.c
index 3c78b22..800e06c 100644
--- a/drivers/gpu/drm/i915/i915_gem_stolen.c
+++ b/drivers/gpu/drm/i915/i915_gem_stolen.c
@@ -137,7 +137,11 @@ static unsigned long i915_stolen_to_physical(struct drm_device *dev)
 		r = devm_request_mem_region(dev->dev, base + 1,
 					    dev_priv->gtt.stolen_size - 1,
 					    "Graphics Stolen Memory");
-		if (r == NULL) {
+		/*
+		 * GEN3 firmware likes to smash pci bridges into the stolen
+		 * range. Apparently this works.
+		 */
+		if (r == NULL && !IS_GEN3(dev)) {
 			DRM_ERROR("conflict detected with stolen region: [0x%08x - 0x%08x]\n",
 				  base, base + (uint32_t)dev_priv->gtt.stolen_size);
 			base = 0;
diff --git a/drivers/gpu/drm/i915/i915_reg.h b/drivers/gpu/drm/i915/i915_reg.h
index 0a3b938..0c83b3d 100644
--- a/drivers/gpu/drm/i915/i915_reg.h
+++ b/drivers/gpu/drm/i915/i915_reg.h
@@ -320,6 +320,7 @@
 #define   PIPE_CONTROL_GLOBAL_GTT_IVB			(1<<24) /* gen7+ */
 #define   PIPE_CONTROL_CS_STALL				(1<<20)
 #define   PIPE_CONTROL_TLB_INVALIDATE			(1<<18)
+#define   PIPE_CONTROL_MEDIA_STATE_CLEAR		(1<<16)
 #define   PIPE_CONTROL_QW_WRITE				(1<<14)
 #define   PIPE_CONTROL_DEPTH_STALL			(1<<13)
 #define   PIPE_CONTROL_WRITE_FLUSH			(1<<12)
diff --git a/drivers/gpu/drm/i915/intel_ringbuffer.c b/drivers/gpu/drm/i915/intel_ringbuffer.c
index d488fc7..d2af1e1 100644
--- a/drivers/gpu/drm/i915/intel_ringbuffer.c
+++ b/drivers/gpu/drm/i915/intel_ringbuffer.c
@@ -334,12 +334,15 @@ gen7_render_ring_flush(struct intel_ring_buffer *ring,
 		flags |= PIPE_CONTROL_VF_CACHE_INVALIDATE;
 		flags |= PIPE_CONTROL_CONST_CACHE_INVALIDATE;
 		flags |= PIPE_CONTROL_STATE_CACHE_INVALIDATE;
+		flags |= PIPE_CONTROL_MEDIA_STATE_CLEAR;
 		/*
 		 * TLB invalidate requires a post-sync write.
 		 */
 		flags |= PIPE_CONTROL_QW_WRITE;
 		flags |= PIPE_CONTROL_GLOBAL_GTT_IVB;
 
+		flags |= PIPE_CONTROL_STALL_AT_SCOREBOARD;
+
 		/* Workaround: we must issue a pipe_control with CS-stall bit
 		 * set before a pipe_control command that has the state cache
 		 * invalidate bit set. */
diff --git a/drivers/gpu/drm/i915/intel_uncore.c b/drivers/gpu/drm/i915/intel_uncore.c
index c879631..b6c063c 100644
--- a/drivers/gpu/drm/i915/intel_uncore.c
+++ b/drivers/gpu/drm/i915/intel_uncore.c
@@ -451,8 +451,8 @@ hsw_unclaimed_reg_check(struct drm_i915_private *dev_priv, u32 reg)
 static void
 assert_device_not_suspended(struct drm_i915_private *dev_priv)
 {
-	WARN(HAS_RUNTIME_PM(dev_priv->dev) && dev_priv->pm.suspended,
-	     "Device suspended\n");
+	WARN_ONCE(HAS_RUNTIME_PM(dev_priv->dev) && dev_priv->pm.suspended,
+		  "Device suspended\n");
 }
 
 #define REG_READ_HEADER(x) \
diff --git a/drivers/gpu/drm/nouveau/core/subdev/mc/nv4c.c b/drivers/gpu/drm/nouveau/core/subdev/mc/nv4c.c
index a75c35c..165401c 100644
--- a/drivers/gpu/drm/nouveau/core/subdev/mc/nv4c.c
+++ b/drivers/gpu/drm/nouveau/core/subdev/mc/nv4c.c
@@ -24,13 +24,6 @@
 
 #include "nv04.h"
 
-static void
-nv4c_mc_msi_rearm(struct nouveau_mc *pmc)
-{
-	struct nv04_mc_priv *priv = (void *)pmc;
-	nv_wr08(priv, 0x088050, 0xff);
-}
-
 struct nouveau_oclass *
 nv4c_mc_oclass = &(struct nouveau_mc_oclass) {
 	.base.handle = NV_SUBDEV(MC, 0x4c),
@@ -41,5 +34,4 @@ nv4c_mc_oclass = &(struct nouveau_mc_oclass) {
 		.fini = _nouveau_mc_fini,
 	},
 	.intr = nv04_mc_intr,
-	.msi_rearm = nv4c_mc_msi_rearm,
 }.base;
diff --git a/drivers/gpu/drm/radeon/atombios_dp.c b/drivers/gpu/drm/radeon/atombios_dp.c
index 5727dbd..b4dbaded 100644
--- a/drivers/gpu/drm/radeon/atombios_dp.c
+++ b/drivers/gpu/drm/radeon/atombios_dp.c
@@ -576,6 +576,10 @@ int radeon_dp_mode_valid_helper(struct drm_connector *connector,
 	struct radeon_connector_atom_dig *dig_connector;
 	int dp_clock;
 
+	if ((mode->clock > 340000) &&
+	    (!radeon_connector_is_dp12_capable(connector)))
+		return MODE_CLOCK_HIGH;
+
 	if (!radeon_connector->con_priv)
 		return MODE_CLOCK_HIGH;
 	dig_connector = radeon_connector->con_priv;
diff --git a/drivers/gpu/drm/radeon/ci_dpm.c b/drivers/gpu/drm/radeon/ci_dpm.c
index 543ba2d..c7c2856 100644
--- a/drivers/gpu/drm/radeon/ci_dpm.c
+++ b/drivers/gpu/drm/radeon/ci_dpm.c
@@ -4733,7 +4733,7 @@ void ci_dpm_disable(struct radeon_device *rdev)
 	ci_enable_spread_spectrum(rdev, false);
 	ci_enable_auto_throttle_source(rdev, RADEON_DPM_AUTO_THROTTLE_SRC_THERMAL, false);
 	ci_stop_dpm(rdev);
-	ci_enable_ds_master_switch(rdev, true);
+	ci_enable_ds_master_switch(rdev, false);
 	ci_enable_ulv(rdev, false);
 	ci_clear_vc(rdev);
 	ci_reset_to_default(rdev);
diff --git a/drivers/gpu/drm/radeon/cik.c b/drivers/gpu/drm/radeon/cik.c
index ddf70d6..8ef67cb 100644
--- a/drivers/gpu/drm/radeon/cik.c
+++ b/drivers/gpu/drm/radeon/cik.c
@@ -5879,6 +5879,7 @@ static void cik_enable_mgcg(struct radeon_device *rdev, bool enable)
 		}
 
 		orig = data = RREG32(RLC_CGTT_MGCG_OVERRIDE);
+		data |= 0x00000001;
 		data &= 0xfffffffd;
 		if (orig != data)
 			WREG32(RLC_CGTT_MGCG_OVERRIDE, data);
@@ -5910,7 +5911,7 @@ static void cik_enable_mgcg(struct radeon_device *rdev, bool enable)
 		}
 	} else {
 		orig = data = RREG32(RLC_CGTT_MGCG_OVERRIDE);
-		data |= 0x00000002;
+		data |= 0x00000003;
 		if (orig != data)
 			WREG32(RLC_CGTT_MGCG_OVERRIDE, data);
 
diff --git a/drivers/gpu/drm/radeon/radeon_ttm.c b/drivers/gpu/drm/radeon/radeon_ttm.c
index 040a2a1..45a9a03 100644
--- a/drivers/gpu/drm/radeon/radeon_ttm.c
+++ b/drivers/gpu/drm/radeon/radeon_ttm.c
@@ -191,7 +191,7 @@ static void radeon_evict_flags(struct ttm_buffer_object *bo,
 	rbo = container_of(bo, struct radeon_bo, tbo);
 	switch (bo->mem.mem_type) {
 	case TTM_PL_VRAM:
-		if (rbo->rdev->ring[RADEON_RING_TYPE_GFX_INDEX].ready == false)
+		if (rbo->rdev->ring[radeon_copy_ring_index(rbo->rdev)].ready == false)
 			radeon_ttm_placement_from_domain(rbo, RADEON_GEM_DOMAIN_CPU);
 		else
 			radeon_ttm_placement_from_domain(rbo, RADEON_GEM_DOMAIN_GTT);
diff --git a/drivers/gpu/drm/ttm/ttm_page_alloc.c b/drivers/gpu/drm/ttm/ttm_page_alloc.c
index cf4bad2..76329d2 100644
--- a/drivers/gpu/drm/ttm/ttm_page_alloc.c
+++ b/drivers/gpu/drm/ttm/ttm_page_alloc.c
@@ -297,11 +297,12 @@ static void ttm_pool_update_free_locked(struct ttm_page_pool *pool,
  *
  * @pool: to free the pages from
  * @free_all: If set to true will free all pages in pool
- * @gfp: GFP flags.
+ * @use_static: Safe to use static buffer
  **/
 static int ttm_page_pool_free(struct ttm_page_pool *pool, unsigned nr_free,
-			      gfp_t gfp)
+			      bool use_static)
 {
+	static struct page *static_buf[NUM_PAGES_TO_ALLOC];
 	unsigned long irq_flags;
 	struct page *p;
 	struct page **pages_to_free;
@@ -311,7 +312,11 @@ static int ttm_page_pool_free(struct ttm_page_pool *pool, unsigned nr_free,
 	if (NUM_PAGES_TO_ALLOC < nr_free)
 		npages_to_free = NUM_PAGES_TO_ALLOC;
 
-	pages_to_free = kmalloc(npages_to_free * sizeof(struct page *), gfp);
+	if (use_static)
+		pages_to_free = static_buf;
+	else
+		pages_to_free = kmalloc(npages_to_free * sizeof(struct page *),
+					GFP_KERNEL);
 	if (!pages_to_free) {
 		pr_err("Failed to allocate memory for pool free operation\n");
 		return 0;
@@ -374,7 +379,8 @@ restart:
 	if (freed_pages)
 		ttm_pages_put(pages_to_free, freed_pages);
 out:
-	kfree(pages_to_free);
+	if (pages_to_free != static_buf)
+		kfree(pages_to_free);
 	return nr_free;
 }
 
@@ -383,8 +389,6 @@ out:
  *
  * XXX: (dchinner) Deadlock warning!
  *
- * We need to pass sc->gfp_mask to ttm_page_pool_free().
- *
  * This code is crying out for a shrinker per pool....
  */
 static unsigned long
@@ -407,8 +411,8 @@ ttm_pool_shrink_scan(struct shrinker *shrink, struct shrink_control *sc)
 		if (shrink_pages == 0)
 			break;
 		pool = &_manager->pools[(i + pool_offset)%NUM_POOLS];
-		shrink_pages = ttm_page_pool_free(pool, nr_free,
-						  sc->gfp_mask);
+		/* OK to use static buffer since global mutex is held. */
+		shrink_pages = ttm_page_pool_free(pool, nr_free, true);
 		freed += nr_free - shrink_pages;
 	}
 	mutex_unlock(&lock);
@@ -710,7 +714,7 @@ static void ttm_put_pages(struct page **pages, unsigned npages, int flags,
 	}
 	spin_unlock_irqrestore(&pool->lock, irq_flags);
 	if (npages)
-		ttm_page_pool_free(pool, npages, GFP_KERNEL);
+		ttm_page_pool_free(pool, npages, false);
 }
 
 /*
@@ -849,9 +853,9 @@ void ttm_page_alloc_fini(void)
 	pr_info("Finalizing pool allocator\n");
 	ttm_pool_mm_shrink_fini(_manager);
 
+	/* OK to use static buffer since global mutex is no longer used. */
 	for (i = 0; i < NUM_POOLS; ++i)
-		ttm_page_pool_free(&_manager->pools[i], FREE_ALL_PAGES,
-				   GFP_KERNEL);
+		ttm_page_pool_free(&_manager->pools[i], FREE_ALL_PAGES, true);
 
 	kobject_put(&_manager->kobj);
 	_manager = NULL;
diff --git a/drivers/gpu/drm/ttm/ttm_page_alloc_dma.c b/drivers/gpu/drm/ttm/ttm_page_alloc_dma.c
index ca65df1..3dfa97d 100644
--- a/drivers/gpu/drm/ttm/ttm_page_alloc_dma.c
+++ b/drivers/gpu/drm/ttm/ttm_page_alloc_dma.c
@@ -411,11 +411,12 @@ static void ttm_dma_page_put(struct dma_pool *pool, struct dma_page *d_page)
  *
  * @pool: to free the pages from
  * @nr_free: If set to true will free all pages in pool
- * @gfp: GFP flags.
+ * @use_static: Safe to use static buffer
  **/
 static unsigned ttm_dma_page_pool_free(struct dma_pool *pool, unsigned nr_free,
-				       gfp_t gfp)
+				       bool use_static)
 {
+	static struct page *static_buf[NUM_PAGES_TO_ALLOC];
 	unsigned long irq_flags;
 	struct dma_page *dma_p, *tmp;
 	struct page **pages_to_free;
@@ -432,7 +433,11 @@ static unsigned ttm_dma_page_pool_free(struct dma_pool *pool, unsigned nr_free,
 			 npages_to_free, nr_free);
 	}
 #endif
-	pages_to_free = kmalloc(npages_to_free * sizeof(struct page *), gfp);
+	if (use_static)
+		pages_to_free = static_buf;
+	else
+		pages_to_free = kmalloc(npages_to_free * sizeof(struct page *),
+					GFP_KERNEL);
 
 	if (!pages_to_free) {
 		pr_err("%s: Failed to allocate memory for pool free operation\n",
@@ -502,7 +507,8 @@ restart:
 	if (freed_pages)
 		ttm_dma_pages_put(pool, &d_pages, pages_to_free, freed_pages);
 out:
-	kfree(pages_to_free);
+	if (pages_to_free != static_buf)
+		kfree(pages_to_free);
 	return nr_free;
 }
 
@@ -531,7 +537,8 @@ static void ttm_dma_free_pool(struct device *dev, enum pool_type type)
 		if (pool->type != type)
 			continue;
 		/* Takes a spinlock.. */
-		ttm_dma_page_pool_free(pool, FREE_ALL_PAGES, GFP_KERNEL);
+		/* OK to use static buffer since global mutex is held. */
+		ttm_dma_page_pool_free(pool, FREE_ALL_PAGES, true);
 		WARN_ON(((pool->npages_in_use + pool->npages_free) != 0));
 		/* This code path is called after _all_ references to the
 		 * struct device has been dropped - so nobody should be
@@ -984,7 +991,7 @@ void ttm_dma_unpopulate(struct ttm_dma_tt *ttm_dma, struct device *dev)
 
 	/* shrink pool if necessary (only on !is_cached pools)*/
 	if (npages)
-		ttm_dma_page_pool_free(pool, npages, GFP_KERNEL);
+		ttm_dma_page_pool_free(pool, npages, false);
 	ttm->state = tt_unpopulated;
 }
 EXPORT_SYMBOL_GPL(ttm_dma_unpopulate);
@@ -994,8 +1001,6 @@ EXPORT_SYMBOL_GPL(ttm_dma_unpopulate);
  *
  * XXX: (dchinner) Deadlock warning!
  *
- * We need to pass sc->gfp_mask to ttm_dma_page_pool_free().
- *
  * I'm getting sadder as I hear more pathetical whimpers about needing per-pool
  * shrinkers
  */
@@ -1028,8 +1033,8 @@ ttm_dma_pool_shrink_scan(struct shrinker *shrink, struct shrink_control *sc)
 		if (++idx < pool_offset)
 			continue;
 		nr_free = shrink_pages;
-		shrink_pages = ttm_dma_page_pool_free(p->pool, nr_free,
-						      sc->gfp_mask);
+		/* OK to use static buffer since global mutex is held. */
+		shrink_pages = ttm_dma_page_pool_free(p->pool, nr_free, true);
 		freed += nr_free - shrink_pages;
 
 		pr_debug("%s: (%s:%d) Asked to shrink %d, have %d more to go\n",
diff --git a/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c b/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c
index 436b013..b65272d 100644
--- a/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c
+++ b/drivers/gpu/drm/vmwgfx/vmwgfx_fence.c
@@ -1049,6 +1049,8 @@ static int vmw_event_fence_action_create(struct drm_file *file_priv,
 	if (ret != 0)
 		goto out_no_queue;
 
+	return 0;
+
 out_no_queue:
 	event->base.destroy(&event->base);
 out_no_event:
@@ -1124,17 +1126,10 @@ int vmw_fence_event_ioctl(struct drm_device *dev, void *data,
 
 	BUG_ON(fence == NULL);
 
-	if (arg->flags & DRM_VMW_FE_FLAG_REQ_TIME)
-		ret = vmw_event_fence_action_create(file_priv, fence,
-						    arg->flags,
-						    arg->user_data,
-						    true);
-	else
-		ret = vmw_event_fence_action_create(file_priv, fence,
-						    arg->flags,
-						    arg->user_data,
-						    true);
-
+	ret = vmw_event_fence_action_create(file_priv, fence,
+					    arg->flags,
+					    arg->user_data,
+					    true);
 	if (unlikely(ret != 0)) {
 		if (ret != -ERESTARTSYS)
 			DRM_ERROR("Failed to attach event to fence.\n");
diff --git a/drivers/infiniband/ulp/isert/ib_isert.c b/drivers/infiniband/ulp/isert/ib_isert.c
index a96cfc3..6014227 100644
--- a/drivers/infiniband/ulp/isert/ib_isert.c
+++ b/drivers/infiniband/ulp/isert/ib_isert.c
@@ -41,6 +41,7 @@ static DEFINE_MUTEX(device_list_mutex);
 static LIST_HEAD(device_list);
 static struct workqueue_struct *isert_rx_wq;
 static struct workqueue_struct *isert_comp_wq;
+static struct workqueue_struct *isert_release_wq;
 
 static void
 isert_unmap_cmd(struct isert_cmd *isert_cmd, struct isert_conn *isert_conn);
@@ -52,6 +53,11 @@ isert_unreg_rdma(struct isert_cmd *isert_cmd, struct isert_conn *isert_conn);
 static int
 isert_reg_rdma(struct iscsi_conn *conn, struct iscsi_cmd *cmd,
 	       struct isert_rdma_wr *wr);
+static int
+isert_rdma_post_recvl(struct isert_conn *isert_conn);
+static int
+isert_rdma_accept(struct isert_conn *isert_conn);
+struct rdma_cm_id *isert_setup_id(struct isert_np *isert_np);
 
 static void
 isert_qp_event_callback(struct ib_event *e, void *context)
@@ -132,12 +138,18 @@ isert_conn_setup_qp(struct isert_conn *isert_conn, struct rdma_cm_id *cma_id)
 	ret = rdma_create_qp(cma_id, isert_conn->conn_pd, &attr);
 	if (ret) {
 		pr_err("rdma_create_qp failed for cma_id %d\n", ret);
-		return ret;
+		goto err;
 	}
 	isert_conn->conn_qp = cma_id->qp;
 	pr_debug("rdma_create_qp() returned success >>>>>>>>>>>>>>>>>>>>>>>>>.\n");
 
 	return 0;
+err:
+	mutex_lock(&device_list_mutex);
+	device->cq_active_qps[min_index]--;
+	mutex_unlock(&device_list_mutex);
+
+	return ret;
 }
 
 static void
@@ -489,8 +501,8 @@ err:
 static int
 isert_connect_request(struct rdma_cm_id *cma_id, struct rdma_cm_event *event)
 {
-	struct iscsi_np *np = cma_id->context;
-	struct isert_np *isert_np = np->np_context;
+	struct isert_np *isert_np = cma_id->context;
+	struct iscsi_np *np = isert_np->np;
 	struct isert_conn *isert_conn;
 	struct isert_device *device;
 	struct ib_device *ib_dev = cma_id->device;
@@ -515,6 +527,7 @@ isert_connect_request(struct rdma_cm_id *cma_id, struct rdma_cm_event *event)
 	isert_conn->state = ISER_CONN_INIT;
 	INIT_LIST_HEAD(&isert_conn->conn_accept_node);
 	init_completion(&isert_conn->conn_login_comp);
+	init_completion(&isert_conn->login_req_comp);
 	init_completion(&isert_conn->conn_wait);
 	init_completion(&isert_conn->conn_wait_comp_err);
 	kref_init(&isert_conn->conn_kref);
@@ -522,7 +535,6 @@ isert_connect_request(struct rdma_cm_id *cma_id, struct rdma_cm_event *event)
 	spin_lock_init(&isert_conn->conn_lock);
 	INIT_LIST_HEAD(&isert_conn->conn_fr_pool);
 
-	cma_id->context = isert_conn;
 	isert_conn->conn_cm_id = cma_id;
 	isert_conn->responder_resources = event->param.conn.responder_resources;
 	isert_conn->initiator_depth = event->param.conn.initiator_depth;
@@ -596,6 +608,14 @@ isert_connect_request(struct rdma_cm_id *cma_id, struct rdma_cm_event *event)
 	if (ret)
 		goto out_conn_dev;
 
+	ret = isert_rdma_post_recvl(isert_conn);
+	if (ret)
+		goto out_conn_dev;
+
+	ret = isert_rdma_accept(isert_conn);
+	if (ret)
+		goto out_conn_dev;
+
 	mutex_lock(&isert_np->np_accept_mutex);
 	list_add_tail(&isert_conn->conn_accept_node, &isert_np->np_accept_list);
 	mutex_unlock(&isert_np->np_accept_mutex);
@@ -620,6 +640,7 @@ out_login_buf:
 	kfree(isert_conn->login_buf);
 out:
 	kfree(isert_conn);
+	rdma_reject(cma_id, NULL, 0);
 	return ret;
 }
 
@@ -635,18 +656,20 @@ isert_connect_release(struct isert_conn *isert_conn)
 	if (device && device->use_fastreg)
 		isert_conn_free_fastreg_pool(isert_conn);
 
+	isert_free_rx_descriptors(isert_conn);
+	rdma_destroy_id(isert_conn->conn_cm_id);
+
 	if (isert_conn->conn_qp) {
 		cq_index = ((struct isert_cq_desc *)
 			isert_conn->conn_qp->recv_cq->cq_context)->cq_index;
 		pr_debug("isert_connect_release: cq_index: %d\n", cq_index);
+		mutex_lock(&device_list_mutex);
 		isert_conn->conn_device->cq_active_qps[cq_index]--;
+		mutex_unlock(&device_list_mutex);
 
-		rdma_destroy_qp(isert_conn->conn_cm_id);
+		ib_destroy_qp(isert_conn->conn_qp);
 	}
 
-	isert_free_rx_descriptors(isert_conn);
-	rdma_destroy_id(isert_conn->conn_cm_id);
-
 	ib_dereg_mr(isert_conn->conn_mr);
 	ib_dealloc_pd(isert_conn->conn_pd);
 
@@ -669,9 +692,19 @@ isert_connect_release(struct isert_conn *isert_conn)
 static void
 isert_connected_handler(struct rdma_cm_id *cma_id)
 {
-	struct isert_conn *isert_conn = cma_id->context;
+	struct isert_conn *isert_conn = cma_id->qp->qp_context;
+
+	pr_info("conn %p\n", isert_conn);
 
-	kref_get(&isert_conn->conn_kref);
+	if (!kref_get_unless_zero(&isert_conn->conn_kref)) {
+		pr_warn("conn %p connect_release is running\n", isert_conn);
+		return;
+	}
+
+	mutex_lock(&isert_conn->conn_mutex);
+	if (isert_conn->state != ISER_CONN_FULL_FEATURE)
+		isert_conn->state = ISER_CONN_UP;
+	mutex_unlock(&isert_conn->conn_mutex);
 }
 
 static void
@@ -692,65 +725,108 @@ isert_put_conn(struct isert_conn *isert_conn)
 	kref_put(&isert_conn->conn_kref, isert_release_conn_kref);
 }
 
+/**
+ * isert_conn_terminate() - Initiate connection termination
+ * @isert_conn: isert connection struct
+ *
+ * Notes:
+ * In case the connection state is FULL_FEATURE, move state
+ * to TEMINATING and start teardown sequence (rdma_disconnect).
+ * In case the connection state is UP, complete flush as well.
+ *
+ * This routine must be called with conn_mutex held. Thus it is
+ * safe to call multiple times.
+ */
 static void
-isert_disconnect_work(struct work_struct *work)
+isert_conn_terminate(struct isert_conn *isert_conn)
 {
-	struct isert_conn *isert_conn = container_of(work,
-				struct isert_conn, conn_logout_work);
+	int err;
 
-	pr_debug("isert_disconnect_work(): >>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>\n");
-	mutex_lock(&isert_conn->conn_mutex);
-	if (isert_conn->state == ISER_CONN_UP)
+	switch (isert_conn->state) {
+	case ISER_CONN_TERMINATING:
+		break;
+	case ISER_CONN_UP:
+		/*
+		 * No flush completions will occur as we didn't
+		 * get to ISER_CONN_FULL_FEATURE yet, complete
+		 * to allow teardown progress.
+		 */
+		complete(&isert_conn->conn_wait_comp_err);
+	case ISER_CONN_FULL_FEATURE: /* FALLTHRU */
+		pr_info("Terminating conn %p state %d\n",
+			   isert_conn, isert_conn->state);
 		isert_conn->state = ISER_CONN_TERMINATING;
-
-	if (isert_conn->post_recv_buf_count == 0 &&
-	    atomic_read(&isert_conn->post_send_buf_count) == 0) {
-		mutex_unlock(&isert_conn->conn_mutex);
-		goto wake_up;
-	}
-	if (!isert_conn->conn_cm_id) {
-		mutex_unlock(&isert_conn->conn_mutex);
-		isert_put_conn(isert_conn);
-		return;
+		err = rdma_disconnect(isert_conn->conn_cm_id);
+		if (err)
+			pr_warn("Failed rdma_disconnect isert_conn %p\n",
+				   isert_conn);
+		break;
+	default:
+		pr_warn("conn %p teminating in state %d\n",
+			   isert_conn, isert_conn->state);
 	}
+}
 
-	if (isert_conn->disconnect) {
-		/* Send DREQ/DREP towards our initiator */
-		rdma_disconnect(isert_conn->conn_cm_id);
-	}
+static int
+isert_np_cma_handler(struct isert_np *isert_np,
+		     enum rdma_cm_event_type event)
+{
+	pr_debug("isert np %p, handling event %d\n", isert_np, event);
 
-	mutex_unlock(&isert_conn->conn_mutex);
+	switch (event) {
+	case RDMA_CM_EVENT_DEVICE_REMOVAL:
+		isert_np->np_cm_id = NULL;
+		break;
+	case RDMA_CM_EVENT_ADDR_CHANGE:
+		isert_np->np_cm_id = isert_setup_id(isert_np);
+		if (IS_ERR(isert_np->np_cm_id)) {
+			pr_err("isert np %p setup id failed: %ld\n",
+				 isert_np, PTR_ERR(isert_np->np_cm_id));
+			isert_np->np_cm_id = NULL;
+		}
+		break;
+	default:
+		pr_err("isert np %p Unexpected event %d\n",
+			  isert_np, event);
+	}
 
-wake_up:
-	complete(&isert_conn->conn_wait);
+	return -1;
 }
 
 static int
-isert_disconnected_handler(struct rdma_cm_id *cma_id, bool disconnect)
+isert_disconnected_handler(struct rdma_cm_id *cma_id,
+			   enum rdma_cm_event_type event)
 {
+	struct isert_np *isert_np = cma_id->context;
 	struct isert_conn *isert_conn;
 
-	if (!cma_id->qp) {
-		struct isert_np *isert_np = cma_id->context;
+	if (isert_np->np_cm_id == cma_id)
+		return isert_np_cma_handler(cma_id->context, event);
 
-		isert_np->np_cm_id = NULL;
-		return -1;
-	}
+	isert_conn = cma_id->qp->qp_context;
 
-	isert_conn = (struct isert_conn *)cma_id->context;
+	mutex_lock(&isert_conn->conn_mutex);
+	isert_conn_terminate(isert_conn);
+	mutex_unlock(&isert_conn->conn_mutex);
 
-	isert_conn->disconnect = disconnect;
-	INIT_WORK(&isert_conn->conn_logout_work, isert_disconnect_work);
-	schedule_work(&isert_conn->conn_logout_work);
+	pr_info("conn %p completing conn_wait\n", isert_conn);
+	complete(&isert_conn->conn_wait);
 
 	return 0;
 }
 
+static void
+isert_connect_error(struct rdma_cm_id *cma_id)
+{
+	struct isert_conn *isert_conn = cma_id->qp->qp_context;
+
+	isert_put_conn(isert_conn);
+}
+
 static int
 isert_cma_handler(struct rdma_cm_id *cma_id, struct rdma_cm_event *event)
 {
 	int ret = 0;
-	bool disconnect = false;
 
 	pr_debug("isert_cma_handler: event %d status %d conn %p id %p\n",
 		 event->event, event->status, cma_id->context, cma_id);
@@ -768,11 +844,14 @@ isert_cma_handler(struct rdma_cm_id *cma_id, struct rdma_cm_event *event)
 	case RDMA_CM_EVENT_ADDR_CHANGE:    /* FALLTHRU */
 	case RDMA_CM_EVENT_DISCONNECTED:   /* FALLTHRU */
 	case RDMA_CM_EVENT_DEVICE_REMOVAL: /* FALLTHRU */
-		disconnect = true;
 	case RDMA_CM_EVENT_TIMEWAIT_EXIT:  /* FALLTHRU */
-		ret = isert_disconnected_handler(cma_id, disconnect);
+		ret = isert_disconnected_handler(cma_id, event->event);
 		break;
+	case RDMA_CM_EVENT_REJECTED:       /* FALLTHRU */
+	case RDMA_CM_EVENT_UNREACHABLE:    /* FALLTHRU */
 	case RDMA_CM_EVENT_CONNECT_ERROR:
+		isert_connect_error(cma_id);
+		break;
 	default:
 		pr_err("Unhandled RDMA CMA event: %d\n", event->event);
 		break;
@@ -906,7 +985,7 @@ isert_init_send_wr(struct isert_conn *isert_conn, struct isert_cmd *isert_cmd,
 	 * bit for every ISERT_COMP_BATCH_COUNT number of ib_post_send() calls.
 	 */
 	mutex_lock(&isert_conn->conn_mutex);
-	if (coalesce && isert_conn->state == ISER_CONN_UP &&
+	if (coalesce && isert_conn->state == ISER_CONN_FULL_FEATURE &&
 	    ++isert_conn->conn_comp_batch < ISERT_COMP_BATCH_COUNT) {
 		tx_desc->llnode_active = true;
 		llist_add(&tx_desc->comp_llnode, &isert_conn->conn_comp_llist);
@@ -1003,7 +1082,10 @@ isert_put_login_tx(struct iscsi_conn *conn, struct iscsi_login *login,
 			if (ret)
 				return ret;
 
-			isert_conn->state = ISER_CONN_UP;
+			/* Now we are in FULL_FEATURE phase */
+			mutex_lock(&isert_conn->conn_mutex);
+			isert_conn->state = ISER_CONN_FULL_FEATURE;
+			mutex_unlock(&isert_conn->conn_mutex);
 			goto post_send;
 		}
 
@@ -1020,18 +1102,17 @@ post_send:
 }
 
 static void
-isert_rx_login_req(struct iser_rx_desc *rx_desc, int rx_buflen,
-		   struct isert_conn *isert_conn)
+isert_rx_login_req(struct isert_conn *isert_conn)
 {
+	struct iser_rx_desc *rx_desc = (void *)isert_conn->login_req_buf;
+	int rx_buflen = isert_conn->login_req_len;
 	struct iscsi_conn *conn = isert_conn->conn;
 	struct iscsi_login *login = conn->conn_login;
 	int size;
 
-	if (!login) {
-		pr_err("conn->conn_login is NULL\n");
-		dump_stack();
-		return;
-	}
+	pr_info("conn %p\n", isert_conn);
+
+	WARN_ON_ONCE(!login);
 
 	if (login->first_request) {
 		struct iscsi_login_req *login_req =
@@ -1394,11 +1475,20 @@ isert_rx_completion(struct iser_rx_desc *desc, struct isert_conn *isert_conn,
 		 hdr->opcode, hdr->itt, hdr->flags,
 		 (int)(xfer_len - ISER_HEADERS_LEN));
 
-	if ((char *)desc == isert_conn->login_req_buf)
-		isert_rx_login_req(desc, xfer_len - ISER_HEADERS_LEN,
-				   isert_conn);
-	else
+	if ((char *)desc == isert_conn->login_req_buf) {
+		isert_conn->login_req_len = xfer_len - ISER_HEADERS_LEN;
+		if (isert_conn->conn) {
+			struct iscsi_login *login = isert_conn->conn->conn_login;
+
+			if (login && !login->first_request)
+				isert_rx_login_req(isert_conn);
+		}
+		mutex_lock(&isert_conn->conn_mutex);
+		complete(&isert_conn->login_req_comp);
+		mutex_unlock(&isert_conn->conn_mutex);
+	} else {
 		isert_rx_do_work(desc, isert_conn);
+	}
 
 	ib_dma_sync_single_for_device(ib_dev, rx_dma, rx_buflen,
 				      DMA_FROM_DEVICE);
@@ -1799,7 +1889,7 @@ isert_cq_rx_comp_err(struct isert_conn *isert_conn)
 		msleep(3000);
 
 	mutex_lock(&isert_conn->conn_mutex);
-	isert_conn->state = ISER_CONN_DOWN;
+	isert_conn_terminate(isert_conn);
 	mutex_unlock(&isert_conn->conn_mutex);
 
 	iscsit_cause_connection_reinstatement(isert_conn->conn, 0);
@@ -2579,13 +2669,51 @@ isert_response_queue(struct iscsi_conn *conn, struct iscsi_cmd *cmd, int state)
 	return ret;
 }
 
+struct rdma_cm_id *
+isert_setup_id(struct isert_np *isert_np)
+{
+	struct iscsi_np *np = isert_np->np;
+	struct rdma_cm_id *id;
+	struct sockaddr *sa;
+	int ret;
+
+	sa = (struct sockaddr *)&np->np_sockaddr;
+	pr_debug("ksockaddr: %p, sa: %p\n", &np->np_sockaddr, sa);
+
+	id = rdma_create_id(isert_cma_handler, isert_np,
+			    RDMA_PS_TCP, IB_QPT_RC);
+	if (IS_ERR(id)) {
+		pr_err("rdma_create_id() failed: %ld\n", PTR_ERR(id));
+		ret = PTR_ERR(id);
+		goto out;
+	}
+	pr_debug("id %p context %p\n", id, id->context);
+
+	ret = rdma_bind_addr(id, sa);
+	if (ret) {
+		pr_err("rdma_bind_addr() failed: %d\n", ret);
+		goto out_id;
+	}
+
+	ret = rdma_listen(id, ISERT_RDMA_LISTEN_BACKLOG);
+	if (ret) {
+		pr_err("rdma_listen() failed: %d\n", ret);
+		goto out_id;
+	}
+
+	return id;
+out_id:
+	rdma_destroy_id(id);
+out:
+	return ERR_PTR(ret);
+}
+
 static int
 isert_setup_np(struct iscsi_np *np,
 	       struct __kernel_sockaddr_storage *ksockaddr)
 {
 	struct isert_np *isert_np;
 	struct rdma_cm_id *isert_lid;
-	struct sockaddr *sa;
 	int ret;
 
 	isert_np = kzalloc(sizeof(struct isert_np), GFP_KERNEL);
@@ -2597,9 +2725,8 @@ isert_setup_np(struct iscsi_np *np,
 	mutex_init(&isert_np->np_accept_mutex);
 	INIT_LIST_HEAD(&isert_np->np_accept_list);
 	init_completion(&isert_np->np_login_comp);
+	isert_np->np = np;
 
-	sa = (struct sockaddr *)ksockaddr;
-	pr_debug("ksockaddr: %p, sa: %p\n", ksockaddr, sa);
 	/*
 	 * Setup the np->np_sockaddr from the passed sockaddr setup
 	 * in iscsi_target_configfs.c code..
@@ -2607,37 +2734,20 @@ isert_setup_np(struct iscsi_np *np,
 	memcpy(&np->np_sockaddr, ksockaddr,
 	       sizeof(struct __kernel_sockaddr_storage));
 
-	isert_lid = rdma_create_id(isert_cma_handler, np, RDMA_PS_TCP,
-				IB_QPT_RC);
+	isert_lid = isert_setup_id(isert_np);
 	if (IS_ERR(isert_lid)) {
-		pr_err("rdma_create_id() for isert_listen_handler failed: %ld\n",
-		       PTR_ERR(isert_lid));
 		ret = PTR_ERR(isert_lid);
 		goto out;
 	}
 
-	ret = rdma_bind_addr(isert_lid, sa);
-	if (ret) {
-		pr_err("rdma_bind_addr() for isert_lid failed: %d\n", ret);
-		goto out_lid;
-	}
-
-	ret = rdma_listen(isert_lid, ISERT_RDMA_LISTEN_BACKLOG);
-	if (ret) {
-		pr_err("rdma_listen() for isert_lid failed: %d\n", ret);
-		goto out_lid;
-	}
-
 	isert_np->np_cm_id = isert_lid;
 	np->np_context = isert_np;
-	pr_debug("Setup isert_lid->context: %p\n", isert_lid->context);
 
 	return 0;
 
-out_lid:
-	rdma_destroy_id(isert_lid);
 out:
 	kfree(isert_np);
+
 	return ret;
 }
 
@@ -2673,7 +2783,15 @@ isert_get_login_rx(struct iscsi_conn *conn, struct iscsi_login *login)
 	struct isert_conn *isert_conn = (struct isert_conn *)conn->context;
 	int ret;
 
-	pr_debug("isert_get_login_rx before conn_login_comp conn: %p\n", conn);
+	pr_info("before login_req comp conn: %p\n", isert_conn);
+	ret = wait_for_completion_interruptible(&isert_conn->login_req_comp);
+	if (ret) {
+		pr_err("isert_conn %p interrupted before got login req\n",
+			  isert_conn);
+		return ret;
+	}
+	reinit_completion(&isert_conn->login_req_comp);
+
 	/*
 	 * For login requests after the first PDU, isert_rx_login_req() will
 	 * kick schedule_delayed_work(&conn->login_work) as the packet is
@@ -2683,11 +2801,15 @@ isert_get_login_rx(struct iscsi_conn *conn, struct iscsi_login *login)
 	if (!login->first_request)
 		return 0;
 
+	isert_rx_login_req(isert_conn);
+
+	pr_info("before conn_login_comp conn: %p\n", conn);
 	ret = wait_for_completion_interruptible(&isert_conn->conn_login_comp);
 	if (ret)
 		return ret;
 
-	pr_debug("isert_get_login_rx processing login->req: %p\n", login->req);
+	pr_info("processing login->req: %p\n", login->req);
+
 	return 0;
 }
 
@@ -2765,17 +2887,10 @@ accept_wait:
 	isert_conn->conn = conn;
 	max_accept = 0;
 
-	ret = isert_rdma_post_recvl(isert_conn);
-	if (ret)
-		return ret;
-
-	ret = isert_rdma_accept(isert_conn);
-	if (ret)
-		return ret;
-
 	isert_set_conn_info(np, conn, isert_conn);
 
-	pr_debug("Processing isert_accept_np: isert_conn: %p\n", isert_conn);
+	pr_debug("Processing isert_conn: %p\n", isert_conn);
+
 	return 0;
 }
 
@@ -2791,6 +2906,24 @@ isert_free_np(struct iscsi_np *np)
 	kfree(isert_np);
 }
 
+static void isert_release_work(struct work_struct *work)
+{
+	struct isert_conn *isert_conn = container_of(work,
+						     struct isert_conn,
+						     release_work);
+
+	pr_info("Starting release conn %p\n", isert_conn);
+
+	wait_for_completion(&isert_conn->conn_wait);
+
+	mutex_lock(&isert_conn->conn_mutex);
+	isert_conn->state = ISER_CONN_DOWN;
+	mutex_unlock(&isert_conn->conn_mutex);
+
+	pr_info("Destroying conn %p\n", isert_conn);
+	isert_put_conn(isert_conn);
+}
+
 static void isert_wait_conn(struct iscsi_conn *conn)
 {
 	struct isert_conn *isert_conn = conn->context;
@@ -2798,10 +2931,6 @@ static void isert_wait_conn(struct iscsi_conn *conn)
 	pr_debug("isert_wait_conn: Starting \n");
 
 	mutex_lock(&isert_conn->conn_mutex);
-	if (isert_conn->conn_cm_id) {
-		pr_debug("Calling rdma_disconnect from isert_wait_conn\n");
-		rdma_disconnect(isert_conn->conn_cm_id);
-	}
 	/*
 	 * Only wait for conn_wait_comp_err if the isert_conn made it
 	 * into full feature phase..
@@ -2810,14 +2939,13 @@ static void isert_wait_conn(struct iscsi_conn *conn)
 		mutex_unlock(&isert_conn->conn_mutex);
 		return;
 	}
-	if (isert_conn->state == ISER_CONN_UP)
-		isert_conn->state = ISER_CONN_TERMINATING;
+	isert_conn_terminate(isert_conn);
 	mutex_unlock(&isert_conn->conn_mutex);
 
 	wait_for_completion(&isert_conn->conn_wait_comp_err);
 
-	wait_for_completion(&isert_conn->conn_wait);
-	isert_put_conn(isert_conn);
+	INIT_WORK(&isert_conn->release_work, isert_release_work);
+	queue_work(isert_release_wq, &isert_conn->release_work);
 }
 
 static void isert_free_conn(struct iscsi_conn *conn)
@@ -2863,10 +2991,21 @@ static int __init isert_init(void)
 		goto destroy_rx_wq;
 	}
 
+	isert_release_wq = alloc_workqueue("isert_release_wq", WQ_UNBOUND,
+					WQ_UNBOUND_MAX_ACTIVE);
+	if (!isert_release_wq) {
+		pr_err("Unable to allocate isert_release_wq\n");
+		ret = -ENOMEM;
+		goto destroy_comp_wq;
+	}
+
 	iscsit_register_transport(&iser_target_transport);
-	pr_debug("iSER_TARGET[0] - Loaded iser_target_transport\n");
+	pr_info("iSER_TARGET[0] - Loaded iser_target_transport\n");
+
 	return 0;
 
+destroy_comp_wq:
+	destroy_workqueue(isert_comp_wq);
 destroy_rx_wq:
 	destroy_workqueue(isert_rx_wq);
 	return ret;
@@ -2875,6 +3014,7 @@ destroy_rx_wq:
 static void __exit isert_exit(void)
 {
 	flush_scheduled_work();
+	destroy_workqueue(isert_release_wq);
 	destroy_workqueue(isert_comp_wq);
 	destroy_workqueue(isert_rx_wq);
 	iscsit_unregister_transport(&iser_target_transport);
diff --git a/drivers/infiniband/ulp/isert/ib_isert.h b/drivers/infiniband/ulp/isert/ib_isert.h
index cbecaab..1178c5b 100644
--- a/drivers/infiniband/ulp/isert/ib_isert.h
+++ b/drivers/infiniband/ulp/isert/ib_isert.h
@@ -23,6 +23,7 @@ enum iser_ib_op_code {
 enum iser_conn_state {
 	ISER_CONN_INIT,
 	ISER_CONN_UP,
+	ISER_CONN_FULL_FEATURE,
 	ISER_CONN_TERMINATING,
 	ISER_CONN_DOWN,
 };
@@ -102,6 +103,7 @@ struct isert_conn {
 	char			*login_req_buf;
 	char			*login_rsp_buf;
 	u64			login_req_dma;
+	int			login_req_len;
 	u64			login_rsp_dma;
 	unsigned int		conn_rx_desc_head;
 	struct iser_rx_desc	*conn_rx_descs;
@@ -109,13 +111,13 @@ struct isert_conn {
 	struct iscsi_conn	*conn;
 	struct list_head	conn_accept_node;
 	struct completion	conn_login_comp;
+	struct completion	login_req_comp;
 	struct iser_tx_desc	conn_login_tx_desc;
 	struct rdma_cm_id	*conn_cm_id;
 	struct ib_pd		*conn_pd;
 	struct ib_mr		*conn_mr;
 	struct ib_qp		*conn_qp;
 	struct isert_device	*conn_device;
-	struct work_struct	conn_logout_work;
 	struct mutex		conn_mutex;
 	struct completion	conn_wait;
 	struct completion	conn_wait_comp_err;
@@ -124,10 +126,10 @@ struct isert_conn {
 	int			conn_fr_pool_size;
 	/* lock to protect fastreg pool */
 	spinlock_t		conn_lock;
+	struct work_struct	release_work;
 #define ISERT_COMP_BATCH_COUNT	8
 	int			conn_comp_batch;
 	struct llist_head	conn_comp_llist;
-	bool                    disconnect;
 };
 
 #define ISERT_MAX_CQ 64
@@ -158,6 +160,7 @@ struct isert_device {
 };
 
 struct isert_np {
+	struct iscsi_np         *np;
 	struct semaphore	np_sem;
 	struct rdma_cm_id	*np_cm_id;
 	struct mutex		np_accept_mutex;
diff --git a/drivers/input/serio/i8042-x86ia64io.h b/drivers/input/serio/i8042-x86ia64io.h
index 8fca488f..c43c46f 100644
--- a/drivers/input/serio/i8042-x86ia64io.h
+++ b/drivers/input/serio/i8042-x86ia64io.h
@@ -408,6 +408,13 @@ static const struct dmi_system_id __initconst i8042_dmi_nomux_table[] = {
 		},
 	},
 	{
+		/* Acer Aspire 7738 */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "Acer"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "Aspire 7738"),
+		},
+	},
+	{
 		/* Gericom Bellagio */
 		.matches = {
 			DMI_MATCH(DMI_SYS_VENDOR, "Gericom"),
@@ -721,6 +728,35 @@ static const struct dmi_system_id __initconst i8042_dmi_dritek_table[] = {
 	{ }
 };
 
+/*
+ * Some laptops need keyboard reset before probing for the trackpad to get
+ * it detected, initialised & finally work.
+ */
+static const struct dmi_system_id __initconst i8042_dmi_kbdreset_table[] = {
+	{
+		/* Gigabyte P35 v2 - Elantech touchpad */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GIGABYTE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "P35V2"),
+		},
+	},
+		{
+		/* Aorus branded Gigabyte X3 Plus - Elantech touchpad */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GIGABYTE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "X3"),
+		},
+	},
+	{
+		/* Gigabyte P34 - Elantech touchpad */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GIGABYTE"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "P34"),
+		},
+	},
+	{ }
+};
+
 #endif /* CONFIG_X86 */
 
 #ifdef CONFIG_PNP
@@ -1016,6 +1052,9 @@ static int __init i8042_platform_init(void)
 	if (dmi_check_system(i8042_dmi_dritek_table))
 		i8042_dritek = true;
 
+	if (dmi_check_system(i8042_dmi_kbdreset_table))
+		i8042_kbdreset = true;
+
 	/*
 	 * A20 was already enabled during early kernel init. But some buggy
 	 * BIOSes (in MSI Laptops) require A20 to be enabled using 8042 to
diff --git a/drivers/input/serio/i8042.c b/drivers/input/serio/i8042.c
index 3807c3e..eb796ff 100644
--- a/drivers/input/serio/i8042.c
+++ b/drivers/input/serio/i8042.c
@@ -67,6 +67,10 @@ static bool i8042_notimeout;
 module_param_named(notimeout, i8042_notimeout, bool, 0);
 MODULE_PARM_DESC(notimeout, "Ignore timeouts signalled by i8042");
 
+static bool i8042_kbdreset;
+module_param_named(kbdreset, i8042_kbdreset, bool, 0);
+MODULE_PARM_DESC(kbdreset, "Reset device connected to KBD port");
+
 #ifdef CONFIG_X86
 static bool i8042_dritek;
 module_param_named(dritek, i8042_dritek, bool, 0);
@@ -790,6 +794,16 @@ static int __init i8042_check_aux(void)
 		return -1;
 
 /*
+ * Reset keyboard (needed on some laptops to successfully detect
+ * touchpad, e.g., some Gigabyte laptop models with Elantech
+ * touchpads).
+ */
+	if (i8042_kbdreset) {
+		pr_warn("Attempting to reset device connected to KBD port\n");
+		i8042_kbd_write(NULL, (unsigned char) 0xff);
+	}
+
+/*
  * Test AUX IRQ delivery to make sure BIOS did not grab the IRQ and
  * used it for a PCI card or somethig else.
  */
diff --git a/drivers/md/bcache/btree.c b/drivers/md/bcache/btree.c
index 5f9c2a6..fbcb622 100644
--- a/drivers/md/bcache/btree.c
+++ b/drivers/md/bcache/btree.c
@@ -199,7 +199,7 @@ void bch_btree_node_read_done(struct btree *b)
 	struct bset *i = btree_bset_first(b);
 	struct btree_iter *iter;
 
-	iter = mempool_alloc(b->c->fill_iter, GFP_NOWAIT);
+	iter = mempool_alloc(b->c->fill_iter, GFP_NOIO);
 	iter->size = b->c->sb.bucket_size / b->c->sb.block_size;
 	iter->used = 0;
 
diff --git a/drivers/media/i2c/smiapp-pll.c b/drivers/media/i2c/smiapp-pll.c
index 2335529..ab5d9a3 100644
--- a/drivers/media/i2c/smiapp-pll.c
+++ b/drivers/media/i2c/smiapp-pll.c
@@ -67,7 +67,7 @@ static void print_pll(struct device *dev, struct smiapp_pll *pll)
 {
 	dev_dbg(dev, "pre_pll_clk_div\t%d\n",  pll->pre_pll_clk_div);
 	dev_dbg(dev, "pll_multiplier \t%d\n",  pll->pll_multiplier);
-	if (pll->flags != SMIAPP_PLL_FLAG_NO_OP_CLOCKS) {
+	if (!(pll->flags & SMIAPP_PLL_FLAG_NO_OP_CLOCKS)) {
 		dev_dbg(dev, "op_sys_clk_div \t%d\n", pll->op_sys_clk_div);
 		dev_dbg(dev, "op_pix_clk_div \t%d\n", pll->op_pix_clk_div);
 	}
@@ -77,7 +77,7 @@ static void print_pll(struct device *dev, struct smiapp_pll *pll)
 	dev_dbg(dev, "ext_clk_freq_hz \t%d\n", pll->ext_clk_freq_hz);
 	dev_dbg(dev, "pll_ip_clk_freq_hz \t%d\n", pll->pll_ip_clk_freq_hz);
 	dev_dbg(dev, "pll_op_clk_freq_hz \t%d\n", pll->pll_op_clk_freq_hz);
-	if (pll->flags & SMIAPP_PLL_FLAG_NO_OP_CLOCKS) {
+	if (!(pll->flags & SMIAPP_PLL_FLAG_NO_OP_CLOCKS)) {
 		dev_dbg(dev, "op_sys_clk_freq_hz \t%d\n",
 			pll->op_sys_clk_freq_hz);
 		dev_dbg(dev, "op_pix_clk_freq_hz \t%d\n",
diff --git a/drivers/media/i2c/smiapp/smiapp-core.c b/drivers/media/i2c/smiapp/smiapp-core.c
index 7026ab0..873d062 100644
--- a/drivers/media/i2c/smiapp/smiapp-core.c
+++ b/drivers/media/i2c/smiapp/smiapp-core.c
@@ -2624,7 +2624,9 @@ static int smiapp_registered(struct v4l2_subdev *subdev)
 		pll->flags |= SMIAPP_PLL_FLAG_OP_PIX_CLOCK_PER_LANE;
 	pll->scale_n = sensor->limits[SMIAPP_LIMIT_SCALER_N_MIN];
 
+	mutex_lock(&sensor->mutex);
 	rval = smiapp_update_mode(sensor);
+	mutex_unlock(&sensor->mutex);
 	if (rval) {
 		dev_err(&client->dev, "update mode failed\n");
 		goto out_nvm_release;
diff --git a/drivers/media/usb/au0828/au0828-cards.c b/drivers/media/usb/au0828/au0828-cards.c
index dd32dec..1d4b110 100644
--- a/drivers/media/usb/au0828/au0828-cards.c
+++ b/drivers/media/usb/au0828/au0828-cards.c
@@ -36,6 +36,11 @@ static void hvr950q_cs5340_audio(void *priv, int enable)
 		au0828_clear(dev, REG_000, 0x10);
 }
 
+/*
+ * WARNING: There's a quirks table at sound/usb/quirks-table.h
+ * that should also be updated every time a new device with V4L2 support
+ * is added here.
+ */
 struct au0828_board au0828_boards[] = {
 	[AU0828_BOARD_UNKNOWN] = {
 		.name	= "Unknown board",
diff --git a/drivers/media/usb/dvb-usb/af9005.c b/drivers/media/usb/dvb-usb/af9005.c
index af176b6..e6d3561 100644
--- a/drivers/media/usb/dvb-usb/af9005.c
+++ b/drivers/media/usb/dvb-usb/af9005.c
@@ -1081,9 +1081,12 @@ static int __init af9005_usb_module_init(void)
 		err("usb_register failed. (%d)", result);
 		return result;
 	}
+#if IS_MODULE(CONFIG_DVB_USB_AF9005) || defined(CONFIG_DVB_USB_AF9005_REMOTE)
+	/* FIXME: convert to todays kernel IR infrastructure */
 	rc_decode = symbol_request(af9005_rc_decode);
 	rc_keys = symbol_request(rc_map_af9005_table);
 	rc_keys_size = symbol_request(rc_map_af9005_table_size);
+#endif
 	if (rc_decode == NULL || rc_keys == NULL || rc_keys_size == NULL) {
 		err("af9005_rc_decode function not found, disabling remote");
 		af9005_properties.rc.legacy.rc_query = NULL;
diff --git a/drivers/media/usb/uvc/uvc_driver.c b/drivers/media/usb/uvc/uvc_driver.c
index 753ad4c..4531441 100644
--- a/drivers/media/usb/uvc/uvc_driver.c
+++ b/drivers/media/usb/uvc/uvc_driver.c
@@ -1603,12 +1603,12 @@ static void uvc_delete(struct uvc_device *dev)
 {
 	struct list_head *p, *n;
 
-	usb_put_intf(dev->intf);
-	usb_put_dev(dev->udev);
-
 	uvc_status_cleanup(dev);
 	uvc_ctrl_cleanup_device(dev);
 
+	usb_put_intf(dev->intf);
+	usb_put_dev(dev->udev);
+
 	if (dev->vdev.dev)
 		v4l2_device_unregister(&dev->vdev);
 #ifdef CONFIG_MEDIA_CONTROLLER
diff --git a/drivers/net/can/usb/kvaser_usb.c b/drivers/net/can/usb/kvaser_usb.c
index e77d110..4e65b35 100644
--- a/drivers/net/can/usb/kvaser_usb.c
+++ b/drivers/net/can/usb/kvaser_usb.c
@@ -1237,6 +1237,9 @@ static int kvaser_usb_close(struct net_device *netdev)
 	if (err)
 		netdev_warn(netdev, "Cannot stop device, error %d\n", err);
 
+	/* reset tx contexts */
+	kvaser_usb_unlink_tx_urbs(priv);
+
 	priv->can.state = CAN_STATE_STOPPED;
 	close_candev(priv->netdev);
 
@@ -1285,12 +1288,14 @@ static netdev_tx_t kvaser_usb_start_xmit(struct sk_buff *skb,
 	if (!urb) {
 		netdev_err(netdev, "No memory left for URBs\n");
 		stats->tx_dropped++;
-		goto nourbmem;
+		dev_kfree_skb(skb);
+		return NETDEV_TX_OK;
 	}
 
 	buf = kmalloc(sizeof(struct kvaser_msg), GFP_ATOMIC);
 	if (!buf) {
 		stats->tx_dropped++;
+		dev_kfree_skb(skb);
 		goto nobufmem;
 	}
 
@@ -1325,6 +1330,7 @@ static netdev_tx_t kvaser_usb_start_xmit(struct sk_buff *skb,
 		}
 	}
 
+	/* This should never happen; it implies a flow control bug */
 	if (!context) {
 		netdev_warn(netdev, "cannot find free context\n");
 		ret =  NETDEV_TX_BUSY;
@@ -1355,9 +1361,6 @@ static netdev_tx_t kvaser_usb_start_xmit(struct sk_buff *skb,
 	if (unlikely(err)) {
 		can_free_echo_skb(netdev, context->echo_index);
 
-		skb = NULL; /* set to NULL to avoid double free in
-			     * dev_kfree_skb(skb) */
-
 		atomic_dec(&priv->active_tx_urbs);
 		usb_unanchor_urb(urb);
 
@@ -1379,8 +1382,6 @@ releasebuf:
 	kfree(buf);
 nobufmem:
 	usb_free_urb(urb);
-nourbmem:
-	dev_kfree_skb(skb);
 	return ret;
 }
 
@@ -1492,6 +1493,10 @@ static int kvaser_usb_init_one(struct usb_interface *intf,
 	struct kvaser_usb_net_priv *priv;
 	int i, err;
 
+	err = kvaser_usb_send_simple_msg(dev, CMD_RESET_CHIP, channel);
+	if (err)
+		return err;
+
 	netdev = alloc_candev(sizeof(*priv), MAX_TX_URBS);
 	if (!netdev) {
 		dev_err(&intf->dev, "Cannot alloc candev\n");
@@ -1595,9 +1600,6 @@ static int kvaser_usb_probe(struct usb_interface *intf,
 
 	usb_set_intfdata(intf, dev);
 
-	for (i = 0; i < MAX_NET_DEVICES; i++)
-		kvaser_usb_send_simple_msg(dev, CMD_RESET_CHIP, i);
-
 	err = kvaser_usb_get_software_info(dev);
 	if (err) {
 		dev_err(&intf->dev,
diff --git a/drivers/net/ethernet/atheros/alx/main.c b/drivers/net/ethernet/atheros/alx/main.c
index 380d249..3e1d7d2 100644
--- a/drivers/net/ethernet/atheros/alx/main.c
+++ b/drivers/net/ethernet/atheros/alx/main.c
@@ -184,15 +184,16 @@ static void alx_schedule_reset(struct alx_priv *alx)
 	schedule_work(&alx->reset_wk);
 }
 
-static bool alx_clean_rx_irq(struct alx_priv *alx, int budget)
+static int alx_clean_rx_irq(struct alx_priv *alx, int budget)
 {
 	struct alx_rx_queue *rxq = &alx->rxq;
 	struct alx_rrd *rrd;
 	struct alx_buffer *rxb;
 	struct sk_buff *skb;
 	u16 length, rfd_cleaned = 0;
+	int work = 0;
 
-	while (budget > 0) {
+	while (work < budget) {
 		rrd = &rxq->rrd[rxq->rrd_read_idx];
 		if (!(rrd->word3 & cpu_to_le32(1 << RRD_UPDATED_SHIFT)))
 			break;
@@ -203,7 +204,7 @@ static bool alx_clean_rx_irq(struct alx_priv *alx, int budget)
 		    ALX_GET_FIELD(le32_to_cpu(rrd->word0),
 				  RRD_NOR) != 1) {
 			alx_schedule_reset(alx);
-			return 0;
+			return work;
 		}
 
 		rxb = &rxq->bufs[rxq->read_idx];
@@ -243,7 +244,7 @@ static bool alx_clean_rx_irq(struct alx_priv *alx, int budget)
 		}
 
 		napi_gro_receive(&alx->napi, skb);
-		budget--;
+		work++;
 
 next_pkt:
 		if (++rxq->read_idx == alx->rx_ringsz)
@@ -258,21 +259,22 @@ next_pkt:
 	if (rfd_cleaned)
 		alx_refill_rx_ring(alx, GFP_ATOMIC);
 
-	return budget > 0;
+	return work;
 }
 
 static int alx_poll(struct napi_struct *napi, int budget)
 {
 	struct alx_priv *alx = container_of(napi, struct alx_priv, napi);
 	struct alx_hw *hw = &alx->hw;
-	bool complete = true;
 	unsigned long flags;
+	bool tx_complete;
+	int work;
 
-	complete = alx_clean_tx_irq(alx) &&
-		   alx_clean_rx_irq(alx, budget);
+	tx_complete = alx_clean_tx_irq(alx);
+	work = alx_clean_rx_irq(alx, budget);
 
-	if (!complete)
-		return 1;
+	if (!tx_complete || work == budget)
+		return budget;
 
 	napi_complete(&alx->napi);
 
@@ -284,7 +286,7 @@ static int alx_poll(struct napi_struct *napi, int budget)
 
 	alx_post_write(hw);
 
-	return 0;
+	return work;
 }
 
 static irqreturn_t alx_intr_handle(struct alx_priv *alx, u32 intr)
diff --git a/drivers/net/ethernet/broadcom/tg3.c b/drivers/net/ethernet/broadcom/tg3.c
index 086eac5..8206113 100644
--- a/drivers/net/ethernet/broadcom/tg3.c
+++ b/drivers/net/ethernet/broadcom/tg3.c
@@ -17731,23 +17731,6 @@ static int tg3_init_one(struct pci_dev *pdev,
 		goto err_out_apeunmap;
 	}
 
-	/*
-	 * Reset chip in case UNDI or EFI driver did not shutdown
-	 * DMA self test will enable WDMAC and we'll see (spurious)
-	 * pending DMA on the PCI bus at that point.
-	 */
-	if ((tr32(HOSTCC_MODE) & HOSTCC_MODE_ENABLE) ||
-	    (tr32(WDMAC_MODE) & WDMAC_MODE_ENABLE)) {
-		tw32(MEMARB_MODE, MEMARB_MODE_ENABLE);
-		tg3_halt(tp, RESET_KIND_SHUTDOWN, 1);
-	}
-
-	err = tg3_test_dma(tp);
-	if (err) {
-		dev_err(&pdev->dev, "DMA engine test failed, aborting\n");
-		goto err_out_apeunmap;
-	}
-
 	intmbx = MAILBOX_INTERRUPT_0 + TG3_64BIT_REG_LOW;
 	rcvmbx = MAILBOX_RCVRET_CON_IDX_0 + TG3_64BIT_REG_LOW;
 	sndmbx = MAILBOX_SNDHOST_PROD_IDX_0 + TG3_64BIT_REG_LOW;
@@ -17792,6 +17775,23 @@ static int tg3_init_one(struct pci_dev *pdev,
 			sndmbx += 0xc;
 	}
 
+	/*
+	 * Reset chip in case UNDI or EFI driver did not shutdown
+	 * DMA self test will enable WDMAC and we'll see (spurious)
+	 * pending DMA on the PCI bus at that point.
+	 */
+	if ((tr32(HOSTCC_MODE) & HOSTCC_MODE_ENABLE) ||
+	    (tr32(WDMAC_MODE) & WDMAC_MODE_ENABLE)) {
+		tw32(MEMARB_MODE, MEMARB_MODE_ENABLE);
+		tg3_halt(tp, RESET_KIND_SHUTDOWN, 1);
+	}
+
+	err = tg3_test_dma(tp);
+	if (err) {
+		dev_err(&pdev->dev, "DMA engine test failed, aborting\n");
+		goto err_out_apeunmap;
+	}
+
 	tg3_init_coal(tp);
 
 	pci_set_drvdata(pdev, dev);
diff --git a/drivers/net/ethernet/cisco/enic/enic_main.c b/drivers/net/ethernet/cisco/enic/enic_main.c
index b740bfc..ff9b423 100644
--- a/drivers/net/ethernet/cisco/enic/enic_main.c
+++ b/drivers/net/ethernet/cisco/enic/enic_main.c
@@ -1044,10 +1044,14 @@ static void enic_rq_indicate_buf(struct vnic_rq *rq,
 				     PKT_HASH_TYPE_L4 : PKT_HASH_TYPE_L3);
 		}
 
-		if ((netdev->features & NETIF_F_RXCSUM) && !csum_not_calc) {
-			skb->csum = htons(checksum);
-			skb->ip_summed = CHECKSUM_COMPLETE;
-		}
+		/* Hardware does not provide whole packet checksum. It only
+		 * provides pseudo checksum. Since hw validates the packet
+		 * checksum but not provide us the checksum value. use
+		 * CHECSUM_UNNECESSARY.
+		 */
+		if ((netdev->features & NETIF_F_RXCSUM) && tcp_udp_csum_ok &&
+		    ipv4_csum_ok)
+			skb->ip_summed = CHECKSUM_UNNECESSARY;
 
 		if (vlan_stripped)
 			__vlan_hwaccel_put_tag(skb, htons(ETH_P_8021Q), vlan_tci);
diff --git a/drivers/net/ethernet/ti/cpsw.c b/drivers/net/ethernet/ti/cpsw.c
index 921b9df..316650c 100644
--- a/drivers/net/ethernet/ti/cpsw.c
+++ b/drivers/net/ethernet/ti/cpsw.c
@@ -596,7 +596,7 @@ static void cpsw_set_promiscious(struct net_device *ndev, bool enable)
 
 			/* Clear all mcast from ALE */
 			cpsw_ale_flush_multicast(ale, ALE_ALL_PORTS <<
-						 priv->host_port);
+						 priv->host_port, -1);
 
 			/* Flood All Unicast Packets to Host port */
 			cpsw_ale_control_set(ale, 0, ALE_P0_UNI_FLOOD, 1);
@@ -620,6 +620,12 @@ static void cpsw_set_promiscious(struct net_device *ndev, bool enable)
 static void cpsw_ndo_set_rx_mode(struct net_device *ndev)
 {
 	struct cpsw_priv *priv = netdev_priv(ndev);
+	int vid;
+
+	if (priv->data.dual_emac)
+		vid = priv->slaves[priv->emac_port].port_vlan;
+	else
+		vid = priv->data.default_vlan;
 
 	if (ndev->flags & IFF_PROMISC) {
 		/* Enable promiscuous mode */
@@ -631,7 +637,8 @@ static void cpsw_ndo_set_rx_mode(struct net_device *ndev)
 	}
 
 	/* Clear all mcast from ALE */
-	cpsw_ale_flush_multicast(priv->ale, ALE_ALL_PORTS << priv->host_port);
+	cpsw_ale_flush_multicast(priv->ale, ALE_ALL_PORTS << priv->host_port,
+				 vid);
 
 	if (!netdev_mc_empty(ndev)) {
 		struct netdev_hw_addr *ha;
@@ -716,6 +723,14 @@ static void cpsw_rx_handler(void *token, int len, int status)
 static irqreturn_t cpsw_interrupt(int irq, void *dev_id)
 {
 	struct cpsw_priv *priv = dev_id;
+	int value = irq - priv->irqs_table[0];
+
+	/* NOTICE: Ending IRQ here. The trick with the 'value' variable above
+	 * is to make sure we will always write the correct value to the EOI
+	 * register. Namely 0 for RX_THRESH Interrupt, 1 for RX Interrupt, 2
+	 * for TX Interrupt and 3 for MISC Interrupt.
+	 */
+	cpdma_ctlr_eoi(priv->dma, value);
 
 	cpsw_intr_disable(priv);
 	if (priv->irq_enabled == true) {
@@ -745,8 +760,6 @@ static int cpsw_poll(struct napi_struct *napi, int budget)
 	int			num_tx, num_rx;
 
 	num_tx = cpdma_chan_process(priv->txch, 128);
-	if (num_tx)
-		cpdma_ctlr_eoi(priv->dma, CPDMA_EOI_TX);
 
 	num_rx = cpdma_chan_process(priv->rxch, budget);
 	if (num_rx < budget) {
@@ -754,7 +767,6 @@ static int cpsw_poll(struct napi_struct *napi, int budget)
 
 		napi_complete(napi);
 		cpsw_intr_enable(priv);
-		cpdma_ctlr_eoi(priv->dma, CPDMA_EOI_RX);
 		prim_cpsw = cpsw_get_slave_priv(priv, 0);
 		if (prim_cpsw->irq_enabled == false) {
 			prim_cpsw->irq_enabled = true;
@@ -1265,8 +1277,6 @@ static int cpsw_ndo_open(struct net_device *ndev)
 	napi_enable(&priv->napi);
 	cpdma_ctlr_start(priv->dma);
 	cpsw_intr_enable(priv);
-	cpdma_ctlr_eoi(priv->dma, CPDMA_EOI_RX);
-	cpdma_ctlr_eoi(priv->dma, CPDMA_EOI_TX);
 
 	if (priv->data.dual_emac)
 		priv->slaves[priv->emac_port].open_stat = true;
@@ -1512,9 +1522,6 @@ static void cpsw_ndo_tx_timeout(struct net_device *ndev)
 	cpdma_chan_start(priv->txch);
 	cpdma_ctlr_int_ctrl(priv->dma, true);
 	cpsw_intr_enable(priv);
-	cpdma_ctlr_eoi(priv->dma, CPDMA_EOI_RX);
-	cpdma_ctlr_eoi(priv->dma, CPDMA_EOI_TX);
-
 }
 
 static int cpsw_ndo_set_mac_address(struct net_device *ndev, void *p)
@@ -1560,9 +1567,6 @@ static void cpsw_ndo_poll_controller(struct net_device *ndev)
 	cpsw_interrupt(ndev->irq, priv);
 	cpdma_ctlr_int_ctrl(priv->dma, true);
 	cpsw_intr_enable(priv);
-	cpdma_ctlr_eoi(priv->dma, CPDMA_EOI_RX);
-	cpdma_ctlr_eoi(priv->dma, CPDMA_EOI_TX);
-
 }
 #endif
 
diff --git a/drivers/net/ethernet/ti/cpsw_ale.c b/drivers/net/ethernet/ti/cpsw_ale.c
index 7f89306..4eceb7e 100644
--- a/drivers/net/ethernet/ti/cpsw_ale.c
+++ b/drivers/net/ethernet/ti/cpsw_ale.c
@@ -236,7 +236,7 @@ static void cpsw_ale_flush_mcast(struct cpsw_ale *ale, u32 *ale_entry,
 		cpsw_ale_set_entry_type(ale_entry, ALE_TYPE_FREE);
 }
 
-int cpsw_ale_flush_multicast(struct cpsw_ale *ale, int port_mask)
+int cpsw_ale_flush_multicast(struct cpsw_ale *ale, int port_mask, int vid)
 {
 	u32 ale_entry[ALE_ENTRY_WORDS];
 	int ret, idx;
@@ -247,6 +247,14 @@ int cpsw_ale_flush_multicast(struct cpsw_ale *ale, int port_mask)
 		if (ret != ALE_TYPE_ADDR && ret != ALE_TYPE_VLAN_ADDR)
 			continue;
 
+		/* if vid passed is -1 then remove all multicast entry from
+		 * the table irrespective of vlan id, if a valid vlan id is
+		 * passed then remove only multicast added to that vlan id.
+		 * if vlan id doesn't match then move on to next entry.
+		 */
+		if (vid != -1 && cpsw_ale_get_vlan_id(ale_entry) != vid)
+			continue;
+
 		if (cpsw_ale_get_mcast(ale_entry)) {
 			u8 addr[6];
 
diff --git a/drivers/net/ethernet/ti/cpsw_ale.h b/drivers/net/ethernet/ti/cpsw_ale.h
index de409c3..e701358 100644
--- a/drivers/net/ethernet/ti/cpsw_ale.h
+++ b/drivers/net/ethernet/ti/cpsw_ale.h
@@ -88,7 +88,7 @@ void cpsw_ale_stop(struct cpsw_ale *ale);
 
 int cpsw_ale_set_ageout(struct cpsw_ale *ale, int ageout);
 int cpsw_ale_flush(struct cpsw_ale *ale, int port_mask);
-int cpsw_ale_flush_multicast(struct cpsw_ale *ale, int port_mask);
+int cpsw_ale_flush_multicast(struct cpsw_ale *ale, int port_mask, int vid);
 int cpsw_ale_add_ucast(struct cpsw_ale *ale, u8 *addr, int port,
 		       int flags, u16 vid);
 int cpsw_ale_del_ucast(struct cpsw_ale *ale, u8 *addr, int port,
diff --git a/drivers/net/team/team.c b/drivers/net/team/team.c
index 979fe43..32efe83 100644
--- a/drivers/net/team/team.c
+++ b/drivers/net/team/team.c
@@ -629,6 +629,7 @@ static int team_change_mode(struct team *team, const char *kind)
 static void team_notify_peers_work(struct work_struct *work)
 {
 	struct team *team;
+	int val;
 
 	team = container_of(work, struct team, notify_peers.dw.work);
 
@@ -636,9 +637,14 @@ static void team_notify_peers_work(struct work_struct *work)
 		schedule_delayed_work(&team->notify_peers.dw, 0);
 		return;
 	}
+	val = atomic_dec_if_positive(&team->notify_peers.count_pending);
+	if (val < 0) {
+		rtnl_unlock();
+		return;
+	}
 	call_netdevice_notifiers(NETDEV_NOTIFY_PEERS, team->dev);
 	rtnl_unlock();
-	if (!atomic_dec_and_test(&team->notify_peers.count_pending))
+	if (val)
 		schedule_delayed_work(&team->notify_peers.dw,
 				      msecs_to_jiffies(team->notify_peers.interval));
 }
@@ -669,6 +675,7 @@ static void team_notify_peers_fini(struct team *team)
 static void team_mcast_rejoin_work(struct work_struct *work)
 {
 	struct team *team;
+	int val;
 
 	team = container_of(work, struct team, mcast_rejoin.dw.work);
 
@@ -676,9 +683,14 @@ static void team_mcast_rejoin_work(struct work_struct *work)
 		schedule_delayed_work(&team->mcast_rejoin.dw, 0);
 		return;
 	}
+	val = atomic_dec_if_positive(&team->mcast_rejoin.count_pending);
+	if (val < 0) {
+		rtnl_unlock();
+		return;
+	}
 	call_netdevice_notifiers(NETDEV_RESEND_IGMP, team->dev);
 	rtnl_unlock();
-	if (!atomic_dec_and_test(&team->mcast_rejoin.count_pending))
+	if (val)
 		schedule_delayed_work(&team->mcast_rejoin.dw,
 				      msecs_to_jiffies(team->mcast_rejoin.interval));
 }
diff --git a/drivers/platform/x86/hp_accel.c b/drivers/platform/x86/hp_accel.c
index 3dc9344..07fbcb0 100644
--- a/drivers/platform/x86/hp_accel.c
+++ b/drivers/platform/x86/hp_accel.c
@@ -237,6 +237,7 @@ static struct dmi_system_id lis3lv02d_dmi_ids[] = {
 	AXIS_DMI_MATCH("HPB64xx", "HP ProBook 64", xy_swap),
 	AXIS_DMI_MATCH("HPB64xx", "HP EliteBook 84", xy_swap),
 	AXIS_DMI_MATCH("HPB65xx", "HP ProBook 65", x_inverted),
+	AXIS_DMI_MATCH("HPZBook15", "HP ZBook 15", x_inverted),
 	{ NULL, }
 /* Laptop models without axis info (yet):
  * "NC6910" "HP Compaq 6910"
diff --git a/drivers/s390/char/con3215.c b/drivers/s390/char/con3215.c
index bb86494..19915c5 100644
--- a/drivers/s390/char/con3215.c
+++ b/drivers/s390/char/con3215.c
@@ -288,12 +288,16 @@ static void raw3215_timeout(unsigned long __data)
 	unsigned long flags;
 
 	spin_lock_irqsave(get_ccwdev_lock(raw->cdev), flags);
-	if (raw->flags & RAW3215_TIMER_RUNS) {
-		del_timer(&raw->timer);
-		raw->flags &= ~RAW3215_TIMER_RUNS;
-		if (!(raw->port.flags & ASYNC_SUSPENDED)) {
-			raw3215_mk_write_req(raw);
-			raw3215_start_io(raw);
+	raw->flags &= ~RAW3215_TIMER_RUNS;
+	if (!(raw->port.flags & ASYNC_SUSPENDED)) {
+		raw3215_mk_write_req(raw);
+		raw3215_start_io(raw);
+		if ((raw->queued_read || raw->queued_write) &&
+		    !(raw->flags & RAW3215_WORKING) &&
+		    !(raw->flags & RAW3215_TIMER_RUNS)) {
+			raw->timer.expires = RAW3215_TIMEOUT + jiffies;
+			add_timer(&raw->timer);
+			raw->flags |= RAW3215_TIMER_RUNS;
 		}
 	}
 	spin_unlock_irqrestore(get_ccwdev_lock(raw->cdev), flags);
@@ -317,17 +321,15 @@ static inline void raw3215_try_io(struct raw3215_info *raw)
 		    (raw->flags & RAW3215_FLUSHING)) {
 			/* execute write requests bigger than minimum size */
 			raw3215_start_io(raw);
-			if (raw->flags & RAW3215_TIMER_RUNS) {
-				del_timer(&raw->timer);
-				raw->flags &= ~RAW3215_TIMER_RUNS;
-			}
-		} else if (!(raw->flags & RAW3215_TIMER_RUNS)) {
-			/* delay small writes */
-			raw->timer.expires = RAW3215_TIMEOUT + jiffies;
-			add_timer(&raw->timer);
-			raw->flags |= RAW3215_TIMER_RUNS;
 		}
 	}
+	if ((raw->queued_read || raw->queued_write) &&
+	    !(raw->flags & RAW3215_WORKING) &&
+	    !(raw->flags & RAW3215_TIMER_RUNS)) {
+		raw->timer.expires = RAW3215_TIMEOUT + jiffies;
+		add_timer(&raw->timer);
+		raw->flags |= RAW3215_TIMER_RUNS;
+	}
 }
 
 /*
@@ -1027,12 +1029,26 @@ static int tty3215_write(struct tty_struct * tty,
 			 const unsigned char *buf, int count)
 {
 	struct raw3215_info *raw;
+	int i, written;
 
 	if (!tty)
 		return 0;
 	raw = (struct raw3215_info *) tty->driver_data;
-	raw3215_write(raw, buf, count);
-	return count;
+	written = count;
+	while (count > 0) {
+		for (i = 0; i < count; i++)
+			if (buf[i] == '\t' || buf[i] == '\n')
+				break;
+		raw3215_write(raw, buf, i);
+		count -= i;
+		buf += i;
+		if (count > 0) {
+			raw3215_putchar(raw, *buf);
+			count--;
+			buf++;
+		}
+	}
+	return written;
 }
 
 /*
@@ -1180,7 +1196,7 @@ static int __init tty3215_init(void)
 	driver->subtype = SYSTEM_TYPE_TTY;
 	driver->init_termios = tty_std_termios;
 	driver->init_termios.c_iflag = IGNBRK | IGNPAR;
-	driver->init_termios.c_oflag = ONLCR | XTABS;
+	driver->init_termios.c_oflag = ONLCR;
 	driver->init_termios.c_lflag = ISIG;
 	driver->flags = TTY_DRIVER_REAL_RAW;
 	tty_set_operations(driver, &tty3215_ops);
diff --git a/drivers/scsi/mpt2sas/mpt2sas_transport.c b/drivers/scsi/mpt2sas/mpt2sas_transport.c
index 410f4a3..72f9c55 100644
--- a/drivers/scsi/mpt2sas/mpt2sas_transport.c
+++ b/drivers/scsi/mpt2sas/mpt2sas_transport.c
@@ -1006,12 +1006,9 @@ mpt2sas_transport_update_links(struct MPT2SAS_ADAPTER *ioc,
 		    &mpt2sas_phy->remote_identify);
 		_transport_add_phy_to_an_existing_port(ioc, sas_node,
 		    mpt2sas_phy, mpt2sas_phy->remote_identify.sas_address);
-	} else {
+	} else
 		memset(&mpt2sas_phy->remote_identify, 0 , sizeof(struct
 		    sas_identify));
-		_transport_del_phy_from_an_existing_port(ioc, sas_node,
-		    mpt2sas_phy);
-	}
 
 	if (mpt2sas_phy->phy)
 		mpt2sas_phy->phy->negotiated_linkrate =
diff --git a/drivers/scsi/mpt3sas/mpt3sas_transport.c b/drivers/scsi/mpt3sas/mpt3sas_transport.c
index 65170cb..55aa597 100644
--- a/drivers/scsi/mpt3sas/mpt3sas_transport.c
+++ b/drivers/scsi/mpt3sas/mpt3sas_transport.c
@@ -1003,12 +1003,9 @@ mpt3sas_transport_update_links(struct MPT3SAS_ADAPTER *ioc,
 		    &mpt3sas_phy->remote_identify);
 		_transport_add_phy_to_an_existing_port(ioc, sas_node,
 		    mpt3sas_phy, mpt3sas_phy->remote_identify.sas_address);
-	} else {
+	} else
 		memset(&mpt3sas_phy->remote_identify, 0 , sizeof(struct
 		    sas_identify));
-		_transport_del_phy_from_an_existing_port(ioc, sas_node,
-		    mpt3sas_phy);
-	}
 
 	if (mpt3sas_phy->phy)
 		mpt3sas_phy->phy->negotiated_linkrate =
diff --git a/drivers/scsi/scsi_devinfo.c b/drivers/scsi/scsi_devinfo.c
index c1d04d4..262ab83 100644
--- a/drivers/scsi/scsi_devinfo.c
+++ b/drivers/scsi/scsi_devinfo.c
@@ -211,6 +211,7 @@ static struct {
 	{"Medion", "Flash XL  MMC/SD", "2.6D", BLIST_FORCELUN},
 	{"MegaRAID", "LD", NULL, BLIST_FORCELUN},
 	{"MICROP", "4110", NULL, BLIST_NOTQ},
+	{"MSFT", "Virtual HD", NULL, BLIST_NO_RSOC},
 	{"MYLEX", "DACARMRB", "*", BLIST_REPORTLUN2},
 	{"nCipher", "Fastness Crypto", NULL, BLIST_FORCELUN},
 	{"NAKAMICH", "MJ-4.8S", NULL, BLIST_FORCELUN | BLIST_SINGLELUN},
diff --git a/drivers/scsi/storvsc_drv.c b/drivers/scsi/storvsc_drv.c
index ed0f899..86b0515 100644
--- a/drivers/scsi/storvsc_drv.c
+++ b/drivers/scsi/storvsc_drv.c
@@ -1690,13 +1690,12 @@ static int storvsc_queuecommand(struct Scsi_Host *host, struct scsi_cmnd *scmnd)
 	if (ret == -EAGAIN) {
 		/* no more space */
 
-		if (cmd_request->bounce_sgl_count) {
+		if (cmd_request->bounce_sgl_count)
 			destroy_bounce_buffer(cmd_request->bounce_sgl,
 					cmd_request->bounce_sgl_count);
 
-			ret = SCSI_MLQUEUE_DEVICE_BUSY;
-			goto queue_error;
-		}
+		ret = SCSI_MLQUEUE_DEVICE_BUSY;
+		goto queue_error;
 	}
 
 	return 0;
diff --git a/drivers/target/iscsi/iscsi_target_login.c b/drivers/target/iscsi/iscsi_target_login.c
index d509aa7..c5d3811 100644
--- a/drivers/target/iscsi/iscsi_target_login.c
+++ b/drivers/target/iscsi/iscsi_target_login.c
@@ -1186,6 +1186,9 @@ old_sess_out:
 		conn->sock = NULL;
 	}
 
+	if (conn->conn_transport->iscsit_wait_conn)
+		conn->conn_transport->iscsit_wait_conn(conn);
+
 	if (conn->conn_transport->iscsit_free_conn)
 		conn->conn_transport->iscsit_free_conn(conn);
 
diff --git a/drivers/target/iscsi/iscsi_target_util.c b/drivers/target/iscsi/iscsi_target_util.c
index ab77f80..1e406af 100644
--- a/drivers/target/iscsi/iscsi_target_util.c
+++ b/drivers/target/iscsi/iscsi_target_util.c
@@ -1356,15 +1356,15 @@ static int iscsit_do_tx_data(
 	struct iscsi_conn *conn,
 	struct iscsi_data_count *count)
 {
-	int data = count->data_length, total_tx = 0, tx_loop = 0, iov_len;
+	int ret, iov_len;
 	struct kvec *iov_p;
 	struct msghdr msg;
 
 	if (!conn || !conn->sock || !conn->conn_ops)
 		return -1;
 
-	if (data <= 0) {
-		pr_err("Data length is: %d\n", data);
+	if (count->data_length <= 0) {
+		pr_err("Data length is: %d\n", count->data_length);
 		return -1;
 	}
 
@@ -1373,20 +1373,16 @@ static int iscsit_do_tx_data(
 	iov_p = count->iov;
 	iov_len = count->iov_count;
 
-	while (total_tx < data) {
-		tx_loop = kernel_sendmsg(conn->sock, &msg, iov_p, iov_len,
-					(data - total_tx));
-		if (tx_loop <= 0) {
-			pr_debug("tx_loop: %d total_tx %d\n",
-				tx_loop, total_tx);
-			return tx_loop;
-		}
-		total_tx += tx_loop;
-		pr_debug("tx_loop: %d, total_tx: %d, data: %d\n",
-					tx_loop, total_tx, data);
+	ret = kernel_sendmsg(conn->sock, &msg, iov_p, iov_len,
+			     count->data_length);
+	if (ret != count->data_length) {
+		pr_err("Unexpected ret: %d send data %d\n",
+		       ret, count->data_length);
+		return -EPIPE;
 	}
+	pr_debug("ret: %d, sent data: %d\n", ret, count->data_length);
 
-	return total_tx;
+	return ret;
 }
 
 int rx_data(
diff --git a/drivers/target/loopback/tcm_loop.c b/drivers/target/loopback/tcm_loop.c
index fadad7c..67c802c 100644
--- a/drivers/target/loopback/tcm_loop.c
+++ b/drivers/target/loopback/tcm_loop.c
@@ -153,18 +153,11 @@ static int tcm_loop_change_queue_type(struct scsi_device *sdev, int tag)
 /*
  * Locate the SAM Task Attr from struct scsi_cmnd *
  */
-static int tcm_loop_sam_attr(struct scsi_cmnd *sc)
-{
-	if (sc->device->tagged_supported) {
-		switch (sc->tag) {
-		case HEAD_OF_QUEUE_TAG:
-			return MSG_HEAD_TAG;
-		case ORDERED_QUEUE_TAG:
-			return MSG_ORDERED_TAG;
-		default:
-			break;
-		}
-	}
+static int tcm_loop_sam_attr(struct scsi_cmnd *sc, int tag)
+{
+	if (sc->device->tagged_supported &&
+	    sc->device->ordered_tags && tag >= 0)
+		return MSG_ORDERED_TAG;
 
 	return MSG_SIMPLE_TAG;
 }
@@ -197,7 +190,7 @@ static void tcm_loop_submission_work(struct work_struct *work)
 		set_host_byte(sc, DID_TRANSPORT_DISRUPTED);
 		goto out_done;
 	}
-	tl_nexus = tl_hba->tl_nexus;
+	tl_nexus = tl_tpg->tl_nexus;
 	if (!tl_nexus) {
 		scmd_printk(KERN_ERR, sc, "TCM_Loop I_T Nexus"
 				" does not exist\n");
@@ -214,7 +207,7 @@ static void tcm_loop_submission_work(struct work_struct *work)
 	}
 	rc = target_submit_cmd_map_sgls(se_cmd, tl_nexus->se_sess, sc->cmnd,
 			&tl_cmd->tl_sense_buf[0], tl_cmd->sc->device->lun,
-			scsi_bufflen(sc), tcm_loop_sam_attr(sc),
+			scsi_bufflen(sc), tcm_loop_sam_attr(sc, tl_cmd->sc_cmd_tag),
 			sc->sc_data_direction, 0,
 			scsi_sglist(sc), scsi_sg_count(sc),
 			sgl_bidi, sgl_bidi_count,
@@ -252,7 +245,7 @@ static int tcm_loop_queuecommand(struct Scsi_Host *sh, struct scsi_cmnd *sc)
 	}
 
 	tl_cmd->sc = sc;
-	tl_cmd->sc_cmd_tag = sc->tag;
+	tl_cmd->sc_cmd_tag = sc->request->tag;
 	INIT_WORK(&tl_cmd->work, tcm_loop_submission_work);
 	queue_work(tcm_loop_workqueue, &tl_cmd->work);
 	return 0;
@@ -263,16 +256,26 @@ static int tcm_loop_queuecommand(struct Scsi_Host *sh, struct scsi_cmnd *sc)
  * to struct scsi_device
  */
 static int tcm_loop_issue_tmr(struct tcm_loop_tpg *tl_tpg,
-			      struct tcm_loop_nexus *tl_nexus,
 			      int lun, int task, enum tcm_tmreq_table tmr)
 {
 	struct se_cmd *se_cmd = NULL;
 	struct se_session *se_sess;
 	struct se_portal_group *se_tpg;
+	struct tcm_loop_nexus *tl_nexus;
 	struct tcm_loop_cmd *tl_cmd = NULL;
 	struct tcm_loop_tmr *tl_tmr = NULL;
 	int ret = TMR_FUNCTION_FAILED, rc;
 
+	/*
+	 * Locate the tl_nexus and se_sess pointers
+	 */
+	tl_nexus = tl_tpg->tl_nexus;
+	if (!tl_nexus) {
+		pr_err("Unable to perform device reset without"
+				" active I_T Nexus\n");
+		return ret;
+	}
+
 	tl_cmd = kmem_cache_zalloc(tcm_loop_cmd_cache, GFP_KERNEL);
 	if (!tl_cmd) {
 		pr_err("Unable to allocate memory for tl_cmd\n");
@@ -288,7 +291,7 @@ static int tcm_loop_issue_tmr(struct tcm_loop_tpg *tl_tpg,
 
 	se_cmd = &tl_cmd->tl_se_cmd;
 	se_tpg = &tl_tpg->tl_se_tpg;
-	se_sess = tl_nexus->se_sess;
+	se_sess = tl_tpg->tl_nexus->se_sess;
 	/*
 	 * Initialize struct se_cmd descriptor from target_core_mod infrastructure
 	 */
@@ -333,7 +336,6 @@ release:
 static int tcm_loop_abort_task(struct scsi_cmnd *sc)
 {
 	struct tcm_loop_hba *tl_hba;
-	struct tcm_loop_nexus *tl_nexus;
 	struct tcm_loop_tpg *tl_tpg;
 	int ret = FAILED;
 
@@ -341,22 +343,9 @@ static int tcm_loop_abort_task(struct scsi_cmnd *sc)
 	 * Locate the tcm_loop_hba_t pointer
 	 */
 	tl_hba = *(struct tcm_loop_hba **)shost_priv(sc->device->host);
-	/*
-	 * Locate the tl_nexus and se_sess pointers
-	 */
-	tl_nexus = tl_hba->tl_nexus;
-	if (!tl_nexus) {
-		pr_err("Unable to perform device reset without"
-				" active I_T Nexus\n");
-		return FAILED;
-	}
-
-	/*
-	 * Locate the tl_tpg pointer from TargetID in sc->device->id
-	 */
 	tl_tpg = &tl_hba->tl_hba_tpgs[sc->device->id];
-	ret = tcm_loop_issue_tmr(tl_tpg, tl_nexus, sc->device->lun,
-				 sc->tag, TMR_ABORT_TASK);
+	ret = tcm_loop_issue_tmr(tl_tpg, sc->device->lun,
+				 sc->request->tag, TMR_ABORT_TASK);
 	return (ret == TMR_FUNCTION_COMPLETE) ? SUCCESS : FAILED;
 }
 
@@ -367,7 +356,6 @@ static int tcm_loop_abort_task(struct scsi_cmnd *sc)
 static int tcm_loop_device_reset(struct scsi_cmnd *sc)
 {
 	struct tcm_loop_hba *tl_hba;
-	struct tcm_loop_nexus *tl_nexus;
 	struct tcm_loop_tpg *tl_tpg;
 	int ret = FAILED;
 
@@ -375,20 +363,9 @@ static int tcm_loop_device_reset(struct scsi_cmnd *sc)
 	 * Locate the tcm_loop_hba_t pointer
 	 */
 	tl_hba = *(struct tcm_loop_hba **)shost_priv(sc->device->host);
-	/*
-	 * Locate the tl_nexus and se_sess pointers
-	 */
-	tl_nexus = tl_hba->tl_nexus;
-	if (!tl_nexus) {
-		pr_err("Unable to perform device reset without"
-				" active I_T Nexus\n");
-		return FAILED;
-	}
-	/*
-	 * Locate the tl_tpg pointer from TargetID in sc->device->id
-	 */
 	tl_tpg = &tl_hba->tl_hba_tpgs[sc->device->id];
-	ret = tcm_loop_issue_tmr(tl_tpg, tl_nexus, sc->device->lun,
+
+	ret = tcm_loop_issue_tmr(tl_tpg, sc->device->lun,
 				 0, TMR_LUN_RESET);
 	return (ret == TMR_FUNCTION_COMPLETE) ? SUCCESS : FAILED;
 }
@@ -995,8 +972,8 @@ static int tcm_loop_make_nexus(
 	struct tcm_loop_nexus *tl_nexus;
 	int ret = -ENOMEM;
 
-	if (tl_tpg->tl_hba->tl_nexus) {
-		pr_debug("tl_tpg->tl_hba->tl_nexus already exists\n");
+	if (tl_tpg->tl_nexus) {
+		pr_debug("tl_tpg->tl_nexus already exists\n");
 		return -EEXIST;
 	}
 	se_tpg = &tl_tpg->tl_se_tpg;
@@ -1031,7 +1008,7 @@ static int tcm_loop_make_nexus(
 	 */
 	__transport_register_session(se_tpg, tl_nexus->se_sess->se_node_acl,
 			tl_nexus->se_sess, tl_nexus);
-	tl_tpg->tl_hba->tl_nexus = tl_nexus;
+	tl_tpg->tl_nexus = tl_nexus;
 	pr_debug("TCM_Loop_ConfigFS: Established I_T Nexus to emulated"
 		" %s Initiator Port: %s\n", tcm_loop_dump_proto_id(tl_hba),
 		name);
@@ -1047,12 +1024,8 @@ static int tcm_loop_drop_nexus(
 {
 	struct se_session *se_sess;
 	struct tcm_loop_nexus *tl_nexus;
-	struct tcm_loop_hba *tl_hba = tpg->tl_hba;
 
-	if (!tl_hba)
-		return -ENODEV;
-
-	tl_nexus = tl_hba->tl_nexus;
+	tl_nexus = tpg->tl_nexus;
 	if (!tl_nexus)
 		return -ENODEV;
 
@@ -1068,13 +1041,13 @@ static int tcm_loop_drop_nexus(
 	}
 
 	pr_debug("TCM_Loop_ConfigFS: Removing I_T Nexus to emulated"
-		" %s Initiator Port: %s\n", tcm_loop_dump_proto_id(tl_hba),
+		" %s Initiator Port: %s\n", tcm_loop_dump_proto_id(tpg->tl_hba),
 		tl_nexus->se_sess->se_node_acl->initiatorname);
 	/*
 	 * Release the SCSI I_T Nexus to the emulated SAS Target Port
 	 */
 	transport_deregister_session(tl_nexus->se_sess);
-	tpg->tl_hba->tl_nexus = NULL;
+	tpg->tl_nexus = NULL;
 	kfree(tl_nexus);
 	return 0;
 }
@@ -1090,7 +1063,7 @@ static ssize_t tcm_loop_tpg_show_nexus(
 	struct tcm_loop_nexus *tl_nexus;
 	ssize_t ret;
 
-	tl_nexus = tl_tpg->tl_hba->tl_nexus;
+	tl_nexus = tl_tpg->tl_nexus;
 	if (!tl_nexus)
 		return -ENODEV;
 
diff --git a/drivers/target/loopback/tcm_loop.h b/drivers/target/loopback/tcm_loop.h
index 54c59d0..6ae49f2 100644
--- a/drivers/target/loopback/tcm_loop.h
+++ b/drivers/target/loopback/tcm_loop.h
@@ -27,11 +27,6 @@ struct tcm_loop_tmr {
 };
 
 struct tcm_loop_nexus {
-	int it_nexus_active;
-	/*
-	 * Pointer to Linux/SCSI HBA from linux/include/scsi_host.h
-	 */
-	struct scsi_host *sh;
 	/*
 	 * Pointer to TCM session for I_T Nexus
 	 */
@@ -51,6 +46,7 @@ struct tcm_loop_tpg {
 	atomic_t tl_tpg_port_count;
 	struct se_portal_group tl_se_tpg;
 	struct tcm_loop_hba *tl_hba;
+	struct tcm_loop_nexus *tl_nexus;
 };
 
 struct tcm_loop_hba {
@@ -59,7 +55,6 @@ struct tcm_loop_hba {
 	struct se_hba_s *se_hba;
 	struct se_lun *tl_hba_lun;
 	struct se_port *tl_hba_lun_sep;
-	struct tcm_loop_nexus *tl_nexus;
 	struct device dev;
 	struct Scsi_Host *sh;
 	struct tcm_loop_tpg tl_hba_tpgs[TL_TPGS_PER_HBA];
diff --git a/drivers/thermal/intel_powerclamp.c b/drivers/thermal/intel_powerclamp.c
index a084325..6e75177 100644
--- a/drivers/thermal/intel_powerclamp.c
+++ b/drivers/thermal/intel_powerclamp.c
@@ -435,7 +435,6 @@ static int clamp_thread(void *arg)
 		 * allowed. thus jiffies are updated properly.
 		 */
 		preempt_disable();
-		tick_nohz_idle_enter();
 		/* mwait until target jiffies is reached */
 		while (time_before(jiffies, target_jiffies)) {
 			unsigned long ecx = 1;
@@ -451,7 +450,6 @@ static int clamp_thread(void *arg)
 			start_critical_timings();
 			atomic_inc(&idle_wakeup_counter);
 		}
-		tick_nohz_idle_exit();
 		preempt_enable();
 	}
 	del_timer_sync(&wakeup_timer);
diff --git a/drivers/usb/dwc3/gadget.c b/drivers/usb/dwc3/gadget.c
index d90c70c..8f6738d 100644
--- a/drivers/usb/dwc3/gadget.c
+++ b/drivers/usb/dwc3/gadget.c
@@ -887,8 +887,7 @@ static void dwc3_prepare_trbs(struct dwc3_ep *dep, bool starting)
 
 				if (i == (request->num_mapped_sgs - 1) ||
 						sg_is_last(s)) {
-					if (list_is_last(&req->list,
-							&dep->request_list))
+					if (list_empty(&dep->request_list))
 						last_one = true;
 					chain = false;
 				}
@@ -906,6 +905,9 @@ static void dwc3_prepare_trbs(struct dwc3_ep *dep, bool starting)
 				if (last_one)
 					break;
 			}
+
+			if (last_one)
+				break;
 		} else {
 			dma = req->request.dma;
 			length = req->request.length;
diff --git a/drivers/usb/host/ehci-sched.c b/drivers/usb/host/ehci-sched.c
index e113fd7..c399606 100644
--- a/drivers/usb/host/ehci-sched.c
+++ b/drivers/usb/host/ehci-sched.c
@@ -1581,6 +1581,10 @@ iso_stream_schedule (
 	else
 		next = (now + 2 + 7) & ~0x07;	/* full frame cache */
 
+	/* If needed, initialize last_iso_frame so that this URB will be seen */
+	if (ehci->isoc_count == 0)
+		ehci->last_iso_frame = now >> 3;
+
 	/*
 	 * Use ehci->last_iso_frame as the base.  There can't be any
 	 * TDs scheduled for earlier than that.
@@ -1671,10 +1675,6 @@ iso_stream_schedule (
 	urb->start_frame = start & (mod - 1);
 	if (!stream->highspeed)
 		urb->start_frame >>= 3;
-
-	/* Make sure scan_isoc() sees these */
-	if (ehci->isoc_count == 0)
-		ehci->last_iso_frame = now >> 3;
 	return status;
 
  fail:
diff --git a/drivers/usb/host/pci-quirks.c b/drivers/usb/host/pci-quirks.c
index 2f3aceb..f4e6b94 100644
--- a/drivers/usb/host/pci-quirks.c
+++ b/drivers/usb/host/pci-quirks.c
@@ -571,7 +571,8 @@ static void quirk_usb_handoff_ohci(struct pci_dev *pdev)
 {
 	void __iomem *base;
 	u32 control;
-	u32 fminterval;
+	u32 fminterval = 0;
+	bool no_fminterval = false;
 	int cnt;
 
 	if (!mmio_resource_enabled(pdev, 0))
@@ -581,6 +582,13 @@ static void quirk_usb_handoff_ohci(struct pci_dev *pdev)
 	if (base == NULL)
 		return;
 
+	/*
+	 * ULi M5237 OHCI controller locks the whole system when accessing
+	 * the OHCI_FMINTERVAL offset.
+	 */
+	if (pdev->vendor == PCI_VENDOR_ID_AL && pdev->device == 0x5237)
+		no_fminterval = true;
+
 	control = readl(base + OHCI_CONTROL);
 
 /* On PA-RISC, PDC can leave IR set incorrectly; ignore it there. */
@@ -619,7 +627,9 @@ static void quirk_usb_handoff_ohci(struct pci_dev *pdev)
 	}
 
 	/* software reset of the controller, preserving HcFmInterval */
-	fminterval = readl(base + OHCI_FMINTERVAL);
+	if (!no_fminterval)
+		fminterval = readl(base + OHCI_FMINTERVAL);
+
 	writel(OHCI_HCR, base + OHCI_CMDSTATUS);
 
 	/* reset requires max 10 us delay */
@@ -628,7 +638,9 @@ static void quirk_usb_handoff_ohci(struct pci_dev *pdev)
 			break;
 		udelay(1);
 	}
-	writel(fminterval, base + OHCI_FMINTERVAL);
+
+	if (!no_fminterval)
+		writel(fminterval, base + OHCI_FMINTERVAL);
 
 	/* Now the controller is safely in SUSPEND and nothing can wake it up */
 	iounmap(base);
diff --git a/drivers/usb/musb/musb_host.c b/drivers/usb/musb/musb_host.c
index abb38c3..6b0fb6a 100644
--- a/drivers/usb/musb/musb_host.c
+++ b/drivers/usb/musb/musb_host.c
@@ -2640,7 +2640,6 @@ void musb_host_cleanup(struct musb *musb)
 	if (musb->port_mode == MUSB_PORT_MODE_GADGET)
 		return;
 	usb_remove_hcd(musb->hcd);
-	musb->hcd = NULL;
 }
 
 void musb_host_free(struct musb *musb)
diff --git a/drivers/usb/serial/console.c b/drivers/usb/serial/console.c
index 8d7fc48..29fa1c3 100644
--- a/drivers/usb/serial/console.c
+++ b/drivers/usb/serial/console.c
@@ -46,6 +46,8 @@ static struct console usbcons;
  * ------------------------------------------------------------
  */
 
+static const struct tty_operations usb_console_fake_tty_ops = {
+};
 
 /*
  * The parsing of the command line works exactly like the
@@ -137,13 +139,17 @@ static int usb_console_setup(struct console *co, char *options)
 				goto reset_open_count;
 			}
 			kref_init(&tty->kref);
-			tty_port_tty_set(&port->port, tty);
 			tty->driver = usb_serial_tty_driver;
 			tty->index = co->index;
+			init_ldsem(&tty->ldisc_sem);
+			INIT_LIST_HEAD(&tty->tty_files);
+			kref_get(&tty->driver->kref);
+			tty->ops = &usb_console_fake_tty_ops;
 			if (tty_init_termios(tty)) {
 				retval = -ENOMEM;
-				goto free_tty;
+				goto put_tty;
 			}
+			tty_port_tty_set(&port->port, tty);
 		}
 
 		/* only call the device specific open if this
@@ -161,7 +167,7 @@ static int usb_console_setup(struct console *co, char *options)
 			serial->type->set_termios(tty, port, &dummy);
 
 			tty_port_tty_set(&port->port, NULL);
-			kfree(tty);
+			tty_kref_put(tty);
 		}
 		set_bit(ASYNCB_INITIALIZED, &port->port.flags);
 	}
@@ -177,8 +183,8 @@ static int usb_console_setup(struct console *co, char *options)
 
  fail:
 	tty_port_tty_set(&port->port, NULL);
- free_tty:
-	kfree(tty);
+ put_tty:
+	tty_kref_put(tty);
  reset_open_count:
 	port->port.count = 0;
 	usb_autopm_put_interface(serial->interface);
diff --git a/drivers/usb/serial/cp210x.c b/drivers/usb/serial/cp210x.c
index 5741e94..9e8708c 100644
--- a/drivers/usb/serial/cp210x.c
+++ b/drivers/usb/serial/cp210x.c
@@ -120,10 +120,12 @@ static const struct usb_device_id id_table[] = {
 	{ USB_DEVICE(0x10C4, 0x85F8) }, /* Virtenio Preon32 */
 	{ USB_DEVICE(0x10C4, 0x8664) }, /* AC-Services CAN-IF */
 	{ USB_DEVICE(0x10C4, 0x8665) }, /* AC-Services OBD-IF */
-	{ USB_DEVICE(0x10C4, 0x8875) }, /* CEL MeshConnect USB Stick */
+	{ USB_DEVICE(0x10C4, 0x8856) },	/* CEL EM357 ZigBee USB Stick - LR */
+	{ USB_DEVICE(0x10C4, 0x8857) },	/* CEL EM357 ZigBee USB Stick */
 	{ USB_DEVICE(0x10C4, 0x88A4) }, /* MMB Networks ZigBee USB Device */
 	{ USB_DEVICE(0x10C4, 0x88A5) }, /* Planet Innovation Ingeni ZigBee USB Device */
 	{ USB_DEVICE(0x10C4, 0x8946) }, /* Ketra N1 Wireless Interface */
+	{ USB_DEVICE(0x10C4, 0x8977) },	/* CEL MeshWorks DevKit Device */
 	{ USB_DEVICE(0x10C4, 0xEA60) }, /* Silicon Labs factory default */
 	{ USB_DEVICE(0x10C4, 0xEA61) }, /* Silicon Labs factory default */
 	{ USB_DEVICE(0x10C4, 0xEA70) }, /* Silicon Labs factory default */
diff --git a/drivers/usb/serial/keyspan.c b/drivers/usb/serial/keyspan.c
index 49101fe..35297a8 100644
--- a/drivers/usb/serial/keyspan.c
+++ b/drivers/usb/serial/keyspan.c
@@ -421,6 +421,8 @@ static void	usa26_instat_callback(struct urb *urb)
 	}
 	port = serial->port[msg->port];
 	p_priv = usb_get_serial_port_data(port);
+	if (!p_priv)
+		goto resubmit;
 
 	/* Update handshaking pin state information */
 	old_dcd_state = p_priv->dcd_state;
@@ -431,7 +433,7 @@ static void	usa26_instat_callback(struct urb *urb)
 
 	if (old_dcd_state != p_priv->dcd_state)
 		tty_port_tty_hangup(&port->port, true);
-
+resubmit:
 	/* Resubmit urb so we continue receiving */
 	err = usb_submit_urb(urb, GFP_ATOMIC);
 	if (err != 0)
@@ -541,6 +543,8 @@ static void	usa28_instat_callback(struct urb *urb)
 	}
 	port = serial->port[msg->port];
 	p_priv = usb_get_serial_port_data(port);
+	if (!p_priv)
+		goto resubmit;
 
 	/* Update handshaking pin state information */
 	old_dcd_state = p_priv->dcd_state;
@@ -551,7 +555,7 @@ static void	usa28_instat_callback(struct urb *urb)
 
 	if (old_dcd_state != p_priv->dcd_state && old_dcd_state)
 		tty_port_tty_hangup(&port->port, true);
-
+resubmit:
 		/* Resubmit urb so we continue receiving */
 	err = usb_submit_urb(urb, GFP_ATOMIC);
 	if (err != 0)
@@ -624,6 +628,8 @@ static void	usa49_instat_callback(struct urb *urb)
 	}
 	port = serial->port[msg->portNumber];
 	p_priv = usb_get_serial_port_data(port);
+	if (!p_priv)
+		goto resubmit;
 
 	/* Update handshaking pin state information */
 	old_dcd_state = p_priv->dcd_state;
@@ -634,7 +640,7 @@ static void	usa49_instat_callback(struct urb *urb)
 
 	if (old_dcd_state != p_priv->dcd_state && old_dcd_state)
 		tty_port_tty_hangup(&port->port, true);
-
+resubmit:
 	/* Resubmit urb so we continue receiving */
 	err = usb_submit_urb(urb, GFP_ATOMIC);
 	if (err != 0)
@@ -872,6 +878,8 @@ static void	usa90_instat_callback(struct urb *urb)
 
 	port = serial->port[0];
 	p_priv = usb_get_serial_port_data(port);
+	if (!p_priv)
+		goto resubmit;
 
 	/* Update handshaking pin state information */
 	old_dcd_state = p_priv->dcd_state;
@@ -882,7 +890,7 @@ static void	usa90_instat_callback(struct urb *urb)
 
 	if (old_dcd_state != p_priv->dcd_state && old_dcd_state)
 		tty_port_tty_hangup(&port->port, true);
-
+resubmit:
 	/* Resubmit urb so we continue receiving */
 	err = usb_submit_urb(urb, GFP_ATOMIC);
 	if (err != 0)
@@ -943,6 +951,8 @@ static void	usa67_instat_callback(struct urb *urb)
 
 	port = serial->port[msg->port];
 	p_priv = usb_get_serial_port_data(port);
+	if (!p_priv)
+		goto resubmit;
 
 	/* Update handshaking pin state information */
 	old_dcd_state = p_priv->dcd_state;
@@ -951,7 +961,7 @@ static void	usa67_instat_callback(struct urb *urb)
 
 	if (old_dcd_state != p_priv->dcd_state && old_dcd_state)
 		tty_port_tty_hangup(&port->port, true);
-
+resubmit:
 	/* Resubmit urb so we continue receiving */
 	err = usb_submit_urb(urb, GFP_ATOMIC);
 	if (err != 0)
diff --git a/drivers/vfio/pci/vfio_pci.c b/drivers/vfio/pci/vfio_pci.c
index 7ba0424..75e1d03 100644
--- a/drivers/vfio/pci/vfio_pci.c
+++ b/drivers/vfio/pci/vfio_pci.c
@@ -810,13 +810,11 @@ static const struct vfio_device_ops vfio_pci_ops = {
 
 static int vfio_pci_probe(struct pci_dev *pdev, const struct pci_device_id *id)
 {
-	u8 type;
 	struct vfio_pci_device *vdev;
 	struct iommu_group *group;
 	int ret;
 
-	pci_read_config_byte(pdev, PCI_HEADER_TYPE, &type);
-	if ((type & PCI_HEADER_TYPE) != PCI_HEADER_TYPE_NORMAL)
+	if (pdev->hdr_type != PCI_HEADER_TYPE_NORMAL)
 		return -EINVAL;
 
 	group = iommu_group_get(&pdev->dev);
diff --git a/drivers/vhost/scsi.c b/drivers/vhost/scsi.c
index 5d0b7b8..486d710 100644
--- a/drivers/vhost/scsi.c
+++ b/drivers/vhost/scsi.c
@@ -861,6 +861,23 @@ vhost_scsi_map_iov_to_sgl(struct tcm_vhost_cmd *cmd,
 	return 0;
 }
 
+static int vhost_scsi_to_tcm_attr(int attr)
+{
+	switch (attr) {
+	case VIRTIO_SCSI_S_SIMPLE:
+		return MSG_SIMPLE_TAG;
+	case VIRTIO_SCSI_S_ORDERED:
+		return MSG_ORDERED_TAG;
+	case VIRTIO_SCSI_S_HEAD:
+		return MSG_HEAD_TAG;
+	case VIRTIO_SCSI_S_ACA:
+		return MSG_ACA_TAG;
+	default:
+		break;
+	}
+	return MSG_SIMPLE_TAG;
+}
+
 static void tcm_vhost_submission_work(struct work_struct *work)
 {
 	struct tcm_vhost_cmd *cmd =
@@ -887,9 +904,10 @@ static void tcm_vhost_submission_work(struct work_struct *work)
 	rc = target_submit_cmd_map_sgls(se_cmd, tv_nexus->tvn_se_sess,
 			cmd->tvc_cdb, &cmd->tvc_sense_buf[0],
 			cmd->tvc_lun, cmd->tvc_exp_data_len,
-			cmd->tvc_task_attr, cmd->tvc_data_direction,
-			TARGET_SCF_ACK_KREF, sg_ptr, cmd->tvc_sgl_count,
-			sg_bidi_ptr, sg_no_bidi, NULL, 0);
+			vhost_scsi_to_tcm_attr(cmd->tvc_task_attr),
+			cmd->tvc_data_direction, TARGET_SCF_ACK_KREF,
+			sg_ptr, cmd->tvc_sgl_count, sg_bidi_ptr, sg_no_bidi,
+			NULL, 0);
 	if (rc < 0) {
 		transport_send_check_condition_and_sense(se_cmd,
 				TCM_LOGICAL_UNIT_COMMUNICATION_FAILURE, 0);
diff --git a/drivers/video/logo/logo.c b/drivers/video/logo/logo.c
index b670cbd..ffe024b 100644
--- a/drivers/video/logo/logo.c
+++ b/drivers/video/logo/logo.c
@@ -21,6 +21,21 @@ static bool nologo;
 module_param(nologo, bool, 0);
 MODULE_PARM_DESC(nologo, "Disables startup logo");
 
+/*
+ * Logos are located in the initdata, and will be freed in kernel_init.
+ * Use late_init to mark the logos as freed to prevent any further use.
+ */
+
+static bool logos_freed;
+
+static int __init fb_logo_late_init(void)
+{
+	logos_freed = true;
+	return 0;
+}
+
+late_initcall(fb_logo_late_init);
+
 /* logo's are marked __initdata. Use __init_refok to tell
  * modpost that it is intended that this function uses data
  * marked __initdata.
@@ -29,7 +44,7 @@ const struct linux_logo * __init_refok fb_find_logo(int depth)
 {
 	const struct linux_logo *logo = NULL;
 
-	if (nologo)
+	if (nologo || logos_freed)
 		return NULL;
 
 	if (depth >= 1) {
diff --git a/fs/lockd/svc.c b/fs/lockd/svc.c
index 223e1cb..59a53f6 100644
--- a/fs/lockd/svc.c
+++ b/fs/lockd/svc.c
@@ -137,10 +137,6 @@ lockd(void *vrqstp)
 
 	dprintk("NFS locking service started (ver " LOCKD_VERSION ").\n");
 
-	if (!nlm_timeout)
-		nlm_timeout = LOCKD_DFLT_TIMEO;
-	nlmsvc_timeout = nlm_timeout * HZ;
-
 	/*
 	 * The main request loop. We don't terminate until the last
 	 * NFS mount or NFS daemon has gone away.
@@ -346,6 +342,10 @@ static struct svc_serv *lockd_create_svc(void)
 		printk(KERN_WARNING
 			"lockd_up: no pid, %d users??\n", nlmsvc_users);
 
+	if (!nlm_timeout)
+		nlm_timeout = LOCKD_DFLT_TIMEO;
+	nlmsvc_timeout = nlm_timeout * HZ;
+
 	serv = svc_create(&nlmsvc_program, LOCKD_BUFSIZE, NULL);
 	if (!serv) {
 		printk(KERN_WARNING "lockd_up: create service failed\n");
diff --git a/fs/nfs/nfs4client.c b/fs/nfs/nfs4client.c
index 1abe4f5..037f957 100644
--- a/fs/nfs/nfs4client.c
+++ b/fs/nfs/nfs4client.c
@@ -565,20 +565,14 @@ static bool nfs4_match_clientids(struct nfs_client *a, struct nfs_client *b)
 }
 
 /*
- * Returns true if the server owners match
+ * Returns true if the server major ids match
  */
 static bool
-nfs4_match_serverowners(struct nfs_client *a, struct nfs_client *b)
+nfs4_check_clientid_trunking(struct nfs_client *a, struct nfs_client *b)
 {
 	struct nfs41_server_owner *o1 = a->cl_serverowner;
 	struct nfs41_server_owner *o2 = b->cl_serverowner;
 
-	if (o1->minor_id != o2->minor_id) {
-		dprintk("NFS: --> %s server owner minor IDs do not match\n",
-			__func__);
-		return false;
-	}
-
 	if (o1->major_id_sz != o2->major_id_sz)
 		goto out_major_mismatch;
 	if (memcmp(o1->major_id, o2->major_id, o1->major_id_sz) != 0)
@@ -654,7 +648,12 @@ int nfs41_walk_client_list(struct nfs_client *new,
 		if (!nfs4_match_clientids(pos, new))
 			continue;
 
-		if (!nfs4_match_serverowners(pos, new))
+		/*
+		 * Note that session trunking is just a special subcase of
+		 * client id trunking. In either case, we want to fall back
+		 * to using the existing nfs_client.
+		 */
+		if (!nfs4_check_clientid_trunking(pos, new))
 			continue;
 
 		atomic_inc(&pos->cl_count);
diff --git a/fs/notify/inode_mark.c b/fs/notify/inode_mark.c
index 74825be..fbb9dfb 100644
--- a/fs/notify/inode_mark.c
+++ b/fs/notify/inode_mark.c
@@ -288,20 +288,25 @@ void fsnotify_unmount_inodes(struct list_head *list)
 		spin_unlock(&inode->i_lock);
 
 		/* In case the dropping of a reference would nuke next_i. */
-		if ((&next_i->i_sb_list != list) &&
-		    atomic_read(&next_i->i_count)) {
+		while (&next_i->i_sb_list != list) {
 			spin_lock(&next_i->i_lock);
-			if (!(next_i->i_state & (I_FREEING | I_WILL_FREE))) {
+			if (!(next_i->i_state & (I_FREEING | I_WILL_FREE)) &&
+						atomic_read(&next_i->i_count)) {
 				__iget(next_i);
 				need_iput = next_i;
+				spin_unlock(&next_i->i_lock);
+				break;
 			}
 			spin_unlock(&next_i->i_lock);
+			next_i = list_entry(next_i->i_sb_list.next,
+						struct inode, i_sb_list);
 		}
 
 		/*
-		 * We can safely drop inode_sb_list_lock here because we hold
-		 * references on both inode and next_i.  Also no new inodes
-		 * will be added since the umount has begun.
+		 * We can safely drop inode_sb_list_lock here because either
+		 * we actually hold references on both inode and next_i or
+		 * end of list.  Also no new inodes will be added since the
+		 * umount has begun.
 		 */
 		spin_unlock(&inode_sb_list_lock);
 
diff --git a/fs/proc/stat.c b/fs/proc/stat.c
index 6f599c6..dbd0272 100644
--- a/fs/proc/stat.c
+++ b/fs/proc/stat.c
@@ -159,7 +159,7 @@ static int show_stat(struct seq_file *p, void *v)
 
 	/* sum again ? it could be updated? */
 	for_each_irq_nr(j)
-		seq_put_decimal_ull(p, ' ', kstat_irqs(j));
+		seq_put_decimal_ull(p, ' ', kstat_irqs_usr(j));
 
 	seq_printf(p,
 		"\nctxt %llu\n"
diff --git a/include/linux/kernel_stat.h b/include/linux/kernel_stat.h
index 51c72be..4b2053a 100644
--- a/include/linux/kernel_stat.h
+++ b/include/linux/kernel_stat.h
@@ -74,6 +74,7 @@ static inline unsigned int kstat_softirqs_cpu(unsigned int irq, int cpu)
  * Number of interrupts per specific IRQ source, since bootup
  */
 extern unsigned int kstat_irqs(unsigned int irq);
+extern unsigned int kstat_irqs_usr(unsigned int irq);
 
 /*
  * Number of interrupts per cpu, since bootup
diff --git a/include/uapi/linux/in6.h b/include/uapi/linux/in6.h
index e9a1d2d..4c399ae 100644
--- a/include/uapi/linux/in6.h
+++ b/include/uapi/linux/in6.h
@@ -149,7 +149,7 @@ struct in6_flowlabel_req {
 /*
  *	IPV6 socket options
  */
-
+#if __UAPI_DEF_IPV6_OPTIONS
 #define IPV6_ADDRFORM		1
 #define IPV6_2292PKTINFO	2
 #define IPV6_2292HOPOPTS	3
@@ -192,6 +192,7 @@ struct in6_flowlabel_req {
 
 #define IPV6_IPSEC_POLICY	34
 #define IPV6_XFRM_POLICY	35
+#endif
 
 /*
  * Multicast:
diff --git a/include/uapi/linux/libc-compat.h b/include/uapi/linux/libc-compat.h
index c140620..e28807a 100644
--- a/include/uapi/linux/libc-compat.h
+++ b/include/uapi/linux/libc-compat.h
@@ -69,6 +69,7 @@
 #define __UAPI_DEF_SOCKADDR_IN6		0
 #define __UAPI_DEF_IPV6_MREQ		0
 #define __UAPI_DEF_IPPROTO_V6		0
+#define __UAPI_DEF_IPV6_OPTIONS		0
 
 #else
 
@@ -82,6 +83,7 @@
 #define __UAPI_DEF_SOCKADDR_IN6		1
 #define __UAPI_DEF_IPV6_MREQ		1
 #define __UAPI_DEF_IPPROTO_V6		1
+#define __UAPI_DEF_IPV6_OPTIONS		1
 
 #endif /* _NETINET_IN_H */
 
@@ -103,6 +105,7 @@
 #define __UAPI_DEF_SOCKADDR_IN6		1
 #define __UAPI_DEF_IPV6_MREQ		1
 #define __UAPI_DEF_IPPROTO_V6		1
+#define __UAPI_DEF_IPV6_OPTIONS		1
 
 /* Definitions for xattr.h */
 #define __UAPI_DEF_XATTR		1
diff --git a/kernel/irq/internals.h b/kernel/irq/internals.h
index 001fa5b..8a160e8 100644
--- a/kernel/irq/internals.h
+++ b/kernel/irq/internals.h
@@ -74,6 +74,14 @@ extern void irq_percpu_disable(struct irq_desc *desc, unsigned int cpu);
 extern void mask_irq(struct irq_desc *desc);
 extern void unmask_irq(struct irq_desc *desc);
 
+#ifdef CONFIG_SPARSE_IRQ
+extern void irq_lock_sparse(void);
+extern void irq_unlock_sparse(void);
+#else
+static inline void irq_lock_sparse(void) { }
+static inline void irq_unlock_sparse(void) { }
+#endif
+
 extern void init_kstat_irqs(struct irq_desc *desc, int node, int nr);
 
 irqreturn_t handle_irq_event_percpu(struct irq_desc *desc, struct irqaction *action);
diff --git a/kernel/irq/irqdesc.c b/kernel/irq/irqdesc.c
index 8ab8e93..07d4551 100644
--- a/kernel/irq/irqdesc.c
+++ b/kernel/irq/irqdesc.c
@@ -131,6 +131,16 @@ static void free_masks(struct irq_desc *desc)
 static inline void free_masks(struct irq_desc *desc) { }
 #endif
 
+void irq_lock_sparse(void)
+{
+	mutex_lock(&sparse_irq_lock);
+}
+
+void irq_unlock_sparse(void)
+{
+	mutex_unlock(&sparse_irq_lock);
+}
+
 static struct irq_desc *alloc_desc(int irq, int node, struct module *owner)
 {
 	struct irq_desc *desc;
@@ -167,6 +177,12 @@ static void free_desc(unsigned int irq)
 
 	unregister_irq_proc(irq, desc);
 
+	/*
+	 * sparse_irq_lock protects also show_interrupts() and
+	 * kstat_irq_usr(). Once we deleted the descriptor from the
+	 * sparse tree we can free it. Access in proc will fail to
+	 * lookup the descriptor.
+	 */
 	mutex_lock(&sparse_irq_lock);
 	delete_irq_desc(irq);
 	mutex_unlock(&sparse_irq_lock);
@@ -489,6 +505,15 @@ void dynamic_irq_cleanup(unsigned int irq)
 	raw_spin_unlock_irqrestore(&desc->lock, flags);
 }
 
+/**
+ * kstat_irqs_cpu - Get the statistics for an interrupt on a cpu
+ * @irq:	The interrupt number
+ * @cpu:	The cpu number
+ *
+ * Returns the sum of interrupt counts on @cpu since boot for
+ * @irq. The caller must ensure that the interrupt is not removed
+ * concurrently.
+ */
 unsigned int kstat_irqs_cpu(unsigned int irq, int cpu)
 {
 	struct irq_desc *desc = irq_to_desc(irq);
@@ -497,6 +522,14 @@ unsigned int kstat_irqs_cpu(unsigned int irq, int cpu)
 			*per_cpu_ptr(desc->kstat_irqs, cpu) : 0;
 }
 
+/**
+ * kstat_irqs - Get the statistics for an interrupt
+ * @irq:	The interrupt number
+ *
+ * Returns the sum of interrupt counts on all cpus since boot for
+ * @irq. The caller must ensure that the interrupt is not removed
+ * concurrently.
+ */
 unsigned int kstat_irqs(unsigned int irq)
 {
 	struct irq_desc *desc = irq_to_desc(irq);
@@ -509,3 +542,22 @@ unsigned int kstat_irqs(unsigned int irq)
 		sum += *per_cpu_ptr(desc->kstat_irqs, cpu);
 	return sum;
 }
+
+/**
+ * kstat_irqs_usr - Get the statistics for an interrupt
+ * @irq:	The interrupt number
+ *
+ * Returns the sum of interrupt counts on all cpus since boot for
+ * @irq. Contrary to kstat_irqs() this can be called from any
+ * preemptible context. It's protected against concurrent removal of
+ * an interrupt descriptor when sparse irqs are enabled.
+ */
+unsigned int kstat_irqs_usr(unsigned int irq)
+{
+	int sum;
+
+	irq_lock_sparse();
+	sum = kstat_irqs(irq);
+	irq_unlock_sparse();
+	return sum;
+}
diff --git a/kernel/irq/proc.c b/kernel/irq/proc.c
index 36f6ee1..095cd72 100644
--- a/kernel/irq/proc.c
+++ b/kernel/irq/proc.c
@@ -15,6 +15,23 @@
 
 #include "internals.h"
 
+/*
+ * Access rules:
+ *
+ * procfs protects read/write of /proc/irq/N/ files against a
+ * concurrent free of the interrupt descriptor. remove_proc_entry()
+ * immediately prevents new read/writes to happen and waits for
+ * already running read/write functions to complete.
+ *
+ * We remove the proc entries first and then delete the interrupt
+ * descriptor from the radix tree and free it. So it is guaranteed
+ * that irq_to_desc(N) is valid as long as the read/writes are
+ * permitted by procfs.
+ *
+ * The read from /proc/interrupts is a different problem because there
+ * is no protection. So the lookup and the access to irqdesc
+ * information must be protected by sparse_irq_lock.
+ */
 static struct proc_dir_entry *root_irq_dir;
 
 #ifdef CONFIG_SMP
@@ -437,9 +454,10 @@ int show_interrupts(struct seq_file *p, void *v)
 		seq_putc(p, '\n');
 	}
 
+	irq_lock_sparse();
 	desc = irq_to_desc(i);
 	if (!desc)
-		return 0;
+		goto outsparse;
 
 	raw_spin_lock_irqsave(&desc->lock, flags);
 	for_each_online_cpu(j)
@@ -479,6 +497,8 @@ int show_interrupts(struct seq_file *p, void *v)
 	seq_putc(p, '\n');
 out:
 	raw_spin_unlock_irqrestore(&desc->lock, flags);
+outsparse:
+	irq_unlock_sparse();
 	return 0;
 }
 #endif
diff --git a/kernel/time/tick-sched.c b/kernel/time/tick-sched.c
index 6558b7a..8c08a6f 100644
--- a/kernel/time/tick-sched.c
+++ b/kernel/time/tick-sched.c
@@ -807,7 +807,6 @@ void tick_nohz_idle_enter(void)
 
 	local_irq_enable();
 }
-EXPORT_SYMBOL_GPL(tick_nohz_idle_enter);
 
 /**
  * tick_nohz_irq_exit - update next tick event from interrupt exit
@@ -934,7 +933,6 @@ void tick_nohz_idle_exit(void)
 
 	local_irq_enable();
 }
-EXPORT_SYMBOL_GPL(tick_nohz_idle_exit);
 
 static int tick_nohz_reprogram(struct tick_sched *ts, ktime_t now)
 {
diff --git a/lib/decompress_bunzip2.c b/lib/decompress_bunzip2.c
index 31c5f76..f504027 100644
--- a/lib/decompress_bunzip2.c
+++ b/lib/decompress_bunzip2.c
@@ -184,7 +184,7 @@ static int INIT get_next_block(struct bunzip_data *bd)
 	if (get_bits(bd, 1))
 		return RETVAL_OBSOLETE_INPUT;
 	origPtr = get_bits(bd, 24);
-	if (origPtr > dbufSize)
+	if (origPtr >= dbufSize)
 		return RETVAL_DATA_ERROR;
 	/* mapping table: if some byte values are never used (encoding things
 	   like ascii text), the compression code removes the gaps to have fewer
diff --git a/net/batman-adv/fragmentation.c b/net/batman-adv/fragmentation.c
index c46387a..e5c5f57 100644
--- a/net/batman-adv/fragmentation.c
+++ b/net/batman-adv/fragmentation.c
@@ -251,7 +251,7 @@ batadv_frag_merge_packets(struct hlist_head *chain, struct sk_buff *skb)
 	kfree(entry);
 
 	/* Make room for the rest of the fragments. */
-	if (pskb_expand_head(skb_out, 0, size - skb->len, GFP_ATOMIC) < 0) {
+	if (pskb_expand_head(skb_out, 0, size - skb_out->len, GFP_ATOMIC) < 0) {
 		kfree_skb(skb_out);
 		skb_out = NULL;
 		goto free;
@@ -434,7 +434,7 @@ bool batadv_frag_send_packet(struct sk_buff *skb,
 	 * fragments larger than BATADV_FRAG_MAX_FRAG_SIZE
 	 */
 	mtu = min_t(unsigned, mtu, BATADV_FRAG_MAX_FRAG_SIZE);
-	max_fragment_size = (mtu - header_size - ETH_HLEN);
+	max_fragment_size = mtu - header_size;
 	max_packet_size = max_fragment_size * BATADV_FRAG_MAX_FRAGMENTS;
 
 	/* Don't even try to fragment, if we need more than 16 fragments */
diff --git a/net/batman-adv/gateway_client.c b/net/batman-adv/gateway_client.c
index 36b9ae6..2393ea7 100644
--- a/net/batman-adv/gateway_client.c
+++ b/net/batman-adv/gateway_client.c
@@ -812,7 +812,7 @@ bool batadv_gw_out_of_range(struct batadv_priv *bat_priv,
 		goto out;
 
 	gw_node = batadv_gw_node_get(bat_priv, orig_dst_node);
-	if (!gw_node->bandwidth_down == 0)
+	if (!gw_node)
 		goto out;
 
 	switch (atomic_read(&bat_priv->gw_mode)) {
diff --git a/net/core/dev.c b/net/core/dev.c
index 3ed11a5..86bb9cc 100644
--- a/net/core/dev.c
+++ b/net/core/dev.c
@@ -1709,6 +1709,7 @@ int dev_forward_skb(struct net_device *dev, struct sk_buff *skb)
 
 	skb_scrub_packet(skb, true);
 	skb->protocol = eth_type_trans(skb, dev);
+	skb_postpull_rcsum(skb, eth_hdr(skb), ETH_HLEN);
 
 	return netif_rx_internal(skb);
 }
@@ -2529,11 +2530,14 @@ netdev_features_t netif_skb_dev_features(struct sk_buff *skb,
 	if (skb_shinfo(skb)->gso_segs > dev->gso_max_segs)
 		features &= ~NETIF_F_GSO_MASK;
 
-	if (protocol == htons(ETH_P_8021Q) || protocol == htons(ETH_P_8021AD)) {
-		struct vlan_ethhdr *veh = (struct vlan_ethhdr *)skb->data;
-		protocol = veh->h_vlan_encapsulated_proto;
-	} else if (!vlan_tx_tag_present(skb)) {
-		return harmonize_features(skb, dev, features);
+	if (!vlan_tx_tag_present(skb)) {
+		if (unlikely(protocol == htons(ETH_P_8021Q) ||
+			     protocol == htons(ETH_P_8021AD))) {
+			struct vlan_ethhdr *veh = (struct vlan_ethhdr *)skb->data;
+			protocol = veh->h_vlan_encapsulated_proto;
+		} else {
+			return harmonize_features(skb, dev, features);
+		}
 	}
 
 	features &= (dev->vlan_features | NETIF_F_HW_VLAN_CTAG_TX |
@@ -4701,9 +4705,14 @@ static void netdev_adjacent_sysfs_del(struct net_device *dev,
 	sysfs_remove_link(&(dev->dev.kobj), linkname);
 }
 
-#define netdev_adjacent_is_neigh_list(dev, dev_list) \
-		(dev_list == &dev->adj_list.upper || \
-		 dev_list == &dev->adj_list.lower)
+static inline bool netdev_adjacent_is_neigh_list(struct net_device *dev,
+						 struct net_device *adj_dev,
+						 struct list_head *dev_list)
+{
+	return (dev_list == &dev->adj_list.upper ||
+		dev_list == &dev->adj_list.lower) &&
+		net_eq(dev_net(dev), dev_net(adj_dev));
+}
 
 static int __netdev_adjacent_dev_insert(struct net_device *dev,
 					struct net_device *adj_dev,
@@ -4733,7 +4742,7 @@ static int __netdev_adjacent_dev_insert(struct net_device *dev,
 	pr_debug("dev_hold for %s, because of link added from %s to %s\n",
 		 adj_dev->name, dev->name, adj_dev->name);
 
-	if (netdev_adjacent_is_neigh_list(dev, dev_list)) {
+	if (netdev_adjacent_is_neigh_list(dev, adj_dev, dev_list)) {
 		ret = netdev_adjacent_sysfs_add(dev, adj_dev, dev_list);
 		if (ret)
 			goto free_adj;
@@ -4754,7 +4763,7 @@ static int __netdev_adjacent_dev_insert(struct net_device *dev,
 	return 0;
 
 remove_symlinks:
-	if (netdev_adjacent_is_neigh_list(dev, dev_list))
+	if (netdev_adjacent_is_neigh_list(dev, adj_dev, dev_list))
 		netdev_adjacent_sysfs_del(dev, adj_dev->name, dev_list);
 free_adj:
 	kfree(adj);
@@ -4787,7 +4796,7 @@ static void __netdev_adjacent_dev_remove(struct net_device *dev,
 	if (adj->master)
 		sysfs_remove_link(&(dev->dev.kobj), "master");
 
-	if (netdev_adjacent_is_neigh_list(dev, dev_list))
+	if (netdev_adjacent_is_neigh_list(dev, adj_dev, dev_list))
 		netdev_adjacent_sysfs_del(dev, adj_dev->name, dev_list);
 
 	list_del_rcu(&adj->list);
@@ -5057,11 +5066,65 @@ void netdev_upper_dev_unlink(struct net_device *dev,
 }
 EXPORT_SYMBOL(netdev_upper_dev_unlink);
 
+void netdev_adjacent_add_links(struct net_device *dev)
+{
+	struct netdev_adjacent *iter;
+
+	struct net *net = dev_net(dev);
+
+	list_for_each_entry(iter, &dev->adj_list.upper, list) {
+		if (!net_eq(net,dev_net(iter->dev)))
+			continue;
+		netdev_adjacent_sysfs_add(iter->dev, dev,
+					  &iter->dev->adj_list.lower);
+		netdev_adjacent_sysfs_add(dev, iter->dev,
+					  &dev->adj_list.upper);
+	}
+
+	list_for_each_entry(iter, &dev->adj_list.lower, list) {
+		if (!net_eq(net,dev_net(iter->dev)))
+			continue;
+		netdev_adjacent_sysfs_add(iter->dev, dev,
+					  &iter->dev->adj_list.upper);
+		netdev_adjacent_sysfs_add(dev, iter->dev,
+					  &dev->adj_list.lower);
+	}
+}
+
+void netdev_adjacent_del_links(struct net_device *dev)
+{
+	struct netdev_adjacent *iter;
+
+	struct net *net = dev_net(dev);
+
+	list_for_each_entry(iter, &dev->adj_list.upper, list) {
+		if (!net_eq(net,dev_net(iter->dev)))
+			continue;
+		netdev_adjacent_sysfs_del(iter->dev, dev->name,
+					  &iter->dev->adj_list.lower);
+		netdev_adjacent_sysfs_del(dev, iter->dev->name,
+					  &dev->adj_list.upper);
+	}
+
+	list_for_each_entry(iter, &dev->adj_list.lower, list) {
+		if (!net_eq(net,dev_net(iter->dev)))
+			continue;
+		netdev_adjacent_sysfs_del(iter->dev, dev->name,
+					  &iter->dev->adj_list.upper);
+		netdev_adjacent_sysfs_del(dev, iter->dev->name,
+					  &dev->adj_list.lower);
+	}
+}
+
 void netdev_adjacent_rename_links(struct net_device *dev, char *oldname)
 {
 	struct netdev_adjacent *iter;
 
+	struct net *net = dev_net(dev);
+
 	list_for_each_entry(iter, &dev->adj_list.upper, list) {
+		if (!net_eq(net,dev_net(iter->dev)))
+			continue;
 		netdev_adjacent_sysfs_del(iter->dev, oldname,
 					  &iter->dev->adj_list.lower);
 		netdev_adjacent_sysfs_add(iter->dev, dev,
@@ -5069,6 +5132,8 @@ void netdev_adjacent_rename_links(struct net_device *dev, char *oldname)
 	}
 
 	list_for_each_entry(iter, &dev->adj_list.lower, list) {
+		if (!net_eq(net,dev_net(iter->dev)))
+			continue;
 		netdev_adjacent_sysfs_del(iter->dev, oldname,
 					  &iter->dev->adj_list.upper);
 		netdev_adjacent_sysfs_add(iter->dev, dev,
@@ -6675,6 +6740,7 @@ int dev_change_net_namespace(struct net_device *dev, struct net *net, const char
 
 	/* Send a netdev-removed uevent to the old namespace */
 	kobject_uevent(&dev->dev.kobj, KOBJ_REMOVE);
+	netdev_adjacent_del_links(dev);
 
 	/* Actually switch the network namespace */
 	dev_net_set(dev, net);
@@ -6689,6 +6755,7 @@ int dev_change_net_namespace(struct net_device *dev, struct net *net, const char
 
 	/* Send a netdev-add uevent to the new namespace */
 	kobject_uevent(&dev->dev.kobj, KOBJ_ADD);
+	netdev_adjacent_add_links(dev);
 
 	/* Fixup kobjects */
 	err = device_rename(&dev->dev, dev->name);
diff --git a/net/core/skbuff.c b/net/core/skbuff.c
index baf6fc4..e2b1bba 100644
--- a/net/core/skbuff.c
+++ b/net/core/skbuff.c
@@ -3937,6 +3937,7 @@ void skb_scrub_packet(struct sk_buff *skb, bool xnet)
 	skb->local_df = 0;
 	skb_dst_drop(skb);
 	skb->mark = 0;
+	skb_init_secmark(skb);
 	secpath_reset(skb);
 	nf_reset(skb);
 	nf_reset_trace(skb);
diff --git a/net/ipv4/ip_gre.c b/net/ipv4/ip_gre.c
index 94213c8..b40b90d 100644
--- a/net/ipv4/ip_gre.c
+++ b/net/ipv4/ip_gre.c
@@ -250,10 +250,6 @@ static netdev_tx_t ipgre_xmit(struct sk_buff *skb,
 	struct ip_tunnel *tunnel = netdev_priv(dev);
 	const struct iphdr *tnl_params;
 
-	skb = gre_handle_offloads(skb, !!(tunnel->parms.o_flags&TUNNEL_CSUM));
-	if (IS_ERR(skb))
-		goto out;
-
 	if (dev->header_ops) {
 		/* Need space for new headers */
 		if (skb_cow_head(skb, dev->needed_headroom -
@@ -266,6 +262,7 @@ static netdev_tx_t ipgre_xmit(struct sk_buff *skb,
 		 * to gre header.
 		 */
 		skb_pull(skb, tunnel->hlen + sizeof(struct iphdr));
+		skb_reset_mac_header(skb);
 	} else {
 		if (skb_cow_head(skb, dev->needed_headroom))
 			goto free_skb;
@@ -273,6 +270,10 @@ static netdev_tx_t ipgre_xmit(struct sk_buff *skb,
 		tnl_params = &tunnel->parms.iph;
 	}
 
+	skb = gre_handle_offloads(skb, !!(tunnel->parms.o_flags&TUNNEL_CSUM));
+	if (IS_ERR(skb))
+		goto out;
+
 	__gre_xmit(skb, dev, tnl_params, skb->protocol);
 
 	return NETDEV_TX_OK;
diff --git a/net/ipv4/tcp_output.c b/net/ipv4/tcp_output.c
index 91b98e5..7efa26b 100644
--- a/net/ipv4/tcp_output.c
+++ b/net/ipv4/tcp_output.c
@@ -1894,7 +1894,7 @@ static bool tcp_write_xmit(struct sock *sk, unsigned int mss_now, int nonagle,
 		if (unlikely(!tcp_snd_wnd_test(tp, skb, mss_now)))
 			break;
 
-		if (tso_segs == 1) {
+		if (tso_segs == 1 || !sk->sk_gso_max_segs) {
 			if (unlikely(!tcp_nagle_test(tp, skb, mss_now,
 						     (tcp_skb_is_last(sk, skb) ?
 						      nonagle : TCP_NAGLE_PUSH))))
@@ -1931,7 +1931,7 @@ static bool tcp_write_xmit(struct sock *sk, unsigned int mss_now, int nonagle,
 		}
 
 		limit = mss_now;
-		if (tso_segs > 1 && !tcp_urg_mode(tp))
+		if (tso_segs > 1 && sk->sk_gso_max_segs && !tcp_urg_mode(tp))
 			limit = tcp_mss_split_point(sk, skb, mss_now,
 						    min_t(unsigned int,
 							  cwnd_quota,
diff --git a/net/netfilter/ipset/ip_set_core.c b/net/netfilter/ipset/ip_set_core.c
index cf99377..53ea164 100644
--- a/net/netfilter/ipset/ip_set_core.c
+++ b/net/netfilter/ipset/ip_set_core.c
@@ -1839,6 +1839,12 @@ ip_set_sockfn_get(struct sock *sk, int optval, void __user *user, int *len)
 	if (*op < IP_SET_OP_VERSION) {
 		/* Check the version at the beginning of operations */
 		struct ip_set_req_version *req_version = data;
+
+		if (*len < sizeof(struct ip_set_req_version)) {
+			ret = -EINVAL;
+			goto done;
+		}
+
 		if (req_version->version != IPSET_PROTOCOL) {
 			ret = -EPROTO;
 			goto done;
diff --git a/net/netlink/af_netlink.c b/net/netlink/af_netlink.c
index 7c177bc..1d52506 100644
--- a/net/netlink/af_netlink.c
+++ b/net/netlink/af_netlink.c
@@ -510,14 +510,14 @@ out:
 	return err;
 }
 
-static void netlink_frame_flush_dcache(const struct nl_mmap_hdr *hdr)
+static void netlink_frame_flush_dcache(const struct nl_mmap_hdr *hdr, unsigned int nm_len)
 {
 #if ARCH_IMPLEMENTS_FLUSH_DCACHE_PAGE == 1
 	struct page *p_start, *p_end;
 
 	/* First page is flushed through netlink_{get,set}_status */
 	p_start = pgvec_to_page(hdr + PAGE_SIZE);
-	p_end   = pgvec_to_page((void *)hdr + NL_MMAP_HDRLEN + hdr->nm_len - 1);
+	p_end   = pgvec_to_page((void *)hdr + NL_MMAP_HDRLEN + nm_len - 1);
 	while (p_start <= p_end) {
 		flush_dcache_page(p_start);
 		p_start++;
@@ -535,9 +535,9 @@ static enum nl_mmap_status netlink_get_status(const struct nl_mmap_hdr *hdr)
 static void netlink_set_status(struct nl_mmap_hdr *hdr,
 			       enum nl_mmap_status status)
 {
+	smp_mb();
 	hdr->nm_status = status;
 	flush_dcache_page(pgvec_to_page(hdr));
-	smp_wmb();
 }
 
 static struct nl_mmap_hdr *
@@ -699,24 +699,16 @@ static int netlink_mmap_sendmsg(struct sock *sk, struct msghdr *msg,
 	struct nl_mmap_hdr *hdr;
 	struct sk_buff *skb;
 	unsigned int maxlen;
-	bool excl = true;
 	int err = 0, len = 0;
 
-	/* Netlink messages are validated by the receiver before processing.
-	 * In order to avoid userspace changing the contents of the message
-	 * after validation, the socket and the ring may only be used by a
-	 * single process, otherwise we fall back to copying.
-	 */
-	if (atomic_long_read(&sk->sk_socket->file->f_count) > 1 ||
-	    atomic_read(&nlk->mapped) > 1)
-		excl = false;
-
 	mutex_lock(&nlk->pg_vec_lock);
 
 	ring   = &nlk->tx_ring;
 	maxlen = ring->frame_size - NL_MMAP_HDRLEN;
 
 	do {
+		unsigned int nm_len;
+
 		hdr = netlink_current_frame(ring, NL_MMAP_STATUS_VALID);
 		if (hdr == NULL) {
 			if (!(msg->msg_flags & MSG_DONTWAIT) &&
@@ -724,35 +716,23 @@ static int netlink_mmap_sendmsg(struct sock *sk, struct msghdr *msg,
 				schedule();
 			continue;
 		}
-		if (hdr->nm_len > maxlen) {
+
+		nm_len = ACCESS_ONCE(hdr->nm_len);
+		if (nm_len > maxlen) {
 			err = -EINVAL;
 			goto out;
 		}
 
-		netlink_frame_flush_dcache(hdr);
+		netlink_frame_flush_dcache(hdr, nm_len);
 
-		if (likely(dst_portid == 0 && dst_group == 0 && excl)) {
-			skb = alloc_skb_head(GFP_KERNEL);
-			if (skb == NULL) {
-				err = -ENOBUFS;
-				goto out;
-			}
-			sock_hold(sk);
-			netlink_ring_setup_skb(skb, sk, ring, hdr);
-			NETLINK_CB(skb).flags |= NETLINK_SKB_TX;
-			__skb_put(skb, hdr->nm_len);
-			netlink_set_status(hdr, NL_MMAP_STATUS_RESERVED);
-			atomic_inc(&ring->pending);
-		} else {
-			skb = alloc_skb(hdr->nm_len, GFP_KERNEL);
-			if (skb == NULL) {
-				err = -ENOBUFS;
-				goto out;
-			}
-			__skb_put(skb, hdr->nm_len);
-			memcpy(skb->data, (void *)hdr + NL_MMAP_HDRLEN, hdr->nm_len);
-			netlink_set_status(hdr, NL_MMAP_STATUS_UNUSED);
+		skb = alloc_skb(nm_len, GFP_KERNEL);
+		if (skb == NULL) {
+			err = -ENOBUFS;
+			goto out;
 		}
+		__skb_put(skb, nm_len);
+		memcpy(skb->data, (void *)hdr + NL_MMAP_HDRLEN, nm_len);
+		netlink_set_status(hdr, NL_MMAP_STATUS_UNUSED);
 
 		netlink_increment_head(ring);
 
@@ -798,7 +778,7 @@ static void netlink_queue_mmaped_skb(struct sock *sk, struct sk_buff *skb)
 	hdr->nm_pid	= NETLINK_CB(skb).creds.pid;
 	hdr->nm_uid	= from_kuid(sk_user_ns(sk), NETLINK_CB(skb).creds.uid);
 	hdr->nm_gid	= from_kgid(sk_user_ns(sk), NETLINK_CB(skb).creds.gid);
-	netlink_frame_flush_dcache(hdr);
+	netlink_frame_flush_dcache(hdr, hdr->nm_len);
 	netlink_set_status(hdr, NL_MMAP_STATUS_VALID);
 
 	NETLINK_CB(skb).flags |= NETLINK_SKB_DELIVERED;
diff --git a/net/wireless/chan.c b/net/wireless/chan.c
index 78559b5..27157a78 100644
--- a/net/wireless/chan.c
+++ b/net/wireless/chan.c
@@ -516,7 +516,7 @@ bool cfg80211_chandef_usable(struct wiphy *wiphy,
 {
 	struct ieee80211_sta_ht_cap *ht_cap;
 	struct ieee80211_sta_vht_cap *vht_cap;
-	u32 width, control_freq;
+	u32 width, control_freq, cap;
 
 	if (WARN_ON(!cfg80211_chandef_valid(chandef)))
 		return false;
@@ -554,7 +554,8 @@ bool cfg80211_chandef_usable(struct wiphy *wiphy,
 			return false;
 		break;
 	case NL80211_CHAN_WIDTH_80P80:
-		if (!(vht_cap->cap & IEEE80211_VHT_CAP_SUPP_CHAN_WIDTH_160_80PLUS80MHZ))
+		cap = vht_cap->cap & IEEE80211_VHT_CAP_SUPP_CHAN_WIDTH_MASK;
+		if (cap != IEEE80211_VHT_CAP_SUPP_CHAN_WIDTH_160_80PLUS80MHZ)
 			return false;
 	case NL80211_CHAN_WIDTH_80:
 		if (!vht_cap->vht_supported)
@@ -565,7 +566,9 @@ bool cfg80211_chandef_usable(struct wiphy *wiphy,
 	case NL80211_CHAN_WIDTH_160:
 		if (!vht_cap->vht_supported)
 			return false;
-		if (!(vht_cap->cap & IEEE80211_VHT_CAP_SUPP_CHAN_WIDTH_160MHZ))
+		cap = vht_cap->cap & IEEE80211_VHT_CAP_SUPP_CHAN_WIDTH_MASK;
+		if (cap != IEEE80211_VHT_CAP_SUPP_CHAN_WIDTH_160MHZ &&
+		    cap != IEEE80211_VHT_CAP_SUPP_CHAN_WIDTH_160_80PLUS80MHZ)
 			return false;
 		prohibited_flags |= IEEE80211_CHAN_NO_160MHZ;
 		width = 160;
diff --git a/net/wireless/reg.c b/net/wireless/reg.c
index 338794e..04d5305 100644
--- a/net/wireless/reg.c
+++ b/net/wireless/reg.c
@@ -1547,7 +1547,7 @@ static enum reg_request_treatment
 reg_process_hint_driver(struct wiphy *wiphy,
 			struct regulatory_request *driver_request)
 {
-	const struct ieee80211_regdomain *regd;
+	const struct ieee80211_regdomain *regd, *tmp;
 	enum reg_request_treatment treatment;
 
 	treatment = __reg_process_hint_driver(driver_request);
@@ -1566,7 +1566,10 @@ reg_process_hint_driver(struct wiphy *wiphy,
 			kfree(driver_request);
 			return REG_REQ_IGNORE;
 		}
+
+		tmp = get_wiphy_regdom(wiphy);
 		rcu_assign_pointer(wiphy->regd, regd);
+		rcu_free_regdom(tmp);
 	}
 
 
@@ -1625,11 +1628,8 @@ __reg_process_hint_country_ie(struct wiphy *wiphy,
 			return REG_REQ_IGNORE;
 		return REG_REQ_ALREADY_SET;
 	}
-	/*
-	 * Two consecutive Country IE hints on the same wiphy.
-	 * This should be picked up early by the driver/stack
-	 */
-	if (WARN_ON(regdom_changes(country_ie_request->alpha2)))
+
+	if (regdom_changes(country_ie_request->alpha2))
 		return REG_REQ_OK;
 	return REG_REQ_ALREADY_SET;
 }
diff --git a/sound/usb/quirks-table.h b/sound/usb/quirks-table.h
index c657752..83bddbd 100644
--- a/sound/usb/quirks-table.h
+++ b/sound/usb/quirks-table.h
@@ -2804,133 +2804,45 @@ YAMAHA_DEVICE(0x7010, "UB99"),
 	}
 },
 
-/* Hauppauge HVR-950Q and HVR-850 */
-{
-	USB_DEVICE_VENDOR_SPEC(0x2040, 0x7200),
-	.match_flags = USB_DEVICE_ID_MATCH_DEVICE |
-		       USB_DEVICE_ID_MATCH_INT_CLASS |
-		       USB_DEVICE_ID_MATCH_INT_SUBCLASS,
-	.bInterfaceClass = USB_CLASS_AUDIO,
-	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL,
-	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) {
-		.vendor_name = "Hauppauge",
-		.product_name = "HVR-950Q",
-		.ifnum = QUIRK_ANY_INTERFACE,
-		.type = QUIRK_AUDIO_ALIGN_TRANSFER,
-	}
-},
-{
-	USB_DEVICE_VENDOR_SPEC(0x2040, 0x7210),
-	.match_flags = USB_DEVICE_ID_MATCH_DEVICE |
-		       USB_DEVICE_ID_MATCH_INT_CLASS |
-		       USB_DEVICE_ID_MATCH_INT_SUBCLASS,
-	.bInterfaceClass = USB_CLASS_AUDIO,
-	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL,
-	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) {
-		.vendor_name = "Hauppauge",
-		.product_name = "HVR-950Q",
-		.ifnum = QUIRK_ANY_INTERFACE,
-		.type = QUIRK_AUDIO_ALIGN_TRANSFER,
-	}
-},
-{
-	USB_DEVICE_VENDOR_SPEC(0x2040, 0x7217),
-	.match_flags = USB_DEVICE_ID_MATCH_DEVICE |
-		       USB_DEVICE_ID_MATCH_INT_CLASS |
-		       USB_DEVICE_ID_MATCH_INT_SUBCLASS,
-	.bInterfaceClass = USB_CLASS_AUDIO,
-	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL,
-	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) {
-		.vendor_name = "Hauppauge",
-		.product_name = "HVR-950Q",
-		.ifnum = QUIRK_ANY_INTERFACE,
-		.type = QUIRK_AUDIO_ALIGN_TRANSFER,
-	}
-},
-{
-	USB_DEVICE_VENDOR_SPEC(0x2040, 0x721b),
-	.match_flags = USB_DEVICE_ID_MATCH_DEVICE |
-		       USB_DEVICE_ID_MATCH_INT_CLASS |
-		       USB_DEVICE_ID_MATCH_INT_SUBCLASS,
-	.bInterfaceClass = USB_CLASS_AUDIO,
-	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL,
-	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) {
-		.vendor_name = "Hauppauge",
-		.product_name = "HVR-950Q",
-		.ifnum = QUIRK_ANY_INTERFACE,
-		.type = QUIRK_AUDIO_ALIGN_TRANSFER,
-	}
-},
-{
-	USB_DEVICE_VENDOR_SPEC(0x2040, 0x721e),
-	.match_flags = USB_DEVICE_ID_MATCH_DEVICE |
-		       USB_DEVICE_ID_MATCH_INT_CLASS |
-		       USB_DEVICE_ID_MATCH_INT_SUBCLASS,
-	.bInterfaceClass = USB_CLASS_AUDIO,
-	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL,
-	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) {
-		.vendor_name = "Hauppauge",
-		.product_name = "HVR-950Q",
-		.ifnum = QUIRK_ANY_INTERFACE,
-		.type = QUIRK_AUDIO_ALIGN_TRANSFER,
-	}
-},
-{
-	USB_DEVICE_VENDOR_SPEC(0x2040, 0x721f),
-	.match_flags = USB_DEVICE_ID_MATCH_DEVICE |
-		       USB_DEVICE_ID_MATCH_INT_CLASS |
-		       USB_DEVICE_ID_MATCH_INT_SUBCLASS,
-	.bInterfaceClass = USB_CLASS_AUDIO,
-	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL,
-	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) {
-		.vendor_name = "Hauppauge",
-		.product_name = "HVR-950Q",
-		.ifnum = QUIRK_ANY_INTERFACE,
-		.type = QUIRK_AUDIO_ALIGN_TRANSFER,
-	}
-},
-{
-	USB_DEVICE_VENDOR_SPEC(0x2040, 0x7240),
-	.match_flags = USB_DEVICE_ID_MATCH_DEVICE |
-		       USB_DEVICE_ID_MATCH_INT_CLASS |
-		       USB_DEVICE_ID_MATCH_INT_SUBCLASS,
-	.bInterfaceClass = USB_CLASS_AUDIO,
-	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL,
-	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) {
-		.vendor_name = "Hauppauge",
-		.product_name = "HVR-850",
-		.ifnum = QUIRK_ANY_INTERFACE,
-		.type = QUIRK_AUDIO_ALIGN_TRANSFER,
-	}
-},
-{
-	USB_DEVICE_VENDOR_SPEC(0x2040, 0x7280),
-	.match_flags = USB_DEVICE_ID_MATCH_DEVICE |
-		       USB_DEVICE_ID_MATCH_INT_CLASS |
-		       USB_DEVICE_ID_MATCH_INT_SUBCLASS,
-	.bInterfaceClass = USB_CLASS_AUDIO,
-	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL,
-	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) {
-		.vendor_name = "Hauppauge",
-		.product_name = "HVR-950Q",
-		.ifnum = QUIRK_ANY_INTERFACE,
-		.type = QUIRK_AUDIO_ALIGN_TRANSFER,
-	}
-},
-{
-	USB_DEVICE_VENDOR_SPEC(0x0fd9, 0x0008),
-	.match_flags = USB_DEVICE_ID_MATCH_DEVICE |
-		       USB_DEVICE_ID_MATCH_INT_CLASS |
-		       USB_DEVICE_ID_MATCH_INT_SUBCLASS,
-	.bInterfaceClass = USB_CLASS_AUDIO,
-	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL,
-	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) {
-		.vendor_name = "Hauppauge",
-		.product_name = "HVR-950Q",
-		.ifnum = QUIRK_ANY_INTERFACE,
-		.type = QUIRK_AUDIO_ALIGN_TRANSFER,
-	}
-},
+/*
+ * Auvitek au0828 devices with audio interface.
+ * This should be kept in sync with drivers/media/usb/au0828/au0828-cards.c
+ * Please notice that some drivers are DVB only, and don't need to be
+ * here. That's the case, for example, of DVICO_FUSIONHDTV7.
+ */
+
+#define AU0828_DEVICE(vid, pid, vname, pname) { \
+	USB_DEVICE_VENDOR_SPEC(vid, pid), \
+	.match_flags = USB_DEVICE_ID_MATCH_DEVICE | \
+		       USB_DEVICE_ID_MATCH_INT_CLASS | \
+		       USB_DEVICE_ID_MATCH_INT_SUBCLASS, \
+	.bInterfaceClass = USB_CLASS_AUDIO, \
+	.bInterfaceSubClass = USB_SUBCLASS_AUDIOCONTROL, \
+	.driver_info = (unsigned long) &(const struct snd_usb_audio_quirk) { \
+		.vendor_name = vname, \
+		.product_name = pname, \
+		.ifnum = QUIRK_ANY_INTERFACE, \
+		.type = QUIRK_AUDIO_ALIGN_TRANSFER, \
+	} \
+}
+
+AU0828_DEVICE(0x2040, 0x7200, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x2040, 0x7240, "Hauppauge", "HVR-850"),
+AU0828_DEVICE(0x2040, 0x7210, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x2040, 0x7217, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x2040, 0x721b, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x2040, 0x721e, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x2040, 0x721f, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x2040, 0x7280, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x0fd9, 0x0008, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x2040, 0x7201, "Hauppauge", "HVR-950Q-MXL"),
+AU0828_DEVICE(0x2040, 0x7211, "Hauppauge", "HVR-950Q-MXL"),
+AU0828_DEVICE(0x2040, 0x7281, "Hauppauge", "HVR-950Q-MXL"),
+AU0828_DEVICE(0x05e1, 0x0480, "Hauppauge", "Woodbury"),
+AU0828_DEVICE(0x2040, 0x8200, "Hauppauge", "Woodbury"),
+AU0828_DEVICE(0x2040, 0x7260, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x2040, 0x7213, "Hauppauge", "HVR-950Q"),
+AU0828_DEVICE(0x2040, 0x7270, "Hauppauge", "HVR-950Q"),
 
 /* Digidesign Mbox */
 {
