diff --git a/Makefile b/Makefile
index 00fffa3..b0963ca 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 14
-SUBLEVEL = 32
+SUBLEVEL = 33
 EXTRAVERSION =
 NAME = Remembering Coco
 
diff --git a/arch/arm/mm/context.c b/arch/arm/mm/context.c
index 6eb97b3..4370933 100644
--- a/arch/arm/mm/context.c
+++ b/arch/arm/mm/context.c
@@ -144,21 +144,17 @@ static void flush_context(unsigned int cpu)
 	/* Update the list of reserved ASIDs and the ASID bitmap. */
 	bitmap_clear(asid_map, 0, NUM_USER_ASIDS);
 	for_each_possible_cpu(i) {
-		if (i == cpu) {
-			asid = 0;
-		} else {
-			asid = atomic64_xchg(&per_cpu(active_asids, i), 0);
-			/*
-			 * If this CPU has already been through a
-			 * rollover, but hasn't run another task in
-			 * the meantime, we must preserve its reserved
-			 * ASID, as this is the only trace we have of
-			 * the process it is still running.
-			 */
-			if (asid == 0)
-				asid = per_cpu(reserved_asids, i);
-			__set_bit(asid & ~ASID_MASK, asid_map);
-		}
+		asid = atomic64_xchg(&per_cpu(active_asids, i), 0);
+		/*
+		 * If this CPU has already been through a
+		 * rollover, but hasn't run another task in
+		 * the meantime, we must preserve its reserved
+		 * ASID, as this is the only trace we have of
+		 * the process it is still running.
+		 */
+		if (asid == 0)
+			asid = per_cpu(reserved_asids, i);
+		__set_bit(asid & ~ASID_MASK, asid_map);
 		per_cpu(reserved_asids, i) = asid;
 	}
 
diff --git a/arch/arm64/include/asm/cputype.h b/arch/arm64/include/asm/cputype.h
index c404fb0..64bc6c6 100644
--- a/arch/arm64/include/asm/cputype.h
+++ b/arch/arm64/include/asm/cputype.h
@@ -77,6 +77,8 @@ static inline u32 __attribute_const__ read_cpuid_cachetype(void)
 	return read_cpuid(CTR_EL0);
 }
 
+void cpuinfo_store_cpu(void);
+
 #endif /* __ASSEMBLY__ */
 
 #endif
diff --git a/arch/arm64/kernel/setup.c b/arch/arm64/kernel/setup.c
index 071c382..1e01d80 100644
--- a/arch/arm64/kernel/setup.c
+++ b/arch/arm64/kernel/setup.c
@@ -41,6 +41,7 @@
 #include <linux/memblock.h>
 #include <linux/of_fdt.h>
 #include <linux/of_platform.h>
+#include <linux/personality.h>
 
 #include <asm/cputype.h>
 #include <asm/elf.h>
@@ -73,7 +74,6 @@ unsigned int compat_elf_hwcap __read_mostly = COMPAT_ELF_HWCAP_DEFAULT;
 #endif
 
 static const char *cpu_name;
-static const char *machine_name;
 phys_addr_t __fdt_pointer __initdata;
 
 /*
@@ -193,6 +193,19 @@ static void __init smp_build_mpidr_hash(void)
 }
 #endif
 
+struct cpuinfo_arm64 {
+	struct cpu	cpu;
+	u32		reg_midr;
+};
+
+static DEFINE_PER_CPU(struct cpuinfo_arm64, cpu_data);
+
+void cpuinfo_store_cpu(void)
+{
+	struct cpuinfo_arm64 *info = this_cpu_ptr(&cpu_data);
+	info->reg_midr = read_cpuid_id();
+}
+
 static void __init setup_processor(void)
 {
 	struct cpu_info *cpu_info;
@@ -213,6 +226,8 @@ static void __init setup_processor(void)
 	sprintf(init_utsname()->machine, ELF_PLATFORM);
 	elf_hwcap = 0;
 
+	cpuinfo_store_cpu();
+
 	/*
 	 * ID_AA64ISAR0_EL1 contains 4-bit wide signed feature blocks.
 	 * The blocks we test below represent incremental functionality
@@ -257,8 +272,6 @@ static void __init setup_machine_fdt(phys_addr_t dt_phys)
 		while (true)
 			cpu_relax();
 	}
-
-	machine_name = of_flat_dt_get_machine_name();
 }
 
 /*
@@ -363,14 +376,12 @@ static int __init arm64_device_init(void)
 }
 arch_initcall(arm64_device_init);
 
-static DEFINE_PER_CPU(struct cpu, cpu_data);
-
 static int __init topology_init(void)
 {
 	int i;
 
 	for_each_possible_cpu(i) {
-		struct cpu *cpu = &per_cpu(cpu_data, i);
+		struct cpu *cpu = &per_cpu(cpu_data.cpu, i);
 		cpu->hotpluggable = 1;
 		register_cpu(cpu, i);
 	}
@@ -391,14 +402,41 @@ static const char *hwcap_str[] = {
 	NULL
 };
 
+#ifdef CONFIG_COMPAT
+static const char *compat_hwcap_str[] = {
+	"swp",
+	"half",
+	"thumb",
+	"26bit",
+	"fastmult",
+	"fpa",
+	"vfp",
+	"edsp",
+	"java",
+	"iwmmxt",
+	"crunch",
+	"thumbee",
+	"neon",
+	"vfpv3",
+	"vfpv3d16",
+	"tls",
+	"vfpv4",
+	"idiva",
+	"idivt",
+	"vfpd32",
+	"lpae",
+	"evtstrm"
+};
+#endif /* CONFIG_COMPAT */
+
 static int c_show(struct seq_file *m, void *v)
 {
-	int i;
-
-	seq_printf(m, "Processor\t: %s rev %d (%s)\n",
-		   cpu_name, read_cpuid_id() & 15, ELF_PLATFORM);
+	int i, j;
 
 	for_each_online_cpu(i) {
+		struct cpuinfo_arm64 *cpuinfo = &per_cpu(cpu_data, i);
+		u32 midr = cpuinfo->reg_midr;
+
 		/*
 		 * glibc reads /proc/cpuinfo to determine the number of
 		 * online processors, looking for lines beginning with
@@ -407,24 +445,33 @@ static int c_show(struct seq_file *m, void *v)
 #ifdef CONFIG_SMP
 		seq_printf(m, "processor\t: %d\n", i);
 #endif
-	}
-
-	/* dump out the processor features */
-	seq_puts(m, "Features\t: ");
-
-	for (i = 0; hwcap_str[i]; i++)
-		if (elf_hwcap & (1 << i))
-			seq_printf(m, "%s ", hwcap_str[i]);
 
-	seq_printf(m, "\nCPU implementer\t: 0x%02x\n", read_cpuid_id() >> 24);
-	seq_printf(m, "CPU architecture: AArch64\n");
-	seq_printf(m, "CPU variant\t: 0x%x\n", (read_cpuid_id() >> 20) & 15);
-	seq_printf(m, "CPU part\t: 0x%03x\n", (read_cpuid_id() >> 4) & 0xfff);
-	seq_printf(m, "CPU revision\t: %d\n", read_cpuid_id() & 15);
-
-	seq_puts(m, "\n");
+		/*
+		 * Dump out the common processor features in a single line.
+		 * Userspace should read the hwcaps with getauxval(AT_HWCAP)
+		 * rather than attempting to parse this, but there's a body of
+		 * software which does already (at least for 32-bit).
+		 */
+		seq_puts(m, "Features\t:");
+		if (personality(current->personality) == PER_LINUX32) {
+#ifdef CONFIG_COMPAT
+			for (j = 0; compat_hwcap_str[j]; j++)
+				if (compat_elf_hwcap & (1 << j))
+					seq_printf(m, " %s", compat_hwcap_str[j]);
+#endif /* CONFIG_COMPAT */
+		} else {
+			for (j = 0; hwcap_str[j]; j++)
+				if (elf_hwcap & (1 << j))
+					seq_printf(m, " %s", hwcap_str[j]);
+		}
+		seq_puts(m, "\n");
 
-	seq_printf(m, "Hardware\t: %s\n", machine_name);
+		seq_printf(m, "CPU implementer\t: 0x%02x\n", (midr >> 24));
+		seq_printf(m, "CPU architecture: 8\n");
+		seq_printf(m, "CPU variant\t: 0x%x\n", ((midr >> 20) & 0xf));
+		seq_printf(m, "CPU part\t: 0x%03x\n", ((midr >> 4) & 0xfff));
+		seq_printf(m, "CPU revision\t: %d\n\n", (midr & 0xf));
+	}
 
 	return 0;
 }
diff --git a/arch/arm64/kernel/smp.c b/arch/arm64/kernel/smp.c
index 7cfb92a..7b9542b 100644
--- a/arch/arm64/kernel/smp.c
+++ b/arch/arm64/kernel/smp.c
@@ -148,6 +148,11 @@ asmlinkage void secondary_start_kernel(void)
 		cpu_ops[cpu]->cpu_postboot();
 
 	/*
+	 * Log the CPU info before it is marked online and might get read.
+	 */
+	cpuinfo_store_cpu();
+
+	/*
 	 * Enable GIC and timers.
 	 */
 	notify_cpu_starting(cpu);
diff --git a/arch/mips/cavium-octeon/smp.c b/arch/mips/cavium-octeon/smp.c
index 67a078f..34467ac 100644
--- a/arch/mips/cavium-octeon/smp.c
+++ b/arch/mips/cavium-octeon/smp.c
@@ -263,9 +263,7 @@ static int octeon_cpu_disable(void)
 
 	set_cpu_online(cpu, false);
 	cpu_clear(cpu, cpu_callin_map);
-	local_irq_disable();
 	octeon_fixup_irqs();
-	local_irq_enable();
 
 	flush_cache_all();
 	local_flush_tlb_all();
diff --git a/arch/mips/kernel/irq_cpu.c b/arch/mips/kernel/irq_cpu.c
index e498f2b..f5598e2 100644
--- a/arch/mips/kernel/irq_cpu.c
+++ b/arch/mips/kernel/irq_cpu.c
@@ -56,6 +56,8 @@ static struct irq_chip mips_cpu_irq_controller = {
 	.irq_mask_ack	= mask_mips_irq,
 	.irq_unmask	= unmask_mips_irq,
 	.irq_eoi	= unmask_mips_irq,
+	.irq_disable	= mask_mips_irq,
+	.irq_enable	= unmask_mips_irq,
 };
 
 /*
@@ -92,6 +94,8 @@ static struct irq_chip mips_mt_cpu_irq_controller = {
 	.irq_mask_ack	= mips_mt_cpu_irq_ack,
 	.irq_unmask	= unmask_mips_irq,
 	.irq_eoi	= unmask_mips_irq,
+	.irq_disable	= mask_mips_irq,
+	.irq_enable	= unmask_mips_irq,
 };
 
 void __init mips_cpu_irq_init(void)
diff --git a/arch/mips/kernel/smp.c b/arch/mips/kernel/smp.c
index 0a022ee..18ed112 100644
--- a/arch/mips/kernel/smp.c
+++ b/arch/mips/kernel/smp.c
@@ -109,10 +109,10 @@ asmlinkage void start_secondary(void)
 	else
 #endif /* CONFIG_MIPS_MT_SMTC */
 	cpu_probe();
-	cpu_report();
 	per_cpu_trap_init(false);
 	mips_clockevent_init();
 	mp_ops->init_secondary();
+	cpu_report();
 
 	/*
 	 * XXX parity protection should be folded in here when it's converted
diff --git a/arch/x86/kvm/vmx.c b/arch/x86/kvm/vmx.c
index de42688..80c22a3 100644
--- a/arch/x86/kvm/vmx.c
+++ b/arch/x86/kvm/vmx.c
@@ -441,6 +441,7 @@ struct vcpu_vmx {
 #endif
 		int           gs_ldt_reload_needed;
 		int           fs_reload_needed;
+		unsigned long vmcs_host_cr4;    /* May not match real cr4 */
 	} host_state;
 	struct {
 		int vm86_active;
@@ -4165,11 +4166,16 @@ static void vmx_set_constant_host_state(struct vcpu_vmx *vmx)
 	u32 low32, high32;
 	unsigned long tmpl;
 	struct desc_ptr dt;
+	unsigned long cr4;
 
 	vmcs_writel(HOST_CR0, read_cr0() & ~X86_CR0_TS);  /* 22.2.3 */
-	vmcs_writel(HOST_CR4, read_cr4());  /* 22.2.3, 22.2.5 */
 	vmcs_writel(HOST_CR3, read_cr3());  /* 22.2.3  FIXME: shadow tables */
 
+	/* Save the most likely value for this task's CR4 in the VMCS. */
+	cr4 = read_cr4();
+	vmcs_writel(HOST_CR4, cr4);			/* 22.2.3, 22.2.5 */
+	vmx->host_state.vmcs_host_cr4 = cr4;
+
 	vmcs_write16(HOST_CS_SELECTOR, __KERNEL_CS);  /* 22.2.4 */
 #ifdef CONFIG_X86_64
 	/*
@@ -7196,7 +7202,7 @@ static void atomic_switch_perf_msrs(struct vcpu_vmx *vmx)
 static void __noclone vmx_vcpu_run(struct kvm_vcpu *vcpu)
 {
 	struct vcpu_vmx *vmx = to_vmx(vcpu);
-	unsigned long debugctlmsr;
+	unsigned long debugctlmsr, cr4;
 
 	/* Record the guest's net vcpu time for enforced NMI injections. */
 	if (unlikely(!cpu_has_virtual_nmis() && vmx->soft_vnmi_blocked))
@@ -7217,6 +7223,12 @@ static void __noclone vmx_vcpu_run(struct kvm_vcpu *vcpu)
 	if (test_bit(VCPU_REGS_RIP, (unsigned long *)&vcpu->arch.regs_dirty))
 		vmcs_writel(GUEST_RIP, vcpu->arch.regs[VCPU_REGS_RIP]);
 
+	cr4 = read_cr4();
+	if (unlikely(cr4 != vmx->host_state.vmcs_host_cr4)) {
+		vmcs_writel(HOST_CR4, cr4);
+		vmx->host_state.vmcs_host_cr4 = cr4;
+	}
+
 	/* When single-stepping over STI and MOV SS, we must clear the
 	 * corresponding interruptibility bits in the guest state. Otherwise
 	 * vmentry fails as it then expects bit 14 (BS) in pending debug
diff --git a/arch/x86/pci/common.c b/arch/x86/pci/common.c
index 981c2db..88f143d 100644
--- a/arch/x86/pci/common.c
+++ b/arch/x86/pci/common.c
@@ -448,6 +448,22 @@ static const struct dmi_system_id pciprobe_dmi_table[] = {
 			DMI_MATCH(DMI_PRODUCT_NAME, "ftServer"),
 		},
 	},
+        {
+                .callback = set_scan_all,
+                .ident = "Stratus/NEC ftServer",
+                .matches = {
+                        DMI_MATCH(DMI_SYS_VENDOR, "NEC"),
+                        DMI_MATCH(DMI_PRODUCT_NAME, "Express5800/R32"),
+                },
+        },
+        {
+                .callback = set_scan_all,
+                .ident = "Stratus/NEC ftServer",
+                .matches = {
+                        DMI_MATCH(DMI_SYS_VENDOR, "NEC"),
+                        DMI_MATCH(DMI_PRODUCT_NAME, "Express5800/R31"),
+                },
+        },
 	{}
 };
 
diff --git a/crypto/crc32c.c b/crypto/crc32c.c
index 06f7018..238f0e6 100644
--- a/crypto/crc32c.c
+++ b/crypto/crc32c.c
@@ -170,3 +170,4 @@ module_exit(crc32c_mod_fini);
 MODULE_AUTHOR("Clay Haapala <chaapala@cisco.com>");
 MODULE_DESCRIPTION("CRC32c (Castagnoli) calculations wrapper for lib/crc32c");
 MODULE_LICENSE("GPL");
+MODULE_ALIAS_CRYPTO("crc32c");
diff --git a/drivers/gpio/gpiolib.c b/drivers/gpio/gpiolib.c
index ccbffd0..8f42bd7 100644
--- a/drivers/gpio/gpiolib.c
+++ b/drivers/gpio/gpiolib.c
@@ -911,6 +911,7 @@ int gpiod_export_link(struct device *dev, const char *name,
 		if (tdev != NULL) {
 			status = sysfs_create_link(&dev->kobj, &tdev->kobj,
 						name);
+			put_device(tdev);
 		} else {
 			status = -ENODEV;
 		}
@@ -958,7 +959,7 @@ int gpiod_sysfs_set_active_low(struct gpio_desc *desc, int value)
 	}
 
 	status = sysfs_set_active_low(desc, dev, value);
-
+	put_device(dev);
 unlock:
 	mutex_unlock(&sysfs_lock);
 
diff --git a/fs/cifs/file.c b/fs/cifs/file.c
index d375322..0218a9b 100644
--- a/fs/cifs/file.c
+++ b/fs/cifs/file.c
@@ -366,6 +366,7 @@ void cifsFileInfo_put(struct cifsFileInfo *cifs_file)
 	struct cifsLockInfo *li, *tmp;
 	struct cifs_fid fid;
 	struct cifs_pending_open open;
+	bool oplock_break_cancelled;
 
 	spin_lock(&cifs_file_list_lock);
 	if (--cifs_file->count > 0) {
@@ -397,7 +398,7 @@ void cifsFileInfo_put(struct cifsFileInfo *cifs_file)
 	}
 	spin_unlock(&cifs_file_list_lock);
 
-	cancel_work_sync(&cifs_file->oplock_break);
+	oplock_break_cancelled = cancel_work_sync(&cifs_file->oplock_break);
 
 	if (!tcon->need_reconnect && !cifs_file->invalidHandle) {
 		struct TCP_Server_Info *server = tcon->ses->server;
@@ -409,6 +410,9 @@ void cifsFileInfo_put(struct cifsFileInfo *cifs_file)
 		_free_xid(xid);
 	}
 
+	if (oplock_break_cancelled)
+		cifs_done_oplock_break(cifsi);
+
 	cifs_del_pending_open(&open);
 
 	/*
diff --git a/fs/ext4/file.c b/fs/ext4/file.c
index 2a8b2e1..589117e 100644
--- a/fs/ext4/file.c
+++ b/fs/ext4/file.c
@@ -100,7 +100,7 @@ ext4_file_dio_write(struct kiocb *iocb, const struct iovec *iov,
 	struct blk_plug plug;
 	int unaligned_aio = 0;
 	ssize_t ret;
-	int overwrite = 0;
+	int *overwrite = iocb->private;
 	size_t length = iov_length(iov, nr_segs);
 
 	if (ext4_test_inode_flag(inode, EXT4_INODE_EXTENTS) &&
@@ -118,8 +118,6 @@ ext4_file_dio_write(struct kiocb *iocb, const struct iovec *iov,
 	mutex_lock(&inode->i_mutex);
 	blk_start_plug(&plug);
 
-	iocb->private = &overwrite;
-
 	/* check whether we do a DIO overwrite or not */
 	if (ext4_should_dioread_nolock(inode) && !unaligned_aio &&
 	    !file->f_mapping->nrpages && pos + length <= i_size_read(inode)) {
@@ -143,7 +141,7 @@ ext4_file_dio_write(struct kiocb *iocb, const struct iovec *iov,
 		 * So we should check these two conditions.
 		 */
 		if (err == len && (map.m_flags & EXT4_MAP_MAPPED))
-			overwrite = 1;
+			*overwrite = 1;
 	}
 
 	ret = __generic_file_aio_write(iocb, iov, nr_segs, &iocb->ki_pos);
@@ -170,6 +168,7 @@ ext4_file_write(struct kiocb *iocb, const struct iovec *iov,
 {
 	struct inode *inode = file_inode(iocb->ki_filp);
 	ssize_t ret;
+	int overwrite = 0;
 
 	/*
 	 * If we have encountered a bitmap-format file, the size limit
@@ -190,6 +189,7 @@ ext4_file_write(struct kiocb *iocb, const struct iovec *iov,
 		}
 	}
 
+	iocb->private = &overwrite;
 	if (unlikely(iocb->ki_filp->f_flags & O_DIRECT))
 		ret = ext4_file_dio_write(iocb, iov, nr_segs, pos);
 	else
diff --git a/fs/nilfs2/nilfs.h b/fs/nilfs2/nilfs.h
index 9bc72de..b02c202 100644
--- a/fs/nilfs2/nilfs.h
+++ b/fs/nilfs2/nilfs.h
@@ -141,7 +141,6 @@ enum {
  * @ti_save: Backup of journal_info field of task_struct
  * @ti_flags: Flags
  * @ti_count: Nest level
- * @ti_garbage:	List of inode to be put when releasing semaphore
  */
 struct nilfs_transaction_info {
 	u32			ti_magic;
@@ -150,7 +149,6 @@ struct nilfs_transaction_info {
 				   one of other filesystems has a bug. */
 	unsigned short		ti_flags;
 	unsigned short		ti_count;
-	struct list_head	ti_garbage;
 };
 
 /* ti_magic */
diff --git a/fs/nilfs2/segment.c b/fs/nilfs2/segment.c
index a1a1916..5bee816 100644
--- a/fs/nilfs2/segment.c
+++ b/fs/nilfs2/segment.c
@@ -305,7 +305,6 @@ static void nilfs_transaction_lock(struct super_block *sb,
 	ti->ti_count = 0;
 	ti->ti_save = cur_ti;
 	ti->ti_magic = NILFS_TI_MAGIC;
-	INIT_LIST_HEAD(&ti->ti_garbage);
 	current->journal_info = ti;
 
 	for (;;) {
@@ -332,8 +331,6 @@ static void nilfs_transaction_unlock(struct super_block *sb)
 
 	up_write(&nilfs->ns_segctor_sem);
 	current->journal_info = ti->ti_save;
-	if (!list_empty(&ti->ti_garbage))
-		nilfs_dispose_list(nilfs, &ti->ti_garbage, 0);
 }
 
 static void *nilfs_segctor_map_segsum_entry(struct nilfs_sc_info *sci,
@@ -746,6 +743,15 @@ static void nilfs_dispose_list(struct the_nilfs *nilfs,
 	}
 }
 
+static void nilfs_iput_work_func(struct work_struct *work)
+{
+	struct nilfs_sc_info *sci = container_of(work, struct nilfs_sc_info,
+						 sc_iput_work);
+	struct the_nilfs *nilfs = sci->sc_super->s_fs_info;
+
+	nilfs_dispose_list(nilfs, &sci->sc_iput_queue, 0);
+}
+
 static int nilfs_test_metadata_dirty(struct the_nilfs *nilfs,
 				     struct nilfs_root *root)
 {
@@ -1899,8 +1905,8 @@ static int nilfs_segctor_collect_dirty_files(struct nilfs_sc_info *sci,
 static void nilfs_segctor_drop_written_files(struct nilfs_sc_info *sci,
 					     struct the_nilfs *nilfs)
 {
-	struct nilfs_transaction_info *ti = current->journal_info;
 	struct nilfs_inode_info *ii, *n;
+	int defer_iput = false;
 
 	spin_lock(&nilfs->ns_inode_lock);
 	list_for_each_entry_safe(ii, n, &sci->sc_dirty_files, i_dirty) {
@@ -1911,9 +1917,24 @@ static void nilfs_segctor_drop_written_files(struct nilfs_sc_info *sci,
 		clear_bit(NILFS_I_BUSY, &ii->i_state);
 		brelse(ii->i_bh);
 		ii->i_bh = NULL;
-		list_move_tail(&ii->i_dirty, &ti->ti_garbage);
+		list_del_init(&ii->i_dirty);
+		if (!ii->vfs_inode.i_nlink) {
+			/*
+			 * Defer calling iput() to avoid a deadlock
+			 * over I_SYNC flag for inodes with i_nlink == 0
+			 */
+			list_add_tail(&ii->i_dirty, &sci->sc_iput_queue);
+			defer_iput = true;
+		} else {
+			spin_unlock(&nilfs->ns_inode_lock);
+			iput(&ii->vfs_inode);
+			spin_lock(&nilfs->ns_inode_lock);
+		}
 	}
 	spin_unlock(&nilfs->ns_inode_lock);
+
+	if (defer_iput)
+		schedule_work(&sci->sc_iput_work);
 }
 
 /*
@@ -2580,6 +2601,8 @@ static struct nilfs_sc_info *nilfs_segctor_new(struct super_block *sb,
 	INIT_LIST_HEAD(&sci->sc_segbufs);
 	INIT_LIST_HEAD(&sci->sc_write_logs);
 	INIT_LIST_HEAD(&sci->sc_gc_inodes);
+	INIT_LIST_HEAD(&sci->sc_iput_queue);
+	INIT_WORK(&sci->sc_iput_work, nilfs_iput_work_func);
 	init_timer(&sci->sc_timer);
 
 	sci->sc_interval = HZ * NILFS_SC_DEFAULT_TIMEOUT;
@@ -2606,6 +2629,8 @@ static void nilfs_segctor_write_out(struct nilfs_sc_info *sci)
 		ret = nilfs_segctor_construct(sci, SC_LSEG_SR);
 		nilfs_transaction_unlock(sci->sc_super);
 
+		flush_work(&sci->sc_iput_work);
+
 	} while (ret && retrycount-- > 0);
 }
 
@@ -2630,6 +2655,9 @@ static void nilfs_segctor_destroy(struct nilfs_sc_info *sci)
 		|| sci->sc_seq_request != sci->sc_seq_done);
 	spin_unlock(&sci->sc_state_lock);
 
+	if (flush_work(&sci->sc_iput_work))
+		flag = true;
+
 	if (flag || !nilfs_segctor_confirm(sci))
 		nilfs_segctor_write_out(sci);
 
@@ -2639,6 +2667,12 @@ static void nilfs_segctor_destroy(struct nilfs_sc_info *sci)
 		nilfs_dispose_list(nilfs, &sci->sc_dirty_files, 1);
 	}
 
+	if (!list_empty(&sci->sc_iput_queue)) {
+		nilfs_warning(sci->sc_super, __func__,
+			      "iput queue is not empty\n");
+		nilfs_dispose_list(nilfs, &sci->sc_iput_queue, 1);
+	}
+
 	WARN_ON(!list_empty(&sci->sc_segbufs));
 	WARN_ON(!list_empty(&sci->sc_write_logs));
 
diff --git a/fs/nilfs2/segment.h b/fs/nilfs2/segment.h
index 38a1d00..a48d6de 100644
--- a/fs/nilfs2/segment.h
+++ b/fs/nilfs2/segment.h
@@ -26,6 +26,7 @@
 #include <linux/types.h>
 #include <linux/fs.h>
 #include <linux/buffer_head.h>
+#include <linux/workqueue.h>
 #include <linux/nilfs2_fs.h>
 #include "nilfs.h"
 
@@ -92,6 +93,8 @@ struct nilfs_segsum_pointer {
  * @sc_nblk_inc: Block count of current generation
  * @sc_dirty_files: List of files to be written
  * @sc_gc_inodes: List of GC inodes having blocks to be written
+ * @sc_iput_queue: list of inodes for which iput should be done
+ * @sc_iput_work: work struct to defer iput call
  * @sc_freesegs: array of segment numbers to be freed
  * @sc_nfreesegs: number of segments on @sc_freesegs
  * @sc_dsync_inode: inode whose data pages are written for a sync operation
@@ -135,6 +138,8 @@ struct nilfs_sc_info {
 
 	struct list_head	sc_dirty_files;
 	struct list_head	sc_gc_inodes;
+	struct list_head	sc_iput_queue;
+	struct work_struct	sc_iput_work;
 
 	__u64		       *sc_freesegs;
 	size_t			sc_nfreesegs;
diff --git a/include/sound/ak4113.h b/include/sound/ak4113.h
index 2609048..3a34f6e 100644
--- a/include/sound/ak4113.h
+++ b/include/sound/ak4113.h
@@ -286,7 +286,7 @@ struct ak4113 {
 	ak4113_write_t *write;
 	ak4113_read_t *read;
 	void *private_data;
-	unsigned int init:1;
+	atomic_t wq_processing;
 	spinlock_t lock;
 	unsigned char regmap[AK4113_WRITABLE_REGS];
 	struct snd_kcontrol *kctls[AK4113_CONTROLS];
diff --git a/include/sound/ak4114.h b/include/sound/ak4114.h
index 52f02a6..069299a 100644
--- a/include/sound/ak4114.h
+++ b/include/sound/ak4114.h
@@ -168,7 +168,7 @@ struct ak4114 {
 	ak4114_write_t * write;
 	ak4114_read_t * read;
 	void * private_data;
-	unsigned int init: 1;
+	atomic_t wq_processing;
 	spinlock_t lock;
 	unsigned char regmap[6];
 	unsigned char txcsb[5];
diff --git a/kernel/smpboot.c b/kernel/smpboot.c
index eb89e18..60d35ac5 100644
--- a/kernel/smpboot.c
+++ b/kernel/smpboot.c
@@ -279,6 +279,7 @@ int smpboot_register_percpu_thread(struct smp_hotplug_thread *plug_thread)
 	unsigned int cpu;
 	int ret = 0;
 
+	get_online_cpus();
 	mutex_lock(&smpboot_threads_lock);
 	for_each_online_cpu(cpu) {
 		ret = __smpboot_create_thread(plug_thread, cpu);
@@ -291,6 +292,7 @@ int smpboot_register_percpu_thread(struct smp_hotplug_thread *plug_thread)
 	list_add(&plug_thread->list, &hotplug_threads);
 out:
 	mutex_unlock(&smpboot_threads_lock);
+	put_online_cpus();
 	return ret;
 }
 EXPORT_SYMBOL_GPL(smpboot_register_percpu_thread);
diff --git a/lib/checksum.c b/lib/checksum.c
index 129775e..8b39e86 100644
--- a/lib/checksum.c
+++ b/lib/checksum.c
@@ -181,6 +181,15 @@ csum_partial_copy(const void *src, void *dst, int len, __wsum sum)
 EXPORT_SYMBOL(csum_partial_copy);
 
 #ifndef csum_tcpudp_nofold
+static inline u32 from64to32(u64 x)
+{
+	/* add up 32-bit and 32-bit for 32+c bit */
+	x = (x & 0xffffffff) + (x >> 32);
+	/* add up carry.. */
+	x = (x & 0xffffffff) + (x >> 32);
+	return (u32)x;
+}
+
 __wsum csum_tcpudp_nofold(__be32 saddr, __be32 daddr,
 			unsigned short len,
 			unsigned short proto,
@@ -195,8 +204,7 @@ __wsum csum_tcpudp_nofold(__be32 saddr, __be32 daddr,
 #else
 	s += (proto + len) << 8;
 #endif
-	s += (s >> 32);
-	return (__force __wsum)s;
+	return (__force __wsum)from64to32(s);
 }
 EXPORT_SYMBOL(csum_tcpudp_nofold);
 #endif
diff --git a/mm/pagewalk.c b/mm/pagewalk.c
index 2beeabf..9056d22 100644
--- a/mm/pagewalk.c
+++ b/mm/pagewalk.c
@@ -199,7 +199,10 @@ int walk_page_range(unsigned long addr, unsigned long end,
 			 */
 			if ((vma->vm_start <= addr) &&
 			    (vma->vm_flags & VM_PFNMAP)) {
-				next = vma->vm_end;
+				if (walk->pte_hole)
+					err = walk->pte_hole(addr, next, walk);
+				if (err)
+					break;
 				pgd = pgd_offset(walk->mm, next);
 				continue;
 			}
diff --git a/scripts/kconfig/menu.c b/scripts/kconfig/menu.c
index db1512a..f53542b 100644
--- a/scripts/kconfig/menu.c
+++ b/scripts/kconfig/menu.c
@@ -545,7 +545,7 @@ static void get_prompt_str(struct gstr *r, struct property *prop,
 {
 	int i, j;
 	struct menu *submenu[8], *menu, *location = NULL;
-	struct jump_key *jump;
+	struct jump_key *jump = NULL;
 
 	str_printf(r, _("Prompt: %s\n"), _(prop->text));
 	menu = prop->menu->parent;
@@ -583,7 +583,7 @@ static void get_prompt_str(struct gstr *r, struct property *prop,
 		str_printf(r, _("  Location:\n"));
 		for (j = 4; --i >= 0; j += 2) {
 			menu = submenu[i];
-			if (head && location && menu == location)
+			if (jump && menu == location)
 				jump->offset = strlen(r->s);
 			str_printf(r, "%*c-> %s", j, ' ',
 				   _(menu_get_prompt(menu)));
diff --git a/sound/i2c/other/ak4113.c b/sound/i2c/other/ak4113.c
index e04e750..7a9149b 100644
--- a/sound/i2c/other/ak4113.c
+++ b/sound/i2c/other/ak4113.c
@@ -56,8 +56,7 @@ static inline unsigned char reg_read(struct ak4113 *ak4113, unsigned char reg)
 
 static void snd_ak4113_free(struct ak4113 *chip)
 {
-	chip->init = 1;	/* don't schedule new work */
-	mb();
+	atomic_inc(&chip->wq_processing);	/* don't schedule new work */
 	cancel_delayed_work_sync(&chip->work);
 	kfree(chip);
 }
@@ -89,6 +88,7 @@ int snd_ak4113_create(struct snd_card *card, ak4113_read_t *read,
 	chip->write = write;
 	chip->private_data = private_data;
 	INIT_DELAYED_WORK(&chip->work, ak4113_stats);
+	atomic_set(&chip->wq_processing, 0);
 
 	for (reg = 0; reg < AK4113_WRITABLE_REGS ; reg++)
 		chip->regmap[reg] = pgm[reg];
@@ -139,13 +139,11 @@ static void ak4113_init_regs(struct ak4113 *chip)
 
 void snd_ak4113_reinit(struct ak4113 *chip)
 {
-	chip->init = 1;
-	mb();
-	flush_delayed_work(&chip->work);
+	if (atomic_inc_return(&chip->wq_processing) == 1)
+		cancel_delayed_work_sync(&chip->work);
 	ak4113_init_regs(chip);
 	/* bring up statistics / event queing */
-	chip->init = 0;
-	if (chip->kctls[0])
+	if (atomic_dec_and_test(&chip->wq_processing))
 		schedule_delayed_work(&chip->work, HZ / 10);
 }
 EXPORT_SYMBOL_GPL(snd_ak4113_reinit);
@@ -632,8 +630,9 @@ static void ak4113_stats(struct work_struct *work)
 {
 	struct ak4113 *chip = container_of(work, struct ak4113, work.work);
 
-	if (!chip->init)
+	if (atomic_inc_return(&chip->wq_processing) == 1)
 		snd_ak4113_check_rate_and_errors(chip, chip->check_flags);
 
-	schedule_delayed_work(&chip->work, HZ / 10);
+	if (atomic_dec_and_test(&chip->wq_processing))
+		schedule_delayed_work(&chip->work, HZ / 10);
 }
diff --git a/sound/i2c/other/ak4114.c b/sound/i2c/other/ak4114.c
index 15ae025..bf515db 100644
--- a/sound/i2c/other/ak4114.c
+++ b/sound/i2c/other/ak4114.c
@@ -66,8 +66,7 @@ static void reg_dump(struct ak4114 *ak4114)
 
 static void snd_ak4114_free(struct ak4114 *chip)
 {
-	chip->init = 1;	/* don't schedule new work */
-	mb();
+	atomic_inc(&chip->wq_processing);	/* don't schedule new work */
 	cancel_delayed_work_sync(&chip->work);
 	kfree(chip);
 }
@@ -100,6 +99,7 @@ int snd_ak4114_create(struct snd_card *card,
 	chip->write = write;
 	chip->private_data = private_data;
 	INIT_DELAYED_WORK(&chip->work, ak4114_stats);
+	atomic_set(&chip->wq_processing, 0);
 
 	for (reg = 0; reg < 6; reg++)
 		chip->regmap[reg] = pgm[reg];
@@ -152,13 +152,11 @@ static void ak4114_init_regs(struct ak4114 *chip)
 
 void snd_ak4114_reinit(struct ak4114 *chip)
 {
-	chip->init = 1;
-	mb();
-	flush_delayed_work(&chip->work);
+	if (atomic_inc_return(&chip->wq_processing) == 1)
+		cancel_delayed_work_sync(&chip->work);
 	ak4114_init_regs(chip);
 	/* bring up statistics / event queing */
-	chip->init = 0;
-	if (chip->kctls[0])
+	if (atomic_dec_and_test(&chip->wq_processing))
 		schedule_delayed_work(&chip->work, HZ / 10);
 }
 
@@ -612,10 +610,10 @@ static void ak4114_stats(struct work_struct *work)
 {
 	struct ak4114 *chip = container_of(work, struct ak4114, work.work);
 
-	if (!chip->init)
+	if (atomic_inc_return(&chip->wq_processing) == 1)
 		snd_ak4114_check_rate_and_errors(chip, chip->check_flags);
-
-	schedule_delayed_work(&chip->work, HZ / 10);
+	if (atomic_dec_and_test(&chip->wq_processing))
+		schedule_delayed_work(&chip->work, HZ / 10);
 }
 
 EXPORT_SYMBOL(snd_ak4114_create);
diff --git a/sound/soc/atmel/atmel_ssc_dai.c b/sound/soc/atmel/atmel_ssc_dai.c
index 1ead3c9..f20e703 100644
--- a/sound/soc/atmel/atmel_ssc_dai.c
+++ b/sound/soc/atmel/atmel_ssc_dai.c
@@ -344,7 +344,6 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 	struct atmel_pcm_dma_params *dma_params;
 	int dir, channels, bits;
 	u32 tfmr, rfmr, tcmr, rcmr;
-	int start_event;
 	int ret;
 
 	/*
@@ -451,19 +450,10 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 		 * The SSC transmit clock is obtained from the BCLK signal on
 		 * on the TK line, and the SSC receive clock is
 		 * generated from the transmit clock.
-		 *
-		 *  For single channel data, one sample is transferred
-		 * on the falling edge of the LRC clock.
-		 * For two channel data, one sample is
-		 * transferred on both edges of the LRC clock.
 		 */
-		start_event = ((channels == 1)
-				? SSC_START_FALLING_RF
-				: SSC_START_EDGE_RF);
-
 		rcmr =	  SSC_BF(RCMR_PERIOD, 0)
 			| SSC_BF(RCMR_STTDLY, START_DELAY)
-			| SSC_BF(RCMR_START, start_event)
+			| SSC_BF(RCMR_START, SSC_START_FALLING_RF)
 			| SSC_BF(RCMR_CKI, SSC_CKI_RISING)
 			| SSC_BF(RCMR_CKO, SSC_CKO_NONE)
 			| SSC_BF(RCMR_CKS, SSC_CKS_CLOCK);
@@ -471,14 +461,14 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 		rfmr =	  SSC_BF(RFMR_FSEDGE, SSC_FSEDGE_POSITIVE)
 			| SSC_BF(RFMR_FSOS, SSC_FSOS_NONE)
 			| SSC_BF(RFMR_FSLEN, 0)
-			| SSC_BF(RFMR_DATNB, 0)
+			| SSC_BF(RFMR_DATNB, (channels - 1))
 			| SSC_BIT(RFMR_MSBF)
 			| SSC_BF(RFMR_LOOP, 0)
 			| SSC_BF(RFMR_DATLEN, (bits - 1));
 
 		tcmr =	  SSC_BF(TCMR_PERIOD, 0)
 			| SSC_BF(TCMR_STTDLY, START_DELAY)
-			| SSC_BF(TCMR_START, start_event)
+			| SSC_BF(TCMR_START, SSC_START_FALLING_RF)
 			| SSC_BF(TCMR_CKI, SSC_CKI_FALLING)
 			| SSC_BF(TCMR_CKO, SSC_CKO_NONE)
 			| SSC_BF(TCMR_CKS, SSC_CKS_PIN);
@@ -487,7 +477,7 @@ static int atmel_ssc_hw_params(struct snd_pcm_substream *substream,
 			| SSC_BF(TFMR_FSDEN, 0)
 			| SSC_BF(TFMR_FSOS, SSC_FSOS_NONE)
 			| SSC_BF(TFMR_FSLEN, 0)
-			| SSC_BF(TFMR_DATNB, 0)
+			| SSC_BF(TFMR_DATNB, (channels - 1))
 			| SSC_BIT(TFMR_MSBF)
 			| SSC_BF(TFMR_DATDEF, 0)
 			| SSC_BF(TFMR_DATLEN, (bits - 1));
diff --git a/sound/soc/codecs/sgtl5000.c b/sound/soc/codecs/sgtl5000.c
index 12528e9..715589f 100644
--- a/sound/soc/codecs/sgtl5000.c
+++ b/sound/soc/codecs/sgtl5000.c
@@ -1521,6 +1521,9 @@ static int sgtl5000_i2c_probe(struct i2c_client *client,
 	if (ret)
 		return ret;
 
+	/* Need 8 clocks before I2C accesses */
+	udelay(1);
+
 	/* read chip information */
 	ret = regmap_read(sgtl5000->regmap, SGTL5000_CHIP_ID, &reg);
 	if (ret)
