diff --git a/Makefile b/Makefile
index 63a5ee8..944db23 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 14
-SUBLEVEL = 26
+SUBLEVEL = 27
 EXTRAVERSION =
 NAME = Remembering Coco
 
diff --git a/arch/powerpc/kernel/vdso32/getcpu.S b/arch/powerpc/kernel/vdso32/getcpu.S
index 47afd08..fe7e97a 100644
--- a/arch/powerpc/kernel/vdso32/getcpu.S
+++ b/arch/powerpc/kernel/vdso32/getcpu.S
@@ -30,8 +30,8 @@
 V_FUNCTION_BEGIN(__kernel_getcpu)
   .cfi_startproc
 	mfspr	r5,SPRN_USPRG3
-	cmpdi	cr0,r3,0
-	cmpdi	cr1,r4,0
+	cmpwi	cr0,r3,0
+	cmpwi	cr1,r4,0
 	clrlwi  r6,r5,16
 	rlwinm  r7,r5,16,31-15,31-0
 	beq	cr0,1f
diff --git a/arch/x86/boot/compressed/Makefile b/arch/x86/boot/compressed/Makefile
index 14fe7cb..b5bb498 100644
--- a/arch/x86/boot/compressed/Makefile
+++ b/arch/x86/boot/compressed/Makefile
@@ -75,7 +75,7 @@ suffix-$(CONFIG_KERNEL_XZ)	:= xz
 suffix-$(CONFIG_KERNEL_LZO) 	:= lzo
 suffix-$(CONFIG_KERNEL_LZ4) 	:= lz4
 
-RUN_SIZE = $(shell objdump -h vmlinux | \
+RUN_SIZE = $(shell $(OBJDUMP) -h vmlinux | \
 	     perl $(srctree)/arch/x86/tools/calc_run_size.pl)
 quiet_cmd_mkpiggy = MKPIGGY $@
       cmd_mkpiggy = $(obj)/mkpiggy $< $(RUN_SIZE) > $@ || ( rm -f $@ ; false )
diff --git a/arch/x86/kernel/cpu/perf_event.c b/arch/x86/kernel/cpu/perf_event.c
index 79f9f84..fb345c4 100644
--- a/arch/x86/kernel/cpu/perf_event.c
+++ b/arch/x86/kernel/cpu/perf_event.c
@@ -118,6 +118,9 @@ static int x86_pmu_extra_regs(u64 config, struct perf_event *event)
 			continue;
 		if (event->attr.config1 & ~er->valid_mask)
 			return -EINVAL;
+		/* Check if the extra msrs can be safely accessed*/
+		if (!er->extra_msr_access)
+			return -ENXIO;
 
 		reg->idx = er->idx;
 		reg->config = event->attr.config1;
diff --git a/arch/x86/kernel/cpu/perf_event.h b/arch/x86/kernel/cpu/perf_event.h
index 4972c24..7876c34 100644
--- a/arch/x86/kernel/cpu/perf_event.h
+++ b/arch/x86/kernel/cpu/perf_event.h
@@ -293,14 +293,16 @@ struct extra_reg {
 	u64			config_mask;
 	u64			valid_mask;
 	int			idx;  /* per_xxx->regs[] reg index */
+	bool			extra_msr_access;
 };
 
 #define EVENT_EXTRA_REG(e, ms, m, vm, i) {	\
-	.event = (e),		\
-	.msr = (ms),		\
-	.config_mask = (m),	\
-	.valid_mask = (vm),	\
-	.idx = EXTRA_REG_##i,	\
+	.event = (e),			\
+	.msr = (ms),			\
+	.config_mask = (m),		\
+	.valid_mask = (vm),		\
+	.idx = EXTRA_REG_##i,		\
+	.extra_msr_access = true,	\
 	}
 
 #define INTEL_EVENT_EXTRA_REG(event, msr, vm, idx)	\
diff --git a/arch/x86/kernel/cpu/perf_event_intel.c b/arch/x86/kernel/cpu/perf_event_intel.c
index 5ee8064..d4c0a0e 100644
--- a/arch/x86/kernel/cpu/perf_event_intel.c
+++ b/arch/x86/kernel/cpu/perf_event_intel.c
@@ -2183,6 +2183,41 @@ static void intel_snb_check_microcode(void)
 	}
 }
 
+/*
+ * Under certain circumstances, access certain MSR may cause #GP.
+ * The function tests if the input MSR can be safely accessed.
+ */
+static bool check_msr(unsigned long msr, u64 mask)
+{
+	u64 val_old, val_new, val_tmp;
+
+	/*
+	 * Read the current value, change it and read it back to see if it
+	 * matches, this is needed to detect certain hardware emulators
+	 * (qemu/kvm) that don't trap on the MSR access and always return 0s.
+	 */
+	if (rdmsrl_safe(msr, &val_old))
+		return false;
+
+	/*
+	 * Only change the bits which can be updated by wrmsrl.
+	 */
+	val_tmp = val_old ^ mask;
+	if (wrmsrl_safe(msr, val_tmp) ||
+	    rdmsrl_safe(msr, &val_new))
+		return false;
+
+	if (val_new != val_tmp)
+		return false;
+
+	/* Here it's sure that the MSR can be safely accessed.
+	 * Restore the old value and return.
+	 */
+	wrmsrl(msr, val_old);
+
+	return true;
+}
+
 static __init void intel_sandybridge_quirk(void)
 {
 	x86_pmu.check_microcode = intel_snb_check_microcode;
@@ -2272,7 +2307,8 @@ __init int intel_pmu_init(void)
 	union cpuid10_ebx ebx;
 	struct event_constraint *c;
 	unsigned int unused;
-	int version;
+	struct extra_reg *er;
+	int version, i;
 
 	if (!cpu_has(&boot_cpu_data, X86_FEATURE_ARCH_PERFMON)) {
 		switch (boot_cpu_data.x86) {
@@ -2578,6 +2614,34 @@ __init int intel_pmu_init(void)
 		}
 	}
 
+	/*
+	 * Access LBR MSR may cause #GP under certain circumstances.
+	 * E.g. KVM doesn't support LBR MSR
+	 * Check all LBT MSR here.
+	 * Disable LBR access if any LBR MSRs can not be accessed.
+	 */
+	if (x86_pmu.lbr_nr && !check_msr(x86_pmu.lbr_tos, 0x3UL))
+		x86_pmu.lbr_nr = 0;
+	for (i = 0; i < x86_pmu.lbr_nr; i++) {
+		if (!(check_msr(x86_pmu.lbr_from + i, 0xffffUL) &&
+		      check_msr(x86_pmu.lbr_to + i, 0xffffUL)))
+			x86_pmu.lbr_nr = 0;
+	}
+
+	/*
+	 * Access extra MSR may cause #GP under certain circumstances.
+	 * E.g. KVM doesn't support offcore event
+	 * Check all extra_regs here.
+	 */
+	if (x86_pmu.extra_regs) {
+		for (er = x86_pmu.extra_regs; er->msr; er++) {
+			er->extra_msr_access = check_msr(er->msr, 0x1ffUL);
+			/* Disable LBR select mapping */
+			if ((er->idx == EXTRA_REG_LBR) && !er->extra_msr_access)
+				x86_pmu.lbr_sel_map = NULL;
+		}
+	}
+
 	/* Support full width counters using alternative MSR range */
 	if (x86_pmu.intel_cap.full_width_write) {
 		x86_pmu.max_period = x86_pmu.cntval_mask;
diff --git a/drivers/ata/ahci.c b/drivers/ata/ahci.c
index e662f14..cc5f102 100644
--- a/drivers/ata/ahci.c
+++ b/drivers/ata/ahci.c
@@ -322,6 +322,9 @@ static const struct pci_device_id ahci_pci_tbl[] = {
 	{ PCI_VDEVICE(INTEL, 0x8c87), board_ahci }, /* 9 Series RAID */
 	{ PCI_VDEVICE(INTEL, 0x8c8e), board_ahci }, /* 9 Series RAID */
 	{ PCI_VDEVICE(INTEL, 0x8c8f), board_ahci }, /* 9 Series RAID */
+	{ PCI_VDEVICE(INTEL, 0x9d03), board_ahci }, /* Sunrise Point-LP AHCI */
+	{ PCI_VDEVICE(INTEL, 0x9d05), board_ahci }, /* Sunrise Point-LP RAID */
+	{ PCI_VDEVICE(INTEL, 0x9d07), board_ahci }, /* Sunrise Point-LP RAID */
 	{ PCI_VDEVICE(INTEL, 0xa103), board_ahci }, /* Sunrise Point-H AHCI */
 	{ PCI_VDEVICE(INTEL, 0xa103), board_ahci }, /* Sunrise Point-H RAID */
 	{ PCI_VDEVICE(INTEL, 0xa105), board_ahci }, /* Sunrise Point-H RAID */
@@ -493,6 +496,7 @@ static const struct pci_device_id ahci_pci_tbl[] = {
 	 * enabled.  https://bugzilla.kernel.org/show_bug.cgi?id=60731
 	 */
 	{ PCI_VDEVICE(SAMSUNG, 0x1600), board_ahci_nomsi },
+	{ PCI_VDEVICE(SAMSUNG, 0xa800), board_ahci_nomsi },
 
 	/* Enmotus */
 	{ PCI_DEVICE(0x1c44, 0x8000), board_ahci },
diff --git a/drivers/ata/sata_fsl.c b/drivers/ata/sata_fsl.c
index fb0b40a..ee2780d 100644
--- a/drivers/ata/sata_fsl.c
+++ b/drivers/ata/sata_fsl.c
@@ -1503,7 +1503,7 @@ static int sata_fsl_probe(struct platform_device *ofdev)
 	host_priv->csr_base = csr_base;
 
 	irq = irq_of_parse_and_map(ofdev->dev.of_node, 0);
-	if (irq < 0) {
+	if (!irq) {
 		dev_err(&ofdev->dev, "invalid irq from platform\n");
 		goto error_exit_with_cleanup;
 	}
diff --git a/drivers/gpu/drm/i915/intel_display.c b/drivers/gpu/drm/i915/intel_display.c
index b6fb3eb..c514690 100644
--- a/drivers/gpu/drm/i915/intel_display.c
+++ b/drivers/gpu/drm/i915/intel_display.c
@@ -3817,7 +3817,6 @@ static void ironlake_crtc_disable(struct drm_crtc *crtc)
 		ironlake_fdi_disable(crtc);
 
 		ironlake_disable_pch_transcoder(dev_priv, pipe);
-		intel_set_pch_fifo_underrun_reporting(dev, pipe, true);
 
 		if (HAS_PCH_CPT(dev)) {
 			/* disable TRANS_DP_CTL */
@@ -3883,7 +3882,6 @@ static void haswell_crtc_disable(struct drm_crtc *crtc)
 
 	if (intel_crtc->config.has_pch_encoder) {
 		lpt_disable_pch_transcoder(dev_priv);
-		intel_set_pch_fifo_underrun_reporting(dev, TRANSCODER_A, true);
 		intel_ddi_fdi_disable(crtc);
 	}
 
diff --git a/drivers/gpu/drm/i915/intel_lvds.c b/drivers/gpu/drm/i915/intel_lvds.c
index 67c9ff3..af49b24 100644
--- a/drivers/gpu/drm/i915/intel_lvds.c
+++ b/drivers/gpu/drm/i915/intel_lvds.c
@@ -905,6 +905,17 @@ void intel_lvds_init(struct drm_device *dev)
 	int pipe;
 	u8 pin;
 
+	/*
+	 * Unlock registers and just leave them unlocked. Do this before
+	 * checking quirk lists to avoid bogus WARNINGs.
+	 */
+	if (HAS_PCH_SPLIT(dev)) {
+		I915_WRITE(PCH_PP_CONTROL,
+			   I915_READ(PCH_PP_CONTROL) | PANEL_UNLOCK_REGS);
+	} else {
+		I915_WRITE(PP_CONTROL,
+			   I915_READ(PP_CONTROL) | PANEL_UNLOCK_REGS);
+	}
 	if (!intel_lvds_supported(dev))
 		return;
 
@@ -1099,17 +1110,6 @@ out:
 	DRM_DEBUG_KMS("detected %s-link lvds configuration\n",
 		      lvds_encoder->is_dual_link ? "dual" : "single");
 
-	/*
-	 * Unlock registers and just
-	 * leave them unlocked
-	 */
-	if (HAS_PCH_SPLIT(dev)) {
-		I915_WRITE(PCH_PP_CONTROL,
-			   I915_READ(PCH_PP_CONTROL) | PANEL_UNLOCK_REGS);
-	} else {
-		I915_WRITE(PP_CONTROL,
-			   I915_READ(PP_CONTROL) | PANEL_UNLOCK_REGS);
-	}
 	lvds_connector->lid_notifier.notifier_call = intel_lid_notify;
 	if (acpi_lid_notifier_register(&lvds_connector->lid_notifier)) {
 		DRM_DEBUG_KMS("lid notifier registration failed\n");
diff --git a/drivers/gpu/drm/radeon/radeon_kms.c b/drivers/gpu/drm/radeon/radeon_kms.c
index 0bc9106..6bffe82 100644
--- a/drivers/gpu/drm/radeon/radeon_kms.c
+++ b/drivers/gpu/drm/radeon/radeon_kms.c
@@ -740,6 +740,8 @@ int radeon_get_vblank_timestamp_kms(struct drm_device *dev, int crtc,
 
 	/* Get associated drm_crtc: */
 	drmcrtc = &rdev->mode_info.crtcs[crtc]->base;
+	if (!drmcrtc)
+		return -EINVAL;
 
 	/* Helper routine in DRM core does all the work: */
 	return drm_calc_vbltimestamp_from_scanoutpos(dev, crtc, max_error,
diff --git a/drivers/i2c/busses/i2c-davinci.c b/drivers/i2c/busses/i2c-davinci.c
index af0b583..e3c6a96 100644
--- a/drivers/i2c/busses/i2c-davinci.c
+++ b/drivers/i2c/busses/i2c-davinci.c
@@ -411,11 +411,9 @@ i2c_davinci_xfer_msg(struct i2c_adapter *adap, struct i2c_msg *msg, int stop)
 	if (dev->cmd_err & DAVINCI_I2C_STR_NACK) {
 		if (msg->flags & I2C_M_IGNORE_NAK)
 			return msg->len;
-		if (stop) {
-			w = davinci_i2c_read_reg(dev, DAVINCI_I2C_MDR_REG);
-			w |= DAVINCI_I2C_MDR_STP;
-			davinci_i2c_write_reg(dev, DAVINCI_I2C_MDR_REG, w);
-		}
+		w = davinci_i2c_read_reg(dev, DAVINCI_I2C_MDR_REG);
+		w |= DAVINCI_I2C_MDR_STP;
+		davinci_i2c_write_reg(dev, DAVINCI_I2C_MDR_REG, w);
 		return -EREMOTEIO;
 	}
 	return -EIO;
diff --git a/drivers/i2c/busses/i2c-omap.c b/drivers/i2c/busses/i2c-omap.c
index 90dcc2e..a686057 100644
--- a/drivers/i2c/busses/i2c-omap.c
+++ b/drivers/i2c/busses/i2c-omap.c
@@ -926,14 +926,12 @@ omap_i2c_isr_thread(int this_irq, void *dev_id)
 		if (stat & OMAP_I2C_STAT_NACK) {
 			err |= OMAP_I2C_STAT_NACK;
 			omap_i2c_ack_stat(dev, OMAP_I2C_STAT_NACK);
-			break;
 		}
 
 		if (stat & OMAP_I2C_STAT_AL) {
 			dev_err(dev->dev, "Arbitration lost\n");
 			err |= OMAP_I2C_STAT_AL;
 			omap_i2c_ack_stat(dev, OMAP_I2C_STAT_AL);
-			break;
 		}
 
 		/*
@@ -958,11 +956,13 @@ omap_i2c_isr_thread(int this_irq, void *dev_id)
 			if (dev->fifo_size)
 				num_bytes = dev->buf_len;
 
-			omap_i2c_receive_data(dev, num_bytes, true);
-
-			if (dev->errata & I2C_OMAP_ERRATA_I207)
+			if (dev->errata & I2C_OMAP_ERRATA_I207) {
 				i2c_omap_errata_i207(dev, stat);
+				num_bytes = (omap_i2c_read_reg(dev,
+					OMAP_I2C_BUFSTAT_REG) >> 8) & 0x3F;
+			}
 
+			omap_i2c_receive_data(dev, num_bytes, true);
 			omap_i2c_ack_stat(dev, OMAP_I2C_STAT_RDR);
 			continue;
 		}
diff --git a/drivers/media/i2c/smiapp/smiapp-core.c b/drivers/media/i2c/smiapp/smiapp-core.c
index 8741cae..7026ab0 100644
--- a/drivers/media/i2c/smiapp/smiapp-core.c
+++ b/drivers/media/i2c/smiapp/smiapp-core.c
@@ -2138,7 +2138,7 @@ static int smiapp_set_selection(struct v4l2_subdev *subdev,
 		ret = smiapp_set_compose(subdev, fh, sel);
 		break;
 	default:
-		BUG();
+		ret = -EINVAL;
 	}
 
 	mutex_unlock(&sensor->mutex);
diff --git a/drivers/net/ethernet/broadcom/tg3.c b/drivers/net/ethernet/broadcom/tg3.c
index 9373f1f..086eac5 100644
--- a/drivers/net/ethernet/broadcom/tg3.c
+++ b/drivers/net/ethernet/broadcom/tg3.c
@@ -8548,7 +8548,8 @@ static int tg3_init_rings(struct tg3 *tp)
 		if (tnapi->rx_rcb)
 			memset(tnapi->rx_rcb, 0, TG3_RX_RCB_RING_BYTES(tp));
 
-		if (tg3_rx_prodring_alloc(tp, &tnapi->prodring)) {
+		if (tnapi->prodring.rx_std &&
+		    tg3_rx_prodring_alloc(tp, &tnapi->prodring)) {
 			tg3_free_rings(tp);
 			return -ENOMEM;
 		}
diff --git a/drivers/net/ethernet/intel/igb/igb_main.c b/drivers/net/ethernet/intel/igb/igb_main.c
index 5ca8c47..206e79d 100644
--- a/drivers/net/ethernet/intel/igb/igb_main.c
+++ b/drivers/net/ethernet/intel/igb/igb_main.c
@@ -1613,6 +1613,8 @@ void igb_power_up_link(struct igb_adapter *adapter)
 		igb_power_up_phy_copper(&adapter->hw);
 	else
 		igb_power_up_serdes_link_82575(&adapter->hw);
+
+	igb_setup_link(&adapter->hw);
 }
 
 /**
diff --git a/drivers/net/ethernet/marvell/mvneta.c b/drivers/net/ethernet/marvell/mvneta.c
index c4c00d9f..96fc7fe 100644
--- a/drivers/net/ethernet/marvell/mvneta.c
+++ b/drivers/net/ethernet/marvell/mvneta.c
@@ -213,7 +213,7 @@
 /* Various constants */
 
 /* Coalescing */
-#define MVNETA_TXDONE_COAL_PKTS		16
+#define MVNETA_TXDONE_COAL_PKTS		1
 #define MVNETA_RX_COAL_PKTS		32
 #define MVNETA_RX_COAL_USEC		100
 
@@ -1612,6 +1612,7 @@ static int mvneta_tx(struct sk_buff *skb, struct net_device *dev)
 	u16 txq_id = skb_get_queue_mapping(skb);
 	struct mvneta_tx_queue *txq = &pp->txqs[txq_id];
 	struct mvneta_tx_desc *tx_desc;
+	int len = skb->len;
 	struct netdev_queue *nq;
 	int frags = 0;
 	u32 tx_cmd;
@@ -1675,7 +1676,7 @@ out:
 
 		u64_stats_update_begin(&stats->syncp);
 		stats->tx_packets++;
-		stats->tx_bytes  += skb->len;
+		stats->tx_bytes  += len;
 		u64_stats_update_end(&stats->syncp);
 	} else {
 		dev->stats.tx_dropped++;
diff --git a/drivers/net/ethernet/mellanox/mlx4/resource_tracker.c b/drivers/net/ethernet/mellanox/mlx4/resource_tracker.c
index 57428a0..1e8a4b4 100644
--- a/drivers/net/ethernet/mellanox/mlx4/resource_tracker.c
+++ b/drivers/net/ethernet/mellanox/mlx4/resource_tracker.c
@@ -1456,7 +1456,7 @@ static int qp_alloc_res(struct mlx4_dev *dev, int slave, int op, int cmd,
 
 	switch (op) {
 	case RES_OP_RESERVE:
-		count = get_param_l(&in_param);
+		count = get_param_l(&in_param) & 0xffffff;
 		align = get_param_h(&in_param);
 		err = mlx4_grant_resource(dev, slave, RES_QP, count, 0);
 		if (err)
diff --git a/drivers/net/vxlan.c b/drivers/net/vxlan.c
index 5441b49..5988910 100644
--- a/drivers/net/vxlan.c
+++ b/drivers/net/vxlan.c
@@ -2106,9 +2106,8 @@ static int vxlan_init(struct net_device *dev)
 	spin_lock(&vn->sock_lock);
 	vs = vxlan_find_sock(dev_net(dev), ipv6 ? AF_INET6 : AF_INET,
 			     vxlan->dst_port);
-	if (vs) {
+	if (vs && atomic_add_unless(&vs->refcnt, 1, 0)) {
 		/* If we have a socket with same port already, reuse it */
-		atomic_inc(&vs->refcnt);
 		vxlan_vs_add_dev(vs, vxlan);
 	} else {
 		/* otherwise make new socket outside of RTNL */
@@ -2574,12 +2573,9 @@ struct vxlan_sock *vxlan_sock_add(struct net *net, __be16 port,
 
 	spin_lock(&vn->sock_lock);
 	vs = vxlan_find_sock(net, ipv6 ? AF_INET6 : AF_INET, port);
-	if (vs) {
-		if (vs->rcv == rcv)
-			atomic_inc(&vs->refcnt);
-		else
+	if (vs && ((vs->rcv != rcv) ||
+		   !atomic_add_unless(&vs->refcnt, 1, 0)))
 			vs = ERR_PTR(-EBUSY);
-	}
 	spin_unlock(&vn->sock_lock);
 
 	if (!vs)
diff --git a/drivers/net/xen-netfront.c b/drivers/net/xen-netfront.c
index e30d800..19db057 100644
--- a/drivers/net/xen-netfront.c
+++ b/drivers/net/xen-netfront.c
@@ -469,9 +469,6 @@ static void xennet_make_frags(struct sk_buff *skb, struct net_device *dev,
 		len = skb_frag_size(frag);
 		offset = frag->page_offset;
 
-		/* Data must not cross a page boundary. */
-		BUG_ON(len + offset > PAGE_SIZE<<compound_order(page));
-
 		/* Skip unused frames from start of page */
 		page += offset >> PAGE_SHIFT;
 		offset &= ~PAGE_MASK;
@@ -479,8 +476,6 @@ static void xennet_make_frags(struct sk_buff *skb, struct net_device *dev,
 		while (len > 0) {
 			unsigned long bytes;
 
-			BUG_ON(offset >= PAGE_SIZE);
-
 			bytes = PAGE_SIZE - offset;
 			if (bytes > len)
 				bytes = len;
diff --git a/drivers/usb/host/xhci-ring.c b/drivers/usb/host/xhci-ring.c
index 1710a86..faa8b98 100644
--- a/drivers/usb/host/xhci-ring.c
+++ b/drivers/usb/host/xhci-ring.c
@@ -1998,22 +1998,13 @@ static int finish_td(struct xhci_hcd *xhci, struct xhci_td *td,
 		ep->stopped_td = td;
 		return 0;
 	} else {
-		if (trb_comp_code == COMP_STALL) {
-			/* The transfer is completed from the driver's
-			 * perspective, but we need to issue a set dequeue
-			 * command for this stalled endpoint to move the dequeue
-			 * pointer past the TD.  We can't do that here because
-			 * the halt condition must be cleared first.  Let the
-			 * USB class driver clear the stall later.
-			 */
-			ep->stopped_td = td;
-			ep->stopped_stream = ep_ring->stream_id;
-		} else if (xhci_requires_manual_halt_cleanup(xhci,
-					ep_ctx, trb_comp_code)) {
-			/* Other types of errors halt the endpoint, but the
-			 * class driver doesn't call usb_reset_endpoint() unless
-			 * the error is -EPIPE.  Clear the halted status in the
-			 * xHCI hardware manually.
+		if (trb_comp_code == COMP_STALL ||
+		    xhci_requires_manual_halt_cleanup(xhci, ep_ctx,
+						      trb_comp_code)) {
+			/* Issue a reset endpoint command to clear the host side
+			 * halt, followed by a set dequeue command to move the
+			 * dequeue pointer past the TD.
+			 * The class driver clears the device side halt later.
 			 */
 			xhci_cleanup_halted_endpoint(xhci,
 					slot_id, ep_index, ep_ring->stream_id,
@@ -2133,9 +2124,7 @@ static int process_ctrl_td(struct xhci_hcd *xhci, struct xhci_td *td,
 		else
 			td->urb->actual_length = 0;
 
-		xhci_cleanup_halted_endpoint(xhci,
-			slot_id, ep_index, 0, td, event_trb);
-		return finish_td(xhci, td, event_trb, event, ep, status, true);
+		return finish_td(xhci, td, event_trb, event, ep, status, false);
 	}
 	/*
 	 * Did we transfer any data, despite the errors that might have
@@ -2689,17 +2678,8 @@ cleanup:
 		if (ret) {
 			urb = td->urb;
 			urb_priv = urb->hcpriv;
-			/* Leave the TD around for the reset endpoint function
-			 * to use(but only if it's not a control endpoint,
-			 * since we already queued the Set TR dequeue pointer
-			 * command for stalled control endpoints).
-			 */
-			if (usb_endpoint_xfer_control(&urb->ep->desc) ||
-				(trb_comp_code != COMP_STALL &&
-					trb_comp_code != COMP_BABBLE))
-				xhci_urb_free_priv(xhci, urb_priv);
-			else
-				kfree(urb_priv);
+
+			xhci_urb_free_priv(xhci, urb_priv);
 
 			usb_hcd_unlink_urb_from_ep(bus_to_hcd(urb->dev->bus), urb);
 			if ((urb->actual_length != urb->transfer_buffer_length &&
diff --git a/drivers/usb/host/xhci.c b/drivers/usb/host/xhci.c
index 17e3987..16f4f8d 100644
--- a/drivers/usb/host/xhci.c
+++ b/drivers/usb/host/xhci.c
@@ -2925,63 +2925,33 @@ void xhci_cleanup_stalled_ring(struct xhci_hcd *xhci,
 	}
 }
 
-/* Deal with stalled endpoints.  The core should have sent the control message
- * to clear the halt condition.  However, we need to make the xHCI hardware
- * reset its sequence number, since a device will expect a sequence number of
- * zero after the halt condition is cleared.
+/* Called when clearing halted device. The core should have sent the control
+ * message to clear the device halt condition. The host side of the halt should
+ * already be cleared with a reset endpoint command issued when the STALL tx
+ * event was received.
+ *
  * Context: in_interrupt
  */
+
 void xhci_endpoint_reset(struct usb_hcd *hcd,
 		struct usb_host_endpoint *ep)
 {
 	struct xhci_hcd *xhci;
-	struct usb_device *udev;
-	unsigned int ep_index;
-	unsigned long flags;
-	int ret;
-	struct xhci_virt_ep *virt_ep;
 
 	xhci = hcd_to_xhci(hcd);
-	udev = (struct usb_device *) ep->hcpriv;
-	/* Called with a root hub endpoint (or an endpoint that wasn't added
-	 * with xhci_add_endpoint()
-	 */
-	if (!ep->hcpriv)
-		return;
-	ep_index = xhci_get_endpoint_index(&ep->desc);
-	virt_ep = &xhci->devs[udev->slot_id]->eps[ep_index];
-	if (!virt_ep->stopped_td) {
-		xhci_dbg_trace(xhci, trace_xhci_dbg_reset_ep,
-			"Endpoint 0x%x not halted, refusing to reset.",
-			ep->desc.bEndpointAddress);
-		return;
-	}
-	if (usb_endpoint_xfer_control(&ep->desc)) {
-		xhci_dbg_trace(xhci, trace_xhci_dbg_reset_ep,
-				"Control endpoint stall already handled.");
-		return;
-	}
 
-	xhci_dbg_trace(xhci, trace_xhci_dbg_reset_ep,
-			"Queueing reset endpoint command");
-	spin_lock_irqsave(&xhci->lock, flags);
-	ret = xhci_queue_reset_ep(xhci, udev->slot_id, ep_index);
 	/*
-	 * Can't change the ring dequeue pointer until it's transitioned to the
-	 * stopped state, which is only upon a successful reset endpoint
-	 * command.  Better hope that last command worked!
+	 * We might need to implement the config ep cmd in xhci 4.8.1 note:
+	 * The Reset Endpoint Command may only be issued to endpoints in the
+	 * Halted state. If software wishes reset the Data Toggle or Sequence
+	 * Number of an endpoint that isn't in the Halted state, then software
+	 * may issue a Configure Endpoint Command with the Drop and Add bits set
+	 * for the target endpoint. that is in the Stopped state.
 	 */
-	if (!ret) {
-		xhci_cleanup_stalled_ring(xhci, udev, ep_index);
-		kfree(virt_ep->stopped_td);
-		xhci_ring_cmd_db(xhci);
-	}
-	virt_ep->stopped_td = NULL;
-	virt_ep->stopped_stream = 0;
-	spin_unlock_irqrestore(&xhci->lock, flags);
 
-	if (ret)
-		xhci_warn(xhci, "FIXME allocate a new ring segment\n");
+	/* For now just print debug to follow the situation */
+	xhci_dbg(xhci, "Endpoint 0x%x ep reset callback called\n",
+		 ep->desc.bEndpointAddress);
 }
 
 static int xhci_check_streams_endpoint(struct xhci_hcd *xhci,
diff --git a/mm/frontswap.c b/mm/frontswap.c
index c30eec5..f2a3571 100644
--- a/mm/frontswap.c
+++ b/mm/frontswap.c
@@ -244,8 +244,10 @@ int __frontswap_store(struct page *page)
 		  the (older) page from frontswap
 		 */
 		inc_frontswap_failed_stores();
-		if (dup)
+		if (dup) {
 			__frontswap_clear(sis, offset);
+			frontswap_ops->invalidate_page(type, offset);
+		}
 	}
 	if (frontswap_writethrough_enabled)
 		/* report failure so swap also writes to swap device */
diff --git a/mm/memory.c b/mm/memory.c
index 492e36f..48d7365 100644
--- a/mm/memory.c
+++ b/mm/memory.c
@@ -808,20 +808,20 @@ copy_one_pte(struct mm_struct *dst_mm, struct mm_struct *src_mm,
 		if (!pte_file(pte)) {
 			swp_entry_t entry = pte_to_swp_entry(pte);
 
-			if (swap_duplicate(entry) < 0)
-				return entry.val;
-
-			/* make sure dst_mm is on swapoff's mmlist. */
-			if (unlikely(list_empty(&dst_mm->mmlist))) {
-				spin_lock(&mmlist_lock);
-				if (list_empty(&dst_mm->mmlist))
-					list_add(&dst_mm->mmlist,
-						 &src_mm->mmlist);
-				spin_unlock(&mmlist_lock);
-			}
-			if (likely(!non_swap_entry(entry)))
+			if (likely(!non_swap_entry(entry))) {
+				if (swap_duplicate(entry) < 0)
+					return entry.val;
+
+				/* make sure dst_mm is on swapoff's mmlist. */
+				if (unlikely(list_empty(&dst_mm->mmlist))) {
+					spin_lock(&mmlist_lock);
+					if (list_empty(&dst_mm->mmlist))
+						list_add(&dst_mm->mmlist,
+							 &src_mm->mmlist);
+					spin_unlock(&mmlist_lock);
+				}
 				rss[MM_SWAPENTS]++;
-			else if (is_migration_entry(entry)) {
+			} else if (is_migration_entry(entry)) {
 				page = migration_entry_to_page(entry);
 
 				if (PageAnon(page))
diff --git a/mm/mmap.c b/mm/mmap.c
index dfe90657..b91ac80 100644
--- a/mm/mmap.c
+++ b/mm/mmap.c
@@ -745,8 +745,11 @@ again:			remove_next = 1 + (end > next->vm_end);
 		 * shrinking vma had, to cover any anon pages imported.
 		 */
 		if (exporter && exporter->anon_vma && !importer->anon_vma) {
-			if (anon_vma_clone(importer, exporter))
-				return -ENOMEM;
+			int error;
+
+			error = anon_vma_clone(importer, exporter);
+			if (error)
+				return error;
 			importer->anon_vma = exporter->anon_vma;
 		}
 	}
@@ -2428,7 +2431,8 @@ static int __split_vma(struct mm_struct * mm, struct vm_area_struct * vma,
 	if (err)
 		goto out_free_vma;
 
-	if (anon_vma_clone(new, vma))
+	err = anon_vma_clone(new, vma);
+	if (err)
 		goto out_free_mpol;
 
 	if (new->vm_file)
diff --git a/mm/rmap.c b/mm/rmap.c
index cdbd312..cab9820 100644
--- a/mm/rmap.c
+++ b/mm/rmap.c
@@ -274,6 +274,7 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 {
 	struct anon_vma_chain *avc;
 	struct anon_vma *anon_vma;
+	int error;
 
 	/* Don't bother if the parent process has no anon_vma here. */
 	if (!pvma->anon_vma)
@@ -283,8 +284,9 @@ int anon_vma_fork(struct vm_area_struct *vma, struct vm_area_struct *pvma)
 	 * First, attach the new VMA to the parent VMA's anon_vmas,
 	 * so rmap can find non-COWed pages in child processes.
 	 */
-	if (anon_vma_clone(vma, pvma))
-		return -ENOMEM;
+	error = anon_vma_clone(vma, pvma);
+	if (error)
+		return error;
 
 	/* Then add our own anon_vma. */
 	anon_vma = anon_vma_alloc();
diff --git a/mm/vmpressure.c b/mm/vmpressure.c
index d4042e7..c5afd57 100644
--- a/mm/vmpressure.c
+++ b/mm/vmpressure.c
@@ -165,6 +165,7 @@ static void vmpressure_work_fn(struct work_struct *work)
 	unsigned long scanned;
 	unsigned long reclaimed;
 
+	spin_lock(&vmpr->sr_lock);
 	/*
 	 * Several contexts might be calling vmpressure(), so it is
 	 * possible that the work was rescheduled again before the old
@@ -173,11 +174,12 @@ static void vmpressure_work_fn(struct work_struct *work)
 	 * here. No need for any locks here since we don't care if
 	 * vmpr->reclaimed is in sync.
 	 */
-	if (!vmpr->scanned)
+	scanned = vmpr->scanned;
+	if (!scanned) {
+		spin_unlock(&vmpr->sr_lock);
 		return;
+	}
 
-	spin_lock(&vmpr->sr_lock);
-	scanned = vmpr->scanned;
 	reclaimed = vmpr->reclaimed;
 	vmpr->scanned = 0;
 	vmpr->reclaimed = 0;
diff --git a/net/core/rtnetlink.c b/net/core/rtnetlink.c
index b0db904..4617586 100644
--- a/net/core/rtnetlink.c
+++ b/net/core/rtnetlink.c
@@ -1453,6 +1453,7 @@ static int do_setlink(const struct sk_buff *skb,
 			goto errout;
 		}
 		if (!netlink_ns_capable(skb, net->user_ns, CAP_NET_ADMIN)) {
+			put_net(net);
 			err = -EPERM;
 			goto errout;
 		}
diff --git a/net/ipv4/gre_offload.c b/net/ipv4/gre_offload.c
index 8c8493e..278836f 100644
--- a/net/ipv4/gre_offload.c
+++ b/net/ipv4/gre_offload.c
@@ -271,6 +271,9 @@ static int gre_gro_complete(struct sk_buff *skb, int nhoff)
 		err = ptype->callbacks.gro_complete(skb, nhoff + grehlen);
 
 	rcu_read_unlock();
+
+	skb_set_inner_mac_header(skb, nhoff + grehlen);
+
 	return err;
 }
 
diff --git a/net/ipv4/ip_vti.c b/net/ipv4/ip_vti.c
index e4a8f76..b0a9cb4 100644
--- a/net/ipv4/ip_vti.c
+++ b/net/ipv4/ip_vti.c
@@ -369,6 +369,7 @@ static struct rtnl_link_ops vti_link_ops __read_mostly = {
 	.validate	= vti_tunnel_validate,
 	.newlink	= vti_newlink,
 	.changelink	= vti_changelink,
+	.dellink        = ip_tunnel_dellink,
 	.get_size	= vti_get_size,
 	.fill_info	= vti_fill_info,
 };
diff --git a/net/ipv6/ip6_gre.c b/net/ipv6/ip6_gre.c
index b27f6d3..4a230b1 100644
--- a/net/ipv6/ip6_gre.c
+++ b/net/ipv6/ip6_gre.c
@@ -508,11 +508,11 @@ static int ip6gre_rcv(struct sk_buff *skb)
 
 		skb->protocol = gre_proto;
 		/* WCCP version 1 and 2 protocol decoding.
-		 * - Change protocol to IP
+		 * - Change protocol to IPv6
 		 * - When dealing with WCCPv2, Skip extra 4 bytes in GRE header
 		 */
 		if (flags == 0 && gre_proto == htons(ETH_P_WCCP)) {
-			skb->protocol = htons(ETH_P_IP);
+			skb->protocol = htons(ETH_P_IPV6);
 			if ((*(h + offset) & 0xF0) != 0x40)
 				offset += 4;
 		}
diff --git a/net/ipv6/ip6_vti.c b/net/ipv6/ip6_vti.c
index 9a5339f..28456c9 100644
--- a/net/ipv6/ip6_vti.c
+++ b/net/ipv6/ip6_vti.c
@@ -825,6 +825,15 @@ static int vti6_newlink(struct net *src_net, struct net_device *dev,
 	return vti6_tnl_create2(dev);
 }
 
+static void vti6_dellink(struct net_device *dev, struct list_head *head)
+{
+	struct net *net = dev_net(dev);
+	struct vti6_net *ip6n = net_generic(net, vti6_net_id);
+
+	if (dev != ip6n->fb_tnl_dev)
+		unregister_netdevice_queue(dev, head);
+}
+
 static int vti6_changelink(struct net_device *dev, struct nlattr *tb[],
 			   struct nlattr *data[])
 {
@@ -900,6 +909,7 @@ static struct rtnl_link_ops vti6_link_ops __read_mostly = {
 	.setup		= vti6_dev_setup,
 	.validate	= vti6_validate,
 	.newlink	= vti6_newlink,
+	.dellink	= vti6_dellink,
 	.changelink	= vti6_changelink,
 	.get_size	= vti6_get_size,
 	.fill_info	= vti6_fill_info,
@@ -945,6 +955,7 @@ static int __net_init vti6_init_net(struct net *net)
 	if (!ip6n->fb_tnl_dev)
 		goto err_alloc_dev;
 	dev_net_set(ip6n->fb_tnl_dev, net);
+	ip6n->fb_tnl_dev->rtnl_link_ops = &vti6_link_ops;
 
 	err = vti6_fb_tnl_dev_init(ip6n->fb_tnl_dev);
 	if (err < 0)
diff --git a/net/mac80211/aes_ccm.c b/net/mac80211/aes_ccm.c
index 7c7df47..f056f9ed 100644
--- a/net/mac80211/aes_ccm.c
+++ b/net/mac80211/aes_ccm.c
@@ -54,6 +54,9 @@ int ieee80211_aes_ccm_decrypt(struct crypto_aead *tfm, u8 *b_0, u8 *aad,
 
 	memset(&aead_req, 0, sizeof(aead_req));
 
+	if (data_len == 0)
+		return -EINVAL;
+
 	sg_init_one(&pt, data, data_len);
 	sg_init_one(&assoc, &aad[2], be16_to_cpup((__be16 *)aad));
 	sg_init_table(ct, 2);
diff --git a/net/sctp/output.c b/net/sctp/output.c
index 8267b06..740ca5f 100644
--- a/net/sctp/output.c
+++ b/net/sctp/output.c
@@ -401,12 +401,12 @@ int sctp_packet_transmit(struct sctp_packet *packet)
 	sk = chunk->skb->sk;
 
 	/* Allocate the new skb.  */
-	nskb = alloc_skb(packet->size + LL_MAX_HEADER, GFP_ATOMIC);
+	nskb = alloc_skb(packet->size + MAX_HEADER, GFP_ATOMIC);
 	if (!nskb)
 		goto nomem;
 
 	/* Make sure the outbound skb has enough header room reserved. */
-	skb_reserve(nskb, packet->overhead + LL_MAX_HEADER);
+	skb_reserve(nskb, packet->overhead + MAX_HEADER);
 
 	/* Set the owning socket so that we know where to get the
 	 * destination IP address.
diff --git a/sound/pci/hda/patch_analog.c b/sound/pci/hda/patch_analog.c
index eaf64ea..1a05efa 100644
--- a/sound/pci/hda/patch_analog.c
+++ b/sound/pci/hda/patch_analog.c
@@ -333,6 +333,7 @@ static const struct hda_fixup ad1986a_fixups[] = {
 
 static const struct snd_pci_quirk ad1986a_fixup_tbl[] = {
 	SND_PCI_QUIRK(0x103c, 0x30af, "HP B2800", AD1986A_FIXUP_LAPTOP_IMIC),
+	SND_PCI_QUIRK(0x1043, 0x1443, "ASUS Z99He", AD1986A_FIXUP_EAPD),
 	SND_PCI_QUIRK(0x1043, 0x1447, "ASUS A8JN", AD1986A_FIXUP_EAPD),
 	SND_PCI_QUIRK_MASK(0x1043, 0xff00, 0x8100, "ASUS P5", AD1986A_FIXUP_3STACK),
 	SND_PCI_QUIRK_MASK(0x1043, 0xff00, 0x8200, "ASUS M2", AD1986A_FIXUP_3STACK),
diff --git a/sound/pci/hda/patch_realtek.c b/sound/pci/hda/patch_realtek.c
index 4c826a4..910f2db 100644
--- a/sound/pci/hda/patch_realtek.c
+++ b/sound/pci/hda/patch_realtek.c
@@ -4554,6 +4554,7 @@ static const struct snd_pci_quirk alc269_fixup_tbl[] = {
 	SND_PCI_QUIRK(0x17aa, 0x2212, "Thinkpad", ALC269_FIXUP_LIMIT_INT_MIC_BOOST),
 	SND_PCI_QUIRK(0x17aa, 0x2214, "Thinkpad", ALC269_FIXUP_LIMIT_INT_MIC_BOOST),
 	SND_PCI_QUIRK(0x17aa, 0x2215, "Thinkpad", ALC269_FIXUP_LIMIT_INT_MIC_BOOST),
+	SND_PCI_QUIRK(0x17aa, 0x3977, "IdeaPad S210", ALC283_FIXUP_INT_MIC),
 	SND_PCI_QUIRK(0x17aa, 0x3978, "IdeaPad Y410P", ALC269_FIXUP_NO_SHUTUP),
 	SND_PCI_QUIRK(0x17aa, 0x5013, "Thinkpad", ALC269_FIXUP_LIMIT_INT_MIC_BOOST),
 	SND_PCI_QUIRK(0x17aa, 0x501a, "Thinkpad", ALC283_FIXUP_INT_MIC),
diff --git a/sound/usb/midi.c b/sound/usb/midi.c
index b901f46..c7aa71e 100644
--- a/sound/usb/midi.c
+++ b/sound/usb/midi.c
@@ -364,6 +364,8 @@ static void snd_usbmidi_error_timer(unsigned long data)
 		if (in && in->error_resubmit) {
 			in->error_resubmit = 0;
 			for (j = 0; j < INPUT_URBS; ++j) {
+				if (atomic_read(&in->urbs[j]->use_count))
+					continue;
 				in->urbs[j]->dev = umidi->dev;
 				snd_usbmidi_submit_urb(in->urbs[j], GFP_ATOMIC);
 			}
