diff --git a/Makefile b/Makefile
index b0963ca..5443481 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 14
-SUBLEVEL = 33
+SUBLEVEL = 34
 EXTRAVERSION =
 NAME = Remembering Coco
 
diff --git a/drivers/media/rc/ir-lirc-codec.c b/drivers/media/rc/ir-lirc-codec.c
index ed2c8a1..98893a8 100644
--- a/drivers/media/rc/ir-lirc-codec.c
+++ b/drivers/media/rc/ir-lirc-codec.c
@@ -42,11 +42,17 @@ static int ir_lirc_decode(struct rc_dev *dev, struct ir_raw_event ev)
 		return -EINVAL;
 
 	/* Packet start */
-	if (ev.reset)
-		return 0;
+	if (ev.reset) {
+		/* Userspace expects a long space event before the start of
+		 * the signal to use as a sync.  This may be done with repeat
+		 * packets and normal samples.  But if a reset has been sent
+		 * then we assume that a long time has passed, so we send a
+		 * space with the maximum time value. */
+		sample = LIRC_SPACE(LIRC_VALUE_MASK);
+		IR_dprintk(2, "delivering reset sync space to lirc_dev\n");
 
 	/* Carrier reports */
-	if (ev.carrier_report) {
+	} else if (ev.carrier_report) {
 		sample = LIRC_FREQUENCY(ev.carrier);
 		IR_dprintk(2, "carrier report (freq: %d)\n", sample);
 
diff --git a/drivers/net/ethernet/broadcom/bnx2x/bnx2x_cmn.c b/drivers/net/ethernet/broadcom/bnx2x/bnx2x_cmn.c
index afa4a1f..a830d42 100644
--- a/drivers/net/ethernet/broadcom/bnx2x/bnx2x_cmn.c
+++ b/drivers/net/ethernet/broadcom/bnx2x/bnx2x_cmn.c
@@ -3131,7 +3131,7 @@ static int bnx2x_poll(struct napi_struct *napi, int budget)
 		}
 #endif
 		if (!bnx2x_fp_lock_napi(fp))
-			return work_done;
+			return budget;
 
 		for_each_cos_in_tx_queue(fp, cos)
 			if (bnx2x_tx_queue_has_work(fp->txdata_ptr[cos]))
diff --git a/drivers/net/ethernet/qlogic/netxen/netxen_nic_main.c b/drivers/net/ethernet/qlogic/netxen/netxen_nic_main.c
index 70849de..5fa076f 100644
--- a/drivers/net/ethernet/qlogic/netxen/netxen_nic_main.c
+++ b/drivers/net/ethernet/qlogic/netxen/netxen_nic_main.c
@@ -2390,7 +2390,10 @@ static int netxen_nic_poll(struct napi_struct *napi, int budget)
 
 	work_done = netxen_process_rcv_ring(sds_ring, budget);
 
-	if ((work_done < budget) && tx_complete) {
+	if (!tx_complete)
+		work_done = budget;
+
+	if (work_done < budget) {
 		napi_complete(&sds_ring->napi);
 		if (test_bit(__NX_DEV_UP, &adapter->state))
 			netxen_nic_enable_int(sds_ring);
diff --git a/drivers/net/ppp/ppp_deflate.c b/drivers/net/ppp/ppp_deflate.c
index 602c625..b5edc7f 100644
--- a/drivers/net/ppp/ppp_deflate.c
+++ b/drivers/net/ppp/ppp_deflate.c
@@ -246,7 +246,7 @@ static int z_compress(void *arg, unsigned char *rptr, unsigned char *obuf,
 	/*
 	 * See if we managed to reduce the size of the packet.
 	 */
-	if (olen < isize) {
+	if (olen < isize && olen <= osize) {
 		state->stats.comp_bytes += olen;
 		state->stats.comp_packets++;
 	} else {
diff --git a/include/net/ip.h b/include/net/ip.h
index 937f196..3446cdd 100644
--- a/include/net/ip.h
+++ b/include/net/ip.h
@@ -38,11 +38,12 @@ struct inet_skb_parm {
 	struct ip_options	opt;		/* Compiled IP options		*/
 	unsigned char		flags;
 
-#define IPSKB_FORWARDED		1
-#define IPSKB_XFRM_TUNNEL_SIZE	2
-#define IPSKB_XFRM_TRANSFORMED	4
-#define IPSKB_FRAG_COMPLETE	8
-#define IPSKB_REROUTED		16
+#define IPSKB_FORWARDED		BIT(0)
+#define IPSKB_XFRM_TUNNEL_SIZE	BIT(1)
+#define IPSKB_XFRM_TRANSFORMED	BIT(2)
+#define IPSKB_FRAG_COMPLETE	BIT(3)
+#define IPSKB_REROUTED		BIT(4)
+#define IPSKB_DOREDIRECT	BIT(5)
 
 	u16			frag_max_size;
 };
@@ -174,7 +175,7 @@ static inline __u8 ip_reply_arg_flowi_flags(const struct ip_reply_arg *arg)
 	return (arg->flags & IP_REPLY_ARG_NOSRCCHECK) ? FLOWI_FLAG_ANYSRC : 0;
 }
 
-void ip_send_unicast_reply(struct net *net, struct sk_buff *skb, __be32 daddr,
+void ip_send_unicast_reply(struct sock *sk, struct sk_buff *skb, __be32 daddr,
 			   __be32 saddr, const struct ip_reply_arg *arg,
 			   unsigned int len);
 
diff --git a/include/net/netns/ipv4.h b/include/net/netns/ipv4.h
index 80f500a..57c2da9 100644
--- a/include/net/netns/ipv4.h
+++ b/include/net/netns/ipv4.h
@@ -47,6 +47,7 @@ struct netns_ipv4 {
 	struct inet_peer_base	*peers;
 	struct tcpm_hash_bucket	*tcp_metrics_hash;
 	unsigned int		tcp_metrics_hash_log;
+	struct sock  * __percpu	*tcp_sk;
 	struct netns_frags	frags;
 #ifdef CONFIG_NETFILTER
 	struct xt_table		*iptable_filter;
diff --git a/net/core/dev.c b/net/core/dev.c
index 86bb9cc..4ed77d7 100644
--- a/net/core/dev.c
+++ b/net/core/dev.c
@@ -6812,10 +6812,20 @@ static int dev_cpu_callback(struct notifier_block *nfb,
 		oldsd->output_queue = NULL;
 		oldsd->output_queue_tailp = &oldsd->output_queue;
 	}
-	/* Append NAPI poll list from offline CPU. */
-	if (!list_empty(&oldsd->poll_list)) {
-		list_splice_init(&oldsd->poll_list, &sd->poll_list);
-		raise_softirq_irqoff(NET_RX_SOFTIRQ);
+	/* Append NAPI poll list from offline CPU, with one exception :
+	 * process_backlog() must be called by cpu owning percpu backlog.
+	 * We properly handle process_queue & input_pkt_queue later.
+	 */
+	while (!list_empty(&oldsd->poll_list)) {
+		struct napi_struct *napi = list_first_entry(&oldsd->poll_list,
+							    struct napi_struct,
+							    poll_list);
+
+		list_del_init(&napi->poll_list);
+		if (napi->poll == process_backlog)
+			napi->state = 0;
+		else
+			____napi_schedule(sd, napi);
 	}
 
 	raise_softirq_irqoff(NET_TX_SOFTIRQ);
@@ -6826,7 +6836,7 @@ static int dev_cpu_callback(struct notifier_block *nfb,
 		netif_rx_internal(skb);
 		input_queue_head_incr(oldsd);
 	}
-	while ((skb = __skb_dequeue(&oldsd->input_pkt_queue))) {
+	while ((skb = skb_dequeue(&oldsd->input_pkt_queue))) {
 		netif_rx_internal(skb);
 		input_queue_head_incr(oldsd);
 	}
diff --git a/net/core/rtnetlink.c b/net/core/rtnetlink.c
index 4617586..a6613ff 100644
--- a/net/core/rtnetlink.c
+++ b/net/core/rtnetlink.c
@@ -2649,12 +2649,16 @@ static int rtnl_bridge_notify(struct net_device *dev, u16 flags)
 			goto errout;
 	}
 
+	if (!skb->len)
+		goto errout;
+
 	rtnl_notify(skb, net, 0, RTNLGRP_LINK, NULL, GFP_ATOMIC);
 	return 0;
 errout:
 	WARN_ON(err == -EMSGSIZE);
 	kfree_skb(skb);
-	rtnl_set_sk_err(net, RTNLGRP_LINK, err);
+	if (err)
+		rtnl_set_sk_err(net, RTNLGRP_LINK, err);
 	return err;
 }
 
diff --git a/net/ipv4/ip_forward.c b/net/ipv4/ip_forward.c
index 1c6bd43..ecb34b5 100644
--- a/net/ipv4/ip_forward.c
+++ b/net/ipv4/ip_forward.c
@@ -178,7 +178,8 @@ int ip_forward(struct sk_buff *skb)
 	 *	We now generate an ICMP HOST REDIRECT giving the route
 	 *	we calculated.
 	 */
-	if (rt->rt_flags&RTCF_DOREDIRECT && !opt->srr && !skb_sec_path(skb))
+	if (IPCB(skb)->flags & IPSKB_DOREDIRECT && !opt->srr &&
+	    !skb_sec_path(skb))
 		ip_rt_send_redirect(skb);
 
 	skb->priority = rt_tos2priority(iph->tos);
diff --git a/net/ipv4/ip_output.c b/net/ipv4/ip_output.c
index 844323b..dd637fc 100644
--- a/net/ipv4/ip_output.c
+++ b/net/ipv4/ip_output.c
@@ -1460,23 +1460,8 @@ static int ip_reply_glue_bits(void *dptr, char *to, int offset,
 /*
  *	Generic function to send a packet as reply to another packet.
  *	Used to send some TCP resets/acks so far.
- *
- *	Use a fake percpu inet socket to avoid false sharing and contention.
  */
-static DEFINE_PER_CPU(struct inet_sock, unicast_sock) = {
-	.sk = {
-		.__sk_common = {
-			.skc_refcnt = ATOMIC_INIT(1),
-		},
-		.sk_wmem_alloc	= ATOMIC_INIT(1),
-		.sk_allocation	= GFP_ATOMIC,
-		.sk_flags	= (1UL << SOCK_USE_WRITE_QUEUE),
-	},
-	.pmtudisc	= IP_PMTUDISC_WANT,
-	.uc_ttl		= -1,
-};
-
-void ip_send_unicast_reply(struct net *net, struct sk_buff *skb, __be32 daddr,
+void ip_send_unicast_reply(struct sock *sk, struct sk_buff *skb, __be32 daddr,
 			   __be32 saddr, const struct ip_reply_arg *arg,
 			   unsigned int len)
 {
@@ -1484,9 +1469,8 @@ void ip_send_unicast_reply(struct net *net, struct sk_buff *skb, __be32 daddr,
 	struct ipcm_cookie ipc;
 	struct flowi4 fl4;
 	struct rtable *rt = skb_rtable(skb);
+	struct net *net = sock_net(sk);
 	struct sk_buff *nskb;
-	struct sock *sk;
-	struct inet_sock *inet;
 	int err;
 
 	if (ip_options_echo(&replyopts.opt.opt, skb))
@@ -1516,15 +1500,11 @@ void ip_send_unicast_reply(struct net *net, struct sk_buff *skb, __be32 daddr,
 	if (IS_ERR(rt))
 		return;
 
-	inet = &get_cpu_var(unicast_sock);
+	inet_sk(sk)->tos = arg->tos;
 
-	inet->tos = arg->tos;
-	sk = &inet->sk;
 	sk->sk_priority = skb->priority;
 	sk->sk_protocol = ip_hdr(skb)->protocol;
 	sk->sk_bound_dev_if = arg->bound_dev_if;
-	sock_net_set(sk, net);
-	__skb_queue_head_init(&sk->sk_write_queue);
 	sk->sk_sndbuf = sysctl_wmem_default;
 	err = ip_append_data(sk, &fl4, ip_reply_glue_bits, arg->iov->iov_base,
 			     len, 0, &ipc, &rt, MSG_DONTWAIT);
@@ -1540,13 +1520,10 @@ void ip_send_unicast_reply(struct net *net, struct sk_buff *skb, __be32 daddr,
 			  arg->csumoffset) = csum_fold(csum_add(nskb->csum,
 								arg->csum));
 		nskb->ip_summed = CHECKSUM_NONE;
-		skb_orphan(nskb);
 		skb_set_queue_mapping(nskb, skb_get_queue_mapping(skb));
 		ip_push_pending_frames(sk, &fl4);
 	}
 out:
-	put_cpu_var(unicast_sock);
-
 	ip_rt_put(rt);
 }
 
diff --git a/net/ipv4/ip_sockglue.c b/net/ipv4/ip_sockglue.c
index 580dd96..135045e 100644
--- a/net/ipv4/ip_sockglue.c
+++ b/net/ipv4/ip_sockglue.c
@@ -426,15 +426,11 @@ int ip_recv_error(struct sock *sk, struct msghdr *msg, int len, int *addr_len)
 
 	memcpy(&errhdr.ee, &serr->ee, sizeof(struct sock_extended_err));
 	sin = &errhdr.offender;
-	sin->sin_family = AF_UNSPEC;
+	memset(sin, 0, sizeof(*sin));
 	if (serr->ee.ee_origin == SO_EE_ORIGIN_ICMP) {
-		struct inet_sock *inet = inet_sk(sk);
-
 		sin->sin_family = AF_INET;
 		sin->sin_addr.s_addr = ip_hdr(skb)->saddr;
-		sin->sin_port = 0;
-		memset(&sin->sin_zero, 0, sizeof(sin->sin_zero));
-		if (inet->cmsg_flags)
+		if (inet_sk(sk)->cmsg_flags)
 			ip_cmsg_recv(msg, skb);
 	}
 
diff --git a/net/ipv4/ping.c b/net/ipv4/ping.c
index 0d33f94..04ce671 100644
--- a/net/ipv4/ping.c
+++ b/net/ipv4/ping.c
@@ -973,8 +973,11 @@ void ping_rcv(struct sk_buff *skb)
 
 	sk = ping_lookup(net, skb, ntohs(icmph->un.echo.id));
 	if (sk != NULL) {
+		struct sk_buff *skb2 = skb_clone(skb, GFP_ATOMIC);
+
 		pr_debug("rcv on socket %p\n", sk);
-		ping_queue_rcv_skb(sk, skb_get(skb));
+		if (skb2)
+			ping_queue_rcv_skb(sk, skb2);
 		sock_put(sk);
 		return;
 	}
diff --git a/net/ipv4/route.c b/net/ipv4/route.c
index 487bb62..b64330f 100644
--- a/net/ipv4/route.c
+++ b/net/ipv4/route.c
@@ -1554,11 +1554,10 @@ static int __mkroute_input(struct sk_buff *skb,
 
 	do_cache = res->fi && !itag;
 	if (out_dev == in_dev && err && IN_DEV_TX_REDIRECTS(out_dev) &&
+	    skb->protocol == htons(ETH_P_IP) &&
 	    (IN_DEV_SHARED_MEDIA(out_dev) ||
-	     inet_addr_onlink(out_dev, saddr, FIB_RES_GW(*res)))) {
-		flags |= RTCF_DOREDIRECT;
-		do_cache = false;
-	}
+	     inet_addr_onlink(out_dev, saddr, FIB_RES_GW(*res))))
+		IPCB(skb)->flags |= IPSKB_DOREDIRECT;
 
 	if (skb->protocol != htons(ETH_P_IP)) {
 		/* Not IP (i.e. ARP). Do not create route, if it is
@@ -2305,6 +2304,8 @@ static int rt_fill_info(struct net *net,  __be32 dst, __be32 src,
 	r->rtm_flags	= (rt->rt_flags & ~0xFFFF) | RTM_F_CLONED;
 	if (rt->rt_flags & RTCF_NOTIFY)
 		r->rtm_flags |= RTM_F_NOTIFY;
+	if (IPCB(skb)->flags & IPSKB_DOREDIRECT)
+		r->rtm_flags |= RTCF_DOREDIRECT;
 
 	if (nla_put_be32(skb, RTA_DST, dst))
 		goto nla_put_failure;
diff --git a/net/ipv4/tcp_ipv4.c b/net/ipv4/tcp_ipv4.c
index a782d5b..b7effad 100644
--- a/net/ipv4/tcp_ipv4.c
+++ b/net/ipv4/tcp_ipv4.c
@@ -691,7 +691,8 @@ static void tcp_v4_send_reset(struct sock *sk, struct sk_buff *skb)
 
 	net = dev_net(skb_dst(skb)->dev);
 	arg.tos = ip_hdr(skb)->tos;
-	ip_send_unicast_reply(net, skb, ip_hdr(skb)->saddr,
+	ip_send_unicast_reply(*this_cpu_ptr(net->ipv4.tcp_sk),
+			      skb, ip_hdr(skb)->saddr,
 			      ip_hdr(skb)->daddr, &arg, arg.iov[0].iov_len);
 
 	TCP_INC_STATS_BH(net, TCP_MIB_OUTSEGS);
@@ -774,7 +775,8 @@ static void tcp_v4_send_ack(struct sk_buff *skb, u32 seq, u32 ack,
 	if (oif)
 		arg.bound_dev_if = oif;
 	arg.tos = tos;
-	ip_send_unicast_reply(net, skb, ip_hdr(skb)->saddr,
+	ip_send_unicast_reply(*this_cpu_ptr(net->ipv4.tcp_sk),
+			      skb, ip_hdr(skb)->saddr,
 			      ip_hdr(skb)->daddr, &arg, arg.iov[0].iov_len);
 
 	TCP_INC_STATS_BH(net, TCP_MIB_OUTSEGS);
@@ -2769,14 +2771,39 @@ struct proto tcp_prot = {
 };
 EXPORT_SYMBOL(tcp_prot);
 
+static void __net_exit tcp_sk_exit(struct net *net)
+{
+	int cpu;
+
+	for_each_possible_cpu(cpu)
+		inet_ctl_sock_destroy(*per_cpu_ptr(net->ipv4.tcp_sk, cpu));
+	free_percpu(net->ipv4.tcp_sk);
+}
+
 static int __net_init tcp_sk_init(struct net *net)
 {
+	int res, cpu;
+
+	net->ipv4.tcp_sk = alloc_percpu(struct sock *);
+	if (!net->ipv4.tcp_sk)
+		return -ENOMEM;
+
+	for_each_possible_cpu(cpu) {
+		struct sock *sk;
+
+		res = inet_ctl_sock_create(&sk, PF_INET, SOCK_RAW,
+					   IPPROTO_TCP, net);
+		if (res)
+			goto fail;
+		*per_cpu_ptr(net->ipv4.tcp_sk, cpu) = sk;
+	}
 	net->ipv4.sysctl_tcp_ecn = 2;
 	return 0;
-}
 
-static void __net_exit tcp_sk_exit(struct net *net)
-{
+fail:
+	tcp_sk_exit(net);
+
+	return res;
 }
 
 static void __net_exit tcp_sk_exit_batch(struct list_head *net_exit_list)
diff --git a/net/ipv4/udp_diag.c b/net/ipv4/udp_diag.c
index 7927db0..4a000f1 100644
--- a/net/ipv4/udp_diag.c
+++ b/net/ipv4/udp_diag.c
@@ -99,11 +99,13 @@ static void udp_dump(struct udp_table *table, struct sk_buff *skb, struct netlin
 	s_slot = cb->args[0];
 	num = s_num = cb->args[1];
 
-	for (slot = s_slot; slot <= table->mask; num = s_num = 0, slot++) {
+	for (slot = s_slot; slot <= table->mask; s_num = 0, slot++) {
 		struct sock *sk;
 		struct hlist_nulls_node *node;
 		struct udp_hslot *hslot = &table->hash[slot];
 
+		num = 0;
+
 		if (hlist_nulls_empty(&hslot->head))
 			continue;
 
diff --git a/net/ipv6/datagram.c b/net/ipv6/datagram.c
index c3bf2d2..841cfa2 100644
--- a/net/ipv6/datagram.c
+++ b/net/ipv6/datagram.c
@@ -382,11 +382,10 @@ int ipv6_recv_error(struct sock *sk, struct msghdr *msg, int len, int *addr_len)
 
 	memcpy(&errhdr.ee, &serr->ee, sizeof(struct sock_extended_err));
 	sin = &errhdr.offender;
-	sin->sin6_family = AF_UNSPEC;
+	memset(sin, 0, sizeof(*sin));
+
 	if (serr->ee.ee_origin != SO_EE_ORIGIN_LOCAL) {
 		sin->sin6_family = AF_INET6;
-		sin->sin6_flowinfo = 0;
-		sin->sin6_port = 0;
 		if (np->rxopt.all)
 			ip6_datagram_recv_common_ctl(sk, msg, skb);
 		if (skb->protocol == htons(ETH_P_IPV6)) {
@@ -397,12 +396,9 @@ int ipv6_recv_error(struct sock *sk, struct msghdr *msg, int len, int *addr_len)
 				ipv6_iface_scope_id(&sin->sin6_addr,
 						    IP6CB(skb)->iif);
 		} else {
-			struct inet_sock *inet = inet_sk(sk);
-
 			ipv6_addr_set_v4mapped(ip_hdr(skb)->saddr,
 					       &sin->sin6_addr);
-			sin->sin6_scope_id = 0;
-			if (inet->cmsg_flags)
+			if (inet_sk(sk)->cmsg_flags)
 				ip_cmsg_recv(msg, skb);
 		}
 	}
diff --git a/net/ipv6/ip6_fib.c b/net/ipv6/ip6_fib.c
index 1e55f5e..7daaeaf 100644
--- a/net/ipv6/ip6_fib.c
+++ b/net/ipv6/ip6_fib.c
@@ -638,6 +638,29 @@ static inline bool rt6_qualify_for_ecmp(struct rt6_info *rt)
 	       RTF_GATEWAY;
 }
 
+static void fib6_purge_rt(struct rt6_info *rt, struct fib6_node *fn,
+			  struct net *net)
+{
+	if (atomic_read(&rt->rt6i_ref) != 1) {
+		/* This route is used as dummy address holder in some split
+		 * nodes. It is not leaked, but it still holds other resources,
+		 * which must be released in time. So, scan ascendant nodes
+		 * and replace dummy references to this route with references
+		 * to still alive ones.
+		 */
+		while (fn) {
+			if (!(fn->fn_flags & RTN_RTINFO) && fn->leaf == rt) {
+				fn->leaf = fib6_find_prefix(net, fn);
+				atomic_inc(&fn->leaf->rt6i_ref);
+				rt6_release(rt);
+			}
+			fn = fn->parent;
+		}
+		/* No more references are possible at this point. */
+		BUG_ON(atomic_read(&rt->rt6i_ref) != 1);
+	}
+}
+
 /*
  *	Insert routing information in a node.
  */
@@ -775,11 +798,12 @@ add:
 		rt->dst.rt6_next = iter->dst.rt6_next;
 		atomic_inc(&rt->rt6i_ref);
 		inet6_rt_notify(RTM_NEWROUTE, rt, info);
-		rt6_release(iter);
 		if (!(fn->fn_flags & RTN_RTINFO)) {
 			info->nl_net->ipv6.rt6_stats->fib_route_nodes++;
 			fn->fn_flags |= RTN_RTINFO;
 		}
+		fib6_purge_rt(iter, fn, info->nl_net);
+		rt6_release(iter);
 	}
 
 	return 0;
@@ -1284,24 +1308,7 @@ static void fib6_del_route(struct fib6_node *fn, struct rt6_info **rtp,
 		fn = fib6_repair_tree(net, fn);
 	}
 
-	if (atomic_read(&rt->rt6i_ref) != 1) {
-		/* This route is used as dummy address holder in some split
-		 * nodes. It is not leaked, but it still holds other resources,
-		 * which must be released in time. So, scan ascendant nodes
-		 * and replace dummy references to this route with references
-		 * to still alive ones.
-		 */
-		while (fn) {
-			if (!(fn->fn_flags & RTN_RTINFO) && fn->leaf == rt) {
-				fn->leaf = fib6_find_prefix(net, fn);
-				atomic_inc(&fn->leaf->rt6i_ref);
-				rt6_release(rt);
-			}
-			fn = fn->parent;
-		}
-		/* No more references are possible at this point. */
-		BUG_ON(atomic_read(&rt->rt6i_ref) != 1);
-	}
+	fib6_purge_rt(rt, fn, net);
 
 	inet6_rt_notify(RTM_DELROUTE, rt, info);
 	rt6_release(rt);
diff --git a/net/ipv6/route.c b/net/ipv6/route.c
index 7cc1102..6f1b850 100644
--- a/net/ipv6/route.c
+++ b/net/ipv6/route.c
@@ -1160,12 +1160,9 @@ static void ip6_rt_update_pmtu(struct dst_entry *dst, struct sock *sk,
 		struct net *net = dev_net(dst->dev);
 
 		rt6->rt6i_flags |= RTF_MODIFIED;
-		if (mtu < IPV6_MIN_MTU) {
-			u32 features = dst_metric(dst, RTAX_FEATURES);
+		if (mtu < IPV6_MIN_MTU)
 			mtu = IPV6_MIN_MTU;
-			features |= RTAX_FEATURE_ALLFRAG;
-			dst_metric_set(dst, RTAX_FEATURES, features);
-		}
+
 		dst_metric_set(dst, RTAX_MTU, mtu);
 		rt6_update_expires(rt6, net->ipv6.sysctl.ip6_rt_mtu_expires);
 	}
diff --git a/net/sctp/associola.c b/net/sctp/associola.c
index d477d47..abc0922 100644
--- a/net/sctp/associola.c
+++ b/net/sctp/associola.c
@@ -1235,7 +1235,6 @@ void sctp_assoc_update(struct sctp_association *asoc,
 	asoc->peer.peer_hmacs = new->peer.peer_hmacs;
 	new->peer.peer_hmacs = NULL;
 
-	sctp_auth_key_put(asoc->asoc_shared_key);
 	sctp_auth_asoc_init_active_key(asoc, GFP_ATOMIC);
 }
 
diff --git a/net/sctp/sm_make_chunk.c b/net/sctp/sm_make_chunk.c
index 43abb64..df06b13 100644
--- a/net/sctp/sm_make_chunk.c
+++ b/net/sctp/sm_make_chunk.c
@@ -2608,7 +2608,7 @@ do_addr_param:
 
 		addr_param = param.v + sizeof(sctp_addip_param_t);
 
-		af = sctp_get_af_specific(param_type2af(param.p->type));
+		af = sctp_get_af_specific(param_type2af(addr_param->p.type));
 		if (af == NULL)
 			break;
 
diff --git a/net/socket.c b/net/socket.c
index a19ae19..1b2c2d6 100644
--- a/net/socket.c
+++ b/net/socket.c
@@ -886,9 +886,6 @@ static ssize_t sock_splice_read(struct file *file, loff_t *ppos,
 static struct sock_iocb *alloc_sock_iocb(struct kiocb *iocb,
 					 struct sock_iocb *siocb)
 {
-	if (!is_sync_kiocb(iocb))
-		BUG();
-
 	siocb->kiocb = iocb;
 	iocb->private = siocb;
 	return siocb;
