From 0f9d760243da06c2a0d258e30033a8c980baf1fc Mon Sep 17 00:00:00 2001
From: Stephan Raue <stephan@openelec.tv>
Date: Mon, 1 Sep 2014 03:16:37 +0200
Subject: [PATCH 11/12] add support to read frequency output if using intel's
 pstate driver

---
 xbmc/utils/CPUInfo.cpp | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/xbmc/utils/CPUInfo.cpp b/xbmc/utils/CPUInfo.cpp
index 7c5b9f8..0536036 100644
--- a/xbmc/utils/CPUInfo.cpp
+++ b/xbmc/utils/CPUInfo.cpp
@@ -269,6 +269,8 @@ CCPUInfo::CCPUInfo(void)
     m_fProcTemperature = fopen("/sys/class/thermal/thermal_zone0/temp", "r");  // On Raspberry PIs
 
   m_fCPUFreq = fopen ("/sys/devices/system/cpu/cpu0/cpufreq/scaling_cur_freq", "r");
+  if (m_fCPUFreq == NULL)
+    m_fCPUFreq = fopen ("/sys/devices/system/cpu/cpu0/cpufreq/cpuinfo_cur_freq", "r");
   if (!m_fCPUFreq)
   {
     m_cpuInfoForFreq = true;
-- 
2.1.4

