diff --git a/Documentation/ramoops.txt b/Documentation/ramoops.txt
index 69b3cac..5d86756 100644
--- a/Documentation/ramoops.txt
+++ b/Documentation/ramoops.txt
@@ -14,11 +14,19 @@ survive after a restart.
 
 1. Ramoops concepts
 
-Ramoops uses a predefined memory area to store the dump. The start and size of
-the memory area are set using two variables:
+Ramoops uses a predefined memory area to store the dump. The start and size
+and type of the memory area are set using three variables:
   * "mem_address" for the start
   * "mem_size" for the size. The memory size will be rounded down to a
   power of two.
+  * "mem_type" to specifiy if the memory type (default is pgprot_writecombine).
+
+Typically the default value of mem_type=0 should be used as that sets the pstore
+mapping to pgprot_writecombine. Setting mem_type=1 attempts to use
+pgprot_noncached, which only works on some platforms. This is because pstore
+depends on atomic operations. At least on ARM, pgprot_noncached causes the
+memory to be mapped strongly ordered, and atomic operations on strongly ordered
+memory are implementation defined, and won't work on many ARMs such as omaps.
 
 The memory area is divided into "record_size" chunks (also rounded down to
 power of two) and each oops/panic writes a "record_size" chunk of
@@ -55,6 +63,7 @@ Setting the ramoops parameters can be done in 2 different manners:
 static struct ramoops_platform_data ramoops_data = {
         .mem_size               = <...>,
         .mem_address            = <...>,
+        .mem_type               = <...>,
         .record_size            = <...>,
         .dump_oops              = <...>,
         .ecc                    = <...>,
diff --git a/Makefile b/Makefile
index a2e572b..7aff64e 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 14
-SUBLEVEL = 28
+SUBLEVEL = 29
 EXTRAVERSION =
 NAME = Remembering Coco
 
diff --git a/arch/arm/boot/dts/dra7.dtsi b/arch/arm/boot/dts/dra7.dtsi
index 767f0e3..f60aeee 100644
--- a/arch/arm/boot/dts/dra7.dtsi
+++ b/arch/arm/boot/dts/dra7.dtsi
@@ -458,7 +458,7 @@
 		};
 
 		wdt2: wdt@4ae14000 {
-			compatible = "ti,omap4-wdt";
+			compatible = "ti,omap3-wdt";
 			reg = <0x4ae14000 0x80>;
 			interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
 			ti,hwmods = "wd_timer2";
diff --git a/arch/arm/boot/dts/s3c6410-mini6410.dts b/arch/arm/boot/dts/s3c6410-mini6410.dts
index 57e00f9..a25debb 100644
--- a/arch/arm/boot/dts/s3c6410-mini6410.dts
+++ b/arch/arm/boot/dts/s3c6410-mini6410.dts
@@ -198,10 +198,6 @@
 	status = "okay";
 };
 
-&pwm {
-	status = "okay";
-};
-
 &pinctrl0 {
 	gpio_leds: gpio-leds {
 		samsung,pins = "gpk-4", "gpk-5", "gpk-6", "gpk-7";
diff --git a/arch/arm/boot/dts/s3c64xx.dtsi b/arch/arm/boot/dts/s3c64xx.dtsi
index 4e3be4d..4f1eff3 100644
--- a/arch/arm/boot/dts/s3c64xx.dtsi
+++ b/arch/arm/boot/dts/s3c64xx.dtsi
@@ -168,7 +168,6 @@
 			clocks = <&clocks PCLK_PWM>;
 			samsung,pwm-outputs = <0>, <1>;
 			#pwm-cells = <3>;
-			status = "disabled";
 		};
 
 		pinctrl0: pinctrl@7f008000 {
diff --git a/arch/arm/configs/multi_v7_defconfig b/arch/arm/configs/multi_v7_defconfig
index ee69829..cf4823b 100644
--- a/arch/arm/configs/multi_v7_defconfig
+++ b/arch/arm/configs/multi_v7_defconfig
@@ -235,6 +235,7 @@ CONFIG_SND_SOC_TEGRA_MAX98090=y
 CONFIG_USB=y
 CONFIG_USB_XHCI_HCD=y
 CONFIG_USB_EHCI_HCD=y
+CONFIG_USB_EHCI_EXYNOS=y
 CONFIG_USB_EHCI_TEGRA=y
 CONFIG_USB_EHCI_HCD_PLATFORM=y
 CONFIG_USB_ISP1760_HCD=y
diff --git a/arch/arm/kernel/setup.c b/arch/arm/kernel/setup.c
index 1e8b030..aab70f6 100644
--- a/arch/arm/kernel/setup.c
+++ b/arch/arm/kernel/setup.c
@@ -1021,6 +1021,15 @@ static int c_show(struct seq_file *m, void *v)
 		seq_printf(m, "model name\t: %s rev %d (%s)\n",
 			   cpu_name, cpuid & 15, elf_platform);
 
+#if defined(CONFIG_SMP)
+		seq_printf(m, "BogoMIPS\t: %lu.%02lu\n",
+			   per_cpu(cpu_data, i).loops_per_jiffy / (500000UL/HZ),
+			   (per_cpu(cpu_data, i).loops_per_jiffy / (5000UL/HZ)) % 100);
+#else
+		seq_printf(m, "BogoMIPS\t: %lu.%02lu\n",
+			   loops_per_jiffy / (500000/HZ),
+			   (loops_per_jiffy / (5000/HZ)) % 100);
+#endif
 		/* dump out the processor features */
 		seq_puts(m, "Features\t: ");
 
diff --git a/arch/arm/kernel/smp.c b/arch/arm/kernel/smp.c
index b7b4c86..8cd3724 100644
--- a/arch/arm/kernel/smp.c
+++ b/arch/arm/kernel/smp.c
@@ -388,8 +388,17 @@ asmlinkage void secondary_start_kernel(void)
 
 void __init smp_cpus_done(unsigned int max_cpus)
 {
-	printk(KERN_INFO "SMP: Total of %d processors activated.\n",
-	       num_online_cpus());
+	int cpu;
+	unsigned long bogosum = 0;
+
+	for_each_online_cpu(cpu)
+		bogosum += per_cpu(cpu_data, cpu).loops_per_jiffy;
+
+	printk(KERN_INFO "SMP: Total of %d processors activated "
+	       "(%lu.%02lu BogoMIPS).\n",
+	       num_online_cpus(),
+	       bogosum / (500000/HZ),
+	       (bogosum / (5000/HZ)) % 100);
 
 	hyp_mode_check();
 }
diff --git a/arch/arm/mach-mvebu/coherency.c b/arch/arm/mach-mvebu/coherency.c
index 4e9d581..c295c10 100644
--- a/arch/arm/mach-mvebu/coherency.c
+++ b/arch/arm/mach-mvebu/coherency.c
@@ -125,6 +125,29 @@ int __init coherency_init(void)
 {
 	struct device_node *np;
 
+	/*
+	 * The coherency fabric is needed:
+	 * - For coherency between processors on Armada XP, so only
+	 *   when SMP is enabled.
+	 * - For coherency between the processor and I/O devices, but
+	 *   this coherency requires many pre-requisites (write
+	 *   allocate cache policy, shareable pages, SMP bit set) that
+	 *   are only meant in SMP situations.
+	 *
+	 * Note that this means that on Armada 370, there is currently
+	 * no way to use hardware I/O coherency, because even when
+	 * CONFIG_SMP is enabled, is_smp() returns false due to the
+	 * Armada 370 being a single-core processor. To lift this
+	 * limitation, we would have to find a way to make the cache
+	 * policy set to write-allocate (on all Armada SoCs), and to
+	 * set the shareable attribute in page tables (on all Armada
+	 * SoCs except the Armada 370). Unfortunately, such decisions
+	 * are taken very early in the kernel boot process, at a point
+	 * where we don't know yet on which SoC we are running.
+	 */
+	if (!is_smp())
+		return 0;
+
 	np = of_find_matching_node(NULL, of_coherency_table);
 	if (np) {
 		struct resource res;
@@ -151,6 +174,9 @@ static int __init coherency_late_init(void)
 {
 	struct device_node *np;
 
+	if (!is_smp())
+		return 0;
+
 	np = of_find_matching_node(NULL, of_coherency_table);
 	if (np) {
 		bus_register_notifier(&platform_bus_type,
diff --git a/arch/arm/mach-omap2/pm44xx.c b/arch/arm/mach-omap2/pm44xx.c
index eefb30c..2b9cff9 100644
--- a/arch/arm/mach-omap2/pm44xx.c
+++ b/arch/arm/mach-omap2/pm44xx.c
@@ -148,26 +148,6 @@ static inline int omap4_init_static_deps(void)
 	struct clockdomain *ducati_clkdm, *l3_2_clkdm;
 	int ret = 0;
 
-	if (omap_rev() == OMAP4430_REV_ES1_0) {
-		WARN(1, "Power Management not supported on OMAP4430 ES1.0\n");
-		return -ENODEV;
-	}
-
-	pr_err("Power Management for TI OMAP4.\n");
-	/*
-	 * OMAP4 chip PM currently works only with certain (newer)
-	 * versions of bootloaders. This is due to missing code in the
-	 * kernel to properly reset and initialize some devices.
-	 * http://www.spinics.net/lists/arm-kernel/msg218641.html
-	 */
-	pr_warn("OMAP4 PM: u-boot >= v2012.07 is required for full PM support\n");
-
-	ret = pwrdm_for_each(pwrdms_setup, NULL);
-	if (ret) {
-		pr_err("Failed to setup powerdomains\n");
-		return ret;
-	}
-
 	/*
 	 * The dynamic dependency between MPUSS -> MEMIF and
 	 * MPUSS -> L4_PER/L3_* and DUCATI -> L3_* doesn't work as
@@ -231,6 +211,15 @@ int __init omap4_pm_init(void)
 
 	pr_info("Power Management for TI OMAP4+ devices.\n");
 
+	/*
+	 * OMAP4 chip PM currently works only with certain (newer)
+	 * versions of bootloaders. This is due to missing code in the
+	 * kernel to properly reset and initialize some devices.
+	 * http://www.spinics.net/lists/arm-kernel/msg218641.html
+	 */
+	if (cpu_is_omap44xx())
+		pr_warn("OMAP4 PM: u-boot >= v2012.07 is required for full PM support\n");
+
 	ret = pwrdm_for_each(pwrdms_setup, NULL);
 	if (ret) {
 		pr_err("Failed to setup powerdomains.\n");
diff --git a/arch/arm64/include/asm/suspend.h b/arch/arm64/include/asm/suspend.h
index e9c149c..456d67c 100644
--- a/arch/arm64/include/asm/suspend.h
+++ b/arch/arm64/include/asm/suspend.h
@@ -21,6 +21,7 @@ struct sleep_save_sp {
 	phys_addr_t save_ptr_stash_phys;
 };
 
+extern int __cpu_suspend(unsigned long arg, int (*fn)(unsigned long));
 extern void cpu_resume(void);
 extern int cpu_suspend(unsigned long);
 
diff --git a/arch/arm64/kernel/sleep.S b/arch/arm64/kernel/sleep.S
index b192572..ede186c 100644
--- a/arch/arm64/kernel/sleep.S
+++ b/arch/arm64/kernel/sleep.S
@@ -49,28 +49,39 @@
 	orr	\dst, \dst, \mask		// dst|=(aff3>>rs3)
 	.endm
 /*
- * Save CPU state for a suspend.  This saves callee registers, and allocates
- * space on the kernel stack to save the CPU specific registers + some
- * other data for resume.
+ * Save CPU state for a suspend and execute the suspend finisher.
+ * On success it will return 0 through cpu_resume - ie through a CPU
+ * soft/hard reboot from the reset vector.
+ * On failure it returns the suspend finisher return value or force
+ * -EOPNOTSUPP if the finisher erroneously returns 0 (the suspend finisher
+ * is not allowed to return, if it does this must be considered failure).
+ * It saves callee registers, and allocates space on the kernel stack
+ * to save the CPU specific registers + some other data for resume.
  *
  *  x0 = suspend finisher argument
+ *  x1 = suspend finisher function pointer
  */
-ENTRY(__cpu_suspend)
+ENTRY(__cpu_suspend_enter)
 	stp	x29, lr, [sp, #-96]!
 	stp	x19, x20, [sp,#16]
 	stp	x21, x22, [sp,#32]
 	stp	x23, x24, [sp,#48]
 	stp	x25, x26, [sp,#64]
 	stp	x27, x28, [sp,#80]
+	/*
+	 * Stash suspend finisher and its argument in x20 and x19
+	 */
+	mov	x19, x0
+	mov	x20, x1
 	mov	x2, sp
 	sub	sp, sp, #CPU_SUSPEND_SZ	// allocate cpu_suspend_ctx
-	mov	x1, sp
+	mov	x0, sp
 	/*
-	 * x1 now points to struct cpu_suspend_ctx allocated on the stack
+	 * x0 now points to struct cpu_suspend_ctx allocated on the stack
 	 */
-	str	x2, [x1, #CPU_CTX_SP]
-	ldr	x2, =sleep_save_sp
-	ldr	x2, [x2, #SLEEP_SAVE_SP_VIRT]
+	str	x2, [x0, #CPU_CTX_SP]
+	ldr	x1, =sleep_save_sp
+	ldr	x1, [x1, #SLEEP_SAVE_SP_VIRT]
 #ifdef CONFIG_SMP
 	mrs	x7, mpidr_el1
 	ldr	x9, =mpidr_hash
@@ -82,11 +93,21 @@ ENTRY(__cpu_suspend)
 	ldp	w3, w4, [x9, #MPIDR_HASH_SHIFTS]
 	ldp	w5, w6, [x9, #(MPIDR_HASH_SHIFTS + 8)]
 	compute_mpidr_hash x8, x3, x4, x5, x6, x7, x10
-	add	x2, x2, x8, lsl #3
+	add	x1, x1, x8, lsl #3
 #endif
-	bl	__cpu_suspend_finisher
+	bl	__cpu_suspend_save
+	/*
+	 * Grab suspend finisher in x20 and its argument in x19
+	 */
+	mov	x0, x19
+	mov	x1, x20
+	/*
+	 * We are ready for power down, fire off the suspend finisher
+	 * in x1, with argument in x0
+	 */
+	blr	x1
         /*
-	 * Never gets here, unless suspend fails.
+	 * Never gets here, unless suspend finisher fails.
 	 * Successful cpu_suspend should return from cpu_resume, returning
 	 * through this code path is considered an error
 	 * If the return value is set to 0 force x0 = -EOPNOTSUPP
@@ -103,7 +124,7 @@ ENTRY(__cpu_suspend)
 	ldp	x27, x28, [sp, #80]
 	ldp	x29, lr, [sp], #96
 	ret
-ENDPROC(__cpu_suspend)
+ENDPROC(__cpu_suspend_enter)
 	.ltorg
 
 /*
@@ -126,14 +147,12 @@ cpu_resume_after_mmu:
 	ret
 ENDPROC(cpu_resume_after_mmu)
 
-	.data
 ENTRY(cpu_resume)
 	bl	el2_setup		// if in EL2 drop to EL1 cleanly
 #ifdef CONFIG_SMP
 	mrs	x1, mpidr_el1
-	adr	x4, mpidr_hash_ptr
-	ldr	x5, [x4]
-	add	x8, x4, x5		// x8 = struct mpidr_hash phys address
+	adrp	x8, mpidr_hash
+	add x8, x8, #:lo12:mpidr_hash // x8 = struct mpidr_hash phys address
         /* retrieve mpidr_hash members to compute the hash */
 	ldr	x2, [x8, #MPIDR_HASH_MASK]
 	ldp	w3, w4, [x8, #MPIDR_HASH_SHIFTS]
@@ -143,14 +162,15 @@ ENTRY(cpu_resume)
 #else
 	mov	x7, xzr
 #endif
-	adr	x0, sleep_save_sp
+	adrp	x0, sleep_save_sp
+	add	x0, x0, #:lo12:sleep_save_sp
 	ldr	x0, [x0, #SLEEP_SAVE_SP_PHYS]
 	ldr	x0, [x0, x7, lsl #3]
 	/* load sp from context */
 	ldr	x2, [x0, #CPU_CTX_SP]
-	adr	x1, sleep_idmap_phys
+	adrp	x1, sleep_idmap_phys
 	/* load physical address of identity map page table in x1 */
-	ldr	x1, [x1]
+	ldr	x1, [x1, #:lo12:sleep_idmap_phys]
 	mov	sp, x2
 	/*
 	 * cpu_do_resume expects x0 to contain context physical address
@@ -159,26 +179,3 @@ ENTRY(cpu_resume)
 	bl	cpu_do_resume		// PC relative jump, MMU off
 	b	cpu_resume_mmu		// Resume MMU, never returns
 ENDPROC(cpu_resume)
-
-	.align 3
-mpidr_hash_ptr:
-	/*
-	 * offset of mpidr_hash symbol from current location
-	 * used to obtain run-time mpidr_hash address with MMU off
-         */
-	.quad	mpidr_hash - .
-/*
- * physical address of identity mapped page tables
- */
-	.type	sleep_idmap_phys, #object
-ENTRY(sleep_idmap_phys)
-	.quad	0
-/*
- * struct sleep_save_sp {
- *	phys_addr_t *save_ptr_stash;
- *	phys_addr_t save_ptr_stash_phys;
- * };
- */
-	.type	sleep_save_sp, #object
-ENTRY(sleep_save_sp)
-	.space	SLEEP_SAVE_SP_SZ	// struct sleep_save_sp
diff --git a/arch/arm64/kernel/suspend.c b/arch/arm64/kernel/suspend.c
index 1fa9ce4..2d6b606 100644
--- a/arch/arm64/kernel/suspend.c
+++ b/arch/arm64/kernel/suspend.c
@@ -5,26 +5,24 @@
 #include <asm/debug-monitors.h>
 #include <asm/pgtable.h>
 #include <asm/memory.h>
+#include <asm/mmu_context.h>
 #include <asm/smp_plat.h>
 #include <asm/suspend.h>
 #include <asm/tlbflush.h>
 
-extern int __cpu_suspend(unsigned long);
+extern int __cpu_suspend_enter(unsigned long arg, int (*fn)(unsigned long));
 /*
- * This is called by __cpu_suspend() to save the state, and do whatever
+ * This is called by __cpu_suspend_enter() to save the state, and do whatever
  * flushing is required to ensure that when the CPU goes to sleep we have
  * the necessary data available when the caches are not searched.
  *
- * @arg: Argument to pass to suspend operations
- * @ptr: CPU context virtual address
- * @save_ptr: address of the location where the context physical address
- *            must be saved
+ * ptr: CPU context virtual address
+ * save_ptr: address of the location where the context physical address
+ *           must be saved
  */
-int __cpu_suspend_finisher(unsigned long arg, struct cpu_suspend_ctx *ptr,
-			   phys_addr_t *save_ptr)
+void notrace __cpu_suspend_save(struct cpu_suspend_ctx *ptr,
+				phys_addr_t *save_ptr)
 {
-	int cpu = smp_processor_id();
-
 	*save_ptr = virt_to_phys(ptr);
 
 	cpu_do_suspend(ptr);
@@ -35,8 +33,6 @@ int __cpu_suspend_finisher(unsigned long arg, struct cpu_suspend_ctx *ptr,
 	 */
 	__flush_dcache_area(ptr, sizeof(*ptr));
 	__flush_dcache_area(save_ptr, sizeof(*save_ptr));
-
-	return cpu_ops[cpu]->cpu_suspend(arg);
 }
 
 /*
@@ -56,15 +52,15 @@ void __init cpu_suspend_set_dbg_restorer(void (*hw_bp_restore)(void *))
 }
 
 /**
- * cpu_suspend
+ * cpu_suspend() - function to enter a low-power state
+ * @arg: argument to pass to CPU suspend operations
  *
- * @arg: argument to pass to the finisher function
+ * Return: 0 on success, -EOPNOTSUPP if CPU suspend hook not initialized, CPU
+ * operations back-end error code otherwise.
  */
 int cpu_suspend(unsigned long arg)
 {
-	struct mm_struct *mm = current->active_mm;
-	int ret, cpu = smp_processor_id();
-	unsigned long flags;
+	int cpu = smp_processor_id();
 
 	/*
 	 * If cpu_ops have not been registered or suspend
@@ -72,6 +68,21 @@ int cpu_suspend(unsigned long arg)
 	 */
 	if (!cpu_ops[cpu] || !cpu_ops[cpu]->cpu_suspend)
 		return -EOPNOTSUPP;
+	return cpu_ops[cpu]->cpu_suspend(arg);
+}
+
+/*
+ * __cpu_suspend
+ *
+ * arg: argument to pass to the finisher function
+ * fn: finisher function pointer
+ *
+ */
+int __cpu_suspend(unsigned long arg, int (*fn)(unsigned long))
+{
+	struct mm_struct *mm = current->active_mm;
+	int ret;
+	unsigned long flags;
 
 	/*
 	 * From this point debug exceptions are disabled to prevent
@@ -86,16 +97,27 @@ int cpu_suspend(unsigned long arg)
 	 * page tables, so that the thread address space is properly
 	 * set-up on function return.
 	 */
-	ret = __cpu_suspend(arg);
+	ret = __cpu_suspend_enter(arg, fn);
 	if (ret == 0) {
-		cpu_switch_mm(mm->pgd, mm);
+		/*
+		 * We are resuming from reset with TTBR0_EL1 set to the
+		 * idmap to enable the MMU; restore the active_mm mappings in
+		 * TTBR0_EL1 unless the active_mm == &init_mm, in which case
+		 * the thread entered __cpu_suspend with TTBR0_EL1 set to
+		 * reserved TTBR0 page tables and should be restored as such.
+		 */
+		if (mm == &init_mm)
+			cpu_set_reserved_ttbr0();
+		else
+			cpu_switch_mm(mm->pgd, mm);
+
 		flush_tlb_all();
 
 		/*
 		 * Restore per-cpu offset before any kernel
 		 * subsystem relying on it has a chance to run.
 		 */
-		set_my_cpu_offset(per_cpu_offset(cpu));
+		set_my_cpu_offset(per_cpu_offset(smp_processor_id()));
 
 		/*
 		 * Restore HW breakpoint registers to sane values
@@ -116,10 +138,10 @@ int cpu_suspend(unsigned long arg)
 	return ret;
 }
 
-extern struct sleep_save_sp sleep_save_sp;
-extern phys_addr_t sleep_idmap_phys;
+struct sleep_save_sp sleep_save_sp;
+phys_addr_t sleep_idmap_phys;
 
-static int cpu_suspend_init(void)
+static int __init cpu_suspend_init(void)
 {
 	void *ctx_ptr;
 
diff --git a/arch/powerpc/kernel/mce_power.c b/arch/powerpc/kernel/mce_power.c
index 27c93f4..fc0927a 100644
--- a/arch/powerpc/kernel/mce_power.c
+++ b/arch/powerpc/kernel/mce_power.c
@@ -78,7 +78,7 @@ static long mce_handle_derror(uint64_t dsisr, uint64_t slb_error_bits)
 	}
 	if (dsisr & P7_DSISR_MC_TLB_MULTIHIT_MFTLB) {
 		if (cur_cpu_spec && cur_cpu_spec->flush_tlb)
-			cur_cpu_spec->flush_tlb(TLBIEL_INVAL_PAGE);
+			cur_cpu_spec->flush_tlb(TLBIEL_INVAL_SET);
 		/* reset error bits */
 		dsisr &= ~P7_DSISR_MC_TLB_MULTIHIT_MFTLB;
 	}
@@ -109,7 +109,7 @@ static long mce_handle_common_ierror(uint64_t srr1)
 		break;
 	case P7_SRR1_MC_IFETCH_TLB_MULTIHIT:
 		if (cur_cpu_spec && cur_cpu_spec->flush_tlb) {
-			cur_cpu_spec->flush_tlb(TLBIEL_INVAL_PAGE);
+			cur_cpu_spec->flush_tlb(TLBIEL_INVAL_SET);
 			handled = 1;
 		}
 		break;
diff --git a/arch/powerpc/kernel/udbg_16550.c b/arch/powerpc/kernel/udbg_16550.c
index 75702e2..f7089fc 100644
--- a/arch/powerpc/kernel/udbg_16550.c
+++ b/arch/powerpc/kernel/udbg_16550.c
@@ -69,8 +69,12 @@ static void udbg_uart_putc(char c)
 
 static int udbg_uart_getc_poll(void)
 {
-	if (!udbg_uart_in || !(udbg_uart_in(UART_LSR) & LSR_DR))
+	if (!udbg_uart_in)
+		return -1;
+
+	if (!(udbg_uart_in(UART_LSR) & LSR_DR))
 		return udbg_uart_in(UART_RBR);
+
 	return -1;
 }
 
diff --git a/arch/x86/include/asm/vsyscall.h b/arch/x86/include/asm/vsyscall.h
index 2a46ca7..2874be9 100644
--- a/arch/x86/include/asm/vsyscall.h
+++ b/arch/x86/include/asm/vsyscall.h
@@ -34,7 +34,7 @@ static inline unsigned int __getcpu(void)
 		native_read_tscp(&p);
 	} else {
 		/* Load per CPU data from GDT */
-		asm("lsl %1,%0" : "=r" (p) : "r" (__PER_CPU_SEG));
+		asm volatile ("lsl %1,%0" : "=r" (p) : "r" (__PER_CPU_SEG));
 	}
 
 	return p;
diff --git a/arch/x86/kernel/cpu/perf_event_intel_uncore.c b/arch/x86/kernel/cpu/perf_event_intel_uncore.c
index 047f540..2f98588 100644
--- a/arch/x86/kernel/cpu/perf_event_intel_uncore.c
+++ b/arch/x86/kernel/cpu/perf_event_intel_uncore.c
@@ -2886,6 +2886,17 @@ static struct intel_uncore_box *uncore_event_to_box(struct perf_event *event)
 	return uncore_pmu_to_box(uncore_event_to_pmu(event), smp_processor_id());
 }
 
+/*
+ * Using uncore_pmu_event_init pmu event_init callback
+ * as a detection point for uncore events.
+ */
+static int uncore_pmu_event_init(struct perf_event *event);
+
+static bool is_uncore_event(struct perf_event *event)
+{
+	return event->pmu->event_init == uncore_pmu_event_init;
+}
+
 static int
 uncore_collect_events(struct intel_uncore_box *box, struct perf_event *leader, bool dogrp)
 {
@@ -2900,13 +2911,18 @@ uncore_collect_events(struct intel_uncore_box *box, struct perf_event *leader, b
 		return -EINVAL;
 
 	n = box->n_events;
-	box->event_list[n] = leader;
-	n++;
+
+	if (is_uncore_event(leader)) {
+		box->event_list[n] = leader;
+		n++;
+	}
+
 	if (!dogrp)
 		return n;
 
 	list_for_each_entry(event, &leader->sibling_list, group_entry) {
-		if (event->state <= PERF_EVENT_STATE_OFF)
+		if (!is_uncore_event(event) ||
+		    event->state <= PERF_EVENT_STATE_OFF)
 			continue;
 
 		if (n >= max_count)
diff --git a/arch/x86/kvm/mmu.c b/arch/x86/kvm/mmu.c
index 49088b8..dcae8fa 100644
--- a/arch/x86/kvm/mmu.c
+++ b/arch/x86/kvm/mmu.c
@@ -4384,7 +4384,7 @@ void kvm_mmu_invalidate_mmio_sptes(struct kvm *kvm)
 	 * zap all shadow pages.
 	 */
 	if (unlikely(kvm_current_mmio_generation(kvm) == 0)) {
-		printk_ratelimited(KERN_INFO "kvm: zapping shadow pages for mmio generation wraparound\n");
+		printk_ratelimited(KERN_DEBUG "kvm: zapping shadow pages for mmio generation wraparound\n");
 		kvm_mmu_invalidate_zap_all_pages(kvm);
 	}
 }
diff --git a/arch/x86/vdso/vma.c b/arch/x86/vdso/vma.c
index 431e875..ab6ba35 100644
--- a/arch/x86/vdso/vma.c
+++ b/arch/x86/vdso/vma.c
@@ -117,30 +117,45 @@ subsys_initcall(init_vdso);
 
 struct linux_binprm;
 
-/* Put the vdso above the (randomized) stack with another randomized offset.
-   This way there is no hole in the middle of address space.
-   To save memory make sure it is still in the same PTE as the stack top.
-   This doesn't give that many random bits */
+/*
+ * Put the vdso above the (randomized) stack with another randomized
+ * offset.  This way there is no hole in the middle of address space.
+ * To save memory make sure it is still in the same PTE as the stack
+ * top.  This doesn't give that many random bits.
+ *
+ * Note that this algorithm is imperfect: the distribution of the vdso
+ * start address within a PMD is biased toward the end.
+ *
+ * Only used for the 64-bit and x32 vdsos.
+ */
 static unsigned long vdso_addr(unsigned long start, unsigned len)
 {
 	unsigned long addr, end;
 	unsigned offset;
-	end = (start + PMD_SIZE - 1) & PMD_MASK;
+
+	/*
+	 * Round up the start address.  It can start out unaligned as a result
+	 * of stack start randomization.
+	 */
+	start = PAGE_ALIGN(start);
+
+	/* Round the lowest possible end address up to a PMD boundary. */
+	end = (start + len + PMD_SIZE - 1) & PMD_MASK;
 	if (end >= TASK_SIZE_MAX)
 		end = TASK_SIZE_MAX;
 	end -= len;
-	/* This loses some more bits than a modulo, but is cheaper */
-	offset = get_random_int() & (PTRS_PER_PTE - 1);
-	addr = start + (offset << PAGE_SHIFT);
-	if (addr >= end)
-		addr = end;
+
+	if (end > start) {
+		offset = get_random_int() % (((end - start) >> PAGE_SHIFT) + 1);
+		addr = start + (offset << PAGE_SHIFT);
+	} else {
+		addr = start;
+	}
 
 	/*
-	 * page-align it here so that get_unmapped_area doesn't
-	 * align it wrongfully again to the next page. addr can come in 4K
-	 * unaligned here as a result of stack start randomization.
+	 * Forcibly align the final address in case we have a hardware
+	 * issue that requires alignment for performance reasons.
 	 */
-	addr = PAGE_ALIGN(addr);
 	addr = align_vdso_addr(addr);
 
 	return addr;
diff --git a/block/blk-mq-cpumap.c b/block/blk-mq-cpumap.c
index f872127..78d3835 100644
--- a/block/blk-mq-cpumap.c
+++ b/block/blk-mq-cpumap.c
@@ -95,7 +95,7 @@ unsigned int *blk_mq_make_queue_map(struct blk_mq_reg *reg)
 	unsigned int *map;
 
 	/* If cpus are offline, map them to first hctx */
-	map = kzalloc_node(sizeof(*map) * num_possible_cpus(), GFP_KERNEL,
+	map = kzalloc_node(sizeof(*map) * nr_cpu_ids, GFP_KERNEL,
 				reg->numa_node);
 	if (!map)
 		return NULL;
diff --git a/block/genhd.c b/block/genhd.c
index e6723bd..a8d586a 100644
--- a/block/genhd.c
+++ b/block/genhd.c
@@ -1070,9 +1070,16 @@ int disk_expand_part_tbl(struct gendisk *disk, int partno)
 	struct disk_part_tbl *old_ptbl = disk->part_tbl;
 	struct disk_part_tbl *new_ptbl;
 	int len = old_ptbl ? old_ptbl->len : 0;
-	int target = partno + 1;
+	int i, target;
 	size_t size;
-	int i;
+
+	/*
+	 * check for int overflow, since we can get here from blkpg_ioctl()
+	 * with a user passed 'partno'.
+	 */
+	target = partno + 1;
+	if (target < 0)
+		return -EINVAL;
 
 	/* disk_max_parts() is zero during initialization, ignore if so */
 	if (disk_max_parts(disk) && target > disk_max_parts(disk))
diff --git a/drivers/acpi/device_pm.c b/drivers/acpi/device_pm.c
index c14a00d..19f6505 100644
--- a/drivers/acpi/device_pm.c
+++ b/drivers/acpi/device_pm.c
@@ -257,7 +257,7 @@ int acpi_bus_init_power(struct acpi_device *device)
 
 	device->power.state = ACPI_STATE_UNKNOWN;
 	if (!acpi_device_is_present(device))
-		return 0;
+		return -ENXIO;
 
 	result = acpi_device_get_power(device, &state);
 	if (result)
diff --git a/drivers/acpi/scan.c b/drivers/acpi/scan.c
index 493a342..666beea 100644
--- a/drivers/acpi/scan.c
+++ b/drivers/acpi/scan.c
@@ -865,7 +865,7 @@ static void acpi_free_power_resources_lists(struct acpi_device *device)
 	if (device->wakeup.flags.valid)
 		acpi_power_resources_list_free(&device->wakeup.resources);
 
-	if (!device->flags.power_manageable)
+	if (!device->power.flags.power_resources)
 		return;
 
 	for (i = ACPI_STATE_D0; i <= ACPI_STATE_D3_HOT; i++) {
@@ -1554,10 +1554,8 @@ static void acpi_bus_get_power_flags(struct acpi_device *device)
 			device->power.flags.power_resources)
 		device->power.states[ACPI_STATE_D3_COLD].flags.os_accessible = 1;
 
-	if (acpi_bus_init_power(device)) {
-		acpi_free_power_resources_lists(device);
+	if (acpi_bus_init_power(device))
 		device->flags.power_manageable = 0;
-	}
 }
 
 static void acpi_bus_get_flags(struct acpi_device *device)
@@ -2043,13 +2041,18 @@ static void acpi_bus_attach(struct acpi_device *device)
 	/* Skip devices that are not present. */
 	if (!acpi_device_is_present(device)) {
 		device->flags.visited = false;
+		device->flags.power_manageable = 0;
 		return;
 	}
 	if (device->handler)
 		goto ok;
 
 	if (!device->flags.initialized) {
-		acpi_bus_update_power(device, NULL);
+		device->flags.power_manageable =
+			device->power.states[ACPI_STATE_D0].flags.valid;
+		if (acpi_bus_init_power(device))
+			device->flags.power_manageable = 0;
+
 		device->flags.initialized = true;
 	}
 	device->flags.visited = false;
diff --git a/drivers/base/bus.c b/drivers/base/bus.c
index 59dc808..45d0fa7 100644
--- a/drivers/base/bus.c
+++ b/drivers/base/bus.c
@@ -254,13 +254,15 @@ static ssize_t store_drivers_probe(struct bus_type *bus,
 				   const char *buf, size_t count)
 {
 	struct device *dev;
+	int err = -EINVAL;
 
 	dev = bus_find_device_by_name(bus, NULL, buf);
 	if (!dev)
 		return -ENODEV;
-	if (bus_rescan_devices_helper(dev, NULL) != 0)
-		return -EINVAL;
-	return count;
+	if (bus_rescan_devices_helper(dev, NULL) == 0)
+		err = count;
+	put_device(dev);
+	return err;
 }
 
 static struct device *next_device(struct klist_iter *i)
diff --git a/drivers/hid/hid-core.c b/drivers/hid/hid-core.c
index 7cd42ea..d92c7d9 100644
--- a/drivers/hid/hid-core.c
+++ b/drivers/hid/hid-core.c
@@ -1743,6 +1743,7 @@ static const struct hid_device_id hid_have_special_driver[] = {
 	{ HID_USB_DEVICE(USB_VENDOR_ID_KYE, USB_DEVICE_ID_KYE_ERGO_525V) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_KYE, USB_DEVICE_ID_KYE_EASYPEN_I405X) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_KYE, USB_DEVICE_ID_KYE_MOUSEPEN_I608X) },
+	{ HID_USB_DEVICE(USB_VENDOR_ID_KYE, USB_DEVICE_ID_KYE_MOUSEPEN_I608X_2) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_KYE, USB_DEVICE_ID_KYE_EASYPEN_M610X) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_LABTEC, USB_DEVICE_ID_LABTEC_WIRELESS_KEYBOARD) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_LCPOWER, USB_DEVICE_ID_LCPOWER_LC1000 ) },
diff --git a/drivers/hid/hid-ids.h b/drivers/hid/hid-ids.h
index 91bc66b..4850da3 100644
--- a/drivers/hid/hid-ids.h
+++ b/drivers/hid/hid-ids.h
@@ -511,6 +511,7 @@
 #define USB_DEVICE_ID_KYE_GPEN_560	0x5003
 #define USB_DEVICE_ID_KYE_EASYPEN_I405X	0x5010
 #define USB_DEVICE_ID_KYE_MOUSEPEN_I608X	0x5011
+#define USB_DEVICE_ID_KYE_MOUSEPEN_I608X_2	0x501a
 #define USB_DEVICE_ID_KYE_EASYPEN_M610X	0x5013
 
 #define USB_VENDOR_ID_LABTEC		0x1020
diff --git a/drivers/hid/hid-input.c b/drivers/hid/hid-input.c
index a713e62..4b87bb1 100644
--- a/drivers/hid/hid-input.c
+++ b/drivers/hid/hid-input.c
@@ -312,6 +312,9 @@ static const struct hid_device_id hid_battery_quirks[] = {
 			       USB_DEVICE_ID_APPLE_ALU_WIRELESS_2011_ANSI),
 	  HID_BATTERY_QUIRK_PERCENT | HID_BATTERY_QUIRK_FEATURE },
 	{ HID_BLUETOOTH_DEVICE(USB_VENDOR_ID_APPLE,
+			       USB_DEVICE_ID_APPLE_ALU_WIRELESS_2011_ISO),
+	  HID_BATTERY_QUIRK_PERCENT | HID_BATTERY_QUIRK_FEATURE },
+	{ HID_BLUETOOTH_DEVICE(USB_VENDOR_ID_APPLE,
 		USB_DEVICE_ID_APPLE_ALU_WIRELESS_ANSI),
 	  HID_BATTERY_QUIRK_PERCENT | HID_BATTERY_QUIRK_FEATURE },
 	{}
diff --git a/drivers/hid/hid-kye.c b/drivers/hid/hid-kye.c
index b92bf01..158fcf5 100644
--- a/drivers/hid/hid-kye.c
+++ b/drivers/hid/hid-kye.c
@@ -323,6 +323,7 @@ static __u8 *kye_report_fixup(struct hid_device *hdev, __u8 *rdesc,
 		}
 		break;
 	case USB_DEVICE_ID_KYE_MOUSEPEN_I608X:
+	case USB_DEVICE_ID_KYE_MOUSEPEN_I608X_2:
 		if (*rsize == MOUSEPEN_I608X_RDESC_ORIG_SIZE) {
 			rdesc = mousepen_i608x_rdesc_fixed;
 			*rsize = sizeof(mousepen_i608x_rdesc_fixed);
@@ -415,6 +416,7 @@ static int kye_probe(struct hid_device *hdev, const struct hid_device_id *id)
 	switch (id->product) {
 	case USB_DEVICE_ID_KYE_EASYPEN_I405X:
 	case USB_DEVICE_ID_KYE_MOUSEPEN_I608X:
+	case USB_DEVICE_ID_KYE_MOUSEPEN_I608X_2:
 	case USB_DEVICE_ID_KYE_EASYPEN_M610X:
 		ret = kye_tablet_enable(hdev);
 		if (ret) {
@@ -446,6 +448,8 @@ static const struct hid_device_id kye_devices[] = {
 	{ HID_USB_DEVICE(USB_VENDOR_ID_KYE,
 				USB_DEVICE_ID_KYE_MOUSEPEN_I608X) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_KYE,
+				USB_DEVICE_ID_KYE_MOUSEPEN_I608X_2) },
+	{ HID_USB_DEVICE(USB_VENDOR_ID_KYE,
 				USB_DEVICE_ID_KYE_EASYPEN_M610X) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_KYE,
 				USB_DEVICE_ID_GENIUS_GILA_GAMING_MOUSE) },
diff --git a/drivers/hid/hid-roccat-pyra.c b/drivers/hid/hid-roccat-pyra.c
index 1a07e07..47d7e74 100644
--- a/drivers/hid/hid-roccat-pyra.c
+++ b/drivers/hid/hid-roccat-pyra.c
@@ -35,6 +35,8 @@ static struct class *pyra_class;
 static void profile_activated(struct pyra_device *pyra,
 		unsigned int new_profile)
 {
+	if (new_profile >= ARRAY_SIZE(pyra->profile_settings))
+		return;
 	pyra->actual_profile = new_profile;
 	pyra->actual_cpi = pyra->profile_settings[pyra->actual_profile].y_cpi;
 }
@@ -257,9 +259,11 @@ static ssize_t pyra_sysfs_write_settings(struct file *fp,
 	if (off != 0 || count != PYRA_SIZE_SETTINGS)
 		return -EINVAL;
 
-	mutex_lock(&pyra->pyra_lock);
-
 	settings = (struct pyra_settings const *)buf;
+	if (settings->startup_profile >= ARRAY_SIZE(pyra->profile_settings))
+		return -EINVAL;
+
+	mutex_lock(&pyra->pyra_lock);
 
 	retval = pyra_set_settings(usb_dev, settings);
 	if (retval) {
diff --git a/drivers/hid/i2c-hid/i2c-hid.c b/drivers/hid/i2c-hid/i2c-hid.c
index 42eebd1..6e5d8fe 100644
--- a/drivers/hid/i2c-hid/i2c-hid.c
+++ b/drivers/hid/i2c-hid/i2c-hid.c
@@ -136,6 +136,7 @@ struct i2c_hid {
 						   * descriptor. */
 	unsigned int		bufsize;	/* i2c buffer size */
 	char			*inbuf;		/* Input buffer */
+	char			*rawbuf;	/* Raw Input buffer */
 	char			*cmdbuf;	/* Command buffer */
 	char			*argsbuf;	/* Command arguments buffer */
 
@@ -355,7 +356,7 @@ static int i2c_hid_hwreset(struct i2c_client *client)
 static void i2c_hid_get_input(struct i2c_hid *ihid)
 {
 	int ret, ret_size;
-	int size = le16_to_cpu(ihid->hdesc.wMaxInputLength);
+	int size = ihid->bufsize;
 
 	ret = i2c_master_recv(ihid->client, ihid->inbuf, size);
 	if (ret != size) {
@@ -482,9 +483,11 @@ static void i2c_hid_find_max_report(struct hid_device *hid, unsigned int type,
 static void i2c_hid_free_buffers(struct i2c_hid *ihid)
 {
 	kfree(ihid->inbuf);
+	kfree(ihid->rawbuf);
 	kfree(ihid->argsbuf);
 	kfree(ihid->cmdbuf);
 	ihid->inbuf = NULL;
+	ihid->rawbuf = NULL;
 	ihid->cmdbuf = NULL;
 	ihid->argsbuf = NULL;
 	ihid->bufsize = 0;
@@ -500,10 +503,11 @@ static int i2c_hid_alloc_buffers(struct i2c_hid *ihid, size_t report_size)
 		       report_size; /* report */
 
 	ihid->inbuf = kzalloc(report_size, GFP_KERNEL);
+	ihid->rawbuf = kzalloc(report_size, GFP_KERNEL);
 	ihid->argsbuf = kzalloc(args_len, GFP_KERNEL);
 	ihid->cmdbuf = kzalloc(sizeof(union command) + args_len, GFP_KERNEL);
 
-	if (!ihid->inbuf || !ihid->argsbuf || !ihid->cmdbuf) {
+	if (!ihid->inbuf || !ihid->rawbuf || !ihid->argsbuf || !ihid->cmdbuf) {
 		i2c_hid_free_buffers(ihid);
 		return -ENOMEM;
 	}
@@ -530,12 +534,12 @@ static int i2c_hid_get_raw_report(struct hid_device *hid,
 
 	ret = i2c_hid_get_report(client,
 			report_type == HID_FEATURE_REPORT ? 0x03 : 0x01,
-			report_number, ihid->inbuf, ask_count);
+			report_number, ihid->rawbuf, ask_count);
 
 	if (ret < 0)
 		return ret;
 
-	ret_count = ihid->inbuf[0] | (ihid->inbuf[1] << 8);
+	ret_count = ihid->rawbuf[0] | (ihid->rawbuf[1] << 8);
 
 	if (ret_count <= 2)
 		return 0;
@@ -544,7 +548,7 @@ static int i2c_hid_get_raw_report(struct hid_device *hid,
 
 	/* The query buffer contains the size, dropping it in the reply */
 	count = min(count, ret_count - 2);
-	memcpy(buf, ihid->inbuf + 2, count);
+	memcpy(buf, ihid->rawbuf + 2, count);
 
 	return count;
 }
diff --git a/drivers/hid/usbhid/hid-quirks.c b/drivers/hid/usbhid/hid-quirks.c
index deb3643..473c0c4 100644
--- a/drivers/hid/usbhid/hid-quirks.c
+++ b/drivers/hid/usbhid/hid-quirks.c
@@ -116,6 +116,7 @@ static const struct hid_blacklist {
 	{ USB_VENDOR_ID_CHICONY, USB_DEVICE_ID_CHICONY_WIRELESS, HID_QUIRK_MULTI_INPUT },
 	{ USB_VENDOR_ID_SIGMA_MICRO, USB_DEVICE_ID_SIGMA_MICRO_KEYBOARD, HID_QUIRK_NO_INIT_REPORTS },
 	{ USB_VENDOR_ID_KYE, USB_DEVICE_ID_KYE_MOUSEPEN_I608X, HID_QUIRK_MULTI_INPUT },
+	{ USB_VENDOR_ID_KYE, USB_DEVICE_ID_KYE_MOUSEPEN_I608X_2, HID_QUIRK_MULTI_INPUT },
 	{ USB_VENDOR_ID_KYE, USB_DEVICE_ID_KYE_EASYPEN_M610X, HID_QUIRK_MULTI_INPUT },
 	{ USB_VENDOR_ID_NTRIG, USB_DEVICE_ID_NTRIG_DUOSENSE, HID_QUIRK_NO_INIT_REPORTS },
 	{ USB_VENDOR_ID_SYNAPTICS, USB_DEVICE_ID_SYNAPTICS_LTS1, HID_QUIRK_NO_INIT_REPORTS },
diff --git a/drivers/hv/channel_mgmt.c b/drivers/hv/channel_mgmt.c
index fa92046..505fe29 100644
--- a/drivers/hv/channel_mgmt.c
+++ b/drivers/hv/channel_mgmt.c
@@ -202,9 +202,16 @@ static void vmbus_process_rescind_offer(struct work_struct *work)
 	unsigned long flags;
 	struct vmbus_channel *primary_channel;
 	struct vmbus_channel_relid_released msg;
+	struct device *dev;
+
+	if (channel->device_obj) {
+		dev = get_device(&channel->device_obj->device);
+		if (dev) {
+			vmbus_device_unregister(channel->device_obj);
+			put_device(dev);
+		}
+	}
 
-	if (channel->device_obj)
-		vmbus_device_unregister(channel->device_obj);
 	memset(&msg, 0, sizeof(struct vmbus_channel_relid_released));
 	msg.child_relid = channel->offermsg.child_relid;
 	msg.header.msgtype = CHANNELMSG_RELID_RELEASED;
diff --git a/drivers/iommu/intel-iommu.c b/drivers/iommu/intel-iommu.c
index 40f6b47..8855ecb 100644
--- a/drivers/iommu/intel-iommu.c
+++ b/drivers/iommu/intel-iommu.c
@@ -1768,7 +1768,7 @@ static int __domain_mapping(struct dmar_domain *domain, unsigned long iov_pfn,
 	struct dma_pte *first_pte = NULL, *pte = NULL;
 	phys_addr_t uninitialized_var(pteval);
 	int addr_width = agaw_to_width(domain->agaw) - VTD_PAGE_SHIFT;
-	unsigned long sg_res;
+	unsigned long sg_res = 0;
 	unsigned int largepage_lvl = 0;
 	unsigned long lvl_pages = 0;
 
@@ -1779,10 +1779,8 @@ static int __domain_mapping(struct dmar_domain *domain, unsigned long iov_pfn,
 
 	prot &= DMA_PTE_READ | DMA_PTE_WRITE | DMA_PTE_SNP;
 
-	if (sg)
-		sg_res = 0;
-	else {
-		sg_res = nr_pages + 1;
+	if (!sg) {
+		sg_res = nr_pages;
 		pteval = ((phys_addr_t)phys_pfn << VTD_PAGE_SHIFT) | prot;
 	}
 
diff --git a/drivers/misc/genwqe/card_utils.c b/drivers/misc/genwqe/card_utils.c
index 6b1a6ef..0c3a647 100644
--- a/drivers/misc/genwqe/card_utils.c
+++ b/drivers/misc/genwqe/card_utils.c
@@ -490,6 +490,8 @@ int genwqe_user_vmap(struct genwqe_dev *cd, struct dma_mapping *m, void *uaddr,
 				 m->nr_pages,
 				 1,		/* write by caller */
 				 m->page_list);	/* ptrs to pages */
+	if (rc < 0)
+		goto fail_get_user_pages;
 
 	/* assumption: get_user_pages can be killed by signals. */
 	if (rc < m->nr_pages) {
diff --git a/drivers/mmc/host/sdhci.c b/drivers/mmc/host/sdhci.c
index 9ddef47..7e01763 100644
--- a/drivers/mmc/host/sdhci.c
+++ b/drivers/mmc/host/sdhci.c
@@ -1343,6 +1343,8 @@ static void sdhci_request(struct mmc_host *mmc, struct mmc_request *mrq)
 
 	sdhci_runtime_pm_get(host);
 
+	present = mmc_gpio_get_cd(host->mmc);
+
 	spin_lock_irqsave(&host->lock, flags);
 
 	WARN_ON(host->mrq != NULL);
@@ -1371,7 +1373,6 @@ static void sdhci_request(struct mmc_host *mmc, struct mmc_request *mrq)
 	 *     zero: cd-gpio is used, and card is removed
 	 *     one: cd-gpio is used, and card is present
 	 */
-	present = mmc_gpio_get_cd(host->mmc);
 	if (present < 0) {
 		/* If polling, assume that the card is always present. */
 		if (host->quirks & SDHCI_QUIRK_BROKEN_CARD_DETECTION)
@@ -2082,15 +2083,18 @@ static void sdhci_card_event(struct mmc_host *mmc)
 {
 	struct sdhci_host *host = mmc_priv(mmc);
 	unsigned long flags;
+	int present;
 
 	/* First check if client has provided their own card event */
 	if (host->ops->card_event)
 		host->ops->card_event(host);
 
+	present = sdhci_do_get_cd(host);
+
 	spin_lock_irqsave(&host->lock, flags);
 
 	/* Check host->mrq first in case we are runtime suspended */
-	if (host->mrq && !sdhci_do_get_cd(host)) {
+	if (host->mrq && !present) {
 		pr_err("%s: Card removed during transfer!\n",
 			mmc_hostname(host->mmc));
 		pr_err("%s: Resetting controller.\n",
diff --git a/drivers/mtd/tests/torturetest.c b/drivers/mtd/tests/torturetest.c
index eeab969..b55bc52 100644
--- a/drivers/mtd/tests/torturetest.c
+++ b/drivers/mtd/tests/torturetest.c
@@ -264,7 +264,9 @@ static int __init tort_init(void)
 		int i;
 		void *patt;
 
-		mtdtest_erase_good_eraseblocks(mtd, bad_ebs, eb, ebcnt);
+		err = mtdtest_erase_good_eraseblocks(mtd, bad_ebs, eb, ebcnt);
+		if (err)
+			goto out;
 
 		/* Check if the eraseblocks contain only 0xFF bytes */
 		if (check) {
diff --git a/drivers/mtd/ubi/upd.c b/drivers/mtd/ubi/upd.c
index ec2c2dc..2a1b6e0 100644
--- a/drivers/mtd/ubi/upd.c
+++ b/drivers/mtd/ubi/upd.c
@@ -133,6 +133,10 @@ int ubi_start_update(struct ubi_device *ubi, struct ubi_volume *vol,
 	ubi_assert(!vol->updating && !vol->changing_leb);
 	vol->updating = 1;
 
+	vol->upd_buf = vmalloc(ubi->leb_size);
+	if (!vol->upd_buf)
+		return -ENOMEM;
+
 	err = set_update_marker(ubi, vol);
 	if (err)
 		return err;
@@ -152,14 +156,12 @@ int ubi_start_update(struct ubi_device *ubi, struct ubi_volume *vol,
 		err = clear_update_marker(ubi, vol, 0);
 		if (err)
 			return err;
+
+		vfree(vol->upd_buf);
 		vol->updating = 0;
 		return 0;
 	}
 
-	vol->upd_buf = vmalloc(ubi->leb_size);
-	if (!vol->upd_buf)
-		return -ENOMEM;
-
 	vol->upd_ebs = div_u64(bytes + vol->usable_leb_size - 1,
 			       vol->usable_leb_size);
 	vol->upd_bytes = bytes;
diff --git a/drivers/mtd/ubi/wl.c b/drivers/mtd/ubi/wl.c
index 02317c1..68b924e 100644
--- a/drivers/mtd/ubi/wl.c
+++ b/drivers/mtd/ubi/wl.c
@@ -1205,7 +1205,6 @@ static int wear_leveling_worker(struct ubi_device *ubi, struct ubi_work *wrk,
 
 	err = do_sync_erase(ubi, e1, vol_id, lnum, 0);
 	if (err) {
-		kmem_cache_free(ubi_wl_entry_slab, e1);
 		if (e2)
 			kmem_cache_free(ubi_wl_entry_slab, e2);
 		goto out_ro;
@@ -1219,10 +1218,8 @@ static int wear_leveling_worker(struct ubi_device *ubi, struct ubi_work *wrk,
 		dbg_wl("PEB %d (LEB %d:%d) was put meanwhile, erase",
 		       e2->pnum, vol_id, lnum);
 		err = do_sync_erase(ubi, e2, vol_id, lnum, 0);
-		if (err) {
-			kmem_cache_free(ubi_wl_entry_slab, e2);
+		if (err)
 			goto out_ro;
-		}
 	}
 
 	dbg_wl("done");
@@ -1258,10 +1255,9 @@ out_not_moved:
 
 	ubi_free_vid_hdr(ubi, vid_hdr);
 	err = do_sync_erase(ubi, e2, vol_id, lnum, torture);
-	if (err) {
-		kmem_cache_free(ubi_wl_entry_slab, e2);
+	if (err)
 		goto out_ro;
-	}
+
 	mutex_unlock(&ubi->move_mutex);
 	return 0;
 
diff --git a/drivers/net/can/usb/peak_usb/pcan_usb_core.c b/drivers/net/can/usb/peak_usb/pcan_usb_core.c
index 0b7a4c3..03e7f0c 100644
--- a/drivers/net/can/usb/peak_usb/pcan_usb_core.c
+++ b/drivers/net/can/usb/peak_usb/pcan_usb_core.c
@@ -734,7 +734,7 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 	dev->cmd_buf = kmalloc(PCAN_USB_MAX_CMD_LEN, GFP_KERNEL);
 	if (!dev->cmd_buf) {
 		err = -ENOMEM;
-		goto lbl_set_intf_data;
+		goto lbl_free_candev;
 	}
 
 	dev->udev = usb_dev;
@@ -773,7 +773,7 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 	err = register_candev(netdev);
 	if (err) {
 		dev_err(&intf->dev, "couldn't register CAN device: %d\n", err);
-		goto lbl_free_cmd_buf;
+		goto lbl_restore_intf_data;
 	}
 
 	if (dev->prev_siblings)
@@ -786,14 +786,14 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 	if (dev->adapter->dev_init) {
 		err = dev->adapter->dev_init(dev);
 		if (err)
-			goto lbl_free_cmd_buf;
+			goto lbl_unregister_candev;
 	}
 
 	/* set bus off */
 	if (dev->adapter->dev_set_bus) {
 		err = dev->adapter->dev_set_bus(dev, 0);
 		if (err)
-			goto lbl_free_cmd_buf;
+			goto lbl_unregister_candev;
 	}
 
 	/* get device number early */
@@ -805,11 +805,14 @@ static int peak_usb_create_dev(struct peak_usb_adapter *peak_usb_adapter,
 
 	return 0;
 
-lbl_free_cmd_buf:
-	kfree(dev->cmd_buf);
+lbl_unregister_candev:
+	unregister_candev(netdev);
 
-lbl_set_intf_data:
+lbl_restore_intf_data:
 	usb_set_intfdata(intf, dev->prev_siblings);
+	kfree(dev->cmd_buf);
+
+lbl_free_candev:
 	free_candev(netdev);
 
 	return err;
diff --git a/drivers/net/can/usb/peak_usb/pcan_usb_pro.c b/drivers/net/can/usb/peak_usb/pcan_usb_pro.c
index 263dd92..f7f796a 100644
--- a/drivers/net/can/usb/peak_usb/pcan_usb_pro.c
+++ b/drivers/net/can/usb/peak_usb/pcan_usb_pro.c
@@ -333,8 +333,6 @@ static int pcan_usb_pro_send_req(struct peak_usb_device *dev, int req_id,
 	if (!(dev->state & PCAN_USB_STATE_CONNECTED))
 		return 0;
 
-	memset(req_addr, '\0', req_size);
-
 	req_type = USB_TYPE_VENDOR | USB_RECIP_OTHER;
 
 	switch (req_id) {
@@ -345,6 +343,7 @@ static int pcan_usb_pro_send_req(struct peak_usb_device *dev, int req_id,
 	default:
 		p = usb_rcvctrlpipe(dev->udev, 0);
 		req_type |= USB_DIR_IN;
+		memset(req_addr, '\0', req_size);
 		break;
 	}
 
diff --git a/drivers/net/wireless/ath/ath5k/qcu.c b/drivers/net/wireless/ath/ath5k/qcu.c
index 0583c69..ddaad71 100644
--- a/drivers/net/wireless/ath/ath5k/qcu.c
+++ b/drivers/net/wireless/ath/ath5k/qcu.c
@@ -225,13 +225,7 @@ ath5k_hw_setup_tx_queue(struct ath5k_hw *ah, enum ath5k_tx_queue queue_type,
 	} else {
 		switch (queue_type) {
 		case AR5K_TX_QUEUE_DATA:
-			for (queue = AR5K_TX_QUEUE_ID_DATA_MIN;
-				ah->ah_txq[queue].tqi_type !=
-				AR5K_TX_QUEUE_INACTIVE; queue++) {
-
-				if (queue > AR5K_TX_QUEUE_ID_DATA_MAX)
-					return -EINVAL;
-			}
+			queue = queue_info->tqi_subtype;
 			break;
 		case AR5K_TX_QUEUE_UAPSD:
 			queue = AR5K_TX_QUEUE_ID_UAPSD;
diff --git a/drivers/net/wireless/ath/ath9k/hw.h b/drivers/net/wireless/ath/ath9k/hw.h
index 0acd4b5..32ae0a4 100644
--- a/drivers/net/wireless/ath/ath9k/hw.h
+++ b/drivers/net/wireless/ath/ath9k/hw.h
@@ -216,8 +216,8 @@
 #define AH_WOW_BEACON_MISS		BIT(3)
 
 enum ath_hw_txq_subtype {
-	ATH_TXQ_AC_BE = 0,
-	ATH_TXQ_AC_BK = 1,
+	ATH_TXQ_AC_BK = 0,
+	ATH_TXQ_AC_BE = 1,
 	ATH_TXQ_AC_VI = 2,
 	ATH_TXQ_AC_VO = 3,
 };
diff --git a/drivers/net/wireless/ath/ath9k/mac.c b/drivers/net/wireless/ath/ath9k/mac.c
index 5f72758..8f93ed3 100644
--- a/drivers/net/wireless/ath/ath9k/mac.c
+++ b/drivers/net/wireless/ath/ath9k/mac.c
@@ -311,14 +311,7 @@ int ath9k_hw_setuptxqueue(struct ath_hw *ah, enum ath9k_tx_queue type,
 		q = ATH9K_NUM_TX_QUEUES - 3;
 		break;
 	case ATH9K_TX_QUEUE_DATA:
-		for (q = 0; q < ATH9K_NUM_TX_QUEUES; q++)
-			if (ah->txq[q].tqi_type ==
-			    ATH9K_TX_QUEUE_INACTIVE)
-				break;
-		if (q == ATH9K_NUM_TX_QUEUES) {
-			ath_err(common, "No available TX queue\n");
-			return -1;
-		}
+		q = qinfo->tqi_subtype;
 		break;
 	default:
 		ath_err(common, "Invalid TX queue type: %u\n", type);
diff --git a/drivers/net/wireless/iwlwifi/mvm/fw-api.h b/drivers/net/wireless/iwlwifi/mvm/fw-api.h
index d8948aa..60dc387 100644
--- a/drivers/net/wireless/iwlwifi/mvm/fw-api.h
+++ b/drivers/net/wireless/iwlwifi/mvm/fw-api.h
@@ -1394,7 +1394,7 @@ enum iwl_sf_scenario {
 #define SF_NUM_TIMEOUT_TYPES 2		/* Aging timer and Idle timer */
 
 /* smart FIFO default values */
-#define SF_W_MARK_SISO 4096
+#define SF_W_MARK_SISO 6144
 #define SF_W_MARK_MIMO2 8192
 #define SF_W_MARK_MIMO3 6144
 #define SF_W_MARK_LEGACY 4096
diff --git a/drivers/pci/probe.c b/drivers/pci/probe.c
index 34dff3a..5b428db 100644
--- a/drivers/pci/probe.c
+++ b/drivers/pci/probe.c
@@ -214,14 +214,17 @@ int __pci_read_base(struct pci_dev *dev, enum pci_bar_type type,
 		res->flags |= IORESOURCE_SIZEALIGN;
 		if (res->flags & IORESOURCE_IO) {
 			l &= PCI_BASE_ADDRESS_IO_MASK;
+			sz &= PCI_BASE_ADDRESS_IO_MASK;
 			mask = PCI_BASE_ADDRESS_IO_MASK & (u32) IO_SPACE_LIMIT;
 		} else {
 			l &= PCI_BASE_ADDRESS_MEM_MASK;
+			sz &= PCI_BASE_ADDRESS_MEM_MASK;
 			mask = (u32)PCI_BASE_ADDRESS_MEM_MASK;
 		}
 	} else {
 		res->flags |= (l & IORESOURCE_ROM_ENABLE);
 		l &= PCI_ROM_ADDRESS_MASK;
+		sz &= PCI_ROM_ADDRESS_MASK;
 		mask = (u32)PCI_ROM_ADDRESS_MASK;
 	}
 
diff --git a/drivers/rtc/rtc-isl12057.c b/drivers/rtc/rtc-isl12057.c
index 7854a65..110eab8 100644
--- a/drivers/rtc/rtc-isl12057.c
+++ b/drivers/rtc/rtc-isl12057.c
@@ -89,7 +89,7 @@ static void isl12057_rtc_regs_to_tm(struct rtc_time *tm, u8 *regs)
 	tm->tm_min = bcd2bin(regs[ISL12057_REG_RTC_MN]);
 
 	if (regs[ISL12057_REG_RTC_HR] & ISL12057_REG_RTC_HR_MIL) { /* AM/PM */
-		tm->tm_hour = bcd2bin(regs[ISL12057_REG_RTC_HR] & 0x0f);
+		tm->tm_hour = bcd2bin(regs[ISL12057_REG_RTC_HR] & 0x1f);
 		if (regs[ISL12057_REG_RTC_HR] & ISL12057_REG_RTC_HR_PM)
 			tm->tm_hour += 12;
 	} else {					    /* 24 hour mode */
@@ -98,7 +98,7 @@ static void isl12057_rtc_regs_to_tm(struct rtc_time *tm, u8 *regs)
 
 	tm->tm_mday = bcd2bin(regs[ISL12057_REG_RTC_DT]);
 	tm->tm_wday = bcd2bin(regs[ISL12057_REG_RTC_DW]) - 1; /* starts at 1 */
-	tm->tm_mon  = bcd2bin(regs[ISL12057_REG_RTC_MO]) - 1; /* starts at 1 */
+	tm->tm_mon  = bcd2bin(regs[ISL12057_REG_RTC_MO] & 0x1f) - 1; /* ditto */
 	tm->tm_year = bcd2bin(regs[ISL12057_REG_RTC_YR]) + 100;
 }
 
diff --git a/drivers/rtc/rtc-sirfsoc.c b/drivers/rtc/rtc-sirfsoc.c
index 3eb3642..d2b1ab3 100644
--- a/drivers/rtc/rtc-sirfsoc.c
+++ b/drivers/rtc/rtc-sirfsoc.c
@@ -290,14 +290,6 @@ static int sirfsoc_rtc_probe(struct platform_device *pdev)
 	rtc_div = ((32768 / RTC_HZ) / 2) - 1;
 	sirfsoc_rtc_iobrg_writel(rtc_div, rtcdrv->rtc_base + RTC_DIV);
 
-	rtcdrv->rtc = devm_rtc_device_register(&pdev->dev, pdev->name,
-			&sirfsoc_rtc_ops, THIS_MODULE);
-	if (IS_ERR(rtcdrv->rtc)) {
-		err = PTR_ERR(rtcdrv->rtc);
-		dev_err(&pdev->dev, "can't register RTC device\n");
-		return err;
-	}
-
 	/* 0x3 -> RTC_CLK */
 	sirfsoc_rtc_iobrg_writel(SIRFSOC_RTC_CLK,
 			rtcdrv->rtc_base + RTC_CLOCK_SWITCH);
@@ -312,6 +304,14 @@ static int sirfsoc_rtc_probe(struct platform_device *pdev)
 	rtcdrv->overflow_rtc =
 		sirfsoc_rtc_iobrg_readl(rtcdrv->rtc_base + RTC_SW_VALUE);
 
+	rtcdrv->rtc = devm_rtc_device_register(&pdev->dev, pdev->name,
+			&sirfsoc_rtc_ops, THIS_MODULE);
+	if (IS_ERR(rtcdrv->rtc)) {
+		err = PTR_ERR(rtcdrv->rtc);
+		dev_err(&pdev->dev, "can't register RTC device\n");
+		return err;
+	}
+
 	rtcdrv->irq = platform_get_irq(pdev, 0);
 	err = devm_request_irq(
 			&pdev->dev,
diff --git a/drivers/spi/spi-fsl-spi.c b/drivers/spi/spi-fsl-spi.c
index 119f7af..4dcb292 100644
--- a/drivers/spi/spi-fsl-spi.c
+++ b/drivers/spi/spi-fsl-spi.c
@@ -362,18 +362,28 @@ static int fsl_spi_bufs(struct spi_device *spi, struct spi_transfer *t,
 static void fsl_spi_do_one_msg(struct spi_message *m)
 {
 	struct spi_device *spi = m->spi;
-	struct spi_transfer *t;
+	struct spi_transfer *t, *first;
 	unsigned int cs_change;
 	const int nsecs = 50;
 	int status;
 
-	cs_change = 1;
-	status = 0;
+	/* Don't allow changes if CS is active */
+	first = list_first_entry(&m->transfers, struct spi_transfer,
+			transfer_list);
 	list_for_each_entry(t, &m->transfers, transfer_list) {
-		if (t->bits_per_word || t->speed_hz) {
-			/* Don't allow changes if CS is active */
+		if ((first->bits_per_word != t->bits_per_word) ||
+			(first->speed_hz != t->speed_hz)) {
 			status = -EINVAL;
+			dev_err(&spi->dev,
+				"bits_per_word/speed_hz should be same for the same SPI transfer\n");
+			return;
+		}
+	}
 
+	cs_change = 1;
+	status = -EINVAL;
+	list_for_each_entry(t, &m->transfers, transfer_list) {
+		if (t->bits_per_word || t->speed_hz) {
 			if (cs_change)
 				status = fsl_spi_setup_transfer(spi, t);
 			if (status < 0)
diff --git a/drivers/tty/n_tty.c b/drivers/tty/n_tty.c
index 28ac3f3..d46b4cc 100644
--- a/drivers/tty/n_tty.c
+++ b/drivers/tty/n_tty.c
@@ -321,7 +321,8 @@ static void n_tty_check_unthrottle(struct tty_struct *tty)
 
 static inline void put_tty_queue(unsigned char c, struct n_tty_data *ldata)
 {
-	*read_buf_addr(ldata, ldata->read_head++) = c;
+	*read_buf_addr(ldata, ldata->read_head) = c;
+	ldata->read_head++;
 }
 
 /**
diff --git a/drivers/tty/serial/samsung.c b/drivers/tty/serial/samsung.c
index 9cd706d..7d3a3f5 100644
--- a/drivers/tty/serial/samsung.c
+++ b/drivers/tty/serial/samsung.c
@@ -544,11 +544,15 @@ static void s3c24xx_serial_pm(struct uart_port *port, unsigned int level,
 			      unsigned int old)
 {
 	struct s3c24xx_uart_port *ourport = to_ourport(port);
+	int timeout = 10000;
 
 	ourport->pm_level = level;
 
 	switch (level) {
 	case 3:
+		while (--timeout && !s3c24xx_serial_txempty_nofifo(port))
+			udelay(100);
+
 		if (!IS_ERR(ourport->baudclk))
 			clk_disable_unprepare(ourport->baudclk);
 
diff --git a/drivers/usb/class/cdc-acm.c b/drivers/usb/class/cdc-acm.c
index 331f06a..d7049c3 100644
--- a/drivers/usb/class/cdc-acm.c
+++ b/drivers/usb/class/cdc-acm.c
@@ -1169,10 +1169,11 @@ next_desc:
 	} else {
 		control_interface = usb_ifnum_to_if(usb_dev, union_header->bMasterInterface0);
 		data_interface = usb_ifnum_to_if(usb_dev, (data_interface_num = union_header->bSlaveInterface0));
-		if (!control_interface || !data_interface) {
-			dev_dbg(&intf->dev, "no interfaces\n");
-			return -ENODEV;
-		}
+	}
+
+	if (!control_interface || !data_interface) {
+		dev_dbg(&intf->dev, "no interfaces\n");
+		return -ENODEV;
 	}
 
 	if (data_interface_num != call_interface_num)
@@ -1448,6 +1449,7 @@ alloc_fail8:
 				&dev_attr_wCountryCodes);
 		device_remove_file(&acm->control->dev,
 				&dev_attr_iCountryCodeRelDate);
+		kfree(acm->country_codes);
 	}
 	device_remove_file(&acm->control->dev, &dev_attr_bmCapabilities);
 alloc_fail7:
diff --git a/drivers/xen/swiotlb-xen.c b/drivers/xen/swiotlb-xen.c
index ebd8f21..9df5d6e 100644
--- a/drivers/xen/swiotlb-xen.c
+++ b/drivers/xen/swiotlb-xen.c
@@ -96,8 +96,6 @@ static inline phys_addr_t xen_bus_to_phys(dma_addr_t baddr)
 	dma_addr_t dma = (dma_addr_t)pfn << PAGE_SHIFT;
 	phys_addr_t paddr = dma;
 
-	BUG_ON(paddr != dma); /* truncation has occurred, should never happen */
-
 	paddr |= baddr & ~PAGE_MASK;
 
 	return paddr;
@@ -447,11 +445,11 @@ static void xen_unmap_single(struct device *hwdev, dma_addr_t dev_addr,
 
 	BUG_ON(dir == DMA_NONE);
 
-	xen_dma_unmap_page(hwdev, paddr, size, dir, attrs);
+	xen_dma_unmap_page(hwdev, dev_addr, size, dir, attrs);
 
 	/* NOTE: We use dev_addr here, not paddr! */
 	if (is_xen_swiotlb_buffer(dev_addr)) {
-		swiotlb_tbl_unmap_single(hwdev, paddr, size, dir);
+		swiotlb_tbl_unmap_single(hwdev, dev_addr, size, dir);
 		return;
 	}
 
@@ -495,14 +493,14 @@ xen_swiotlb_sync_single(struct device *hwdev, dma_addr_t dev_addr,
 	BUG_ON(dir == DMA_NONE);
 
 	if (target == SYNC_FOR_CPU)
-		xen_dma_sync_single_for_cpu(hwdev, paddr, size, dir);
+		xen_dma_sync_single_for_cpu(hwdev, dev_addr, size, dir);
 
 	/* NOTE: We use dev_addr here, not paddr! */
 	if (is_xen_swiotlb_buffer(dev_addr))
 		swiotlb_tbl_sync_single(hwdev, paddr, size, dir, target);
 
 	if (target == SYNC_FOR_DEVICE)
-		xen_dma_sync_single_for_cpu(hwdev, paddr, size, dir);
+		xen_dma_sync_single_for_device(hwdev, dev_addr, size, dir);
 
 	if (dir != DMA_FROM_DEVICE)
 		return;
diff --git a/fs/btrfs/delayed-inode.c b/fs/btrfs/delayed-inode.c
index 451b00c..12e3556 100644
--- a/fs/btrfs/delayed-inode.c
+++ b/fs/btrfs/delayed-inode.c
@@ -1854,6 +1854,14 @@ int btrfs_delayed_delete_inode_ref(struct inode *inode)
 {
 	struct btrfs_delayed_node *delayed_node;
 
+	/*
+	 * we don't do delayed inode updates during log recovery because it
+	 * leads to enospc problems.  This means we also can't do
+	 * delayed inode refs
+	 */
+	if (BTRFS_I(inode)->root->fs_info->log_root_recovering)
+		return -EAGAIN;
+
 	delayed_node = btrfs_get_or_create_delayed_node(inode);
 	if (IS_ERR(delayed_node))
 		return PTR_ERR(delayed_node);
diff --git a/fs/ceph/addr.c b/fs/ceph/addr.c
index b53278c..94a85ee 100644
--- a/fs/ceph/addr.c
+++ b/fs/ceph/addr.c
@@ -676,7 +676,7 @@ static int ceph_writepages_start(struct address_space *mapping,
 	int rc = 0;
 	unsigned wsize = 1 << inode->i_blkbits;
 	struct ceph_osd_request *req = NULL;
-	int do_sync;
+	int do_sync = 0;
 	u64 truncate_size, snap_size;
 	u32 truncate_seq;
 
diff --git a/fs/ceph/mds_client.c b/fs/ceph/mds_client.c
index f4f050a..339c412 100644
--- a/fs/ceph/mds_client.c
+++ b/fs/ceph/mds_client.c
@@ -1461,15 +1461,18 @@ static void discard_cap_releases(struct ceph_mds_client *mdsc,
 
 	dout("discard_cap_releases mds%d\n", session->s_mds);
 
-	/* zero out the in-progress message */
-	msg = list_first_entry(&session->s_cap_releases,
-			       struct ceph_msg, list_head);
-	head = msg->front.iov_base;
-	num = le32_to_cpu(head->num);
-	dout("discard_cap_releases mds%d %p %u\n", session->s_mds, msg, num);
-	head->num = cpu_to_le32(0);
-	msg->front.iov_len = sizeof(*head);
-	session->s_num_cap_releases += num;
+	if (!list_empty(&session->s_cap_releases)) {
+		/* zero out the in-progress message */
+		msg = list_first_entry(&session->s_cap_releases,
+					struct ceph_msg, list_head);
+		head = msg->front.iov_base;
+		num = le32_to_cpu(head->num);
+		dout("discard_cap_releases mds%d %p %u\n",
+		     session->s_mds, msg, num);
+		head->num = cpu_to_le32(0);
+		msg->front.iov_len = sizeof(*head);
+		session->s_num_cap_releases += num;
+	}
 
 	/* requeue completed messages */
 	while (!list_empty(&session->s_cap_releases_done)) {
diff --git a/fs/fs-writeback.c b/fs/fs-writeback.c
index a163159..23a51f0 100644
--- a/fs/fs-writeback.c
+++ b/fs/fs-writeback.c
@@ -476,12 +476,28 @@ __writeback_single_inode(struct inode *inode, struct writeback_control *wbc)
 	 * write_inode()
 	 */
 	spin_lock(&inode->i_lock);
-	/* Clear I_DIRTY_PAGES if we've written out all dirty pages */
-	if (!mapping_tagged(mapping, PAGECACHE_TAG_DIRTY))
-		inode->i_state &= ~I_DIRTY_PAGES;
+
 	dirty = inode->i_state & I_DIRTY;
-	inode->i_state &= ~(I_DIRTY_SYNC | I_DIRTY_DATASYNC);
+	inode->i_state &= ~I_DIRTY;
+
+	/*
+	 * Paired with smp_mb() in __mark_inode_dirty().  This allows
+	 * __mark_inode_dirty() to test i_state without grabbing i_lock -
+	 * either they see the I_DIRTY bits cleared or we see the dirtied
+	 * inode.
+	 *
+	 * I_DIRTY_PAGES is always cleared together above even if @mapping
+	 * still has dirty pages.  The flag is reinstated after smp_mb() if
+	 * necessary.  This guarantees that either __mark_inode_dirty()
+	 * sees clear I_DIRTY_PAGES or we see PAGECACHE_TAG_DIRTY.
+	 */
+	smp_mb();
+
+	if (mapping_tagged(mapping, PAGECACHE_TAG_DIRTY))
+		inode->i_state |= I_DIRTY_PAGES;
+
 	spin_unlock(&inode->i_lock);
+
 	/* Don't write the inode if only I_DIRTY_PAGES was set */
 	if (dirty & (I_DIRTY_SYNC | I_DIRTY_DATASYNC)) {
 		int err = write_inode(inode, wbc);
@@ -1145,12 +1161,11 @@ void __mark_inode_dirty(struct inode *inode, int flags)
 	}
 
 	/*
-	 * make sure that changes are seen by all cpus before we test i_state
-	 * -- mikulas
+	 * Paired with smp_mb() in __writeback_single_inode() for the
+	 * following lockless i_state test.  See there for details.
 	 */
 	smp_mb();
 
-	/* avoid the locking if we can */
 	if ((inode->i_state & flags) == flags)
 		return;
 
diff --git a/fs/nfsd/nfs4state.c b/fs/nfsd/nfs4state.c
index 34d2a1f..daa53da 100644
--- a/fs/nfsd/nfs4state.c
+++ b/fs/nfsd/nfs4state.c
@@ -1209,15 +1209,14 @@ static int copy_cred(struct svc_cred *target, struct svc_cred *source)
 	return 0;
 }
 
-static long long
+static int
 compare_blob(const struct xdr_netobj *o1, const struct xdr_netobj *o2)
 {
-	long long res;
-
-	res = o1->len - o2->len;
-	if (res)
-		return res;
-	return (long long)memcmp(o1->data, o2->data, o1->len);
+	if (o1->len < o2->len)
+		return -1;
+	if (o1->len > o2->len)
+		return 1;
+	return memcmp(o1->data, o2->data, o1->len);
 }
 
 static int same_name(const char *n1, const char *n2)
@@ -1401,7 +1400,7 @@ add_clp_to_name_tree(struct nfs4_client *new_clp, struct rb_root *root)
 static struct nfs4_client *
 find_clp_in_name_tree(struct xdr_netobj *name, struct rb_root *root)
 {
-	long long cmp;
+	int cmp;
 	struct rb_node *node = root->rb_node;
 	struct nfs4_client *clp;
 
diff --git a/fs/nfsd/nfs4xdr.c b/fs/nfsd/nfs4xdr.c
index 8657335..dd1afa3 100644
--- a/fs/nfsd/nfs4xdr.c
+++ b/fs/nfsd/nfs4xdr.c
@@ -1809,6 +1809,9 @@ static __be32 nfsd4_encode_components_esc(char sep, char *components,
 		}
 		else
 			end++;
+		if (found_esc)
+			end = next;
+
 		str = end;
 	}
 	*pp = p;
diff --git a/fs/nilfs2/inode.c b/fs/nilfs2/inode.c
index 1e0bbae..09480c53 100644
--- a/fs/nilfs2/inode.c
+++ b/fs/nilfs2/inode.c
@@ -49,6 +49,8 @@ struct nilfs_iget_args {
 	int for_gc;
 };
 
+static int nilfs_iget_test(struct inode *inode, void *opaque);
+
 void nilfs_inode_add_blocks(struct inode *inode, int n)
 {
 	struct nilfs_root *root = NILFS_I(inode)->i_root;
@@ -347,6 +349,17 @@ const struct address_space_operations nilfs_aops = {
 	.is_partially_uptodate  = block_is_partially_uptodate,
 };
 
+static int nilfs_insert_inode_locked(struct inode *inode,
+				     struct nilfs_root *root,
+				     unsigned long ino)
+{
+	struct nilfs_iget_args args = {
+		.ino = ino, .root = root, .cno = 0, .for_gc = 0
+	};
+
+	return insert_inode_locked4(inode, ino, nilfs_iget_test, &args);
+}
+
 struct inode *nilfs_new_inode(struct inode *dir, umode_t mode)
 {
 	struct super_block *sb = dir->i_sb;
@@ -382,7 +395,7 @@ struct inode *nilfs_new_inode(struct inode *dir, umode_t mode)
 	if (S_ISREG(mode) || S_ISDIR(mode) || S_ISLNK(mode)) {
 		err = nilfs_bmap_read(ii->i_bmap, NULL);
 		if (err < 0)
-			goto failed_bmap;
+			goto failed_after_creation;
 
 		set_bit(NILFS_I_BMAP, &ii->i_state);
 		/* No lock is needed; iget() ensures it. */
@@ -398,21 +411,24 @@ struct inode *nilfs_new_inode(struct inode *dir, umode_t mode)
 	spin_lock(&nilfs->ns_next_gen_lock);
 	inode->i_generation = nilfs->ns_next_generation++;
 	spin_unlock(&nilfs->ns_next_gen_lock);
-	insert_inode_hash(inode);
+	if (nilfs_insert_inode_locked(inode, root, ino) < 0) {
+		err = -EIO;
+		goto failed_after_creation;
+	}
 
 	err = nilfs_init_acl(inode, dir);
 	if (unlikely(err))
-		goto failed_acl; /* never occur. When supporting
+		goto failed_after_creation; /* never occur. When supporting
 				    nilfs_init_acl(), proper cancellation of
 				    above jobs should be considered */
 
 	return inode;
 
- failed_acl:
- failed_bmap:
+ failed_after_creation:
 	clear_nlink(inode);
+	unlock_new_inode(inode);
 	iput(inode);  /* raw_inode will be deleted through
-			 generic_delete_inode() */
+			 nilfs_evict_inode() */
 	goto failed;
 
  failed_ifile_create_inode:
@@ -460,8 +476,8 @@ int nilfs_read_inode_common(struct inode *inode,
 	inode->i_atime.tv_nsec = le32_to_cpu(raw_inode->i_mtime_nsec);
 	inode->i_ctime.tv_nsec = le32_to_cpu(raw_inode->i_ctime_nsec);
 	inode->i_mtime.tv_nsec = le32_to_cpu(raw_inode->i_mtime_nsec);
-	if (inode->i_nlink == 0 && inode->i_mode == 0)
-		return -EINVAL; /* this inode is deleted */
+	if (inode->i_nlink == 0)
+		return -ESTALE; /* this inode is deleted */
 
 	inode->i_blocks = le64_to_cpu(raw_inode->i_blocks);
 	ii->i_flags = le32_to_cpu(raw_inode->i_flags);
diff --git a/fs/nilfs2/namei.c b/fs/nilfs2/namei.c
index 9de78f0..0f84b25 100644
--- a/fs/nilfs2/namei.c
+++ b/fs/nilfs2/namei.c
@@ -51,9 +51,11 @@ static inline int nilfs_add_nondir(struct dentry *dentry, struct inode *inode)
 	int err = nilfs_add_link(dentry, inode);
 	if (!err) {
 		d_instantiate(dentry, inode);
+		unlock_new_inode(inode);
 		return 0;
 	}
 	inode_dec_link_count(inode);
+	unlock_new_inode(inode);
 	iput(inode);
 	return err;
 }
@@ -182,6 +184,7 @@ out:
 out_fail:
 	drop_nlink(inode);
 	nilfs_mark_inode_dirty(inode);
+	unlock_new_inode(inode);
 	iput(inode);
 	goto out;
 }
@@ -201,11 +204,15 @@ static int nilfs_link(struct dentry *old_dentry, struct inode *dir,
 	inode_inc_link_count(inode);
 	ihold(inode);
 
-	err = nilfs_add_nondir(dentry, inode);
-	if (!err)
+	err = nilfs_add_link(dentry, inode);
+	if (!err) {
+		d_instantiate(dentry, inode);
 		err = nilfs_transaction_commit(dir->i_sb);
-	else
+	} else {
+		inode_dec_link_count(inode);
+		iput(inode);
 		nilfs_transaction_abort(dir->i_sb);
+	}
 
 	return err;
 }
@@ -243,6 +250,7 @@ static int nilfs_mkdir(struct inode *dir, struct dentry *dentry, umode_t mode)
 
 	nilfs_mark_inode_dirty(inode);
 	d_instantiate(dentry, inode);
+	unlock_new_inode(inode);
 out:
 	if (!err)
 		err = nilfs_transaction_commit(dir->i_sb);
@@ -255,6 +263,7 @@ out_fail:
 	drop_nlink(inode);
 	drop_nlink(inode);
 	nilfs_mark_inode_dirty(inode);
+	unlock_new_inode(inode);
 	iput(inode);
 out_dir:
 	drop_nlink(dir);
diff --git a/fs/ocfs2/aops.c b/fs/ocfs2/aops.c
index aeb44e8..bb6ee06 100644
--- a/fs/ocfs2/aops.c
+++ b/fs/ocfs2/aops.c
@@ -899,7 +899,7 @@ void ocfs2_unlock_and_free_pages(struct page **pages, int num_pages)
 	}
 }
 
-static void ocfs2_free_write_ctxt(struct ocfs2_write_ctxt *wc)
+static void ocfs2_unlock_pages(struct ocfs2_write_ctxt *wc)
 {
 	int i;
 
@@ -920,7 +920,11 @@ static void ocfs2_free_write_ctxt(struct ocfs2_write_ctxt *wc)
 		page_cache_release(wc->w_target_page);
 	}
 	ocfs2_unlock_and_free_pages(wc->w_pages, wc->w_num_pages);
+}
 
+static void ocfs2_free_write_ctxt(struct ocfs2_write_ctxt *wc)
+{
+	ocfs2_unlock_pages(wc);
 	brelse(wc->w_di_bh);
 	kfree(wc);
 }
@@ -2045,11 +2049,19 @@ out_write_size:
 	di->i_mtime_nsec = di->i_ctime_nsec = cpu_to_le32(inode->i_mtime.tv_nsec);
 	ocfs2_journal_dirty(handle, wc->w_di_bh);
 
+	/* unlock pages before dealloc since it needs acquiring j_trans_barrier
+	 * lock, or it will cause a deadlock since journal commit threads holds
+	 * this lock and will ask for the page lock when flushing the data.
+	 * put it here to preserve the unlock order.
+	 */
+	ocfs2_unlock_pages(wc);
+
 	ocfs2_commit_trans(osb, handle);
 
 	ocfs2_run_deallocs(osb, &wc->w_dealloc);
 
-	ocfs2_free_write_ctxt(wc);
+	brelse(wc->w_di_bh);
+	kfree(wc);
 
 	return copied;
 }
diff --git a/fs/ocfs2/namei.c b/fs/ocfs2/namei.c
index feed025f..b242762 100644
--- a/fs/ocfs2/namei.c
+++ b/fs/ocfs2/namei.c
@@ -94,6 +94,14 @@ static int ocfs2_create_symlink_data(struct ocfs2_super *osb,
 				     struct inode *inode,
 				     const char *symname);
 
+static int ocfs2_double_lock(struct ocfs2_super *osb,
+			     struct buffer_head **bh1,
+			     struct inode *inode1,
+			     struct buffer_head **bh2,
+			     struct inode *inode2,
+			     int rename);
+
+static void ocfs2_double_unlock(struct inode *inode1, struct inode *inode2);
 /* An orphan dir name is an 8 byte value, printed as a hex string */
 #define OCFS2_ORPHAN_NAMELEN ((int)(2 * sizeof(u64)))
 
@@ -656,8 +664,10 @@ static int ocfs2_link(struct dentry *old_dentry,
 {
 	handle_t *handle;
 	struct inode *inode = old_dentry->d_inode;
+	struct inode *old_dir = old_dentry->d_parent->d_inode;
 	int err;
 	struct buffer_head *fe_bh = NULL;
+	struct buffer_head *old_dir_bh = NULL;
 	struct buffer_head *parent_fe_bh = NULL;
 	struct ocfs2_dinode *fe = NULL;
 	struct ocfs2_super *osb = OCFS2_SB(dir->i_sb);
@@ -674,19 +684,33 @@ static int ocfs2_link(struct dentry *old_dentry,
 
 	dquot_initialize(dir);
 
-	err = ocfs2_inode_lock_nested(dir, &parent_fe_bh, 1, OI_LS_PARENT);
+	err = ocfs2_double_lock(osb, &old_dir_bh, old_dir,
+			&parent_fe_bh, dir, 0);
 	if (err < 0) {
 		if (err != -ENOENT)
 			mlog_errno(err);
 		return err;
 	}
 
+	/* make sure both dirs have bhs
+	 * get an extra ref on old_dir_bh if old==new */
+	if (!parent_fe_bh) {
+		if (old_dir_bh) {
+			parent_fe_bh = old_dir_bh;
+			get_bh(parent_fe_bh);
+		} else {
+			mlog(ML_ERROR, "%s: no old_dir_bh!\n", osb->uuid_str);
+			err = -EIO;
+			goto out;
+		}
+	}
+
 	if (!dir->i_nlink) {
 		err = -ENOENT;
 		goto out;
 	}
 
-	err = ocfs2_lookup_ino_from_name(dir, old_dentry->d_name.name,
+	err = ocfs2_lookup_ino_from_name(old_dir, old_dentry->d_name.name,
 			old_dentry->d_name.len, &old_de_ino);
 	if (err) {
 		err = -ENOENT;
@@ -779,10 +803,11 @@ out_unlock_inode:
 	ocfs2_inode_unlock(inode, 1);
 
 out:
-	ocfs2_inode_unlock(dir, 1);
+	ocfs2_double_unlock(old_dir, dir);
 
 	brelse(fe_bh);
 	brelse(parent_fe_bh);
+	brelse(old_dir_bh);
 
 	ocfs2_free_dir_lookup_result(&lookup);
 
@@ -991,14 +1016,15 @@ leave:
 }
 
 /*
- * The only place this should be used is rename!
+ * The only place this should be used is rename and link!
  * if they have the same id, then the 1st one is the only one locked.
  */
 static int ocfs2_double_lock(struct ocfs2_super *osb,
 			     struct buffer_head **bh1,
 			     struct inode *inode1,
 			     struct buffer_head **bh2,
-			     struct inode *inode2)
+			     struct inode *inode2,
+			     int rename)
 {
 	int status;
 	struct ocfs2_inode_info *oi1 = OCFS2_I(inode1);
@@ -1028,7 +1054,7 @@ static int ocfs2_double_lock(struct ocfs2_super *osb,
 		}
 		/* lock id2 */
 		status = ocfs2_inode_lock_nested(inode2, bh2, 1,
-						 OI_LS_RENAME1);
+				rename == 1 ? OI_LS_RENAME1 : OI_LS_PARENT);
 		if (status < 0) {
 			if (status != -ENOENT)
 				mlog_errno(status);
@@ -1037,7 +1063,8 @@ static int ocfs2_double_lock(struct ocfs2_super *osb,
 	}
 
 	/* lock id1 */
-	status = ocfs2_inode_lock_nested(inode1, bh1, 1, OI_LS_RENAME2);
+	status = ocfs2_inode_lock_nested(inode1, bh1, 1,
+			rename == 1 ?  OI_LS_RENAME2 : OI_LS_PARENT);
 	if (status < 0) {
 		/*
 		 * An error return must mean that no cluster locks
@@ -1137,7 +1164,7 @@ static int ocfs2_rename(struct inode *old_dir,
 
 	/* if old and new are the same, this'll just do one lock. */
 	status = ocfs2_double_lock(osb, &old_dir_bh, old_dir,
-				   &new_dir_bh, new_dir);
+				   &new_dir_bh, new_dir, 1);
 	if (status < 0) {
 		mlog_errno(status);
 		goto bail;
diff --git a/fs/pstore/ram.c b/fs/pstore/ram.c
index fa8cef2..e7d95f9 100644
--- a/fs/pstore/ram.c
+++ b/fs/pstore/ram.c
@@ -61,6 +61,11 @@ module_param(mem_size, ulong, 0400);
 MODULE_PARM_DESC(mem_size,
 		"size of reserved RAM used to store oops/panic logs");
 
+static unsigned int mem_type;
+module_param(mem_type, uint, 0600);
+MODULE_PARM_DESC(mem_type,
+		"set to 1 to try to use unbuffered memory (default 0)");
+
 static int dump_oops = 1;
 module_param(dump_oops, int, 0600);
 MODULE_PARM_DESC(dump_oops,
@@ -79,6 +84,7 @@ struct ramoops_context {
 	struct persistent_ram_zone *fprz;
 	phys_addr_t phys_addr;
 	unsigned long size;
+	unsigned int memtype;
 	size_t record_size;
 	size_t console_size;
 	size_t ftrace_size;
@@ -353,7 +359,8 @@ static int ramoops_init_przs(struct device *dev, struct ramoops_context *cxt,
 		size_t sz = cxt->record_size;
 
 		cxt->przs[i] = persistent_ram_new(*paddr, sz, 0,
-						  &cxt->ecc_info);
+						  &cxt->ecc_info,
+						  cxt->memtype);
 		if (IS_ERR(cxt->przs[i])) {
 			err = PTR_ERR(cxt->przs[i]);
 			dev_err(dev, "failed to request mem region (0x%zx@0x%llx): %d\n",
@@ -383,7 +390,7 @@ static int ramoops_init_prz(struct device *dev, struct ramoops_context *cxt,
 		return -ENOMEM;
 	}
 
-	*prz = persistent_ram_new(*paddr, sz, sig, &cxt->ecc_info);
+	*prz = persistent_ram_new(*paddr, sz, sig, &cxt->ecc_info, cxt->memtype);
 	if (IS_ERR(*prz)) {
 		int err = PTR_ERR(*prz);
 
@@ -431,6 +438,7 @@ static int ramoops_probe(struct platform_device *pdev)
 	cxt->dump_read_cnt = 0;
 	cxt->size = pdata->mem_size;
 	cxt->phys_addr = pdata->mem_address;
+	cxt->memtype = pdata->mem_type;
 	cxt->record_size = pdata->record_size;
 	cxt->console_size = pdata->console_size;
 	cxt->ftrace_size = pdata->ftrace_size;
@@ -561,6 +569,7 @@ static void ramoops_register_dummy(void)
 
 	dummy_data->mem_size = mem_size;
 	dummy_data->mem_address = mem_address;
+	dummy_data->mem_type = 0;
 	dummy_data->record_size = record_size;
 	dummy_data->console_size = ramoops_console_size;
 	dummy_data->ftrace_size = ramoops_ftrace_size;
diff --git a/fs/pstore/ram_core.c b/fs/pstore/ram_core.c
index de272d4..bda61a7 100644
--- a/fs/pstore/ram_core.c
+++ b/fs/pstore/ram_core.c
@@ -380,7 +380,8 @@ void persistent_ram_zap(struct persistent_ram_zone *prz)
 	persistent_ram_update_header_ecc(prz);
 }
 
-static void *persistent_ram_vmap(phys_addr_t start, size_t size)
+static void *persistent_ram_vmap(phys_addr_t start, size_t size,
+		unsigned int memtype)
 {
 	struct page **pages;
 	phys_addr_t page_start;
@@ -392,7 +393,10 @@ static void *persistent_ram_vmap(phys_addr_t start, size_t size)
 	page_start = start - offset_in_page(start);
 	page_count = DIV_ROUND_UP(size + offset_in_page(start), PAGE_SIZE);
 
-	prot = pgprot_noncached(PAGE_KERNEL);
+	if (memtype)
+		prot = pgprot_noncached(PAGE_KERNEL);
+	else
+		prot = pgprot_writecombine(PAGE_KERNEL);
 
 	pages = kmalloc(sizeof(struct page *) * page_count, GFP_KERNEL);
 	if (!pages) {
@@ -411,8 +415,11 @@ static void *persistent_ram_vmap(phys_addr_t start, size_t size)
 	return vaddr;
 }
 
-static void *persistent_ram_iomap(phys_addr_t start, size_t size)
+static void *persistent_ram_iomap(phys_addr_t start, size_t size,
+		unsigned int memtype)
 {
+	void *va;
+
 	if (!request_mem_region(start, size, "persistent_ram")) {
 		pr_err("request mem region (0x%llx@0x%llx) failed\n",
 			(unsigned long long)size, (unsigned long long)start);
@@ -422,19 +429,24 @@ static void *persistent_ram_iomap(phys_addr_t start, size_t size)
 	buffer_start_add = buffer_start_add_locked;
 	buffer_size_add = buffer_size_add_locked;
 
-	return ioremap(start, size);
+	if (memtype)
+		va = ioremap(start, size);
+	else
+		va = ioremap_wc(start, size);
+
+	return va;
 }
 
 static int persistent_ram_buffer_map(phys_addr_t start, phys_addr_t size,
-		struct persistent_ram_zone *prz)
+		struct persistent_ram_zone *prz, int memtype)
 {
 	prz->paddr = start;
 	prz->size = size;
 
 	if (pfn_valid(start >> PAGE_SHIFT))
-		prz->vaddr = persistent_ram_vmap(start, size);
+		prz->vaddr = persistent_ram_vmap(start, size, memtype);
 	else
-		prz->vaddr = persistent_ram_iomap(start, size);
+		prz->vaddr = persistent_ram_iomap(start, size, memtype);
 
 	if (!prz->vaddr) {
 		pr_err("%s: Failed to map 0x%llx pages at 0x%llx\n", __func__,
@@ -502,7 +514,8 @@ void persistent_ram_free(struct persistent_ram_zone *prz)
 }
 
 struct persistent_ram_zone *persistent_ram_new(phys_addr_t start, size_t size,
-			u32 sig, struct persistent_ram_ecc_info *ecc_info)
+			u32 sig, struct persistent_ram_ecc_info *ecc_info,
+			unsigned int memtype)
 {
 	struct persistent_ram_zone *prz;
 	int ret = -ENOMEM;
@@ -513,7 +526,7 @@ struct persistent_ram_zone *persistent_ram_new(phys_addr_t start, size_t size,
 		goto err;
 	}
 
-	ret = persistent_ram_buffer_map(start, size, prz);
+	ret = persistent_ram_buffer_map(start, size, prz, memtype);
 	if (ret)
 		goto err;
 
diff --git a/include/linux/mm.h b/include/linux/mm.h
index d5039da..46b8ab5 100644
--- a/include/linux/mm.h
+++ b/include/linux/mm.h
@@ -1866,7 +1866,7 @@ extern int expand_downwards(struct vm_area_struct *vma,
 #if VM_GROWSUP
 extern int expand_upwards(struct vm_area_struct *vma, unsigned long address);
 #else
-  #define expand_upwards(vma, address) do { } while (0)
+  #define expand_upwards(vma, address) (0)
 #endif
 
 /* Look up the first VMA which satisfies  addr < vm_end,  NULL if none. */
diff --git a/include/linux/pstore_ram.h b/include/linux/pstore_ram.h
index 9974975..4af3fdc 100644
--- a/include/linux/pstore_ram.h
+++ b/include/linux/pstore_ram.h
@@ -53,7 +53,8 @@ struct persistent_ram_zone {
 };
 
 struct persistent_ram_zone *persistent_ram_new(phys_addr_t start, size_t size,
-			u32 sig, struct persistent_ram_ecc_info *ecc_info);
+			u32 sig, struct persistent_ram_ecc_info *ecc_info,
+			unsigned int memtype);
 void persistent_ram_free(struct persistent_ram_zone *prz);
 void persistent_ram_zap(struct persistent_ram_zone *prz);
 
@@ -76,6 +77,7 @@ ssize_t persistent_ram_ecc_string(struct persistent_ram_zone *prz,
 struct ramoops_platform_data {
 	unsigned long	mem_size;
 	unsigned long	mem_address;
+	unsigned int	mem_type;
 	unsigned long	record_size;
 	unsigned long	console_size;
 	unsigned long	ftrace_size;
diff --git a/include/trace/events/sched.h b/include/trace/events/sched.h
index 67e1bbf..dc7bb01 100644
--- a/include/trace/events/sched.h
+++ b/include/trace/events/sched.h
@@ -100,7 +100,7 @@ static inline long __trace_sched_switch_state(struct task_struct *p)
 	/*
 	 * For all intents and purposes a preempted task is a running task.
 	 */
-	if (task_preempt_count(p) & PREEMPT_ACTIVE)
+	if (preempt_count() & PREEMPT_ACTIVE)
 		state = TASK_RUNNING | TASK_STATE_MAX;
 #endif
 
diff --git a/kernel/events/core.c b/kernel/events/core.c
index 4bbb27a..69cffb4 100644
--- a/kernel/events/core.c
+++ b/kernel/events/core.c
@@ -7240,11 +7240,11 @@ SYSCALL_DEFINE5(perf_event_open,
 
 	if (move_group) {
 		synchronize_rcu();
-		perf_install_in_context(ctx, group_leader, event->cpu);
+		perf_install_in_context(ctx, group_leader, group_leader->cpu);
 		get_ctx(ctx);
 		list_for_each_entry(sibling, &group_leader->sibling_list,
 				    group_entry) {
-			perf_install_in_context(ctx, sibling, event->cpu);
+			perf_install_in_context(ctx, sibling, sibling->cpu);
 			get_ctx(ctx);
 		}
 	}
diff --git a/kernel/sched/deadline.c b/kernel/sched/deadline.c
index 37dac98..8d3c5dd 100644
--- a/kernel/sched/deadline.c
+++ b/kernel/sched/deadline.c
@@ -550,24 +550,7 @@ void init_dl_task_timer(struct sched_dl_entity *dl_se)
 static
 int dl_runtime_exceeded(struct rq *rq, struct sched_dl_entity *dl_se)
 {
-	int dmiss = dl_time_before(dl_se->deadline, rq_clock(rq));
-	int rorun = dl_se->runtime <= 0;
-
-	if (!rorun && !dmiss)
-		return 0;
-
-	/*
-	 * If we are beyond our current deadline and we are still
-	 * executing, then we have already used some of the runtime of
-	 * the next instance. Thus, if we do not account that, we are
-	 * stealing bandwidth from the system at each deadline miss!
-	 */
-	if (dmiss) {
-		dl_se->runtime = rorun ? dl_se->runtime : 0;
-		dl_se->runtime -= rq_clock(rq) - dl_se->deadline;
-	}
-
-	return 1;
+	return (dl_se->runtime <= 0);
 }
 
 extern bool sched_rt_bandwidth_account(struct rt_rq *rt_rq);
@@ -806,10 +789,10 @@ enqueue_dl_entity(struct sched_dl_entity *dl_se,
 	 * parameters of the task might need updating. Otherwise,
 	 * we want a replenishment of its runtime.
 	 */
-	if (!dl_se->dl_new && flags & ENQUEUE_REPLENISH)
-		replenish_dl_entity(dl_se, pi_se);
-	else
+	if (dl_se->dl_new || flags & ENQUEUE_WAKEUP)
 		update_dl_entity(dl_se, pi_se);
+	else if (flags & ENQUEUE_REPLENISH)
+		replenish_dl_entity(dl_se, pi_se);
 
 	__enqueue_dl_entity(dl_se);
 }
diff --git a/mm/memory.c b/mm/memory.c
index 48d7365..924429e 100644
--- a/mm/memory.c
+++ b/mm/memory.c
@@ -3204,7 +3204,7 @@ static inline int check_stack_guard_page(struct vm_area_struct *vma, unsigned lo
 		if (prev && prev->vm_end == address)
 			return prev->vm_flags & VM_GROWSDOWN ? 0 : -ENOMEM;
 
-		expand_downwards(vma, address - PAGE_SIZE);
+		return expand_downwards(vma, address - PAGE_SIZE);
 	}
 	if ((vma->vm_flags & VM_GROWSUP) && address + PAGE_SIZE == vma->vm_end) {
 		struct vm_area_struct *next = vma->vm_next;
@@ -3213,7 +3213,7 @@ static inline int check_stack_guard_page(struct vm_area_struct *vma, unsigned lo
 		if (next && next->vm_start == address + PAGE_SIZE)
 			return next->vm_flags & VM_GROWSUP ? 0 : -ENOMEM;
 
-		expand_upwards(vma, address + PAGE_SIZE);
+		return expand_upwards(vma, address + PAGE_SIZE);
 	}
 	return 0;
 }
diff --git a/mm/mmap.c b/mm/mmap.c
index b91ac80..085bcd8 100644
--- a/mm/mmap.c
+++ b/mm/mmap.c
@@ -2058,14 +2058,17 @@ static int acct_stack_growth(struct vm_area_struct *vma, unsigned long size, uns
 {
 	struct mm_struct *mm = vma->vm_mm;
 	struct rlimit *rlim = current->signal->rlim;
-	unsigned long new_start;
+	unsigned long new_start, actual_size;
 
 	/* address space limit tests */
 	if (!may_expand_vm(mm, grow))
 		return -ENOMEM;
 
 	/* Stack limit test */
-	if (size > ACCESS_ONCE(rlim[RLIMIT_STACK].rlim_cur))
+	actual_size = size;
+	if (size && (vma->vm_flags & (VM_GROWSUP | VM_GROWSDOWN)))
+		actual_size -= PAGE_SIZE;
+	if (actual_size > ACCESS_ONCE(rlim[RLIMIT_STACK].rlim_cur))
 		return -ENOMEM;
 
 	/* mlock limit tests */
diff --git a/mm/vmscan.c b/mm/vmscan.c
index deb139e..be6a689 100644
--- a/mm/vmscan.c
+++ b/mm/vmscan.c
@@ -2860,18 +2860,20 @@ static bool prepare_kswapd_sleep(pg_data_t *pgdat, int order, long remaining,
 		return false;
 
 	/*
-	 * There is a potential race between when kswapd checks its watermarks
-	 * and a process gets throttled. There is also a potential race if
-	 * processes get throttled, kswapd wakes, a large process exits therby
-	 * balancing the zones that causes kswapd to miss a wakeup. If kswapd
-	 * is going to sleep, no process should be sleeping on pfmemalloc_wait
-	 * so wake them now if necessary. If necessary, processes will wake
-	 * kswapd and get throttled again
+	 * The throttled processes are normally woken up in balance_pgdat() as
+	 * soon as pfmemalloc_watermark_ok() is true. But there is a potential
+	 * race between when kswapd checks the watermarks and a process gets
+	 * throttled. There is also a potential race if processes get
+	 * throttled, kswapd wakes, a large process exits thereby balancing the
+	 * zones, which causes kswapd to exit balance_pgdat() before reaching
+	 * the wake up checks. If kswapd is going to sleep, no process should
+	 * be sleeping on pfmemalloc_wait, so wake them now if necessary. If
+	 * the wake up is premature, processes will wake kswapd and get
+	 * throttled again. The difference from wake ups in balance_pgdat() is
+	 * that here we are under prepare_to_wait().
 	 */
-	if (waitqueue_active(&pgdat->pfmemalloc_wait)) {
-		wake_up(&pgdat->pfmemalloc_wait);
-		return false;
-	}
+	if (waitqueue_active(&pgdat->pfmemalloc_wait))
+		wake_up_all(&pgdat->pfmemalloc_wait);
 
 	return pgdat_balanced(pgdat, order, classzone_idx);
 }
diff --git a/scripts/kernel-doc b/scripts/kernel-doc
index da058da..2438cc3 100755
--- a/scripts/kernel-doc
+++ b/scripts/kernel-doc
@@ -1753,7 +1753,7 @@ sub dump_struct($$) {
 	# strip kmemcheck_bitfield_{begin,end}.*;
 	$members =~ s/kmemcheck_bitfield_.*?;//gos;
 	# strip attributes
-	$members =~ s/__aligned\s*\(.+\)//gos;
+	$members =~ s/__aligned\s*\([^;]*\)//gos;
 
 	create_parameterlist($members, ';', $file);
 	check_sections($file, $declaration_name, "struct", $sectcheck, $struct_actual, $nested);
diff --git a/sound/pci/hda/hda_codec.c b/sound/pci/hda/hda_codec.c
index dafcf82..f6e5c4e 100644
--- a/sound/pci/hda/hda_codec.c
+++ b/sound/pci/hda/hda_codec.c
@@ -338,8 +338,10 @@ int snd_hda_get_sub_nodes(struct hda_codec *codec, hda_nid_t nid,
 	unsigned int parm;
 
 	parm = snd_hda_param_read(codec, nid, AC_PAR_NODE_COUNT);
-	if (parm == -1)
+	if (parm == -1) {
+		*start_id = 0;
 		return 0;
+	}
 	*start_id = (parm >> 16) & 0x7fff;
 	return (int)(parm & 0x7fff);
 }
diff --git a/sound/pci/hda/patch_sigmatel.c b/sound/pci/hda/patch_sigmatel.c
index 15270a2..12f28d7 100644
--- a/sound/pci/hda/patch_sigmatel.c
+++ b/sound/pci/hda/patch_sigmatel.c
@@ -593,9 +593,9 @@ static void stac_store_hints(struct hda_codec *codec)
 			spec->gpio_mask;
 	}
 	if (get_int_hint(codec, "gpio_dir", &spec->gpio_dir))
-		spec->gpio_mask &= spec->gpio_mask;
-	if (get_int_hint(codec, "gpio_data", &spec->gpio_data))
 		spec->gpio_dir &= spec->gpio_mask;
+	if (get_int_hint(codec, "gpio_data", &spec->gpio_data))
+		spec->gpio_data &= spec->gpio_mask;
 	if (get_int_hint(codec, "eapd_mask", &spec->eapd_mask))
 		spec->eapd_mask &= spec->gpio_mask;
 	if (get_int_hint(codec, "gpio_mute", &spec->gpio_mute))
diff --git a/sound/soc/codecs/max98090.c b/sound/soc/codecs/max98090.c
index ddfb0fd..9dd260f 100644
--- a/sound/soc/codecs/max98090.c
+++ b/sound/soc/codecs/max98090.c
@@ -1378,8 +1378,8 @@ static const struct snd_soc_dapm_route max98090_dapm_routes[] = {
 	{"STENL Mux", "Sidetone Left", "DMICL"},
 	{"STENR Mux", "Sidetone Right", "ADCR"},
 	{"STENR Mux", "Sidetone Right", "DMICR"},
-	{"DACL", "NULL", "STENL Mux"},
-	{"DACR", "NULL", "STENL Mux"},
+	{"DACL", NULL, "STENL Mux"},
+	{"DACR", NULL, "STENL Mux"},
 
 	{"AIFINL", NULL, "SHDN"},
 	{"AIFINR", NULL, "SHDN"},
diff --git a/sound/soc/codecs/sigmadsp.c b/sound/soc/codecs/sigmadsp.c
index 4068f24..bb3878c 100644
--- a/sound/soc/codecs/sigmadsp.c
+++ b/sound/soc/codecs/sigmadsp.c
@@ -176,6 +176,13 @@ static int _process_sigma_firmware(struct device *dev,
 		goto done;
 	}
 
+	if (ssfw_head->version != 1) {
+		dev_err(dev,
+			"Failed to load firmware: Invalid version %d. Supported firmware versions: 1\n",
+			ssfw_head->version);
+		goto done;
+	}
+
 	crc = crc32(0, fw->data + sizeof(*ssfw_head),
 			fw->size - sizeof(*ssfw_head));
 	pr_debug("%s: crc=%x\n", __func__, crc);
diff --git a/sound/soc/dwc/designware_i2s.c b/sound/soc/dwc/designware_i2s.c
index 25c31f1..2f63575 100644
--- a/sound/soc/dwc/designware_i2s.c
+++ b/sound/soc/dwc/designware_i2s.c
@@ -263,6 +263,19 @@ static void dw_i2s_shutdown(struct snd_pcm_substream *substream,
 	snd_soc_dai_set_dma_data(dai, substream, NULL);
 }
 
+static int dw_i2s_prepare(struct snd_pcm_substream *substream,
+			  struct snd_soc_dai *dai)
+{
+	struct dw_i2s_dev *dev = snd_soc_dai_get_drvdata(dai);
+
+	if (substream->stream == SNDRV_PCM_STREAM_PLAYBACK)
+		i2s_write_reg(dev->i2s_base, TXFFR, 1);
+	else
+		i2s_write_reg(dev->i2s_base, RXFFR, 1);
+
+	return 0;
+}
+
 static int dw_i2s_trigger(struct snd_pcm_substream *substream,
 		int cmd, struct snd_soc_dai *dai)
 {
@@ -294,6 +307,7 @@ static struct snd_soc_dai_ops dw_i2s_dai_ops = {
 	.startup	= dw_i2s_startup,
 	.shutdown	= dw_i2s_shutdown,
 	.hw_params	= dw_i2s_hw_params,
+	.prepare	= dw_i2s_prepare,
 	.trigger	= dw_i2s_trigger,
 };
 
diff --git a/sound/usb/mixer_maps.c b/sound/usb/mixer_maps.c
index d1d72ff..621bc9e 100644
--- a/sound/usb/mixer_maps.c
+++ b/sound/usb/mixer_maps.c
@@ -328,8 +328,11 @@ static struct usbmix_name_map gamecom780_map[] = {
 	{}
 };
 
-static const struct usbmix_name_map kef_x300a_map[] = {
-	{ 10, NULL }, /* firmware locks up (?) when we try to access this FU */
+/* some (all?) SCMS USB3318 devices are affected by a firmware lock up
+ * when anything attempts to access FU 10 (control)
+ */
+static const struct usbmix_name_map scms_usb3318_map[] = {
+	{ 10, NULL },
 	{ 0 }
 };
 
@@ -425,8 +428,14 @@ static struct usbmix_ctl_map usbmix_ctl_maps[] = {
 		.map = ebox44_map,
 	},
 	{
+		/* KEF X300A */
 		.id = USB_ID(0x27ac, 0x1000),
-		.map = kef_x300a_map,
+		.map = scms_usb3318_map,
+	},
+	{
+		/* Arcam rPAC */
+		.id = USB_ID(0x25c4, 0x0003),
+		.map = scms_usb3318_map,
 	},
 	{ 0 } /* terminator */
 };
diff --git a/tools/perf/util/hist.h b/tools/perf/util/hist.h
index a59743f..0001c9a 100644
--- a/tools/perf/util/hist.h
+++ b/tools/perf/util/hist.h
@@ -36,6 +36,7 @@ struct events_stats {
 	u32 nr_invalid_chains;
 	u32 nr_unknown_id;
 	u32 nr_unprocessable_samples;
+	u32 nr_unordered_events;
 };
 
 enum hist_column {
diff --git a/tools/perf/util/session.c b/tools/perf/util/session.c
index 5da6ce7..c1f20e9 100644
--- a/tools/perf/util/session.c
+++ b/tools/perf/util/session.c
@@ -638,8 +638,7 @@ int perf_session_queue_event(struct perf_session *s, union perf_event *event,
 		return -ETIME;
 
 	if (timestamp < s->ordered_samples.last_flush) {
-		printf("Warning: Timestamp below last timeslice flush\n");
-		return -EINVAL;
+		s->stats.nr_unordered_events++;
 	}
 
 	if (!list_empty(sc)) {
@@ -1135,6 +1134,8 @@ static void perf_session__warn_about_errors(const struct perf_session *session,
 			    "Do you have a KVM guest running and not using 'perf kvm'?\n",
 			    session->stats.nr_unprocessable_samples);
 	}
+	if (session->stats.nr_unordered_events != 0)
+		ui__warning("%u out of order events recorded.\n", session->stats.nr_unordered_events);
 }
 
 volatile int session_done;
