From 5a59cc60d323c3b50f3afa4b9949f97f2bd05ed0 Mon Sep 17 00:00:00 2001
From: fritsch <Peter.Fruehberger@gmail.com>
Date: Thu, 11 Jun 2015 11:02:01 +0300
Subject: [PATCH] i915_irq: enable legacy turbo

---
 drivers/gpu/drm/i915/i915_irq.c | 7 +------
 1 file changed, 1 insertion(+), 6 deletions(-)

diff --git a/drivers/gpu/drm/i915/i915_irq.c b/drivers/gpu/drm/i915/i915_irq.c
index 6d49443..2367009 100644
--- a/drivers/gpu/drm/i915/i915_irq.c
+++ b/drivers/gpu/drm/i915/i915_irq.c
@@ -4235,12 +4235,7 @@ void intel_irq_init(struct drm_i915_private *dev_priv)
 	INIT_WORK(&dev_priv->rps.work, gen6_pm_rps_work);
 	INIT_WORK(&dev_priv->l3_parity.error_work, ivybridge_parity_work);
 
-	/* Let's track the enabled rps events */
-	if (IS_VALLEYVIEW(dev_priv) && !IS_CHERRYVIEW(dev_priv))
-		/* WaGsvRC0ResidencyMethod:vlv */
-		dev_priv->pm_rps_events = GEN6_PM_RP_DOWN_EI_EXPIRED | GEN6_PM_RP_UP_EI_EXPIRED;
-	else
-		dev_priv->pm_rps_events = GEN6_PM_RPS_EVENTS;
+	dev_priv->pm_rps_events = GEN6_PM_RPS_EVENTS;
 
 	INIT_DELAYED_WORK(&dev_priv->gpu_error.hangcheck_work,
 			  i915_hangcheck_elapsed);
-- 
2.1.4

