diff -urN a/boards.cfg b/boards.cfg
--- a/boards.cfg	2014-04-13 01:27:26.000000000 +0200
+++ b/boards.cfg	2014-08-23 16:58:28.000000000 +0200
@@ -301,6 +301,7 @@
 Active  arm         armv7          mx6         freescale       mx6qsabreauto       mx6qsabreauto                        mx6qsabreauto:IMX_CONFIG=board/freescale/mx6qsabreauto/imximage.cfg,MX6Q                                                          Fabio Estevam <fabio.estevam@freescale.com>
 Active  arm         armv7          mx6         freescale       mx6sabresd          mx6dlsabresd                         mx6sabresd:IMX_CONFIG=board/boundary/nitrogen6x/nitrogen6dl.cfg,MX6DL                                                             Fabio Estevam <fabio.estevam@freescale.com>
 Active  arm         armv7          mx6         freescale       mx6sabresd          mx6qsabresd                          mx6sabresd:IMX_CONFIG=board/freescale/imx/ddr/mx6q_4x_mt41j128.cfg,MX6Q                                                           Fabio Estevam <fabio.estevam@freescale.com>
+Active  arm         armv7          mx6         freescale       mx6sabresd          matrix                               mx6sabresd:IMX_CONFIG=board/boundary/nitrogen6x/nitrogen6q2g.cfg,MX6Q,DDR_MB=2048                                                 -
 Active  arm         armv7          mx6         freescale       mx6slevk            mx6slevk                             mx6slevk:IMX_CONFIG=board/freescale/mx6slevk/imximage.cfg,MX6SL                                                                   Fabio Estevam <fabio.estevam@freescale.com>
 Active  arm         armv7          mx6         freescale       titanium            titanium                             titanium:IMX_CONFIG=board/freescale/titanium/imximage.cfg                                                                         Stefan Roese <sr@denx.de>
 Active  arm         armv7          mx6         solidrun        mx6_c1              mx6_c1solo                           mx6_c1:IMX_CONFIG=board/solidrun/mx6_c1/mx6_c1solo.cfg,MX6S,DDR_MB=512
diff -urN a/include/configs/mx6sabresd.h b/include/configs/mx6sabresd.h
--- a/include/configs/mx6sabresd.h	2014-04-13 01:27:26.000000000 +0200
+++ b/include/configs/mx6sabresd.h	2014-08-23 17:01:13.000000000 +0200
@@ -17,17 +17,17 @@
 #define CONFIG_CONSOLE_DEV		"ttymxc0"
 #define CONFIG_MMCROOT			"/dev/mmcblk1p2"
 #if defined(CONFIG_MX6Q)
-#define CONFIG_DEFAULT_FDT_FILE	"imx6q-sabresd.dtb"
+#define CONFIG_DEFAULT_FDT_FILE	"imx6q-tbs2910.dtb"
 #elif defined(CONFIG_MX6DL)
 #define CONFIG_DEFAULT_FDT_FILE	"imx6dl-sabresd.dtb"
 #endif
-#define PHYS_SDRAM_SIZE		(1u * 1024 * 1024 * 1024)
+#define PHYS_SDRAM_SIZE		(2u * 1024 * 1024 * 1024)
 
 #include "mx6sabre_common.h"
 
 #define CONFIG_SYS_FSL_USDHC_NUM	3
 #if defined(CONFIG_ENV_IS_IN_MMC)
-#define CONFIG_SYS_MMC_ENV_DEV		1	/* SDHC3 */
+#define CONFIG_SYS_MMC_ENV_DEV		2	/* eMMC/uSDHC4 */ 
 #endif
 
 /* Framebuffer */

diff -urN a/include/configs/mx6sabre_common.h b/include/configs/mx6sabre_common.h
--- a/include/configs/mx6sabre_common.h	2014-03-20 18:04:26.942867502 -0600
+++ b/include/configs/mx6sabre_common.h	2014-03-20 18:04:49.350866727 -0600
@@ -61,7 +61,7 @@
 #define IMX_FEC_BASE			ENET_BASE_ADDR
 #define CONFIG_FEC_XCV_TYPE		RGMII
 #define CONFIG_ETHPRIME			"FEC"
-#define CONFIG_FEC_MXC_PHYADDR		1
+#define CONFIG_FEC_MXC_PHYADDR		4
 
 #define CONFIG_PHYLIB
 #define CONFIG_PHY_ATHEROS
 
