diff --git a/Documentation/devicetree/bindings/interrupt-controller/interrupts.txt b/Documentation/devicetree/bindings/interrupt-controller/interrupts.txt
index 1486497a24c1..ce6a1a072028 100644
--- a/Documentation/devicetree/bindings/interrupt-controller/interrupts.txt
+++ b/Documentation/devicetree/bindings/interrupt-controller/interrupts.txt
@@ -4,11 +4,13 @@ Specifying interrupt information for devices
 1) Interrupt client nodes
 -------------------------
 
-Nodes that describe devices which generate interrupts must contain an either an
-"interrupts" property or an "interrupts-extended" property. These properties
-contain a list of interrupt specifiers, one per output interrupt. The format of
-the interrupt specifier is determined by the interrupt controller to which the
-interrupts are routed; see section 2 below for details.
+Nodes that describe devices which generate interrupts must contain an
+"interrupts" property, an "interrupts-extended" property, or both. If both are
+present, the latter should take precedence; the former may be provided simply
+for compatibility with software that does not recognize the latter. These
+properties contain a list of interrupt specifiers, one per output interrupt. The
+format of the interrupt specifier is determined by the interrupt controller to
+which the interrupts are routed; see section 2 below for details.
 
   Example:
 	interrupt-parent = <&intc1>;
diff --git a/Makefile b/Makefile
index b1746b486646..beb7e6f0803b 100644
--- a/Makefile
+++ b/Makefile
@@ -1,6 +1,6 @@
 VERSION = 3
 PATCHLEVEL = 14
-SUBLEVEL = 19
+SUBLEVEL = 20
 EXTRAVERSION =
 NAME = Remembering Coco
 
diff --git a/arch/arm/boot/dts/dra7-evm.dts b/arch/arm/boot/dts/dra7-evm.dts
index 904dcf5973f3..9381754b35cc 100644
--- a/arch/arm/boot/dts/dra7-evm.dts
+++ b/arch/arm/boot/dts/dra7-evm.dts
@@ -50,13 +50,13 @@
 
 	mcspi1_pins: pinmux_mcspi1_pins {
 		pinctrl-single,pins = <
-			0x3a4 (PIN_INPUT | MUX_MODE0) /* spi2_clk */
-			0x3a8 (PIN_INPUT | MUX_MODE0) /* spi2_d1 */
-			0x3ac (PIN_INPUT | MUX_MODE0) /* spi2_d0 */
-			0x3b0 (PIN_INPUT_SLEW | MUX_MODE0) /* spi2_cs0 */
-			0x3b4 (PIN_INPUT_SLEW | MUX_MODE0) /* spi2_cs1 */
-			0x3b8 (PIN_INPUT_SLEW | MUX_MODE6) /* spi2_cs2 */
-			0x3bc (PIN_INPUT_SLEW | MUX_MODE6) /* spi2_cs3 */
+			0x3a4 (PIN_INPUT | MUX_MODE0) /* spi1_sclk */
+			0x3a8 (PIN_INPUT | MUX_MODE0) /* spi1_d1 */
+			0x3ac (PIN_INPUT | MUX_MODE0) /* spi1_d0 */
+			0x3b0 (PIN_INPUT_SLEW | MUX_MODE0) /* spi1_cs0 */
+			0x3b4 (PIN_INPUT_SLEW | MUX_MODE0) /* spi1_cs1 */
+			0x3b8 (PIN_INPUT_SLEW | MUX_MODE6) /* spi1_cs2.hdmi1_hpd */
+			0x3bc (PIN_INPUT_SLEW | MUX_MODE6) /* spi1_cs3.hdmi1_cec */
 		>;
 	};
 
diff --git a/arch/arm/boot/dts/dra7.dtsi b/arch/arm/boot/dts/dra7.dtsi
index 1fd75aa4639d..767f0e376f4d 100644
--- a/arch/arm/boot/dts/dra7.dtsi
+++ b/arch/arm/boot/dts/dra7.dtsi
@@ -178,7 +178,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 		};
 
 		gpio2: gpio@48055000 {
@@ -189,7 +189,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 		};
 
 		gpio3: gpio@48057000 {
@@ -200,7 +200,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 		};
 
 		gpio4: gpio@48059000 {
@@ -211,7 +211,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 		};
 
 		gpio5: gpio@4805b000 {
@@ -222,7 +222,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 		};
 
 		gpio6: gpio@4805d000 {
@@ -233,7 +233,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 		};
 
 		gpio7: gpio@48051000 {
@@ -244,7 +244,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 		};
 
 		gpio8: gpio@48053000 {
@@ -255,7 +255,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 		};
 
 		uart1: serial@4806a000 {
diff --git a/arch/arm/include/asm/tls.h b/arch/arm/include/asm/tls.h
index 83259b873333..5f833f7adba1 100644
--- a/arch/arm/include/asm/tls.h
+++ b/arch/arm/include/asm/tls.h
@@ -1,6 +1,9 @@
 #ifndef __ASMARM_TLS_H
 #define __ASMARM_TLS_H
 
+#include <linux/compiler.h>
+#include <asm/thread_info.h>
+
 #ifdef __ASSEMBLY__
 #include <asm/asm-offsets.h>
 	.macro switch_tls_none, base, tp, tpuser, tmp1, tmp2
@@ -50,6 +53,49 @@
 #endif
 
 #ifndef __ASSEMBLY__
+
+static inline void set_tls(unsigned long val)
+{
+	struct thread_info *thread;
+
+	thread = current_thread_info();
+
+	thread->tp_value[0] = val;
+
+	/*
+	 * This code runs with preemption enabled and therefore must
+	 * be reentrant with respect to switch_tls.
+	 *
+	 * We need to ensure ordering between the shadow state and the
+	 * hardware state, so that we don't corrupt the hardware state
+	 * with a stale shadow state during context switch.
+	 *
+	 * If we're preempted here, switch_tls will load TPIDRURO from
+	 * thread_info upon resuming execution and the following mcr
+	 * is merely redundant.
+	 */
+	barrier();
+
+	if (!tls_emu) {
+		if (has_tls_reg) {
+			asm("mcr p15, 0, %0, c13, c0, 3"
+			    : : "r" (val));
+		} else {
+#ifdef CONFIG_KUSER_HELPERS
+			/*
+			 * User space must never try to access this
+			 * directly.  Expect your app to break
+			 * eventually if you do so.  The user helper
+			 * at 0xffff0fe0 must be used instead.  (see
+			 * entry-armv.S for details)
+			 */
+			*((unsigned int *)0xffff0ff0) = val;
+#endif
+		}
+
+	}
+}
+
 static inline unsigned long get_tpuser(void)
 {
 	unsigned long reg = 0;
@@ -59,5 +105,23 @@ static inline unsigned long get_tpuser(void)
 
 	return reg;
 }
+
+static inline void set_tpuser(unsigned long val)
+{
+	/* Since TPIDRURW is fully context-switched (unlike TPIDRURO),
+	 * we need not update thread_info.
+	 */
+	if (has_tls_reg && !tls_emu) {
+		asm("mcr p15, 0, %0, c13, c0, 2"
+		    : : "r" (val));
+	}
+}
+
+static inline void flush_tls(void)
+{
+	set_tls(0);
+	set_tpuser(0);
+}
+
 #endif
 #endif	/* __ASMARM_TLS_H */
diff --git a/arch/arm/kernel/irq.c b/arch/arm/kernel/irq.c
index 9723d17b8f38..1e782bdeee49 100644
--- a/arch/arm/kernel/irq.c
+++ b/arch/arm/kernel/irq.c
@@ -163,7 +163,7 @@ static bool migrate_one_irq(struct irq_desc *desc)
 	c = irq_data_get_irq_chip(d);
 	if (!c->irq_set_affinity)
 		pr_debug("IRQ%u: unable to set affinity\n", d->irq);
-	else if (c->irq_set_affinity(d, affinity, true) == IRQ_SET_MASK_OK && ret)
+	else if (c->irq_set_affinity(d, affinity, false) == IRQ_SET_MASK_OK && ret)
 		cpumask_copy(d->affinity, affinity);
 
 	return ret;
diff --git a/arch/arm/kernel/process.c b/arch/arm/kernel/process.c
index 92f7b15dd221..5f6e650ec9ab 100644
--- a/arch/arm/kernel/process.c
+++ b/arch/arm/kernel/process.c
@@ -334,6 +334,8 @@ void flush_thread(void)
 	memset(&tsk->thread.debug, 0, sizeof(struct debug_info));
 	memset(&thread->fpstate, 0, sizeof(union fp_state));
 
+	flush_tls();
+
 	thread_notify(THREAD_NOTIFY_FLUSH, thread);
 }
 
diff --git a/arch/arm/kernel/thumbee.c b/arch/arm/kernel/thumbee.c
index 7b8403b76666..80f0d69205e7 100644
--- a/arch/arm/kernel/thumbee.c
+++ b/arch/arm/kernel/thumbee.c
@@ -45,7 +45,7 @@ static int thumbee_notifier(struct notifier_block *self, unsigned long cmd, void
 
 	switch (cmd) {
 	case THREAD_NOTIFY_FLUSH:
-		thread->thumbee_state = 0;
+		teehbr_write(0);
 		break;
 	case THREAD_NOTIFY_SWITCH:
 		current_thread_info()->thumbee_state = teehbr_read();
diff --git a/arch/arm/kernel/traps.c b/arch/arm/kernel/traps.c
index 172ee18ff124..9265b8bb529a 100644
--- a/arch/arm/kernel/traps.c
+++ b/arch/arm/kernel/traps.c
@@ -578,7 +578,6 @@ do_cache_op(unsigned long start, unsigned long end, int flags)
 #define NR(x) ((__ARM_NR_##x) - __ARM_NR_BASE)
 asmlinkage int arm_syscall(int no, struct pt_regs *regs)
 {
-	struct thread_info *thread = current_thread_info();
 	siginfo_t info;
 
 	if ((no >> 16) != (__ARM_NR_BASE>> 16))
@@ -629,21 +628,7 @@ asmlinkage int arm_syscall(int no, struct pt_regs *regs)
 		return regs->ARM_r0;
 
 	case NR(set_tls):
-		thread->tp_value[0] = regs->ARM_r0;
-		if (tls_emu)
-			return 0;
-		if (has_tls_reg) {
-			asm ("mcr p15, 0, %0, c13, c0, 3"
-				: : "r" (regs->ARM_r0));
-		} else {
-			/*
-			 * User space must never try to access this directly.
-			 * Expect your app to break eventually if you do so.
-			 * The user helper at 0xffff0fe0 must be used instead.
-			 * (see entry-armv.S for details)
-			 */
-			*((unsigned int *)0xffff0ff0) = regs->ARM_r0;
-		}
+		set_tls(regs->ARM_r0);
 		return 0;
 
 #ifdef CONFIG_NEEDS_SYSCALL_FOR_CMPXCHG
diff --git a/arch/arm/kvm/handle_exit.c b/arch/arm/kvm/handle_exit.c
index 0de91fc6de0f..ec4fa868a7ba 100644
--- a/arch/arm/kvm/handle_exit.c
+++ b/arch/arm/kvm/handle_exit.c
@@ -89,6 +89,8 @@ static int kvm_handle_wfx(struct kvm_vcpu *vcpu, struct kvm_run *run)
 	else
 		kvm_vcpu_block(vcpu);
 
+	kvm_skip_instr(vcpu, kvm_vcpu_trap_il_is32bit(vcpu));
+
 	return 1;
 }
 
diff --git a/arch/arm/kvm/init.S b/arch/arm/kvm/init.S
index 1b9844d369cc..ee4f7447a1d3 100644
--- a/arch/arm/kvm/init.S
+++ b/arch/arm/kvm/init.S
@@ -98,6 +98,10 @@ __do_hyp_init:
 	mrc	p15, 0, r0, c10, c2, 1
 	mcr	p15, 4, r0, c10, c2, 1
 
+	@ Invalidate the stale TLBs from Bootloader
+	mcr	p15, 4, r0, c8, c7, 0	@ TLBIALLH
+	dsb	ish
+
 	@ Set the HSCTLR to:
 	@  - ARM/THUMB exceptions: Kernel config (Thumb-2 kernel)
 	@  - Endianness: Kernel config
diff --git a/arch/arm/mach-omap2/omap_hwmod.c b/arch/arm/mach-omap2/omap_hwmod.c
index c914b0052fb9..4551efd28f8d 100644
--- a/arch/arm/mach-omap2/omap_hwmod.c
+++ b/arch/arm/mach-omap2/omap_hwmod.c
@@ -3349,6 +3349,9 @@ int __init omap_hwmod_register_links(struct omap_hwmod_ocp_if **ois)
 	if (!ois)
 		return 0;
 
+	if (ois[0] == NULL) /* Empty list */
+		return 0;
+
 	if (!linkspace) {
 		if (_alloc_linkspace(ois)) {
 			pr_err("omap_hwmod: could not allocate link space\n");
diff --git a/arch/arm/mach-omap2/omap_hwmod_7xx_data.c b/arch/arm/mach-omap2/omap_hwmod_7xx_data.c
index 810c205d668b..2e35ff99f60e 100644
--- a/arch/arm/mach-omap2/omap_hwmod_7xx_data.c
+++ b/arch/arm/mach-omap2/omap_hwmod_7xx_data.c
@@ -35,6 +35,7 @@
 #include "i2c.h"
 #include "mmc.h"
 #include "wd_timer.h"
+#include "soc.h"
 
 /* Base offset for all DRA7XX interrupts external to MPUSS */
 #define DRA7XX_IRQ_GIC_START	32
@@ -2707,7 +2708,6 @@ static struct omap_hwmod_ocp_if *dra7xx_hwmod_ocp_ifs[] __initdata = {
 	&dra7xx_l4_per3__usb_otg_ss1,
 	&dra7xx_l4_per3__usb_otg_ss2,
 	&dra7xx_l4_per3__usb_otg_ss3,
-	&dra7xx_l4_per3__usb_otg_ss4,
 	&dra7xx_l3_main_1__vcp1,
 	&dra7xx_l4_per2__vcp1,
 	&dra7xx_l3_main_1__vcp2,
@@ -2716,8 +2716,26 @@ static struct omap_hwmod_ocp_if *dra7xx_hwmod_ocp_ifs[] __initdata = {
 	NULL,
 };
 
+static struct omap_hwmod_ocp_if *dra74x_hwmod_ocp_ifs[] __initdata = {
+	&dra7xx_l4_per3__usb_otg_ss4,
+	NULL,
+};
+
+static struct omap_hwmod_ocp_if *dra72x_hwmod_ocp_ifs[] __initdata = {
+	NULL,
+};
+
 int __init dra7xx_hwmod_init(void)
 {
+	int ret;
+
 	omap_hwmod_init();
-	return omap_hwmod_register_links(dra7xx_hwmod_ocp_ifs);
+	ret = omap_hwmod_register_links(dra7xx_hwmod_ocp_ifs);
+
+	if (!ret && soc_is_dra74x())
+		return omap_hwmod_register_links(dra74x_hwmod_ocp_ifs);
+	else if (!ret && soc_is_dra72x())
+		return omap_hwmod_register_links(dra72x_hwmod_ocp_ifs);
+
+	return ret;
 }
diff --git a/arch/arm/mach-omap2/soc.h b/arch/arm/mach-omap2/soc.h
index 076bd90a6ce0..8a9be09d9f38 100644
--- a/arch/arm/mach-omap2/soc.h
+++ b/arch/arm/mach-omap2/soc.h
@@ -245,6 +245,8 @@ IS_AM_SUBCLASS(437x, 0x437)
 #define soc_is_omap54xx()		0
 #define soc_is_omap543x()		0
 #define soc_is_dra7xx()			0
+#define soc_is_dra74x()			0
+#define soc_is_dra72x()			0
 
 #if defined(MULTI_OMAP2)
 # if defined(CONFIG_ARCH_OMAP2)
@@ -393,7 +395,11 @@ IS_OMAP_TYPE(3430, 0x3430)
 
 #if defined(CONFIG_SOC_DRA7XX)
 #undef soc_is_dra7xx
+#undef soc_is_dra74x
+#undef soc_is_dra72x
 #define soc_is_dra7xx()	(of_machine_is_compatible("ti,dra7"))
+#define soc_is_dra74x()	(of_machine_is_compatible("ti,dra74"))
+#define soc_is_dra72x()	(of_machine_is_compatible("ti,dra72"))
 #endif
 
 /* Various silicon revisions for omap2 */
diff --git a/arch/arm/mm/abort-ev6.S b/arch/arm/mm/abort-ev6.S
index 3815a8262af0..8c48c5c22a33 100644
--- a/arch/arm/mm/abort-ev6.S
+++ b/arch/arm/mm/abort-ev6.S
@@ -17,12 +17,6 @@
  */
 	.align	5
 ENTRY(v6_early_abort)
-#ifdef CONFIG_CPU_V6
-	sub	r1, sp, #4			@ Get unused stack location
-	strex	r0, r1, [r1]			@ Clear the exclusive monitor
-#elif defined(CONFIG_CPU_32v6K)
-	clrex
-#endif
 	mrc	p15, 0, r1, c5, c0, 0		@ get FSR
 	mrc	p15, 0, r0, c6, c0, 0		@ get FAR
 /*
diff --git a/arch/arm/mm/abort-ev7.S b/arch/arm/mm/abort-ev7.S
index 703375277ba6..4812ad054214 100644
--- a/arch/arm/mm/abort-ev7.S
+++ b/arch/arm/mm/abort-ev7.S
@@ -13,12 +13,6 @@
  */
 	.align	5
 ENTRY(v7_early_abort)
-	/*
-	 * The effect of data aborts on on the exclusive access monitor are
-	 * UNPREDICTABLE. Do a CLREX to clear the state
-	 */
-	clrex
-
 	mrc	p15, 0, r1, c5, c0, 0		@ get FSR
 	mrc	p15, 0, r0, c6, c0, 0		@ get FAR
 
diff --git a/arch/arm/mm/alignment.c b/arch/arm/mm/alignment.c
index 924036473b16..d301662b7b32 100644
--- a/arch/arm/mm/alignment.c
+++ b/arch/arm/mm/alignment.c
@@ -40,6 +40,7 @@
  * This code is not portable to processors with late data abort handling.
  */
 #define CODING_BITS(i)	(i & 0x0e000000)
+#define COND_BITS(i)	(i & 0xf0000000)
 
 #define LDST_I_BIT(i)	(i & (1 << 26))		/* Immediate constant	*/
 #define LDST_P_BIT(i)	(i & (1 << 24))		/* Preindex		*/
@@ -817,6 +818,8 @@ do_alignment(unsigned long addr, unsigned int fsr, struct pt_regs *regs)
 		break;
 
 	case 0x04000000:	/* ldr or str immediate */
+		if (COND_BITS(instr) == 0xf0000000) /* NEON VLDn, VSTn */
+			goto bad;
 		offset.un = OFFSET_BITS(instr);
 		handler = do_alignment_ldrstr;
 		break;
diff --git a/arch/arm64/include/asm/hw_breakpoint.h b/arch/arm64/include/asm/hw_breakpoint.h
index d064047612b1..52b484b6aa1a 100644
--- a/arch/arm64/include/asm/hw_breakpoint.h
+++ b/arch/arm64/include/asm/hw_breakpoint.h
@@ -79,7 +79,6 @@ static inline void decode_ctrl_reg(u32 reg,
  */
 #define ARM_MAX_BRP		16
 #define ARM_MAX_WRP		16
-#define ARM_MAX_HBP_SLOTS	(ARM_MAX_BRP + ARM_MAX_WRP)
 
 /* Virtual debug register bases. */
 #define AARCH64_DBG_REG_BVR	0
diff --git a/arch/arm64/kernel/irq.c b/arch/arm64/kernel/irq.c
index 0f08dfd69ebc..dfa6e3e74fdd 100644
--- a/arch/arm64/kernel/irq.c
+++ b/arch/arm64/kernel/irq.c
@@ -97,19 +97,15 @@ static bool migrate_one_irq(struct irq_desc *desc)
 	if (irqd_is_per_cpu(d) || !cpumask_test_cpu(smp_processor_id(), affinity))
 		return false;
 
-	if (cpumask_any_and(affinity, cpu_online_mask) >= nr_cpu_ids)
+	if (cpumask_any_and(affinity, cpu_online_mask) >= nr_cpu_ids) {
+		affinity = cpu_online_mask;
 		ret = true;
+	}
 
-	/*
-	 * when using forced irq_set_affinity we must ensure that the cpu
-	 * being offlined is not present in the affinity mask, it may be
-	 * selected as the target CPU otherwise
-	 */
-	affinity = cpu_online_mask;
 	c = irq_data_get_irq_chip(d);
 	if (!c->irq_set_affinity)
 		pr_debug("IRQ%u: unable to set affinity\n", d->irq);
-	else if (c->irq_set_affinity(d, affinity, true) == IRQ_SET_MASK_OK && ret)
+	else if (c->irq_set_affinity(d, affinity, false) == IRQ_SET_MASK_OK && ret)
 		cpumask_copy(d->affinity, affinity);
 
 	return ret;
diff --git a/arch/arm64/kernel/process.c b/arch/arm64/kernel/process.c
index 1c0a9be2ffa8..6e7e579c629d 100644
--- a/arch/arm64/kernel/process.c
+++ b/arch/arm64/kernel/process.c
@@ -187,9 +187,27 @@ void exit_thread(void)
 {
 }
 
+static void tls_thread_flush(void)
+{
+	asm ("msr tpidr_el0, xzr");
+
+	if (is_compat_task()) {
+		current->thread.tp_value = 0;
+
+		/*
+		 * We need to ensure ordering between the shadow state and the
+		 * hardware state, so that we don't corrupt the hardware state
+		 * with a stale shadow state during context switch.
+		 */
+		barrier();
+		asm ("msr tpidrro_el0, xzr");
+	}
+}
+
 void flush_thread(void)
 {
 	fpsimd_flush_thread();
+	tls_thread_flush();
 	flush_ptrace_hw_breakpoint(current);
 }
 
diff --git a/arch/arm64/kernel/ptrace.c b/arch/arm64/kernel/ptrace.c
index 7a50b86464cc..b1269dac1289 100644
--- a/arch/arm64/kernel/ptrace.c
+++ b/arch/arm64/kernel/ptrace.c
@@ -81,7 +81,8 @@ static void ptrace_hbptriggered(struct perf_event *bp,
 			break;
 		}
 	}
-	for (i = ARM_MAX_BRP; i < ARM_MAX_HBP_SLOTS && !bp; ++i) {
+
+	for (i = 0; i < ARM_MAX_WRP; ++i) {
 		if (current->thread.debug.hbp_watch[i] == bp) {
 			info.si_errno = -((i << 1) + 1);
 			break;
diff --git a/arch/arm64/kernel/sys_compat.c b/arch/arm64/kernel/sys_compat.c
index 26e9c4eeaba8..78039927c807 100644
--- a/arch/arm64/kernel/sys_compat.c
+++ b/arch/arm64/kernel/sys_compat.c
@@ -79,6 +79,12 @@ long compat_arm_syscall(struct pt_regs *regs)
 
 	case __ARM_NR_compat_set_tls:
 		current->thread.tp_value = regs->regs[0];
+
+		/*
+		 * Protect against register corruption from context switch.
+		 * See comment in tls_thread_flush.
+		 */
+		barrier();
 		asm ("msr tpidrro_el0, %0" : : "r" (regs->regs[0]));
 		return 0;
 
diff --git a/arch/arm64/kvm/handle_exit.c b/arch/arm64/kvm/handle_exit.c
index 7bc41eab4c64..fd9aeba99683 100644
--- a/arch/arm64/kvm/handle_exit.c
+++ b/arch/arm64/kvm/handle_exit.c
@@ -62,6 +62,8 @@ static int kvm_handle_wfx(struct kvm_vcpu *vcpu, struct kvm_run *run)
 	else
 		kvm_vcpu_block(vcpu);
 
+	kvm_skip_instr(vcpu, kvm_vcpu_trap_il_is32bit(vcpu));
+
 	return 1;
 }
 
diff --git a/arch/arm64/kvm/hyp-init.S b/arch/arm64/kvm/hyp-init.S
index 2b0244d65c16..12e26f358c31 100644
--- a/arch/arm64/kvm/hyp-init.S
+++ b/arch/arm64/kvm/hyp-init.S
@@ -74,6 +74,10 @@ __do_hyp_init:
 	msr	mair_el2, x4
 	isb
 
+	/* Invalidate the stale TLBs from Bootloader */
+	tlbi	alle2
+	dsb	sy
+
 	mrs	x4, sctlr_el2
 	and	x4, x4, #SCTLR_EL2_EE	// preserve endianness of EL2
 	ldr	x5, =SCTLR_EL2_FLAGS
diff --git a/arch/mips/boot/compressed/decompress.c b/arch/mips/boot/compressed/decompress.c
index c00c4ddf4514..5244cecf1e45 100644
--- a/arch/mips/boot/compressed/decompress.c
+++ b/arch/mips/boot/compressed/decompress.c
@@ -13,6 +13,7 @@
 
 #include <linux/types.h>
 #include <linux/kernel.h>
+#include <linux/string.h>
 
 #include <asm/addrspace.h>
 
diff --git a/arch/mips/kernel/mcount.S b/arch/mips/kernel/mcount.S
index 539b6294b613..8f89ff4ed524 100644
--- a/arch/mips/kernel/mcount.S
+++ b/arch/mips/kernel/mcount.S
@@ -123,7 +123,11 @@ NESTED(_mcount, PT_SIZE, ra)
 	 nop
 #endif
 	b	ftrace_stub
+#ifdef CONFIG_32BIT
+	 addiu sp, sp, 8
+#else
 	 nop
+#endif
 
 static_trace:
 	MCOUNT_SAVE_REGS
@@ -133,6 +137,9 @@ static_trace:
 	 move	a1, AT		/* arg2: parent's return address */
 
 	MCOUNT_RESTORE_REGS
+#ifdef CONFIG_32BIT
+	addiu sp, sp, 8
+#endif
 	.globl ftrace_stub
 ftrace_stub:
 	RETURN_BACK
@@ -177,6 +184,11 @@ NESTED(ftrace_graph_caller, PT_SIZE, ra)
 	jal	prepare_ftrace_return
 	 nop
 	MCOUNT_RESTORE_REGS
+#ifndef CONFIG_DYNAMIC_FTRACE
+#ifdef CONFIG_32BIT
+	addiu sp, sp, 8
+#endif
+#endif
 	RETURN_BACK
 	END(ftrace_graph_caller)
 
diff --git a/arch/parisc/Makefile b/arch/parisc/Makefile
index 7187664034c3..5db8882f732c 100644
--- a/arch/parisc/Makefile
+++ b/arch/parisc/Makefile
@@ -48,7 +48,12 @@ cflags-y	:= -pipe
 
 # These flags should be implied by an hppa-linux configuration, but they
 # are not in gcc 3.2.
-cflags-y	+= -mno-space-regs -mfast-indirect-calls
+cflags-y	+= -mno-space-regs
+
+# -mfast-indirect-calls is only relevant for 32-bit kernels.
+ifndef CONFIG_64BIT
+cflags-y	+= -mfast-indirect-calls
+endif
 
 # Currently we save and restore fpregs on all kernel entry/interruption paths.
 # If that gets optimized, we might need to disable the use of fpregs in the
diff --git a/arch/parisc/kernel/syscall.S b/arch/parisc/kernel/syscall.S
index 838786011037..7ef22e3387e0 100644
--- a/arch/parisc/kernel/syscall.S
+++ b/arch/parisc/kernel/syscall.S
@@ -74,7 +74,7 @@ ENTRY(linux_gateway_page)
 	/* ADDRESS 0xb0 to 0xb8, lws uses two insns for entry */
 	/* Light-weight-syscall entry must always be located at 0xb0 */
 	/* WARNING: Keep this number updated with table size changes */
-#define __NR_lws_entries (2)
+#define __NR_lws_entries (3)
 
 lws_entry:
 	gate	lws_start, %r0		/* increase privilege */
@@ -502,7 +502,7 @@ lws_exit:
 
 	
 	/***************************************************
-		Implementing CAS as an atomic operation:
+		Implementing 32bit CAS as an atomic operation:
 
 		%r26 - Address to examine
 		%r25 - Old value to check (old)
@@ -659,6 +659,230 @@ cas_action:
 	ASM_EXCEPTIONTABLE_ENTRY(2b-linux_gateway_page, 3b-linux_gateway_page)
 
 
+	/***************************************************
+		New CAS implementation which uses pointers and variable size
+		information. The value pointed by old and new MUST NOT change
+		while performing CAS. The lock only protect the value at %r26.
+
+		%r26 - Address to examine
+		%r25 - Pointer to the value to check (old)
+		%r24 - Pointer to the value to set (new)
+		%r23 - Size of the variable (0/1/2/3 for 8/16/32/64 bit)
+		%r28 - Return non-zero on failure
+		%r21 - Kernel error code
+
+		%r21 has the following meanings:
+
+		EAGAIN - CAS is busy, ldcw failed, try again.
+		EFAULT - Read or write failed.
+
+		Scratch: r20, r22, r28, r29, r1, fr4 (32bit for 64bit CAS only)
+
+	****************************************************/
+
+	/* ELF32 Process entry path */
+lws_compare_and_swap_2:
+#ifdef CONFIG_64BIT
+	/* Clip the input registers */
+	depdi	0, 31, 32, %r26
+	depdi	0, 31, 32, %r25
+	depdi	0, 31, 32, %r24
+	depdi	0, 31, 32, %r23
+#endif
+
+	/* Check the validity of the size pointer */
+	subi,>>= 4, %r23, %r0
+	b,n	lws_exit_nosys
+
+	/* Jump to the functions which will load the old and new values into
+	   registers depending on the their size */
+	shlw	%r23, 2, %r29
+	blr	%r29, %r0
+	nop
+
+	/* 8bit load */
+4:	ldb	0(%sr3,%r25), %r25
+	b	cas2_lock_start
+5:	ldb	0(%sr3,%r24), %r24
+	nop
+	nop
+	nop
+	nop
+	nop
+
+	/* 16bit load */
+6:	ldh	0(%sr3,%r25), %r25
+	b	cas2_lock_start
+7:	ldh	0(%sr3,%r24), %r24
+	nop
+	nop
+	nop
+	nop
+	nop
+
+	/* 32bit load */
+8:	ldw	0(%sr3,%r25), %r25
+	b	cas2_lock_start
+9:	ldw	0(%sr3,%r24), %r24
+	nop
+	nop
+	nop
+	nop
+	nop
+
+	/* 64bit load */
+#ifdef CONFIG_64BIT
+10:	ldd	0(%sr3,%r25), %r25
+11:	ldd	0(%sr3,%r24), %r24
+#else
+	/* Load new value into r22/r23 - high/low */
+10:	ldw	0(%sr3,%r25), %r22
+11:	ldw	4(%sr3,%r25), %r23
+	/* Load new value into fr4 for atomic store later */
+12:	flddx	0(%sr3,%r24), %fr4
+#endif
+
+cas2_lock_start:
+	/* Load start of lock table */
+	ldil	L%lws_lock_start, %r20
+	ldo	R%lws_lock_start(%r20), %r28
+
+	/* Extract four bits from r26 and hash lock (Bits 4-7) */
+	extru  %r26, 27, 4, %r20
+
+	/* Find lock to use, the hash is either one of 0 to
+	   15, multiplied by 16 (keep it 16-byte aligned)
+	   and add to the lock table offset. */
+	shlw	%r20, 4, %r20
+	add	%r20, %r28, %r20
+
+	rsm	PSW_SM_I, %r0			/* Disable interrupts */
+	/* COW breaks can cause contention on UP systems */
+	LDCW	0(%sr2,%r20), %r28		/* Try to acquire the lock */
+	cmpb,<>,n	%r0, %r28, cas2_action	/* Did we get it? */
+cas2_wouldblock:
+	ldo	2(%r0), %r28			/* 2nd case */
+	ssm	PSW_SM_I, %r0
+	b	lws_exit			/* Contended... */
+	ldo	-EAGAIN(%r0), %r21		/* Spin in userspace */
+
+	/*
+		prev = *addr;
+		if ( prev == old )
+		  *addr = new;
+		return prev;
+	*/
+
+	/* NOTES:
+		This all works becuse intr_do_signal
+		and schedule both check the return iasq
+		and see that we are on the kernel page
+		so this process is never scheduled off
+		or is ever sent any signal of any sort,
+		thus it is wholly atomic from usrspaces
+		perspective
+	*/
+cas2_action:
+	/* Jump to the correct function */
+	blr	%r29, %r0
+	/* Set %r28 as non-zero for now */
+	ldo	1(%r0),%r28
+
+	/* 8bit CAS */
+13:	ldb,ma	0(%sr3,%r26), %r29
+	sub,=	%r29, %r25, %r0
+	b,n	cas2_end
+14:	stb,ma	%r24, 0(%sr3,%r26)
+	b	cas2_end
+	copy	%r0, %r28
+	nop
+	nop
+
+	/* 16bit CAS */
+15:	ldh,ma	0(%sr3,%r26), %r29
+	sub,=	%r29, %r25, %r0
+	b,n	cas2_end
+16:	sth,ma	%r24, 0(%sr3,%r26)
+	b	cas2_end
+	copy	%r0, %r28
+	nop
+	nop
+
+	/* 32bit CAS */
+17:	ldw,ma	0(%sr3,%r26), %r29
+	sub,=	%r29, %r25, %r0
+	b,n	cas2_end
+18:	stw,ma	%r24, 0(%sr3,%r26)
+	b	cas2_end
+	copy	%r0, %r28
+	nop
+	nop
+
+	/* 64bit CAS */
+#ifdef CONFIG_64BIT
+19:	ldd,ma	0(%sr3,%r26), %r29
+	sub,=	%r29, %r25, %r0
+	b,n	cas2_end
+20:	std,ma	%r24, 0(%sr3,%r26)
+	copy	%r0, %r28
+#else
+	/* Compare first word */
+19:	ldw,ma	0(%sr3,%r26), %r29
+	sub,=	%r29, %r22, %r0
+	b,n	cas2_end
+	/* Compare second word */
+20:	ldw,ma	4(%sr3,%r26), %r29
+	sub,=	%r29, %r23, %r0
+	b,n	cas2_end
+	/* Perform the store */
+21:	fstdx	%fr4, 0(%sr3,%r26)
+	copy	%r0, %r28
+#endif
+
+cas2_end:
+	/* Free lock */
+	stw,ma	%r20, 0(%sr2,%r20)
+	/* Enable interrupts */
+	ssm	PSW_SM_I, %r0
+	/* Return to userspace, set no error */
+	b	lws_exit
+	copy	%r0, %r21
+
+22:
+	/* Error occurred on load or store */
+	/* Free lock */
+	stw	%r20, 0(%sr2,%r20)
+	ssm	PSW_SM_I, %r0
+	ldo	1(%r0),%r28
+	b	lws_exit
+	ldo	-EFAULT(%r0),%r21	/* set errno */
+	nop
+	nop
+	nop
+
+	/* Exception table entries, for the load and store, return EFAULT.
+	   Each of the entries must be relocated. */
+	ASM_EXCEPTIONTABLE_ENTRY(4b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(5b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(6b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(7b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(8b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(9b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(10b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(11b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(13b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(14b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(15b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(16b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(17b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(18b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(19b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(20b-linux_gateway_page, 22b-linux_gateway_page)
+#ifndef CONFIG_64BIT
+	ASM_EXCEPTIONTABLE_ENTRY(12b-linux_gateway_page, 22b-linux_gateway_page)
+	ASM_EXCEPTIONTABLE_ENTRY(21b-linux_gateway_page, 22b-linux_gateway_page)
+#endif
+
 	/* Make sure nothing else is placed on this page */
 	.align PAGE_SIZE
 END(linux_gateway_page)
@@ -675,8 +899,9 @@ ENTRY(end_linux_gateway_page)
 	/* Light-weight-syscall table */
 	/* Start of lws table. */
 ENTRY(lws_table)
-	LWS_ENTRY(compare_and_swap32)	/* 0 - ELF32 Atomic compare and swap */
-	LWS_ENTRY(compare_and_swap64)	/* 1 - ELF64 Atomic compare and swap */
+	LWS_ENTRY(compare_and_swap32)		/* 0 - ELF32 Atomic 32bit CAS */
+	LWS_ENTRY(compare_and_swap64)		/* 1 - ELF64 Atomic 32bit CAS */
+	LWS_ENTRY(compare_and_swap_2)		/* 2 - ELF32 Atomic 64bit CAS */
 END(lws_table)
 	/* End of lws table */
 
diff --git a/arch/powerpc/include/asm/ptrace.h b/arch/powerpc/include/asm/ptrace.h
index 279b80f3bb29..c0c61fa9cd9e 100644
--- a/arch/powerpc/include/asm/ptrace.h
+++ b/arch/powerpc/include/asm/ptrace.h
@@ -47,6 +47,12 @@
 				 STACK_FRAME_OVERHEAD + KERNEL_REDZONE_SIZE)
 #define STACK_FRAME_MARKER	12
 
+#if defined(_CALL_ELF) && _CALL_ELF == 2
+#define STACK_FRAME_MIN_SIZE	32
+#else
+#define STACK_FRAME_MIN_SIZE	STACK_FRAME_OVERHEAD
+#endif
+
 /* Size of dummy stack frame allocated when calling signal handler. */
 #define __SIGNAL_FRAMESIZE	128
 #define __SIGNAL_FRAMESIZE32	64
@@ -60,6 +66,7 @@
 #define STACK_FRAME_REGS_MARKER	ASM_CONST(0x72656773)
 #define STACK_INT_FRAME_SIZE	(sizeof(struct pt_regs) + STACK_FRAME_OVERHEAD)
 #define STACK_FRAME_MARKER	2
+#define STACK_FRAME_MIN_SIZE	STACK_FRAME_OVERHEAD
 
 /* Size of stack frame allocated when calling signal handler. */
 #define __SIGNAL_FRAMESIZE	64
diff --git a/arch/powerpc/include/asm/spinlock.h b/arch/powerpc/include/asm/spinlock.h
index 35aa339410bd..4dbe072eecbe 100644
--- a/arch/powerpc/include/asm/spinlock.h
+++ b/arch/powerpc/include/asm/spinlock.h
@@ -61,6 +61,7 @@ static __always_inline int arch_spin_value_unlocked(arch_spinlock_t lock)
 
 static inline int arch_spin_is_locked(arch_spinlock_t *lock)
 {
+	smp_mb();
 	return !arch_spin_value_unlocked(*lock);
 }
 
diff --git a/arch/powerpc/lib/locks.c b/arch/powerpc/lib/locks.c
index 0c9c8d7d0734..170a0346f756 100644
--- a/arch/powerpc/lib/locks.c
+++ b/arch/powerpc/lib/locks.c
@@ -70,12 +70,16 @@ void __rw_yield(arch_rwlock_t *rw)
 
 void arch_spin_unlock_wait(arch_spinlock_t *lock)
 {
+	smp_mb();
+
 	while (lock->slock) {
 		HMT_low();
 		if (SHARED_PROCESSOR)
 			__spin_yield(lock);
 	}
 	HMT_medium();
+
+	smp_mb();
 }
 
 EXPORT_SYMBOL(arch_spin_unlock_wait);
diff --git a/arch/powerpc/perf/callchain.c b/arch/powerpc/perf/callchain.c
index 74d1e780748b..2396dda282cd 100644
--- a/arch/powerpc/perf/callchain.c
+++ b/arch/powerpc/perf/callchain.c
@@ -35,7 +35,7 @@ static int valid_next_sp(unsigned long sp, unsigned long prev_sp)
 		return 0;		/* must be 16-byte aligned */
 	if (!validate_sp(sp, current, STACK_FRAME_OVERHEAD))
 		return 0;
-	if (sp >= prev_sp + STACK_FRAME_OVERHEAD)
+	if (sp >= prev_sp + STACK_FRAME_MIN_SIZE)
 		return 1;
 	/*
 	 * sp could decrease when we jump off an interrupt stack
diff --git a/arch/s390/mm/pgtable.c b/arch/s390/mm/pgtable.c
index 3584ed9b20a1..e309c5c41158 100644
--- a/arch/s390/mm/pgtable.c
+++ b/arch/s390/mm/pgtable.c
@@ -810,11 +810,21 @@ int set_guest_storage_key(struct mm_struct *mm, unsigned long addr,
 	pte_t *ptep;
 
 	down_read(&mm->mmap_sem);
+retry:
 	ptep = get_locked_pte(current->mm, addr, &ptl);
 	if (unlikely(!ptep)) {
 		up_read(&mm->mmap_sem);
 		return -EFAULT;
 	}
+	if (!(pte_val(*ptep) & _PAGE_INVALID) &&
+	     (pte_val(*ptep) & _PAGE_PROTECT)) {
+			pte_unmap_unlock(*ptep, ptl);
+			if (fixup_user_fault(current, mm, addr, FAULT_FLAG_WRITE)) {
+				up_read(&mm->mmap_sem);
+				return -EFAULT;
+			}
+			goto retry;
+		}
 
 	new = old = pgste_get_lock(ptep);
 	pgste_val(new) &= ~(PGSTE_GR_BIT | PGSTE_GC_BIT |
diff --git a/arch/x86/boot/compressed/aslr.c b/arch/x86/boot/compressed/aslr.c
index 4dbf967da50d..6cfcf2a2eb93 100644
--- a/arch/x86/boot/compressed/aslr.c
+++ b/arch/x86/boot/compressed/aslr.c
@@ -183,12 +183,27 @@ static void mem_avoid_init(unsigned long input, unsigned long input_size,
 static bool mem_avoid_overlap(struct mem_vector *img)
 {
 	int i;
+	struct setup_data *ptr;
 
 	for (i = 0; i < MEM_AVOID_MAX; i++) {
 		if (mem_overlaps(img, &mem_avoid[i]))
 			return true;
 	}
 
+	/* Avoid all entries in the setup_data linked list. */
+	ptr = (struct setup_data *)(unsigned long)real_mode->hdr.setup_data;
+	while (ptr) {
+		struct mem_vector avoid;
+
+		avoid.start = (u64)ptr;
+		avoid.size = sizeof(*ptr) + ptr->len;
+
+		if (mem_overlaps(img, &avoid))
+			return true;
+
+		ptr = (struct setup_data *)(unsigned long)ptr->next;
+	}
+
 	return false;
 }
 
diff --git a/arch/x86/include/asm/fixmap.h b/arch/x86/include/asm/fixmap.h
index 7252cd339175..6762a55b798a 100644
--- a/arch/x86/include/asm/fixmap.h
+++ b/arch/x86/include/asm/fixmap.h
@@ -123,14 +123,14 @@ enum fixed_addresses {
 	__end_of_permanent_fixed_addresses,
 
 	/*
-	 * 256 temporary boot-time mappings, used by early_ioremap(),
+	 * 512 temporary boot-time mappings, used by early_ioremap(),
 	 * before ioremap() is functional.
 	 *
-	 * If necessary we round it up to the next 256 pages boundary so
+	 * If necessary we round it up to the next 512 pages boundary so
 	 * that we can have a single pgd entry and a single pte table:
 	 */
 #define NR_FIX_BTMAPS		64
-#define FIX_BTMAPS_SLOTS	4
+#define FIX_BTMAPS_SLOTS	8
 #define TOTAL_FIX_BTMAPS	(NR_FIX_BTMAPS * FIX_BTMAPS_SLOTS)
 	FIX_BTMAP_END =
 	 (__end_of_permanent_fixed_addresses ^
diff --git a/arch/x86/include/asm/pgtable_64.h b/arch/x86/include/asm/pgtable_64.h
index e22c1dbf7feb..d869931bde62 100644
--- a/arch/x86/include/asm/pgtable_64.h
+++ b/arch/x86/include/asm/pgtable_64.h
@@ -19,6 +19,7 @@ extern pud_t level3_ident_pgt[512];
 extern pmd_t level2_kernel_pgt[512];
 extern pmd_t level2_fixmap_pgt[512];
 extern pmd_t level2_ident_pgt[512];
+extern pte_t level1_fixmap_pgt[512];
 extern pgd_t init_level4_pgt[];
 
 #define swapper_pg_dir init_level4_pgt
diff --git a/arch/x86/kernel/cpu/perf_event_intel_rapl.c b/arch/x86/kernel/cpu/perf_event_intel_rapl.c
index 5ad35ad94d0f..95700e52061d 100644
--- a/arch/x86/kernel/cpu/perf_event_intel_rapl.c
+++ b/arch/x86/kernel/cpu/perf_event_intel_rapl.c
@@ -511,6 +511,7 @@ static int rapl_cpu_prepare(int cpu)
 	struct rapl_pmu *pmu = per_cpu(rapl_pmu, cpu);
 	int phys_id = topology_physical_package_id(cpu);
 	u64 ms;
+	u64 msr_rapl_power_unit_bits;
 
 	if (pmu)
 		return 0;
@@ -518,6 +519,9 @@ static int rapl_cpu_prepare(int cpu)
 	if (phys_id < 0)
 		return -1;
 
+	if (!rdmsrl_safe(MSR_RAPL_POWER_UNIT, &msr_rapl_power_unit_bits))
+		return -1;
+
 	pmu = kzalloc_node(sizeof(*pmu), GFP_KERNEL, cpu_to_node(cpu));
 	if (!pmu)
 		return -1;
@@ -531,8 +535,7 @@ static int rapl_cpu_prepare(int cpu)
 	 *
 	 * we cache in local PMU instance
 	 */
-	rdmsrl(MSR_RAPL_POWER_UNIT, pmu->hw_unit);
-	pmu->hw_unit = (pmu->hw_unit >> 8) & 0x1FULL;
+	pmu->hw_unit = (msr_rapl_power_unit_bits >> 8) & 0x1FULL;
 	pmu->pmu = &rapl_pmu_class;
 
 	/*
@@ -649,7 +652,9 @@ static int __init rapl_pmu_init(void)
 	get_online_cpus();
 
 	for_each_online_cpu(cpu) {
-		rapl_cpu_prepare(cpu);
+		ret = rapl_cpu_prepare(cpu);
+		if (ret)
+			goto out;
 		rapl_cpu_init(cpu);
 	}
 
@@ -672,6 +677,7 @@ static int __init rapl_pmu_init(void)
 		hweight32(rapl_cntr_mask),
 		ktime_to_ms(pmu->timer_interval));
 
+out:
 	put_online_cpus();
 
 	return 0;
diff --git a/arch/x86/kernel/smpboot.c b/arch/x86/kernel/smpboot.c
index 395be6d8bbde..682876533ed9 100644
--- a/arch/x86/kernel/smpboot.c
+++ b/arch/x86/kernel/smpboot.c
@@ -1287,6 +1287,9 @@ static void remove_siblinginfo(int cpu)
 
 	for_each_cpu(sibling, cpu_sibling_mask(cpu))
 		cpumask_clear_cpu(cpu, cpu_sibling_mask(sibling));
+	for_each_cpu(sibling, cpu_llc_shared_mask(cpu))
+		cpumask_clear_cpu(cpu, cpu_llc_shared_mask(sibling));
+	cpumask_clear(cpu_llc_shared_mask(cpu));
 	cpumask_clear(cpu_sibling_mask(cpu));
 	cpumask_clear(cpu_core_mask(cpu));
 	c->phys_proc_id = 0;
diff --git a/arch/x86/xen/mmu.c b/arch/x86/xen/mmu.c
index 2423ef04ffea..c83da6fb2dee 100644
--- a/arch/x86/xen/mmu.c
+++ b/arch/x86/xen/mmu.c
@@ -1866,12 +1866,11 @@ static void __init check_pt_base(unsigned long *pt_base, unsigned long *pt_end,
  *
  * We can construct this by grafting the Xen provided pagetable into
  * head_64.S's preconstructed pagetables.  We copy the Xen L2's into
- * level2_ident_pgt, level2_kernel_pgt and level2_fixmap_pgt.  This
- * means that only the kernel has a physical mapping to start with -
- * but that's enough to get __va working.  We need to fill in the rest
- * of the physical mapping once some sort of allocator has been set
- * up.
- * NOTE: for PVH, the page tables are native.
+ * level2_ident_pgt, and level2_kernel_pgt.  This means that only the
+ * kernel has a physical mapping to start with - but that's enough to
+ * get __va working.  We need to fill in the rest of the physical
+ * mapping once some sort of allocator has been set up.  NOTE: for
+ * PVH, the page tables are native.
  */
 void __init xen_setup_kernel_pagetable(pgd_t *pgd, unsigned long max_pfn)
 {
@@ -1902,8 +1901,11 @@ void __init xen_setup_kernel_pagetable(pgd_t *pgd, unsigned long max_pfn)
 		/* L3_i[0] -> level2_ident_pgt */
 		convert_pfn_mfn(level3_ident_pgt);
 		/* L3_k[510] -> level2_kernel_pgt
-		 * L3_i[511] -> level2_fixmap_pgt */
+		 * L3_k[511] -> level2_fixmap_pgt */
 		convert_pfn_mfn(level3_kernel_pgt);
+
+		/* L3_k[511][506] -> level1_fixmap_pgt */
+		convert_pfn_mfn(level2_fixmap_pgt);
 	}
 	/* We get [511][511] and have Xen's version of level2_kernel_pgt */
 	l3 = m2v(pgd[pgd_index(__START_KERNEL_map)].pgd);
@@ -1913,21 +1915,15 @@ void __init xen_setup_kernel_pagetable(pgd_t *pgd, unsigned long max_pfn)
 	addr[1] = (unsigned long)l3;
 	addr[2] = (unsigned long)l2;
 	/* Graft it onto L4[272][0]. Note that we creating an aliasing problem:
-	 * Both L4[272][0] and L4[511][511] have entries that point to the same
+	 * Both L4[272][0] and L4[511][510] have entries that point to the same
 	 * L2 (PMD) tables. Meaning that if you modify it in __va space
 	 * it will be also modified in the __ka space! (But if you just
 	 * modify the PMD table to point to other PTE's or none, then you
 	 * are OK - which is what cleanup_highmap does) */
 	copy_page(level2_ident_pgt, l2);
-	/* Graft it onto L4[511][511] */
+	/* Graft it onto L4[511][510] */
 	copy_page(level2_kernel_pgt, l2);
 
-	/* Get [511][510] and graft that in level2_fixmap_pgt */
-	l3 = m2v(pgd[pgd_index(__START_KERNEL_map + PMD_SIZE)].pgd);
-	l2 = m2v(l3[pud_index(__START_KERNEL_map + PMD_SIZE)].pud);
-	copy_page(level2_fixmap_pgt, l2);
-	/* Note that we don't do anything with level1_fixmap_pgt which
-	 * we don't need. */
 	if (!xen_feature(XENFEAT_auto_translated_physmap)) {
 		/* Make pagetable pieces RO */
 		set_page_prot(init_level4_pgt, PAGE_KERNEL_RO);
@@ -1937,6 +1933,7 @@ void __init xen_setup_kernel_pagetable(pgd_t *pgd, unsigned long max_pfn)
 		set_page_prot(level2_ident_pgt, PAGE_KERNEL_RO);
 		set_page_prot(level2_kernel_pgt, PAGE_KERNEL_RO);
 		set_page_prot(level2_fixmap_pgt, PAGE_KERNEL_RO);
+		set_page_prot(level1_fixmap_pgt, PAGE_KERNEL_RO);
 
 		/* Pin down new L4 */
 		pin_pagetable_pfn(MMUEXT_PIN_L4_TABLE,
diff --git a/arch/xtensa/include/asm/pgtable.h b/arch/xtensa/include/asm/pgtable.h
index 216446295ada..51230ba97bef 100644
--- a/arch/xtensa/include/asm/pgtable.h
+++ b/arch/xtensa/include/asm/pgtable.h
@@ -67,7 +67,12 @@
 #define VMALLOC_START		0xC0000000
 #define VMALLOC_END		0xC7FEFFFF
 #define TLBTEMP_BASE_1		0xC7FF0000
-#define TLBTEMP_BASE_2		0xC7FF8000
+#define TLBTEMP_BASE_2		(TLBTEMP_BASE_1 + DCACHE_WAY_SIZE)
+#if 2 * DCACHE_WAY_SIZE > ICACHE_WAY_SIZE
+#define TLBTEMP_SIZE		(2 * DCACHE_WAY_SIZE)
+#else
+#define TLBTEMP_SIZE		ICACHE_WAY_SIZE
+#endif
 
 /*
  * For the Xtensa architecture, the PTE layout is as follows:
diff --git a/arch/xtensa/include/asm/uaccess.h b/arch/xtensa/include/asm/uaccess.h
index fd686dc45d1a..c7211e7e182d 100644
--- a/arch/xtensa/include/asm/uaccess.h
+++ b/arch/xtensa/include/asm/uaccess.h
@@ -52,7 +52,12 @@
  */
 	.macro	get_fs	ad, sp
 	GET_CURRENT(\ad,\sp)
+#if THREAD_CURRENT_DS > 1020
+	addi	\ad, \ad, TASK_THREAD
+	l32i	\ad, \ad, THREAD_CURRENT_DS - TASK_THREAD
+#else
 	l32i	\ad, \ad, THREAD_CURRENT_DS
+#endif
 	.endm
 
 /*
diff --git a/arch/xtensa/include/uapi/asm/ioctls.h b/arch/xtensa/include/uapi/asm/ioctls.h
index b4cb1100c0fb..a47909f0c34b 100644
--- a/arch/xtensa/include/uapi/asm/ioctls.h
+++ b/arch/xtensa/include/uapi/asm/ioctls.h
@@ -28,17 +28,17 @@
 #define TCSETSW		0x5403
 #define TCSETSF		0x5404
 
-#define TCGETA		_IOR('t', 23, struct termio)
-#define TCSETA		_IOW('t', 24, struct termio)
-#define TCSETAW		_IOW('t', 25, struct termio)
-#define TCSETAF		_IOW('t', 28, struct termio)
+#define TCGETA		0x80127417	/* _IOR('t', 23, struct termio) */
+#define TCSETA		0x40127418	/* _IOW('t', 24, struct termio) */
+#define TCSETAW		0x40127419	/* _IOW('t', 25, struct termio) */
+#define TCSETAF		0x4012741C	/* _IOW('t', 28, struct termio) */
 
 #define TCSBRK		_IO('t', 29)
 #define TCXONC		_IO('t', 30)
 #define TCFLSH		_IO('t', 31)
 
-#define TIOCSWINSZ	_IOW('t', 103, struct winsize)
-#define TIOCGWINSZ	_IOR('t', 104, struct winsize)
+#define TIOCSWINSZ	0x40087467	/* _IOW('t', 103, struct winsize) */
+#define TIOCGWINSZ	0x80087468	/* _IOR('t', 104, struct winsize) */
 #define	TIOCSTART	_IO('t', 110)		/* start output, like ^Q */
 #define	TIOCSTOP	_IO('t', 111)		/* stop output, like ^S */
 #define TIOCOUTQ        _IOR('t', 115, int)     /* output queue size */
@@ -88,7 +88,6 @@
 #define TIOCSETD	_IOW('T', 35, int)
 #define TIOCGETD	_IOR('T', 36, int)
 #define TCSBRKP		_IOW('T', 37, int)   /* Needed for POSIX tcsendbreak()*/
-#define TIOCTTYGSTRUCT	_IOR('T', 38, struct tty_struct) /* For debugging only*/
 #define TIOCSBRK	_IO('T', 39) 	     /* BSD compatibility */
 #define TIOCCBRK	_IO('T', 40)	     /* BSD compatibility */
 #define TIOCGSID	_IOR('T', 41, pid_t) /* Return the session ID of FD*/
@@ -114,8 +113,10 @@
 #define TIOCSERGETLSR   _IOR('T', 89, unsigned int) /* Get line status reg. */
   /* ioctl (fd, TIOCSERGETLSR, &result) where result may be as below */
 # define TIOCSER_TEMT    0x01		     /* Transmitter physically empty */
-#define TIOCSERGETMULTI _IOR('T', 90, struct serial_multiport_struct) /* Get multiport config  */
-#define TIOCSERSETMULTI _IOW('T', 91, struct serial_multiport_struct) /* Set multiport config */
+#define TIOCSERGETMULTI 0x80a8545a /* Get multiport config  */
+			/* _IOR('T', 90, struct serial_multiport_struct) */
+#define TIOCSERSETMULTI 0x40a8545b /* Set multiport config */
+			/* _IOW('T', 91, struct serial_multiport_struct) */
 
 #define TIOCMIWAIT	_IO('T', 92) /* wait for a change on serial input line(s) */
 #define TIOCGICOUNT	0x545D	/* read serial port inline interrupt counts */
diff --git a/arch/xtensa/kernel/entry.S b/arch/xtensa/kernel/entry.S
index ef7f4990722b..a06b7efaae82 100644
--- a/arch/xtensa/kernel/entry.S
+++ b/arch/xtensa/kernel/entry.S
@@ -1001,9 +1001,8 @@ ENTRY(fast_syscall_xtensa)
 	movi	a7, 4			# sizeof(unsigned int)
 	access_ok a3, a7, a0, a2, .Leac	# a0: scratch reg, a2: sp
 
-	addi	a6, a6, -1		# assuming SYS_XTENSA_ATOMIC_SET = 1
-	_bgeui	a6, SYS_XTENSA_COUNT - 1, .Lill
-	_bnei	a6, SYS_XTENSA_ATOMIC_CMP_SWP - 1, .Lnswp
+	_bgeui	a6, SYS_XTENSA_COUNT, .Lill
+	_bnei	a6, SYS_XTENSA_ATOMIC_CMP_SWP, .Lnswp
 
 	/* Fall through for ATOMIC_CMP_SWP. */
 
@@ -1015,27 +1014,26 @@ TRY	s32i	a5, a3, 0		# different, modify value
 	l32i	a7, a2, PT_AREG7	# restore a7
 	l32i	a0, a2, PT_AREG0	# restore a0
 	movi	a2, 1			# and return 1
-	addi	a6, a6, 1		# restore a6 (really necessary?)
 	rfe
 
 1:	l32i	a7, a2, PT_AREG7	# restore a7
 	l32i	a0, a2, PT_AREG0	# restore a0
 	movi	a2, 0			# return 0 (note that we cannot set
-	addi	a6, a6, 1		# restore a6 (really necessary?)
 	rfe
 
 .Lnswp:	/* Atomic set, add, and exg_add. */
 
 TRY	l32i	a7, a3, 0		# orig
+	addi	a6, a6, -SYS_XTENSA_ATOMIC_SET
 	add	a0, a4, a7		# + arg
 	moveqz	a0, a4, a6		# set
+	addi	a6, a6, SYS_XTENSA_ATOMIC_SET
 TRY	s32i	a0, a3, 0		# write new value
 
 	mov	a0, a2
 	mov	a2, a7
 	l32i	a7, a0, PT_AREG7	# restore a7
 	l32i	a0, a0, PT_AREG0	# restore a0
-	addi	a6, a6, 1		# restore a6 (really necessary?)
 	rfe
 
 CATCH
@@ -1044,7 +1042,7 @@ CATCH
 	movi	a2, -EFAULT
 	rfe
 
-.Lill:	l32i	a7, a2, PT_AREG0	# restore a7
+.Lill:	l32i	a7, a2, PT_AREG7	# restore a7
 	l32i	a0, a2, PT_AREG0	# restore a0
 	movi	a2, -EINVAL
 	rfe
@@ -1565,7 +1563,7 @@ ENTRY(fast_second_level_miss)
 	rsr	a0, excvaddr
 	bltu	a0, a3, 2f
 
-	addi	a1, a0, -(2 << (DCACHE_ALIAS_ORDER + PAGE_SHIFT))
+	addi	a1, a0, -TLBTEMP_SIZE
 	bgeu	a1, a3, 2f
 
 	/* Check if we have to restore an ITLB mapping. */
@@ -1820,7 +1818,6 @@ ENTRY(_switch_to)
 
 	entry	a1, 16
 
-	mov	a10, a2			# preserve 'prev' (a2)
 	mov	a11, a3			# and 'next' (a3)
 
 	l32i	a4, a2, TASK_THREAD_INFO
@@ -1828,8 +1825,14 @@ ENTRY(_switch_to)
 
 	save_xtregs_user a4 a6 a8 a9 a12 a13 THREAD_XTREGS_USER
 
-	s32i	a0, a10, THREAD_RA	# save return address
-	s32i	a1, a10, THREAD_SP	# save stack pointer
+#if THREAD_RA > 1020 || THREAD_SP > 1020
+	addi	a10, a2, TASK_THREAD
+	s32i	a0, a10, THREAD_RA - TASK_THREAD	# save return address
+	s32i	a1, a10, THREAD_SP - TASK_THREAD	# save stack pointer
+#else
+	s32i	a0, a2, THREAD_RA	# save return address
+	s32i	a1, a2, THREAD_SP	# save stack pointer
+#endif
 
 	/* Disable ints while we manipulate the stack pointer. */
 
@@ -1870,7 +1873,6 @@ ENTRY(_switch_to)
 	load_xtregs_user a5 a6 a8 a9 a12 a13 THREAD_XTREGS_USER
 
 	wsr	a14, ps
-	mov	a2, a10			# return 'prev'
 	rsync
 
 	retw
diff --git a/arch/xtensa/kernel/pci-dma.c b/arch/xtensa/kernel/pci-dma.c
index 2d9cc6dbfd78..e8b76b8e4b29 100644
--- a/arch/xtensa/kernel/pci-dma.c
+++ b/arch/xtensa/kernel/pci-dma.c
@@ -49,9 +49,8 @@ dma_alloc_coherent(struct device *dev,size_t size,dma_addr_t *handle,gfp_t flag)
 
 	/* We currently don't support coherent memory outside KSEG */
 
-	if (ret < XCHAL_KSEG_CACHED_VADDR
-	    || ret >= XCHAL_KSEG_CACHED_VADDR + XCHAL_KSEG_SIZE)
-		BUG();
+	BUG_ON(ret < XCHAL_KSEG_CACHED_VADDR ||
+	       ret > XCHAL_KSEG_CACHED_VADDR + XCHAL_KSEG_SIZE - 1);
 
 
 	if (ret != 0) {
@@ -68,10 +67,11 @@ EXPORT_SYMBOL(dma_alloc_coherent);
 void dma_free_coherent(struct device *hwdev, size_t size,
 			 void *vaddr, dma_addr_t dma_handle)
 {
-	long addr=(long)vaddr+XCHAL_KSEG_CACHED_VADDR-XCHAL_KSEG_BYPASS_VADDR;
+	unsigned long addr = (unsigned long)vaddr +
+		XCHAL_KSEG_CACHED_VADDR - XCHAL_KSEG_BYPASS_VADDR;
 
-	if (addr < 0 || addr >= XCHAL_KSEG_SIZE)
-		BUG();
+	BUG_ON(addr < XCHAL_KSEG_CACHED_VADDR ||
+	       addr > XCHAL_KSEG_CACHED_VADDR + XCHAL_KSEG_SIZE - 1);
 
 	free_pages(addr, get_order(size));
 }
diff --git a/block/cfq-iosched.c b/block/cfq-iosched.c
index 744833b630c6..91c25f261c91 100644
--- a/block/cfq-iosched.c
+++ b/block/cfq-iosched.c
@@ -1275,12 +1275,16 @@ __cfq_group_service_tree_add(struct cfq_rb_root *st, struct cfq_group *cfqg)
 static void
 cfq_update_group_weight(struct cfq_group *cfqg)
 {
-	BUG_ON(!RB_EMPTY_NODE(&cfqg->rb_node));
-
 	if (cfqg->new_weight) {
 		cfqg->weight = cfqg->new_weight;
 		cfqg->new_weight = 0;
 	}
+}
+
+static void
+cfq_update_group_leaf_weight(struct cfq_group *cfqg)
+{
+	BUG_ON(!RB_EMPTY_NODE(&cfqg->rb_node));
 
 	if (cfqg->new_leaf_weight) {
 		cfqg->leaf_weight = cfqg->new_leaf_weight;
@@ -1299,7 +1303,7 @@ cfq_group_service_tree_add(struct cfq_rb_root *st, struct cfq_group *cfqg)
 	/* add to the service tree */
 	BUG_ON(!RB_EMPTY_NODE(&cfqg->rb_node));
 
-	cfq_update_group_weight(cfqg);
+	cfq_update_group_leaf_weight(cfqg);
 	__cfq_group_service_tree_add(st, cfqg);
 
 	/*
@@ -1323,6 +1327,7 @@ cfq_group_service_tree_add(struct cfq_rb_root *st, struct cfq_group *cfqg)
 	 */
 	while ((parent = cfqg_parent(pos))) {
 		if (propagate) {
+			cfq_update_group_weight(pos);
 			propagate = !parent->nr_active++;
 			parent->children_weight += pos->weight;
 		}
diff --git a/block/genhd.c b/block/genhd.c
index 791f41943132..e6723bd4d7a1 100644
--- a/block/genhd.c
+++ b/block/genhd.c
@@ -28,10 +28,10 @@ struct kobject *block_depr;
 /* for extended dynamic devt allocation, currently only one major is used */
 #define NR_EXT_DEVT		(1 << MINORBITS)
 
-/* For extended devt allocation.  ext_devt_mutex prevents look up
+/* For extended devt allocation.  ext_devt_lock prevents look up
  * results from going away underneath its user.
  */
-static DEFINE_MUTEX(ext_devt_mutex);
+static DEFINE_SPINLOCK(ext_devt_lock);
 static DEFINE_IDR(ext_devt_idr);
 
 static struct device_type disk_type;
@@ -420,9 +420,13 @@ int blk_alloc_devt(struct hd_struct *part, dev_t *devt)
 	}
 
 	/* allocate ext devt */
-	mutex_lock(&ext_devt_mutex);
-	idx = idr_alloc(&ext_devt_idr, part, 0, NR_EXT_DEVT, GFP_KERNEL);
-	mutex_unlock(&ext_devt_mutex);
+	idr_preload(GFP_KERNEL);
+
+	spin_lock(&ext_devt_lock);
+	idx = idr_alloc(&ext_devt_idr, part, 0, NR_EXT_DEVT, GFP_NOWAIT);
+	spin_unlock(&ext_devt_lock);
+
+	idr_preload_end();
 	if (idx < 0)
 		return idx == -ENOSPC ? -EBUSY : idx;
 
@@ -441,15 +445,13 @@ int blk_alloc_devt(struct hd_struct *part, dev_t *devt)
  */
 void blk_free_devt(dev_t devt)
 {
-	might_sleep();
-
 	if (devt == MKDEV(0, 0))
 		return;
 
 	if (MAJOR(devt) == BLOCK_EXT_MAJOR) {
-		mutex_lock(&ext_devt_mutex);
+		spin_lock(&ext_devt_lock);
 		idr_remove(&ext_devt_idr, blk_mangle_minor(MINOR(devt)));
-		mutex_unlock(&ext_devt_mutex);
+		spin_unlock(&ext_devt_lock);
 	}
 }
 
@@ -665,7 +667,6 @@ void del_gendisk(struct gendisk *disk)
 		sysfs_remove_link(block_depr, dev_name(disk_to_dev(disk)));
 	pm_runtime_set_memalloc_noio(disk_to_dev(disk), false);
 	device_del(disk_to_dev(disk));
-	blk_free_devt(disk_to_dev(disk)->devt);
 }
 EXPORT_SYMBOL(del_gendisk);
 
@@ -690,13 +691,13 @@ struct gendisk *get_gendisk(dev_t devt, int *partno)
 	} else {
 		struct hd_struct *part;
 
-		mutex_lock(&ext_devt_mutex);
+		spin_lock(&ext_devt_lock);
 		part = idr_find(&ext_devt_idr, blk_mangle_minor(MINOR(devt)));
 		if (part && get_disk(part_to_disk(part))) {
 			*partno = part->partno;
 			disk = part_to_disk(part);
 		}
-		mutex_unlock(&ext_devt_mutex);
+		spin_unlock(&ext_devt_lock);
 	}
 
 	return disk;
@@ -1098,6 +1099,7 @@ static void disk_release(struct device *dev)
 {
 	struct gendisk *disk = dev_to_disk(dev);
 
+	blk_free_devt(dev->devt);
 	disk_release_events(disk);
 	kfree(disk->random);
 	disk_replace_part_tbl(disk, NULL);
diff --git a/block/partition-generic.c b/block/partition-generic.c
index 789cdea05893..0d9e5f97f0a8 100644
--- a/block/partition-generic.c
+++ b/block/partition-generic.c
@@ -211,6 +211,7 @@ static const struct attribute_group *part_attr_groups[] = {
 static void part_release(struct device *dev)
 {
 	struct hd_struct *p = dev_to_part(dev);
+	blk_free_devt(dev->devt);
 	free_part_stats(p);
 	free_part_info(p);
 	kfree(p);
@@ -253,7 +254,6 @@ void delete_partition(struct gendisk *disk, int partno)
 	rcu_assign_pointer(ptbl->last_lookup, NULL);
 	kobject_put(part->holder_dir);
 	device_del(part_to_dev(part));
-	blk_free_devt(part_devt(part));
 
 	hd_struct_put(part);
 }
diff --git a/block/partitions/aix.c b/block/partitions/aix.c
index 43be471d9b1d..0931f5136ab2 100644
--- a/block/partitions/aix.c
+++ b/block/partitions/aix.c
@@ -253,7 +253,7 @@ int aix_partition(struct parsed_partitions *state)
 				continue;
 			}
 			lv_ix = be16_to_cpu(p->lv_ix) - 1;
-			if (lv_ix > state->limit) {
+			if (lv_ix >= state->limit) {
 				cur_lv_ix = -1;
 				continue;
 			}
diff --git a/drivers/acpi/acpi_cmos_rtc.c b/drivers/acpi/acpi_cmos_rtc.c
index 84190ed89c04..aff69d9bfcbf 100644
--- a/drivers/acpi/acpi_cmos_rtc.c
+++ b/drivers/acpi/acpi_cmos_rtc.c
@@ -35,7 +35,7 @@ acpi_cmos_rtc_space_handler(u32 function, acpi_physical_address address,
 		      void *handler_context, void *region_context)
 {
 	int i;
-	u8 *value = (u8 *)&value64;
+	u8 *value = (u8 *)value64;
 
 	if (address > 0xff || !value64)
 		return AE_BAD_PARAMETER;
diff --git a/drivers/acpi/acpica/aclocal.h b/drivers/acpi/acpica/aclocal.h
index d95ca5449ace..e6ab104afe42 100644
--- a/drivers/acpi/acpica/aclocal.h
+++ b/drivers/acpi/acpica/aclocal.h
@@ -254,6 +254,7 @@ struct acpi_create_field_info {
 	u32 field_bit_position;
 	u32 field_bit_length;
 	u16 resource_length;
+	u16 pin_number_index;
 	u8 field_flags;
 	u8 attribute;
 	u8 field_type;
diff --git a/drivers/acpi/acpica/acobject.h b/drivers/acpi/acpica/acobject.h
index cc7ab6dd724e..a47cc78ffd4f 100644
--- a/drivers/acpi/acpica/acobject.h
+++ b/drivers/acpi/acpica/acobject.h
@@ -263,6 +263,7 @@ struct acpi_object_region_field {
 	ACPI_OBJECT_COMMON_HEADER ACPI_COMMON_FIELD_INFO u16 resource_length;
 	union acpi_operand_object *region_obj;	/* Containing op_region object */
 	u8 *resource_buffer;	/* resource_template for serial regions/fields */
+	u16 pin_number_index;	/* Index relative to previous Connection/Template */
 };
 
 struct acpi_object_bank_field {
diff --git a/drivers/acpi/acpica/dsfield.c b/drivers/acpi/acpica/dsfield.c
index e7a57c554e84..9af55bd6c4d7 100644
--- a/drivers/acpi/acpica/dsfield.c
+++ b/drivers/acpi/acpica/dsfield.c
@@ -360,6 +360,7 @@ acpi_ds_get_field_names(struct acpi_create_field_info *info,
 			 */
 			info->resource_buffer = NULL;
 			info->connection_node = NULL;
+			info->pin_number_index = 0;
 
 			/*
 			 * A Connection() is either an actual resource descriptor (buffer)
@@ -437,6 +438,7 @@ acpi_ds_get_field_names(struct acpi_create_field_info *info,
 			}
 
 			info->field_bit_position += info->field_bit_length;
+			info->pin_number_index++;	/* Index relative to previous Connection() */
 			break;
 
 		default:
diff --git a/drivers/acpi/acpica/evregion.c b/drivers/acpi/acpica/evregion.c
index 144cbb9b73bc..cd4b231ae760 100644
--- a/drivers/acpi/acpica/evregion.c
+++ b/drivers/acpi/acpica/evregion.c
@@ -142,6 +142,7 @@ acpi_ev_address_space_dispatch(union acpi_operand_object *region_obj,
 	union acpi_operand_object *region_obj2;
 	void *region_context = NULL;
 	struct acpi_connection_info *context;
+	acpi_physical_address address;
 
 	ACPI_FUNCTION_TRACE(ev_address_space_dispatch);
 
@@ -231,25 +232,23 @@ acpi_ev_address_space_dispatch(union acpi_operand_object *region_obj,
 	/* We have everything we need, we can invoke the address space handler */
 
 	handler = handler_desc->address_space.handler;
-
-	ACPI_DEBUG_PRINT((ACPI_DB_OPREGION,
-			  "Handler %p (@%p) Address %8.8X%8.8X [%s]\n",
-			  &region_obj->region.handler->address_space, handler,
-			  ACPI_FORMAT_NATIVE_UINT(region_obj->region.address +
-						  region_offset),
-			  acpi_ut_get_region_name(region_obj->region.
-						  space_id)));
+	address = (region_obj->region.address + region_offset);
 
 	/*
 	 * Special handling for generic_serial_bus and general_purpose_io:
 	 * There are three extra parameters that must be passed to the
 	 * handler via the context:
-	 *   1) Connection buffer, a resource template from Connection() op.
-	 *   2) Length of the above buffer.
-	 *   3) Actual access length from the access_as() op.
+	 *   1) Connection buffer, a resource template from Connection() op
+	 *   2) Length of the above buffer
+	 *   3) Actual access length from the access_as() op
+	 *
+	 * In addition, for general_purpose_io, the Address and bit_width fields
+	 * are defined as follows:
+	 *   1) Address is the pin number index of the field (bit offset from
+	 *      the previous Connection)
+	 *   2) bit_width is the actual bit length of the field (number of pins)
 	 */
-	if (((region_obj->region.space_id == ACPI_ADR_SPACE_GSBUS) ||
-	     (region_obj->region.space_id == ACPI_ADR_SPACE_GPIO)) &&
+	if ((region_obj->region.space_id == ACPI_ADR_SPACE_GSBUS) &&
 	    context && field_obj) {
 
 		/* Get the Connection (resource_template) buffer */
@@ -258,6 +257,24 @@ acpi_ev_address_space_dispatch(union acpi_operand_object *region_obj,
 		context->length = field_obj->field.resource_length;
 		context->access_length = field_obj->field.access_length;
 	}
+	if ((region_obj->region.space_id == ACPI_ADR_SPACE_GPIO) &&
+	    context && field_obj) {
+
+		/* Get the Connection (resource_template) buffer */
+
+		context->connection = field_obj->field.resource_buffer;
+		context->length = field_obj->field.resource_length;
+		context->access_length = field_obj->field.access_length;
+		address = field_obj->field.pin_number_index;
+		bit_width = field_obj->field.bit_length;
+	}
+
+	ACPI_DEBUG_PRINT((ACPI_DB_OPREGION,
+			  "Handler %p (@%p) Address %8.8X%8.8X [%s]\n",
+			  &region_obj->region.handler->address_space, handler,
+			  ACPI_FORMAT_NATIVE_UINT(address),
+			  acpi_ut_get_region_name(region_obj->region.
+						  space_id)));
 
 	if (!(handler_desc->address_space.handler_flags &
 	      ACPI_ADDR_HANDLER_DEFAULT_INSTALLED)) {
@@ -271,9 +288,7 @@ acpi_ev_address_space_dispatch(union acpi_operand_object *region_obj,
 
 	/* Call the handler */
 
-	status = handler(function,
-			 (region_obj->region.address + region_offset),
-			 bit_width, value, context,
+	status = handler(function, address, bit_width, value, context,
 			 region_obj2->extra.region_context);
 
 	if (ACPI_FAILURE(status)) {
diff --git a/drivers/acpi/acpica/exfield.c b/drivers/acpi/acpica/exfield.c
index cfd875243421..d36894a228b1 100644
--- a/drivers/acpi/acpica/exfield.c
+++ b/drivers/acpi/acpica/exfield.c
@@ -178,6 +178,37 @@ acpi_ex_read_data_from_field(struct acpi_walk_state *walk_state,
 		buffer = &buffer_desc->integer.value;
 	}
 
+	if ((obj_desc->common.type == ACPI_TYPE_LOCAL_REGION_FIELD) &&
+	    (obj_desc->field.region_obj->region.space_id ==
+	     ACPI_ADR_SPACE_GPIO)) {
+		/*
+		 * For GPIO (general_purpose_io), the Address will be the bit offset
+		 * from the previous Connection() operator, making it effectively a
+		 * pin number index. The bit_length is the length of the field, which
+		 * is thus the number of pins.
+		 */
+		ACPI_DEBUG_PRINT((ACPI_DB_BFIELD,
+				  "GPIO FieldRead [FROM]:  Pin %u Bits %u\n",
+				  obj_desc->field.pin_number_index,
+				  obj_desc->field.bit_length));
+
+		/* Lock entire transaction if requested */
+
+		acpi_ex_acquire_global_lock(obj_desc->common_field.field_flags);
+
+		/* Perform the write */
+
+		status = acpi_ex_access_region(obj_desc, 0,
+					       (u64 *)buffer, ACPI_READ);
+		acpi_ex_release_global_lock(obj_desc->common_field.field_flags);
+		if (ACPI_FAILURE(status)) {
+			acpi_ut_remove_reference(buffer_desc);
+		} else {
+			*ret_buffer_desc = buffer_desc;
+		}
+		return_ACPI_STATUS(status);
+	}
+
 	ACPI_DEBUG_PRINT((ACPI_DB_BFIELD,
 			  "FieldRead [TO]:   Obj %p, Type %X, Buf %p, ByteLen %X\n",
 			  obj_desc, obj_desc->common.type, buffer,
@@ -325,6 +356,42 @@ acpi_ex_write_data_to_field(union acpi_operand_object *source_desc,
 
 		*result_desc = buffer_desc;
 		return_ACPI_STATUS(status);
+	} else if ((obj_desc->common.type == ACPI_TYPE_LOCAL_REGION_FIELD) &&
+		   (obj_desc->field.region_obj->region.space_id ==
+		    ACPI_ADR_SPACE_GPIO)) {
+		/*
+		 * For GPIO (general_purpose_io), we will bypass the entire field
+		 * mechanism and handoff the bit address and bit width directly to
+		 * the handler. The Address will be the bit offset
+		 * from the previous Connection() operator, making it effectively a
+		 * pin number index. The bit_length is the length of the field, which
+		 * is thus the number of pins.
+		 */
+		if (source_desc->common.type != ACPI_TYPE_INTEGER) {
+			return_ACPI_STATUS(AE_AML_OPERAND_TYPE);
+		}
+
+		ACPI_DEBUG_PRINT((ACPI_DB_BFIELD,
+				  "GPIO FieldWrite [FROM]: (%s:%X), Val %.8X  [TO]:  Pin %u Bits %u\n",
+				  acpi_ut_get_type_name(source_desc->common.
+							type),
+				  source_desc->common.type,
+				  (u32)source_desc->integer.value,
+				  obj_desc->field.pin_number_index,
+				  obj_desc->field.bit_length));
+
+		buffer = &source_desc->integer.value;
+
+		/* Lock entire transaction if requested */
+
+		acpi_ex_acquire_global_lock(obj_desc->common_field.field_flags);
+
+		/* Perform the write */
+
+		status = acpi_ex_access_region(obj_desc, 0,
+					       (u64 *)buffer, ACPI_WRITE);
+		acpi_ex_release_global_lock(obj_desc->common_field.field_flags);
+		return_ACPI_STATUS(status);
 	}
 
 	/* Get a pointer to the data to be written */
diff --git a/drivers/acpi/acpica/exprep.c b/drivers/acpi/acpica/exprep.c
index 5a588611ab48..8c88cfdec441 100644
--- a/drivers/acpi/acpica/exprep.c
+++ b/drivers/acpi/acpica/exprep.c
@@ -484,6 +484,8 @@ acpi_status acpi_ex_prep_field_value(struct acpi_create_field_info *info)
 			obj_desc->field.resource_length = info->resource_length;
 		}
 
+		obj_desc->field.pin_number_index = info->pin_number_index;
+
 		/* Allow full data read from EC address space */
 
 		if ((obj_desc->field.region_obj->region.space_id ==
diff --git a/drivers/acpi/container.c b/drivers/acpi/container.c
index 368f9ddb8480..e4a6f78f3bbc 100644
--- a/drivers/acpi/container.c
+++ b/drivers/acpi/container.c
@@ -96,6 +96,13 @@ static void container_device_detach(struct acpi_device *adev)
 		device_unregister(dev);
 }
 
+static void container_device_online(struct acpi_device *adev)
+{
+	struct device *dev = acpi_driver_data(adev);
+
+	kobject_uevent(&dev->kobj, KOBJ_ONLINE);
+}
+
 static struct acpi_scan_handler container_handler = {
 	.ids = container_device_ids,
 	.attach = container_device_attach,
@@ -103,6 +110,7 @@ static struct acpi_scan_handler container_handler = {
 	.hotplug = {
 		.enabled = true,
 		.demand_offline = true,
+		.notify_online = container_device_online,
 	},
 };
 
diff --git a/drivers/acpi/scan.c b/drivers/acpi/scan.c
index 92d5184e3654..493a342efa44 100644
--- a/drivers/acpi/scan.c
+++ b/drivers/acpi/scan.c
@@ -106,7 +106,7 @@ static int create_modalias(struct acpi_device *acpi_dev, char *modalias,
 	list_for_each_entry(id, &acpi_dev->pnp.ids, list) {
 		count = snprintf(&modalias[len], size, "%s:", id->id);
 		if (count < 0)
-			return EINVAL;
+			return -EINVAL;
 		if (count >= size)
 			return -ENOMEM;
 		len += count;
@@ -2068,6 +2068,9 @@ static void acpi_bus_attach(struct acpi_device *device)
  ok:
 	list_for_each_entry(child, &device->children, node)
 		acpi_bus_attach(child);
+
+	if (device->handler && device->handler->hotplug.notify_online)
+		device->handler->hotplug.notify_online(device);
 }
 
 /**
diff --git a/drivers/ata/ahci.c b/drivers/ata/ahci.c
index b54f8b3c7924..00663d60f6d4 100644
--- a/drivers/ata/ahci.c
+++ b/drivers/ata/ahci.c
@@ -306,6 +306,14 @@ static const struct pci_device_id ahci_pci_tbl[] = {
 	{ PCI_VDEVICE(INTEL, 0x9c85), board_ahci }, /* Wildcat Point-LP RAID */
 	{ PCI_VDEVICE(INTEL, 0x9c87), board_ahci }, /* Wildcat Point-LP RAID */
 	{ PCI_VDEVICE(INTEL, 0x9c8f), board_ahci }, /* Wildcat Point-LP RAID */
+	{ PCI_VDEVICE(INTEL, 0x8c82), board_ahci }, /* 9 Series AHCI */
+	{ PCI_VDEVICE(INTEL, 0x8c83), board_ahci }, /* 9 Series AHCI */
+	{ PCI_VDEVICE(INTEL, 0x8c84), board_ahci }, /* 9 Series RAID */
+	{ PCI_VDEVICE(INTEL, 0x8c85), board_ahci }, /* 9 Series RAID */
+	{ PCI_VDEVICE(INTEL, 0x8c86), board_ahci }, /* 9 Series RAID */
+	{ PCI_VDEVICE(INTEL, 0x8c87), board_ahci }, /* 9 Series RAID */
+	{ PCI_VDEVICE(INTEL, 0x8c8e), board_ahci }, /* 9 Series RAID */
+	{ PCI_VDEVICE(INTEL, 0x8c8f), board_ahci }, /* 9 Series RAID */
 
 	/* JMicron 360/1/3/5/6, match class to avoid IDE function */
 	{ PCI_VENDOR_ID_JMICRON, PCI_ANY_ID, PCI_ANY_ID, PCI_ANY_ID,
@@ -443,6 +451,8 @@ static const struct pci_device_id ahci_pci_tbl[] = {
 	{ PCI_DEVICE(PCI_VENDOR_ID_MARVELL_EXT, 0x917a),
 	  .driver_data = board_ahci_yes_fbs },			/* 88se9172 */
 	{ PCI_DEVICE(PCI_VENDOR_ID_MARVELL_EXT, 0x9172),
+	  .driver_data = board_ahci_yes_fbs },			/* 88se9182 */
+	{ PCI_DEVICE(PCI_VENDOR_ID_MARVELL_EXT, 0x9182),
 	  .driver_data = board_ahci_yes_fbs },			/* 88se9172 */
 	{ PCI_DEVICE(PCI_VENDOR_ID_MARVELL_EXT, 0x9192),
 	  .driver_data = board_ahci_yes_fbs },			/* 88se9172 on some Gigabyte */
diff --git a/drivers/ata/ata_piix.c b/drivers/ata/ata_piix.c
index 6334c8d7c3f1..39f76b987c75 100644
--- a/drivers/ata/ata_piix.c
+++ b/drivers/ata/ata_piix.c
@@ -340,6 +340,14 @@ static const struct pci_device_id piix_pci_tbl[] = {
 	{ 0x8086, 0x0F21, PCI_ANY_ID, PCI_ANY_ID, 0, 0, ich8_2port_sata_byt },
 	/* SATA Controller IDE (Coleto Creek) */
 	{ 0x8086, 0x23a6, PCI_ANY_ID, PCI_ANY_ID, 0, 0, ich8_2port_sata },
+	/* SATA Controller IDE (9 Series) */
+	{ 0x8086, 0x8c88, PCI_ANY_ID, PCI_ANY_ID, 0, 0, ich8_2port_sata_snb },
+	/* SATA Controller IDE (9 Series) */
+	{ 0x8086, 0x8c89, PCI_ANY_ID, PCI_ANY_ID, 0, 0, ich8_2port_sata_snb },
+	/* SATA Controller IDE (9 Series) */
+	{ 0x8086, 0x8c80, PCI_ANY_ID, PCI_ANY_ID, 0, 0, ich8_sata_snb },
+	/* SATA Controller IDE (9 Series) */
+	{ 0x8086, 0x8c81, PCI_ANY_ID, PCI_ANY_ID, 0, 0, ich8_sata_snb },
 
 	{ }	/* terminate list */
 };
diff --git a/drivers/ata/libata-core.c b/drivers/ata/libata-core.c
index f7616036663b..538574f98e22 100644
--- a/drivers/ata/libata-core.c
+++ b/drivers/ata/libata-core.c
@@ -4227,7 +4227,7 @@ static const struct ata_blacklist_entry ata_device_blacklist [] = {
 	{ "Micron_M500*",		NULL,	ATA_HORKAGE_NO_NCQ_TRIM, },
 	{ "Crucial_CT???M500SSD*",	NULL,	ATA_HORKAGE_NO_NCQ_TRIM, },
 	{ "Micron_M550*",		NULL,	ATA_HORKAGE_NO_NCQ_TRIM, },
-	{ "Crucial_CT???M550SSD*",	NULL,	ATA_HORKAGE_NO_NCQ_TRIM, },
+	{ "Crucial_CT*M550SSD*",	NULL,	ATA_HORKAGE_NO_NCQ_TRIM, },
 
 	/*
 	 * Some WD SATA-I drives spin up and down erratically when the link
diff --git a/drivers/ata/pata_scc.c b/drivers/ata/pata_scc.c
index f35f15f4d83e..f7badaa39eb6 100644
--- a/drivers/ata/pata_scc.c
+++ b/drivers/ata/pata_scc.c
@@ -586,7 +586,7 @@ static int scc_wait_after_reset(struct ata_link *link, unsigned int devmask,
  *	Note: Original code is ata_bus_softreset().
  */
 
-static unsigned int scc_bus_softreset(struct ata_port *ap, unsigned int devmask,
+static int scc_bus_softreset(struct ata_port *ap, unsigned int devmask,
                                       unsigned long deadline)
 {
 	struct ata_ioports *ioaddr = &ap->ioaddr;
@@ -600,9 +600,7 @@ static unsigned int scc_bus_softreset(struct ata_port *ap, unsigned int devmask,
 	udelay(20);
 	out_be32(ioaddr->ctl_addr, ap->ctl);
 
-	scc_wait_after_reset(&ap->link, devmask, deadline);
-
-	return 0;
+	return scc_wait_after_reset(&ap->link, devmask, deadline);
 }
 
 /**
@@ -619,7 +617,8 @@ static int scc_softreset(struct ata_link *link, unsigned int *classes,
 {
 	struct ata_port *ap = link->ap;
 	unsigned int slave_possible = ap->flags & ATA_FLAG_SLAVE_POSS;
-	unsigned int devmask = 0, err_mask;
+	unsigned int devmask = 0;
+	int rc;
 	u8 err;
 
 	DPRINTK("ENTER\n");
@@ -635,9 +634,9 @@ static int scc_softreset(struct ata_link *link, unsigned int *classes,
 
 	/* issue bus reset */
 	DPRINTK("about to softreset, devmask=%x\n", devmask);
-	err_mask = scc_bus_softreset(ap, devmask, deadline);
-	if (err_mask) {
-		ata_port_err(ap, "SRST failed (err_mask=0x%x)\n", err_mask);
+	rc = scc_bus_softreset(ap, devmask, deadline);
+	if (rc) {
+		ata_port_err(ap, "SRST failed (err_mask=0x%x)\n", rc);
 		return -EIO;
 	}
 
diff --git a/drivers/base/regmap/regcache.c b/drivers/base/regmap/regcache.c
index d4dd77134814..154e7a8c0a04 100644
--- a/drivers/base/regmap/regcache.c
+++ b/drivers/base/regmap/regcache.c
@@ -701,7 +701,7 @@ int regcache_sync_block(struct regmap *map, void *block,
 			unsigned int block_base, unsigned int start,
 			unsigned int end)
 {
-	if (regmap_can_raw_write(map))
+	if (regmap_can_raw_write(map) && !map->use_single_rw)
 		return regcache_sync_block_raw(map, block, cache_present,
 					       block_base, start, end);
 	else
diff --git a/drivers/base/regmap/regmap.c b/drivers/base/regmap/regmap.c
index 6a19515f8a45..2ea056c09aeb 100644
--- a/drivers/base/regmap/regmap.c
+++ b/drivers/base/regmap/regmap.c
@@ -105,7 +105,7 @@ bool regmap_readable(struct regmap *map, unsigned int reg)
 
 bool regmap_volatile(struct regmap *map, unsigned int reg)
 {
-	if (!regmap_readable(map, reg))
+	if (!map->format.format_write && !regmap_readable(map, reg))
 		return false;
 
 	if (map->volatile_reg)
diff --git a/drivers/clk/clk.c b/drivers/clk/clk.c
index b94a311e5ab6..f9c4632d4dd3 100644
--- a/drivers/clk/clk.c
+++ b/drivers/clk/clk.c
@@ -1487,6 +1487,7 @@ static struct clk *clk_propagate_rate_change(struct clk *clk, unsigned long even
 static void clk_change_rate(struct clk *clk)
 {
 	struct clk *child;
+	struct hlist_node *tmp;
 	unsigned long old_rate;
 	unsigned long best_parent_rate = 0;
 	bool skip_set_rate = false;
@@ -1525,7 +1526,11 @@ static void clk_change_rate(struct clk *clk)
 	if (clk->notifier_count && old_rate != clk->rate)
 		__clk_notify(clk, POST_RATE_CHANGE, old_rate, clk->rate);
 
-	hlist_for_each_entry(child, &clk->children, child_node) {
+	/*
+	 * Use safe iteration, as change_rate can actually swap parents
+	 * for certain clock types.
+	 */
+	hlist_for_each_entry_safe(child, tmp, &clk->children, child_node) {
 		/* Skip children who will be reparented to another clock */
 		if (child->new_parent && child->new_parent != clk)
 			continue;
diff --git a/drivers/clk/qcom/mmcc-msm8960.c b/drivers/clk/qcom/mmcc-msm8960.c
index 9be47a829144..f3c95d648a53 100644
--- a/drivers/clk/qcom/mmcc-msm8960.c
+++ b/drivers/clk/qcom/mmcc-msm8960.c
@@ -37,6 +37,8 @@
 #define P_PLL2	2
 #define P_PLL3	3
 
+#define F_MN(f, s, _m, _n) { .freq = f, .src = s, .m = _m, .n = _n }
+
 static u8 mmcc_pxo_pll8_pll2_map[] = {
 	[P_PXO]		= 0,
 	[P_PLL8]	= 2,
@@ -58,8 +60,8 @@ static u8 mmcc_pxo_pll8_pll2_pll3_map[] = {
 
 static const char *mmcc_pxo_pll8_pll2_pll3[] = {
 	"pxo",
-	"pll2",
 	"pll8_vote",
+	"pll2",
 	"pll3",
 };
 
@@ -709,18 +711,18 @@ static struct clk_branch csiphy2_timer_clk = {
 };
 
 static struct freq_tbl clk_tbl_gfx2d[] = {
-	{  27000000, P_PXO,  1,  0 },
-	{  48000000, P_PLL8, 1,  8 },
-	{  54857000, P_PLL8, 1,  7 },
-	{  64000000, P_PLL8, 1,  6 },
-	{  76800000, P_PLL8, 1,  5 },
-	{  96000000, P_PLL8, 1,  4 },
-	{ 128000000, P_PLL8, 1,  3 },
-	{ 145455000, P_PLL2, 2, 11 },
-	{ 160000000, P_PLL2, 1,  5 },
-	{ 177778000, P_PLL2, 2,  9 },
-	{ 200000000, P_PLL2, 1,  4 },
-	{ 228571000, P_PLL2, 2,  7 },
+	F_MN( 27000000, P_PXO,  1,  0),
+	F_MN( 48000000, P_PLL8, 1,  8),
+	F_MN( 54857000, P_PLL8, 1,  7),
+	F_MN( 64000000, P_PLL8, 1,  6),
+	F_MN( 76800000, P_PLL8, 1,  5),
+	F_MN( 96000000, P_PLL8, 1,  4),
+	F_MN(128000000, P_PLL8, 1,  3),
+	F_MN(145455000, P_PLL2, 2, 11),
+	F_MN(160000000, P_PLL2, 1,  5),
+	F_MN(177778000, P_PLL2, 2,  9),
+	F_MN(200000000, P_PLL2, 1,  4),
+	F_MN(228571000, P_PLL2, 2,  7),
 	{ }
 };
 
@@ -841,22 +843,22 @@ static struct clk_branch gfx2d1_clk = {
 };
 
 static struct freq_tbl clk_tbl_gfx3d[] = {
-	{  27000000, P_PXO,  1,  0 },
-	{  48000000, P_PLL8, 1,  8 },
-	{  54857000, P_PLL8, 1,  7 },
-	{  64000000, P_PLL8, 1,  6 },
-	{  76800000, P_PLL8, 1,  5 },
-	{  96000000, P_PLL8, 1,  4 },
-	{ 128000000, P_PLL8, 1,  3 },
-	{ 145455000, P_PLL2, 2, 11 },
-	{ 160000000, P_PLL2, 1,  5 },
-	{ 177778000, P_PLL2, 2,  9 },
-	{ 200000000, P_PLL2, 1,  4 },
-	{ 228571000, P_PLL2, 2,  7 },
-	{ 266667000, P_PLL2, 1,  3 },
-	{ 300000000, P_PLL3, 1,  4 },
-	{ 320000000, P_PLL2, 2,  5 },
-	{ 400000000, P_PLL2, 1,  2 },
+	F_MN( 27000000, P_PXO,  1,  0),
+	F_MN( 48000000, P_PLL8, 1,  8),
+	F_MN( 54857000, P_PLL8, 1,  7),
+	F_MN( 64000000, P_PLL8, 1,  6),
+	F_MN( 76800000, P_PLL8, 1,  5),
+	F_MN( 96000000, P_PLL8, 1,  4),
+	F_MN(128000000, P_PLL8, 1,  3),
+	F_MN(145455000, P_PLL2, 2, 11),
+	F_MN(160000000, P_PLL2, 1,  5),
+	F_MN(177778000, P_PLL2, 2,  9),
+	F_MN(200000000, P_PLL2, 1,  4),
+	F_MN(228571000, P_PLL2, 2,  7),
+	F_MN(266667000, P_PLL2, 1,  3),
+	F_MN(300000000, P_PLL3, 1,  4),
+	F_MN(320000000, P_PLL2, 2,  5),
+	F_MN(400000000, P_PLL2, 1,  2),
 	{ }
 };
 
@@ -896,7 +898,7 @@ static struct clk_dyn_rcg gfx3d_src = {
 		.hw.init = &(struct clk_init_data){
 			.name = "gfx3d_src",
 			.parent_names = mmcc_pxo_pll8_pll2_pll3,
-			.num_parents = 3,
+			.num_parents = 4,
 			.ops = &clk_dyn_rcg_ops,
 		},
 	},
@@ -994,7 +996,7 @@ static struct clk_rcg jpegd_src = {
 	.ns_reg = 0x00ac,
 	.p = {
 		.pre_div_shift = 12,
-		.pre_div_width = 2,
+		.pre_div_width = 4,
 	},
 	.s = {
 		.src_sel_shift = 0,
@@ -1114,7 +1116,7 @@ static struct clk_branch mdp_lut_clk = {
 		.enable_reg = 0x016c,
 		.enable_mask = BIT(0),
 		.hw.init = &(struct clk_init_data){
-			.parent_names = (const char *[]){ "mdp_clk" },
+			.parent_names = (const char *[]){ "mdp_src" },
 			.num_parents = 1,
 			.name = "mdp_lut_clk",
 			.ops = &clk_branch_ops,
@@ -1341,15 +1343,15 @@ static struct clk_branch hdmi_app_clk = {
 };
 
 static struct freq_tbl clk_tbl_vcodec[] = {
-	{  27000000, P_PXO,  1,  0 },
-	{  32000000, P_PLL8, 1, 12 },
-	{  48000000, P_PLL8, 1,  8 },
-	{  54860000, P_PLL8, 1,  7 },
-	{  96000000, P_PLL8, 1,  4 },
-	{ 133330000, P_PLL2, 1,  6 },
-	{ 200000000, P_PLL2, 1,  4 },
-	{ 228570000, P_PLL2, 2,  7 },
-	{ 266670000, P_PLL2, 1,  3 },
+	F_MN( 27000000, P_PXO,  1,  0),
+	F_MN( 32000000, P_PLL8, 1, 12),
+	F_MN( 48000000, P_PLL8, 1,  8),
+	F_MN( 54860000, P_PLL8, 1,  7),
+	F_MN( 96000000, P_PLL8, 1,  4),
+	F_MN(133330000, P_PLL2, 1,  6),
+	F_MN(200000000, P_PLL2, 1,  4),
+	F_MN(228570000, P_PLL2, 2,  7),
+	F_MN(266670000, P_PLL2, 1,  3),
 	{ }
 };
 
diff --git a/drivers/cpufreq/cpufreq.c b/drivers/cpufreq/cpufreq.c
index 153f4b92cc05..415923606164 100644
--- a/drivers/cpufreq/cpufreq.c
+++ b/drivers/cpufreq/cpufreq.c
@@ -1225,6 +1225,8 @@ err_get_freq:
 		per_cpu(cpufreq_cpu_data, j) = NULL;
 	write_unlock_irqrestore(&cpufreq_driver_lock, flags);
 
+	up_write(&policy->rwsem);
+
 	if (cpufreq_driver->exit)
 		cpufreq_driver->exit(policy);
 err_set_policy_cpu:
diff --git a/drivers/dma/TODO b/drivers/dma/TODO
index 734ed0206cd5..b8045cd42ee1 100644
--- a/drivers/dma/TODO
+++ b/drivers/dma/TODO
@@ -7,7 +7,6 @@ TODO for slave dma
 	- imx-dma
 	- imx-sdma
 	- mxs-dma.c
-	- dw_dmac
 	- intel_mid_dma
 4. Check other subsystems for dma drivers and merge/move to dmaengine
 5. Remove dma_slave_config's dma direction.
diff --git a/drivers/dma/dw/core.c b/drivers/dma/dw/core.c
index 01a200cd0189..b0972b3869c7 100644
--- a/drivers/dma/dw/core.c
+++ b/drivers/dma/dw/core.c
@@ -279,6 +279,15 @@ static void dwc_dostart(struct dw_dma_chan *dwc, struct dw_desc *first)
 	channel_set_bit(dw, CH_EN, dwc->mask);
 }
 
+static void dwc_dostart_first_queued(struct dw_dma_chan *dwc)
+{
+	if (list_empty(&dwc->queue))
+		return;
+
+	list_move(dwc->queue.next, &dwc->active_list);
+	dwc_dostart(dwc, dwc_first_active(dwc));
+}
+
 /*----------------------------------------------------------------------*/
 
 static void
@@ -335,10 +344,7 @@ static void dwc_complete_all(struct dw_dma *dw, struct dw_dma_chan *dwc)
 	 * the completed ones.
 	 */
 	list_splice_init(&dwc->active_list, &list);
-	if (!list_empty(&dwc->queue)) {
-		list_move(dwc->queue.next, &dwc->active_list);
-		dwc_dostart(dwc, dwc_first_active(dwc));
-	}
+	dwc_dostart_first_queued(dwc);
 
 	spin_unlock_irqrestore(&dwc->lock, flags);
 
@@ -467,10 +473,7 @@ static void dwc_scan_descriptors(struct dw_dma *dw, struct dw_dma_chan *dwc)
 	/* Try to continue after resetting the channel... */
 	dwc_chan_disable(dw, dwc);
 
-	if (!list_empty(&dwc->queue)) {
-		list_move(dwc->queue.next, &dwc->active_list);
-		dwc_dostart(dwc, dwc_first_active(dwc));
-	}
+	dwc_dostart_first_queued(dwc);
 	spin_unlock_irqrestore(&dwc->lock, flags);
 }
 
@@ -677,17 +680,9 @@ static dma_cookie_t dwc_tx_submit(struct dma_async_tx_descriptor *tx)
 	 * possible, perhaps even appending to those already submitted
 	 * for DMA. But this is hard to do in a race-free manner.
 	 */
-	if (list_empty(&dwc->active_list)) {
-		dev_vdbg(chan2dev(tx->chan), "%s: started %u\n", __func__,
-				desc->txd.cookie);
-		list_add_tail(&desc->desc_node, &dwc->active_list);
-		dwc_dostart(dwc, dwc_first_active(dwc));
-	} else {
-		dev_vdbg(chan2dev(tx->chan), "%s: queued %u\n", __func__,
-				desc->txd.cookie);
 
-		list_add_tail(&desc->desc_node, &dwc->queue);
-	}
+	dev_vdbg(chan2dev(tx->chan), "%s: queued %u\n", __func__, desc->txd.cookie);
+	list_add_tail(&desc->desc_node, &dwc->queue);
 
 	spin_unlock_irqrestore(&dwc->lock, flags);
 
@@ -1092,9 +1087,12 @@ dwc_tx_status(struct dma_chan *chan,
 static void dwc_issue_pending(struct dma_chan *chan)
 {
 	struct dw_dma_chan	*dwc = to_dw_dma_chan(chan);
+	unsigned long		flags;
 
-	if (!list_empty(&dwc->queue))
-		dwc_scan_descriptors(to_dw_dma(chan->device), dwc);
+	spin_lock_irqsave(&dwc->lock, flags);
+	if (list_empty(&dwc->active_list))
+		dwc_dostart_first_queued(dwc);
+	spin_unlock_irqrestore(&dwc->lock, flags);
 }
 
 static int dwc_alloc_chan_resources(struct dma_chan *chan)
diff --git a/drivers/gpu/drm/ast/ast_main.c b/drivers/gpu/drm/ast/ast_main.c
index 50535fd5a88d..d830b38e54f6 100644
--- a/drivers/gpu/drm/ast/ast_main.c
+++ b/drivers/gpu/drm/ast/ast_main.c
@@ -100,7 +100,7 @@ static int ast_detect_chip(struct drm_device *dev)
 			}
 			ast->vga2_clone = false;
 		} else {
-			ast->chip = 2000;
+			ast->chip = AST2000;
 			DRM_INFO("AST 2000 detected\n");
 		}
 	}
diff --git a/drivers/gpu/drm/i915/i915_gem.c b/drivers/gpu/drm/i915/i915_gem.c
index 3ecb332e7cfa..7410a507eacc 100644
--- a/drivers/gpu/drm/i915/i915_gem.c
+++ b/drivers/gpu/drm/i915/i915_gem.c
@@ -1426,10 +1426,13 @@ unlock:
 out:
 	switch (ret) {
 	case -EIO:
-		/* If this -EIO is due to a gpu hang, give the reset code a
-		 * chance to clean up the mess. Otherwise return the proper
-		 * SIGBUS. */
-		if (i915_terminally_wedged(&dev_priv->gpu_error)) {
+		/*
+		 * We eat errors when the gpu is terminally wedged to avoid
+		 * userspace unduly crashing (gl has no provisions for mmaps to
+		 * fail). But any other -EIO isn't ours (e.g. swap in failure)
+		 * and so needs to be reported.
+		 */
+		if (!i915_terminally_wedged(&dev_priv->gpu_error)) {
 			ret = VM_FAULT_SIGBUS;
 			break;
 		}
diff --git a/drivers/gpu/drm/i915/intel_bios.c b/drivers/gpu/drm/i915/intel_bios.c
index f22041973f3a..08105fddfd2a 100644
--- a/drivers/gpu/drm/i915/intel_bios.c
+++ b/drivers/gpu/drm/i915/intel_bios.c
@@ -839,7 +839,7 @@ init_vbt_defaults(struct drm_i915_private *dev_priv)
 	}
 }
 
-static int __init intel_no_opregion_vbt_callback(const struct dmi_system_id *id)
+static int intel_no_opregion_vbt_callback(const struct dmi_system_id *id)
 {
 	DRM_DEBUG_KMS("Falling back to manually reading VBT from "
 		      "VBIOS ROM for %s\n",
diff --git a/drivers/gpu/drm/i915/intel_crt.c b/drivers/gpu/drm/i915/intel_crt.c
index b19ddacbe19d..834847527982 100644
--- a/drivers/gpu/drm/i915/intel_crt.c
+++ b/drivers/gpu/drm/i915/intel_crt.c
@@ -750,7 +750,7 @@ static const struct drm_encoder_funcs intel_crt_enc_funcs = {
 	.destroy = intel_encoder_destroy,
 };
 
-static int __init intel_no_crt_dmi_callback(const struct dmi_system_id *id)
+static int intel_no_crt_dmi_callback(const struct dmi_system_id *id)
 {
 	DRM_INFO("Skipping CRT initialization for %s\n", id->ident);
 	return 1;
diff --git a/drivers/gpu/drm/i915/intel_lvds.c b/drivers/gpu/drm/i915/intel_lvds.c
index eb8f64b5fb85..67c9ff389989 100644
--- a/drivers/gpu/drm/i915/intel_lvds.c
+++ b/drivers/gpu/drm/i915/intel_lvds.c
@@ -544,7 +544,7 @@ static const struct drm_encoder_funcs intel_lvds_enc_funcs = {
 	.destroy = intel_encoder_destroy,
 };
 
-static int __init intel_no_lvds_dmi_callback(const struct dmi_system_id *id)
+static int intel_no_lvds_dmi_callback(const struct dmi_system_id *id)
 {
 	DRM_INFO("Skipping LVDS initialization for %s\n", id->ident);
 	return 1;
diff --git a/drivers/gpu/drm/i915/intel_ringbuffer.c b/drivers/gpu/drm/i915/intel_ringbuffer.c
index 31b36c5ac894..d488fc71ef49 100644
--- a/drivers/gpu/drm/i915/intel_ringbuffer.c
+++ b/drivers/gpu/drm/i915/intel_ringbuffer.c
@@ -475,6 +475,9 @@ static int init_ring_common(struct intel_ring_buffer *ring)
 		}
 	}
 
+	/* Enforce ordering by reading HEAD register back */
+	I915_READ_HEAD(ring);
+
 	/* Initialize the ring. This must happen _after_ we've cleared the ring
 	 * registers with the above sequence (the readback of the HEAD registers
 	 * also enforces ordering), otherwise the hw might lose the new ring
diff --git a/drivers/gpu/drm/i915/intel_tv.c b/drivers/gpu/drm/i915/intel_tv.c
index 365c7c47c46c..9c9606c8bb1a 100644
--- a/drivers/gpu/drm/i915/intel_tv.c
+++ b/drivers/gpu/drm/i915/intel_tv.c
@@ -854,6 +854,10 @@ intel_enable_tv(struct intel_encoder *encoder)
 	struct drm_device *dev = encoder->base.dev;
 	struct drm_i915_private *dev_priv = dev->dev_private;
 
+	/* Prevents vblank waits from timing out in intel_tv_detect_type() */
+	intel_wait_for_vblank(encoder->base.dev,
+			      to_intel_crtc(encoder->base.crtc)->pipe);
+
 	I915_WRITE(TV_CTL, I915_READ(TV_CTL) | TV_ENC_ENABLE);
 }
 
diff --git a/drivers/gpu/drm/nouveau/nouveau_vga.c b/drivers/gpu/drm/nouveau/nouveau_vga.c
index 471347edc27e..a92fb01459c9 100644
--- a/drivers/gpu/drm/nouveau/nouveau_vga.c
+++ b/drivers/gpu/drm/nouveau/nouveau_vga.c
@@ -100,7 +100,16 @@ void
 nouveau_vga_fini(struct nouveau_drm *drm)
 {
 	struct drm_device *dev = drm->dev;
+	bool runtime = false;
+
+	if (nouveau_runtime_pm == 1)
+		runtime = true;
+	if ((nouveau_runtime_pm == -1) && (nouveau_is_optimus() || nouveau_is_v1_dsm()))
+		runtime = true;
+
 	vga_switcheroo_unregister_client(dev->pdev);
+	if (runtime && nouveau_is_v1_dsm() && !nouveau_is_optimus())
+		vga_switcheroo_fini_domain_pm_ops(drm->dev->dev);
 	vga_client_register(dev->pdev, NULL, NULL, NULL);
 }
 
diff --git a/drivers/gpu/drm/radeon/ci_dpm.c b/drivers/gpu/drm/radeon/ci_dpm.c
index 5fa854c84d62..543ba2d4a659 100644
--- a/drivers/gpu/drm/radeon/ci_dpm.c
+++ b/drivers/gpu/drm/radeon/ci_dpm.c
@@ -851,6 +851,9 @@ static int ci_set_thermal_temperature_range(struct radeon_device *rdev,
 	WREG32_SMC(CG_THERMAL_CTRL, tmp);
 #endif
 
+	rdev->pm.dpm.thermal.min_temp = low_temp;
+	rdev->pm.dpm.thermal.max_temp = high_temp;
+
 	return 0;
 }
 
@@ -922,7 +925,18 @@ static void ci_get_leakage_voltages(struct radeon_device *rdev)
 	pi->vddc_leakage.count = 0;
 	pi->vddci_leakage.count = 0;
 
-	if (radeon_atom_get_leakage_id_from_vbios(rdev, &leakage_id) == 0) {
+	if (rdev->pm.dpm.platform_caps & ATOM_PP_PLATFORM_CAP_EVV) {
+		for (i = 0; i < CISLANDS_MAX_LEAKAGE_COUNT; i++) {
+			virtual_voltage_id = ATOM_VIRTUAL_VOLTAGE_ID0 + i;
+			if (radeon_atom_get_voltage_evv(rdev, virtual_voltage_id, &vddc) != 0)
+				continue;
+			if (vddc != 0 && vddc != virtual_voltage_id) {
+				pi->vddc_leakage.actual_voltage[pi->vddc_leakage.count] = vddc;
+				pi->vddc_leakage.leakage_id[pi->vddc_leakage.count] = virtual_voltage_id;
+				pi->vddc_leakage.count++;
+			}
+		}
+	} else if (radeon_atom_get_leakage_id_from_vbios(rdev, &leakage_id) == 0) {
 		for (i = 0; i < CISLANDS_MAX_LEAKAGE_COUNT; i++) {
 			virtual_voltage_id = ATOM_VIRTUAL_VOLTAGE_ID0 + i;
 			if (radeon_atom_get_leakage_vddc_based_on_leakage_params(rdev, &vddc, &vddci,
diff --git a/drivers/gpu/drm/radeon/cik.c b/drivers/gpu/drm/radeon/cik.c
index 7b3537c55c77..ab5c26575622 100644
--- a/drivers/gpu/drm/radeon/cik.c
+++ b/drivers/gpu/drm/radeon/cik.c
@@ -4392,7 +4392,7 @@ struct bonaire_mqd
  */
 static int cik_cp_compute_resume(struct radeon_device *rdev)
 {
-	int r, i, idx;
+	int r, i, j, idx;
 	u32 tmp;
 	bool use_doorbell = true;
 	u64 hqd_gpu_addr;
@@ -4511,7 +4511,7 @@ static int cik_cp_compute_resume(struct radeon_device *rdev)
 		mqd->queue_state.cp_hqd_pq_wptr= 0;
 		if (RREG32(CP_HQD_ACTIVE) & 1) {
 			WREG32(CP_HQD_DEQUEUE_REQUEST, 1);
-			for (i = 0; i < rdev->usec_timeout; i++) {
+			for (j = 0; j < rdev->usec_timeout; j++) {
 				if (!(RREG32(CP_HQD_ACTIVE) & 1))
 					break;
 				udelay(1);
@@ -5545,12 +5545,13 @@ static void cik_vm_decode_fault(struct radeon_device *rdev,
 void cik_vm_flush(struct radeon_device *rdev, int ridx, struct radeon_vm *vm)
 {
 	struct radeon_ring *ring = &rdev->ring[ridx];
+	int usepfp = (ridx == RADEON_RING_TYPE_GFX_INDEX);
 
 	if (vm == NULL)
 		return;
 
 	radeon_ring_write(ring, PACKET3(PACKET3_WRITE_DATA, 3));
-	radeon_ring_write(ring, (WRITE_DATA_ENGINE_SEL(0) |
+	radeon_ring_write(ring, (WRITE_DATA_ENGINE_SEL(usepfp) |
 				 WRITE_DATA_DST_SEL(0)));
 	if (vm->id < 8) {
 		radeon_ring_write(ring,
@@ -5600,7 +5601,7 @@ void cik_vm_flush(struct radeon_device *rdev, int ridx, struct radeon_vm *vm)
 	radeon_ring_write(ring, 1 << vm->id);
 
 	/* compute doesn't have PFP */
-	if (ridx == RADEON_RING_TYPE_GFX_INDEX) {
+	if (usepfp) {
 		/* sync PFP to ME, otherwise we might get invalid PFP reads */
 		radeon_ring_write(ring, PACKET3(PACKET3_PFP_SYNC_ME, 0));
 		radeon_ring_write(ring, 0x0);
diff --git a/drivers/gpu/drm/radeon/cik_sdma.c b/drivers/gpu/drm/radeon/cik_sdma.c
index aac8f487e6df..66ba713ba7d7 100644
--- a/drivers/gpu/drm/radeon/cik_sdma.c
+++ b/drivers/gpu/drm/radeon/cik_sdma.c
@@ -461,13 +461,6 @@ int cik_sdma_resume(struct radeon_device *rdev)
 {
 	int r;
 
-	/* Reset dma */
-	WREG32(SRBM_SOFT_RESET, SOFT_RESET_SDMA | SOFT_RESET_SDMA1);
-	RREG32(SRBM_SOFT_RESET);
-	udelay(50);
-	WREG32(SRBM_SOFT_RESET, 0);
-	RREG32(SRBM_SOFT_RESET);
-
 	r = cik_sdma_load_microcode(rdev);
 	if (r)
 		return r;
diff --git a/drivers/gpu/drm/radeon/ni_dma.c b/drivers/gpu/drm/radeon/ni_dma.c
index 7cf96b15377f..94fa49e974eb 100644
--- a/drivers/gpu/drm/radeon/ni_dma.c
+++ b/drivers/gpu/drm/radeon/ni_dma.c
@@ -191,12 +191,6 @@ int cayman_dma_resume(struct radeon_device *rdev)
 	u32 reg_offset, wb_offset;
 	int i, r;
 
-	/* Reset dma */
-	WREG32(SRBM_SOFT_RESET, SOFT_RESET_DMA | SOFT_RESET_DMA1);
-	RREG32(SRBM_SOFT_RESET);
-	udelay(50);
-	WREG32(SRBM_SOFT_RESET, 0);
-
 	for (i = 0; i < 2; i++) {
 		if (i == 0) {
 			ring = &rdev->ring[R600_RING_TYPE_DMA_INDEX];
diff --git a/drivers/gpu/drm/radeon/r600_dma.c b/drivers/gpu/drm/radeon/r600_dma.c
index b2d4c91e6272..99495513f6b1 100644
--- a/drivers/gpu/drm/radeon/r600_dma.c
+++ b/drivers/gpu/drm/radeon/r600_dma.c
@@ -124,15 +124,6 @@ int r600_dma_resume(struct radeon_device *rdev)
 	u32 rb_bufsz;
 	int r;
 
-	/* Reset dma */
-	if (rdev->family >= CHIP_RV770)
-		WREG32(SRBM_SOFT_RESET, RV770_SOFT_RESET_DMA);
-	else
-		WREG32(SRBM_SOFT_RESET, SOFT_RESET_DMA);
-	RREG32(SRBM_SOFT_RESET);
-	udelay(50);
-	WREG32(SRBM_SOFT_RESET, 0);
-
 	WREG32(DMA_SEM_INCOMPLETE_TIMER_CNTL, 0);
 	WREG32(DMA_SEM_WAIT_FAIL_TIMER_CNTL, 0);
 
diff --git a/drivers/gpu/drm/radeon/radeon.h b/drivers/gpu/drm/radeon/radeon.h
index 08e86f90c9a4..b837e9f9f8ce 100644
--- a/drivers/gpu/drm/radeon/radeon.h
+++ b/drivers/gpu/drm/radeon/radeon.h
@@ -294,6 +294,9 @@ int radeon_atom_get_leakage_vddc_based_on_leakage_params(struct radeon_device *r
 							 u16 *vddc, u16 *vddci,
 							 u16 virtual_voltage_id,
 							 u16 vbios_voltage_id);
+int radeon_atom_get_voltage_evv(struct radeon_device *rdev,
+				u16 virtual_voltage_id,
+				u16 *voltage);
 int radeon_atom_round_to_true_voltage(struct radeon_device *rdev,
 				      u8 voltage_type,
 				      u16 nominal_voltage,
diff --git a/drivers/gpu/drm/radeon/radeon_atombios.c b/drivers/gpu/drm/radeon/radeon_atombios.c
index 30844814c25a..e2de749327ad 100644
--- a/drivers/gpu/drm/radeon/radeon_atombios.c
+++ b/drivers/gpu/drm/radeon/radeon_atombios.c
@@ -447,6 +447,13 @@ static bool radeon_atom_apply_quirks(struct drm_device *dev,
 		}
 	}
 
+	/* Fujitsu D3003-S2 board lists DVI-I as DVI-I and VGA */
+	if ((dev->pdev->device == 0x9805) &&
+	    (dev->pdev->subsystem_vendor == 0x1734) &&
+	    (dev->pdev->subsystem_device == 0x11bd)) {
+		if (*connector_type == DRM_MODE_CONNECTOR_VGA)
+			return false;
+	}
 
 	return true;
 }
@@ -1955,7 +1962,7 @@ static const char *thermal_controller_names[] = {
 	"adm1032",
 	"adm1030",
 	"max6649",
-	"lm64",
+	"lm63", /* lm64 */
 	"f75375",
 	"asc7xxx",
 };
@@ -1966,7 +1973,7 @@ static const char *pp_lib_thermal_controller_names[] = {
 	"adm1032",
 	"adm1030",
 	"max6649",
-	"lm64",
+	"lm63", /* lm64 */
 	"f75375",
 	"RV6xx",
 	"RV770",
@@ -2273,19 +2280,31 @@ static void radeon_atombios_add_pplib_thermal_controller(struct radeon_device *r
 				 (controller->ucFanParameters &
 				  ATOM_PP_FANPARAMETERS_NOFAN) ? "without" : "with");
 			rdev->pm.int_thermal_type = THERMAL_TYPE_KV;
-		} else if ((controller->ucType ==
-			    ATOM_PP_THERMALCONTROLLER_EXTERNAL_GPIO) ||
-			   (controller->ucType ==
-			    ATOM_PP_THERMALCONTROLLER_ADT7473_WITH_INTERNAL) ||
-			   (controller->ucType ==
-			    ATOM_PP_THERMALCONTROLLER_EMC2103_WITH_INTERNAL)) {
-			DRM_INFO("Special thermal controller config\n");
+		} else if (controller->ucType ==
+			   ATOM_PP_THERMALCONTROLLER_EXTERNAL_GPIO) {
+			DRM_INFO("External GPIO thermal controller %s fan control\n",
+				 (controller->ucFanParameters &
+				  ATOM_PP_FANPARAMETERS_NOFAN) ? "without" : "with");
+			rdev->pm.int_thermal_type = THERMAL_TYPE_EXTERNAL_GPIO;
+		} else if (controller->ucType ==
+			   ATOM_PP_THERMALCONTROLLER_ADT7473_WITH_INTERNAL) {
+			DRM_INFO("ADT7473 with internal thermal controller %s fan control\n",
+				 (controller->ucFanParameters &
+				  ATOM_PP_FANPARAMETERS_NOFAN) ? "without" : "with");
+			rdev->pm.int_thermal_type = THERMAL_TYPE_ADT7473_WITH_INTERNAL;
+		} else if (controller->ucType ==
+			   ATOM_PP_THERMALCONTROLLER_EMC2103_WITH_INTERNAL) {
+			DRM_INFO("EMC2103 with internal thermal controller %s fan control\n",
+				 (controller->ucFanParameters &
+				  ATOM_PP_FANPARAMETERS_NOFAN) ? "without" : "with");
+			rdev->pm.int_thermal_type = THERMAL_TYPE_EMC2103_WITH_INTERNAL;
 		} else if (controller->ucType < ARRAY_SIZE(pp_lib_thermal_controller_names)) {
 			DRM_INFO("Possible %s thermal controller at 0x%02x %s fan control\n",
 				 pp_lib_thermal_controller_names[controller->ucType],
 				 controller->ucI2cAddress >> 1,
 				 (controller->ucFanParameters &
 				  ATOM_PP_FANPARAMETERS_NOFAN) ? "without" : "with");
+			rdev->pm.int_thermal_type = THERMAL_TYPE_EXTERNAL;
 			i2c_bus = radeon_lookup_i2c_gpio(rdev, controller->ucI2cLine);
 			rdev->pm.i2c_bus = radeon_i2c_lookup(rdev, &i2c_bus);
 			if (rdev->pm.i2c_bus) {
@@ -3228,6 +3247,41 @@ int radeon_atom_get_leakage_vddc_based_on_leakage_params(struct radeon_device *r
 	return 0;
 }
 
+union get_voltage_info {
+	struct  _GET_VOLTAGE_INFO_INPUT_PARAMETER_V1_2 in;
+	struct  _GET_EVV_VOLTAGE_INFO_OUTPUT_PARAMETER_V1_2 evv_out;
+};
+
+int radeon_atom_get_voltage_evv(struct radeon_device *rdev,
+				u16 virtual_voltage_id,
+				u16 *voltage)
+{
+	int index = GetIndexIntoMasterTable(COMMAND, GetVoltageInfo);
+	u32 entry_id;
+	u32 count = rdev->pm.dpm.dyn_state.vddc_dependency_on_sclk.count;
+	union get_voltage_info args;
+
+	for (entry_id = 0; entry_id < count; entry_id++) {
+		if (rdev->pm.dpm.dyn_state.vddc_dependency_on_sclk.entries[entry_id].v ==
+		    virtual_voltage_id)
+			break;
+	}
+
+	if (entry_id >= count)
+		return -EINVAL;
+
+	args.in.ucVoltageType = VOLTAGE_TYPE_VDDC;
+	args.in.ucVoltageMode = ATOM_GET_VOLTAGE_EVV_VOLTAGE;
+	args.in.ulSCLKFreq =
+		cpu_to_le32(rdev->pm.dpm.dyn_state.vddc_dependency_on_sclk.entries[entry_id].clk);
+
+	atom_execute_table(rdev->mode_info.atom_context, index, (uint32_t *)&args);
+
+	*voltage = le16_to_cpu(args.evv_out.usVoltageLevel);
+
+	return 0;
+}
+
 int radeon_atom_get_voltage_gpio_settings(struct radeon_device *rdev,
 					  u16 voltage_level, u8 voltage_type,
 					  u32 *gpio_value, u32 *gpio_mask)
diff --git a/drivers/gpu/drm/radeon/radeon_device.c b/drivers/gpu/drm/radeon/radeon_device.c
index 0bf6f4a2bb97..e39026cc7d07 100644
--- a/drivers/gpu/drm/radeon/radeon_device.c
+++ b/drivers/gpu/drm/radeon/radeon_device.c
@@ -1314,7 +1314,7 @@ int radeon_device_init(struct radeon_device *rdev,
 
 	r = radeon_init(rdev);
 	if (r)
-		return r;
+		goto failed;
 
 	r = radeon_ib_ring_tests(rdev);
 	if (r)
@@ -1334,7 +1334,7 @@ int radeon_device_init(struct radeon_device *rdev,
 		radeon_agp_disable(rdev);
 		r = radeon_init(rdev);
 		if (r)
-			return r;
+			goto failed;
 	}
 
 	if ((radeon_testing & 1)) {
@@ -1356,6 +1356,11 @@ int radeon_device_init(struct radeon_device *rdev,
 			DRM_INFO("radeon: acceleration disabled, skipping benchmarks\n");
 	}
 	return 0;
+
+failed:
+	if (runtime)
+		vga_switcheroo_fini_domain_pm_ops(rdev->dev);
+	return r;
 }
 
 static void radeon_debugfs_remove_files(struct radeon_device *rdev);
@@ -1376,6 +1381,8 @@ void radeon_device_fini(struct radeon_device *rdev)
 	radeon_bo_evict_vram(rdev);
 	radeon_fini(rdev);
 	vga_switcheroo_unregister_client(rdev->pdev);
+	if (rdev->flags & RADEON_IS_PX)
+		vga_switcheroo_fini_domain_pm_ops(rdev->dev);
 	vga_client_register(rdev->pdev, NULL, NULL, NULL);
 	if (rdev->rio_mem)
 		pci_iounmap(rdev->pdev, rdev->rio_mem);
@@ -1600,7 +1607,6 @@ int radeon_gpu_reset(struct radeon_device *rdev)
 	radeon_save_bios_scratch_regs(rdev);
 	/* block TTM */
 	resched = ttm_bo_lock_delayed_workqueue(&rdev->mman.bdev);
-	radeon_pm_suspend(rdev);
 	radeon_suspend(rdev);
 
 	for (i = 0; i < RADEON_NUM_RINGS; ++i) {
@@ -1646,9 +1652,24 @@ retry:
 		}
 	}
 
-	radeon_pm_resume(rdev);
+	if ((rdev->pm.pm_method == PM_METHOD_DPM) && rdev->pm.dpm_enabled) {
+		/* do dpm late init */
+		r = radeon_pm_late_init(rdev);
+		if (r) {
+			rdev->pm.dpm_enabled = false;
+			DRM_ERROR("radeon_pm_late_init failed, disabling dpm\n");
+		}
+	} else {
+		/* resume old pm late */
+		radeon_pm_resume(rdev);
+	}
+
 	drm_helper_resume_force_mode(rdev->ddev);
 
+	/* set the power state here in case we are a PX system or headless */
+	if ((rdev->pm.pm_method == PM_METHOD_DPM) && rdev->pm.dpm_enabled)
+		radeon_pm_compute_clocks(rdev);
+
 	ttm_bo_unlock_delayed_workqueue(&rdev->mman.bdev, resched);
 	if (r) {
 		/* bad news, how to tell it to userspace ? */
diff --git a/drivers/gpu/drm/radeon/radeon_kms.c b/drivers/gpu/drm/radeon/radeon_kms.c
index ea34a31d3bc8..0bc9106ef435 100644
--- a/drivers/gpu/drm/radeon/radeon_kms.c
+++ b/drivers/gpu/drm/radeon/radeon_kms.c
@@ -254,7 +254,14 @@ static int radeon_info_ioctl(struct drm_device *dev, void *data, struct drm_file
 		}
 		break;
 	case RADEON_INFO_ACCEL_WORKING2:
-		*value = rdev->accel_working;
+		if (rdev->family == CHIP_HAWAII) {
+			if (rdev->accel_working)
+				*value = 2;
+			else
+				*value = 0;
+		} else {
+			*value = rdev->accel_working;
+		}
 		break;
 	case RADEON_INFO_TILING_CONFIG:
 		if (rdev->family >= CHIP_BONAIRE)
diff --git a/drivers/gpu/drm/radeon/radeon_pm.c b/drivers/gpu/drm/radeon/radeon_pm.c
index f77d9d0d54b5..cfb513f933d5 100644
--- a/drivers/gpu/drm/radeon/radeon_pm.c
+++ b/drivers/gpu/drm/radeon/radeon_pm.c
@@ -458,10 +458,6 @@ static ssize_t radeon_get_dpm_state(struct device *dev,
 	struct radeon_device *rdev = ddev->dev_private;
 	enum radeon_pm_state_type pm = rdev->pm.dpm.user_state;
 
-	if  ((rdev->flags & RADEON_IS_PX) &&
-	     (ddev->switch_power_state != DRM_SWITCH_POWER_ON))
-		return snprintf(buf, PAGE_SIZE, "off\n");
-
 	return snprintf(buf, PAGE_SIZE, "%s\n",
 			(pm == POWER_STATE_TYPE_BATTERY) ? "battery" :
 			(pm == POWER_STATE_TYPE_BALANCED) ? "balanced" : "performance");
@@ -475,11 +471,6 @@ static ssize_t radeon_set_dpm_state(struct device *dev,
 	struct drm_device *ddev = dev_get_drvdata(dev);
 	struct radeon_device *rdev = ddev->dev_private;
 
-	/* Can't set dpm state when the card is off */
-	if  ((rdev->flags & RADEON_IS_PX) &&
-	     (ddev->switch_power_state != DRM_SWITCH_POWER_ON))
-		return -EINVAL;
-
 	mutex_lock(&rdev->pm.mutex);
 	if (strncmp("battery", buf, strlen("battery")) == 0)
 		rdev->pm.dpm.user_state = POWER_STATE_TYPE_BATTERY;
@@ -493,7 +484,12 @@ static ssize_t radeon_set_dpm_state(struct device *dev,
 		goto fail;
 	}
 	mutex_unlock(&rdev->pm.mutex);
-	radeon_pm_compute_clocks(rdev);
+
+	/* Can't set dpm state when the card is off */
+	if (!(rdev->flags & RADEON_IS_PX) ||
+	    (ddev->switch_power_state == DRM_SWITCH_POWER_ON))
+		radeon_pm_compute_clocks(rdev);
+
 fail:
 	return count;
 }
@@ -1276,10 +1272,6 @@ int radeon_pm_init(struct radeon_device *rdev)
 	case CHIP_RS780:
 	case CHIP_RS880:
 	case CHIP_RV770:
-	case CHIP_BARTS:
-	case CHIP_TURKS:
-	case CHIP_CAICOS:
-	case CHIP_CAYMAN:
 		/* DPM requires the RLC, RV770+ dGPU requires SMC */
 		if (!rdev->rlc_fw)
 			rdev->pm.pm_method = PM_METHOD_PROFILE;
@@ -1303,6 +1295,10 @@ int radeon_pm_init(struct radeon_device *rdev)
 	case CHIP_PALM:
 	case CHIP_SUMO:
 	case CHIP_SUMO2:
+	case CHIP_BARTS:
+	case CHIP_TURKS:
+	case CHIP_CAICOS:
+	case CHIP_CAYMAN:
 	case CHIP_ARUBA:
 	case CHIP_TAHITI:
 	case CHIP_PITCAIRN:
diff --git a/drivers/gpu/drm/radeon/radeon_semaphore.c b/drivers/gpu/drm/radeon/radeon_semaphore.c
index 9006b32d5eed..eb7b60047e86 100644
--- a/drivers/gpu/drm/radeon/radeon_semaphore.c
+++ b/drivers/gpu/drm/radeon/radeon_semaphore.c
@@ -34,7 +34,7 @@
 int radeon_semaphore_create(struct radeon_device *rdev,
 			    struct radeon_semaphore **semaphore)
 {
-	uint32_t *cpu_addr;
+	uint64_t *cpu_addr;
 	int i, r;
 
 	*semaphore = kmalloc(sizeof(struct radeon_semaphore), GFP_KERNEL);
diff --git a/drivers/gpu/drm/radeon/si.c b/drivers/gpu/drm/radeon/si.c
index ea93393374df..559564c1dc97 100644
--- a/drivers/gpu/drm/radeon/si.c
+++ b/drivers/gpu/drm/radeon/si.c
@@ -4810,7 +4810,7 @@ void si_vm_flush(struct radeon_device *rdev, int ridx, struct radeon_vm *vm)
 
 	/* write new base address */
 	radeon_ring_write(ring, PACKET3(PACKET3_WRITE_DATA, 3));
-	radeon_ring_write(ring, (WRITE_DATA_ENGINE_SEL(0) |
+	radeon_ring_write(ring, (WRITE_DATA_ENGINE_SEL(1) |
 				 WRITE_DATA_DST_SEL(0)));
 
 	if (vm->id < 8) {
diff --git a/drivers/gpu/drm/radeon/trinity_dpm.c b/drivers/gpu/drm/radeon/trinity_dpm.c
index 2da0e17eb960..d9cfa09b2e3f 100644
--- a/drivers/gpu/drm/radeon/trinity_dpm.c
+++ b/drivers/gpu/drm/radeon/trinity_dpm.c
@@ -1877,7 +1877,16 @@ int trinity_dpm_init(struct radeon_device *rdev)
 	for (i = 0; i < SUMO_MAX_HARDWARE_POWERLEVELS; i++)
 		pi->at[i] = TRINITY_AT_DFLT;
 
-	pi->enable_bapm = false;
+	/* There are stability issues reported on with
+	 * bapm enabled when switching between AC and battery
+	 * power.  At the same time, some MSI boards hang
+	 * if it's not enabled and dpm is enabled.  Just enable
+	 * it for MSI boards right now.
+	 */
+	if (rdev->pdev->subsystem_vendor == 0x1462)
+		pi->enable_bapm = true;
+	else
+		pi->enable_bapm = false;
 	pi->enable_nbps_policy = true;
 	pi->enable_sclk_ds = true;
 	pi->enable_gfx_power_gating = true;
diff --git a/drivers/gpu/drm/tilcdc/tilcdc_drv.c b/drivers/gpu/drm/tilcdc/tilcdc_drv.c
index 171a8203892c..0644429f8559 100644
--- a/drivers/gpu/drm/tilcdc/tilcdc_drv.c
+++ b/drivers/gpu/drm/tilcdc/tilcdc_drv.c
@@ -122,6 +122,7 @@ static int tilcdc_unload(struct drm_device *dev)
 	struct tilcdc_drm_private *priv = dev->dev_private;
 	struct tilcdc_module *mod, *cur;
 
+	drm_fbdev_cma_fini(priv->fbdev);
 	drm_kms_helper_poll_fini(dev);
 	drm_mode_config_cleanup(dev);
 	drm_vblank_cleanup(dev);
@@ -628,10 +629,10 @@ static int __init tilcdc_drm_init(void)
 static void __exit tilcdc_drm_fini(void)
 {
 	DBG("fini");
-	tilcdc_tfp410_fini();
-	tilcdc_slave_fini();
-	tilcdc_panel_fini();
 	platform_driver_unregister(&tilcdc_platform_driver);
+	tilcdc_panel_fini();
+	tilcdc_slave_fini();
+	tilcdc_tfp410_fini();
 }
 
 late_initcall(tilcdc_drm_init);
diff --git a/drivers/gpu/drm/tilcdc/tilcdc_panel.c b/drivers/gpu/drm/tilcdc/tilcdc_panel.c
index 86c67329b605..b085dcc54fb5 100644
--- a/drivers/gpu/drm/tilcdc/tilcdc_panel.c
+++ b/drivers/gpu/drm/tilcdc/tilcdc_panel.c
@@ -151,6 +151,7 @@ struct panel_connector {
 static void panel_connector_destroy(struct drm_connector *connector)
 {
 	struct panel_connector *panel_connector = to_panel_connector(connector);
+	drm_sysfs_connector_remove(connector);
 	drm_connector_cleanup(connector);
 	kfree(panel_connector);
 }
@@ -285,10 +286,8 @@ static void panel_destroy(struct tilcdc_module *mod)
 {
 	struct panel_module *panel_mod = to_panel_module(mod);
 
-	if (panel_mod->timings) {
+	if (panel_mod->timings)
 		display_timings_release(panel_mod->timings);
-		kfree(panel_mod->timings);
-	}
 
 	tilcdc_module_cleanup(mod);
 	kfree(panel_mod->info);
diff --git a/drivers/gpu/drm/tilcdc/tilcdc_slave.c b/drivers/gpu/drm/tilcdc/tilcdc_slave.c
index 595068ba2d5e..2f83ffb7f37e 100644
--- a/drivers/gpu/drm/tilcdc/tilcdc_slave.c
+++ b/drivers/gpu/drm/tilcdc/tilcdc_slave.c
@@ -166,6 +166,7 @@ struct slave_connector {
 static void slave_connector_destroy(struct drm_connector *connector)
 {
 	struct slave_connector *slave_connector = to_slave_connector(connector);
+	drm_sysfs_connector_remove(connector);
 	drm_connector_cleanup(connector);
 	kfree(slave_connector);
 }
diff --git a/drivers/gpu/drm/tilcdc/tilcdc_tfp410.c b/drivers/gpu/drm/tilcdc/tilcdc_tfp410.c
index c38b56b268ac..ce75ac8de4f8 100644
--- a/drivers/gpu/drm/tilcdc/tilcdc_tfp410.c
+++ b/drivers/gpu/drm/tilcdc/tilcdc_tfp410.c
@@ -167,6 +167,7 @@ struct tfp410_connector {
 static void tfp410_connector_destroy(struct drm_connector *connector)
 {
 	struct tfp410_connector *tfp410_connector = to_tfp410_connector(connector);
+	drm_sysfs_connector_remove(connector);
 	drm_connector_cleanup(connector);
 	kfree(tfp410_connector);
 }
diff --git a/drivers/gpu/drm/ttm/ttm_page_alloc.c b/drivers/gpu/drm/ttm/ttm_page_alloc.c
index 863bef9f9234..cf4bad2c1d59 100644
--- a/drivers/gpu/drm/ttm/ttm_page_alloc.c
+++ b/drivers/gpu/drm/ttm/ttm_page_alloc.c
@@ -297,8 +297,10 @@ static void ttm_pool_update_free_locked(struct ttm_page_pool *pool,
  *
  * @pool: to free the pages from
  * @free_all: If set to true will free all pages in pool
+ * @gfp: GFP flags.
  **/
-static int ttm_page_pool_free(struct ttm_page_pool *pool, unsigned nr_free)
+static int ttm_page_pool_free(struct ttm_page_pool *pool, unsigned nr_free,
+			      gfp_t gfp)
 {
 	unsigned long irq_flags;
 	struct page *p;
@@ -309,8 +311,7 @@ static int ttm_page_pool_free(struct ttm_page_pool *pool, unsigned nr_free)
 	if (NUM_PAGES_TO_ALLOC < nr_free)
 		npages_to_free = NUM_PAGES_TO_ALLOC;
 
-	pages_to_free = kmalloc(npages_to_free * sizeof(struct page *),
-			GFP_KERNEL);
+	pages_to_free = kmalloc(npages_to_free * sizeof(struct page *), gfp);
 	if (!pages_to_free) {
 		pr_err("Failed to allocate memory for pool free operation\n");
 		return 0;
@@ -382,32 +383,35 @@ out:
  *
  * XXX: (dchinner) Deadlock warning!
  *
- * ttm_page_pool_free() does memory allocation using GFP_KERNEL.  that means
- * this can deadlock when called a sc->gfp_mask that is not equal to
- * GFP_KERNEL.
+ * We need to pass sc->gfp_mask to ttm_page_pool_free().
  *
  * This code is crying out for a shrinker per pool....
  */
 static unsigned long
 ttm_pool_shrink_scan(struct shrinker *shrink, struct shrink_control *sc)
 {
-	static atomic_t start_pool = ATOMIC_INIT(0);
+	static DEFINE_MUTEX(lock);
+	static unsigned start_pool;
 	unsigned i;
-	unsigned pool_offset = atomic_add_return(1, &start_pool);
+	unsigned pool_offset;
 	struct ttm_page_pool *pool;
 	int shrink_pages = sc->nr_to_scan;
 	unsigned long freed = 0;
 
-	pool_offset = pool_offset % NUM_POOLS;
+	if (!mutex_trylock(&lock))
+		return SHRINK_STOP;
+	pool_offset = ++start_pool % NUM_POOLS;
 	/* select start pool in round robin fashion */
 	for (i = 0; i < NUM_POOLS; ++i) {
 		unsigned nr_free = shrink_pages;
 		if (shrink_pages == 0)
 			break;
 		pool = &_manager->pools[(i + pool_offset)%NUM_POOLS];
-		shrink_pages = ttm_page_pool_free(pool, nr_free);
+		shrink_pages = ttm_page_pool_free(pool, nr_free,
+						  sc->gfp_mask);
 		freed += nr_free - shrink_pages;
 	}
+	mutex_unlock(&lock);
 	return freed;
 }
 
@@ -706,7 +710,7 @@ static void ttm_put_pages(struct page **pages, unsigned npages, int flags,
 	}
 	spin_unlock_irqrestore(&pool->lock, irq_flags);
 	if (npages)
-		ttm_page_pool_free(pool, npages);
+		ttm_page_pool_free(pool, npages, GFP_KERNEL);
 }
 
 /*
@@ -846,7 +850,8 @@ void ttm_page_alloc_fini(void)
 	ttm_pool_mm_shrink_fini(_manager);
 
 	for (i = 0; i < NUM_POOLS; ++i)
-		ttm_page_pool_free(&_manager->pools[i], FREE_ALL_PAGES);
+		ttm_page_pool_free(&_manager->pools[i], FREE_ALL_PAGES,
+				   GFP_KERNEL);
 
 	kobject_put(&_manager->kobj);
 	_manager = NULL;
diff --git a/drivers/gpu/drm/ttm/ttm_page_alloc_dma.c b/drivers/gpu/drm/ttm/ttm_page_alloc_dma.c
index fb8259f69839..ca65df144765 100644
--- a/drivers/gpu/drm/ttm/ttm_page_alloc_dma.c
+++ b/drivers/gpu/drm/ttm/ttm_page_alloc_dma.c
@@ -411,8 +411,10 @@ static void ttm_dma_page_put(struct dma_pool *pool, struct dma_page *d_page)
  *
  * @pool: to free the pages from
  * @nr_free: If set to true will free all pages in pool
+ * @gfp: GFP flags.
  **/
-static unsigned ttm_dma_page_pool_free(struct dma_pool *pool, unsigned nr_free)
+static unsigned ttm_dma_page_pool_free(struct dma_pool *pool, unsigned nr_free,
+				       gfp_t gfp)
 {
 	unsigned long irq_flags;
 	struct dma_page *dma_p, *tmp;
@@ -430,8 +432,7 @@ static unsigned ttm_dma_page_pool_free(struct dma_pool *pool, unsigned nr_free)
 			 npages_to_free, nr_free);
 	}
 #endif
-	pages_to_free = kmalloc(npages_to_free * sizeof(struct page *),
-			GFP_KERNEL);
+	pages_to_free = kmalloc(npages_to_free * sizeof(struct page *), gfp);
 
 	if (!pages_to_free) {
 		pr_err("%s: Failed to allocate memory for pool free operation\n",
@@ -530,7 +531,7 @@ static void ttm_dma_free_pool(struct device *dev, enum pool_type type)
 		if (pool->type != type)
 			continue;
 		/* Takes a spinlock.. */
-		ttm_dma_page_pool_free(pool, FREE_ALL_PAGES);
+		ttm_dma_page_pool_free(pool, FREE_ALL_PAGES, GFP_KERNEL);
 		WARN_ON(((pool->npages_in_use + pool->npages_free) != 0));
 		/* This code path is called after _all_ references to the
 		 * struct device has been dropped - so nobody should be
@@ -983,7 +984,7 @@ void ttm_dma_unpopulate(struct ttm_dma_tt *ttm_dma, struct device *dev)
 
 	/* shrink pool if necessary (only on !is_cached pools)*/
 	if (npages)
-		ttm_dma_page_pool_free(pool, npages);
+		ttm_dma_page_pool_free(pool, npages, GFP_KERNEL);
 	ttm->state = tt_unpopulated;
 }
 EXPORT_SYMBOL_GPL(ttm_dma_unpopulate);
@@ -993,10 +994,7 @@ EXPORT_SYMBOL_GPL(ttm_dma_unpopulate);
  *
  * XXX: (dchinner) Deadlock warning!
  *
- * ttm_dma_page_pool_free() does GFP_KERNEL memory allocation, and so attention
- * needs to be paid to sc->gfp_mask to determine if this can be done or not.
- * GFP_KERNEL memory allocation in a GFP_ATOMIC reclaim context woul dbe really
- * bad.
+ * We need to pass sc->gfp_mask to ttm_dma_page_pool_free().
  *
  * I'm getting sadder as I hear more pathetical whimpers about needing per-pool
  * shrinkers
@@ -1004,9 +1002,9 @@ EXPORT_SYMBOL_GPL(ttm_dma_unpopulate);
 static unsigned long
 ttm_dma_pool_shrink_scan(struct shrinker *shrink, struct shrink_control *sc)
 {
-	static atomic_t start_pool = ATOMIC_INIT(0);
+	static unsigned start_pool;
 	unsigned idx = 0;
-	unsigned pool_offset = atomic_add_return(1, &start_pool);
+	unsigned pool_offset;
 	unsigned shrink_pages = sc->nr_to_scan;
 	struct device_pools *p;
 	unsigned long freed = 0;
@@ -1014,8 +1012,11 @@ ttm_dma_pool_shrink_scan(struct shrinker *shrink, struct shrink_control *sc)
 	if (list_empty(&_manager->pools))
 		return SHRINK_STOP;
 
-	mutex_lock(&_manager->lock);
-	pool_offset = pool_offset % _manager->npools;
+	if (!mutex_trylock(&_manager->lock))
+		return SHRINK_STOP;
+	if (!_manager->npools)
+		goto out;
+	pool_offset = ++start_pool % _manager->npools;
 	list_for_each_entry(p, &_manager->pools, pools) {
 		unsigned nr_free;
 
@@ -1027,13 +1028,15 @@ ttm_dma_pool_shrink_scan(struct shrinker *shrink, struct shrink_control *sc)
 		if (++idx < pool_offset)
 			continue;
 		nr_free = shrink_pages;
-		shrink_pages = ttm_dma_page_pool_free(p->pool, nr_free);
+		shrink_pages = ttm_dma_page_pool_free(p->pool, nr_free,
+						      sc->gfp_mask);
 		freed += nr_free - shrink_pages;
 
 		pr_debug("%s: (%s:%d) Asked to shrink %d, have %d more to go\n",
 			 p->pool->dev_name, p->pool->name, current->pid,
 			 nr_free, shrink_pages);
 	}
+out:
 	mutex_unlock(&_manager->lock);
 	return freed;
 }
@@ -1044,7 +1047,8 @@ ttm_dma_pool_shrink_count(struct shrinker *shrink, struct shrink_control *sc)
 	struct device_pools *p;
 	unsigned long count = 0;
 
-	mutex_lock(&_manager->lock);
+	if (!mutex_trylock(&_manager->lock))
+		return 0;
 	list_for_each_entry(p, &_manager->pools, pools)
 		count += p->pool->npages_free;
 	mutex_unlock(&_manager->lock);
diff --git a/drivers/gpu/drm/vmwgfx/vmwgfx_fifo.c b/drivers/gpu/drm/vmwgfx/vmwgfx_fifo.c
index 6ccd993e26bf..6eae14d2a3f7 100644
--- a/drivers/gpu/drm/vmwgfx/vmwgfx_fifo.c
+++ b/drivers/gpu/drm/vmwgfx/vmwgfx_fifo.c
@@ -180,8 +180,9 @@ void vmw_fifo_release(struct vmw_private *dev_priv, struct vmw_fifo_state *fifo)
 
 	mutex_lock(&dev_priv->hw_mutex);
 
+	vmw_write(dev_priv, SVGA_REG_SYNC, SVGA_SYNC_GENERIC);
 	while (vmw_read(dev_priv, SVGA_REG_BUSY) != 0)
-		vmw_write(dev_priv, SVGA_REG_SYNC, SVGA_SYNC_GENERIC);
+		;
 
 	dev_priv->last_read_seqno = ioread32(fifo_mem + SVGA_FIFO_FENCE);
 
diff --git a/drivers/gpu/vga/vga_switcheroo.c b/drivers/gpu/vga/vga_switcheroo.c
index 6866448083b2..37ac7b5dbd06 100644
--- a/drivers/gpu/vga/vga_switcheroo.c
+++ b/drivers/gpu/vga/vga_switcheroo.c
@@ -660,6 +660,12 @@ int vga_switcheroo_init_domain_pm_ops(struct device *dev, struct dev_pm_domain *
 }
 EXPORT_SYMBOL(vga_switcheroo_init_domain_pm_ops);
 
+void vga_switcheroo_fini_domain_pm_ops(struct device *dev)
+{
+	dev->pm_domain = NULL;
+}
+EXPORT_SYMBOL(vga_switcheroo_fini_domain_pm_ops);
+
 static int vga_switcheroo_runtime_resume_hdmi_audio(struct device *dev)
 {
 	struct pci_dev *pdev = to_pci_dev(dev);
diff --git a/drivers/hid/hid-logitech-dj.c b/drivers/hid/hid-logitech-dj.c
index 0b14d3261531..5da115a6fd22 100644
--- a/drivers/hid/hid-logitech-dj.c
+++ b/drivers/hid/hid-logitech-dj.c
@@ -687,7 +687,6 @@ static int logi_dj_raw_event(struct hid_device *hdev,
 	struct dj_receiver_dev *djrcv_dev = hid_get_drvdata(hdev);
 	struct dj_report *dj_report = (struct dj_report *) data;
 	unsigned long flags;
-	bool report_processed = false;
 
 	dbg_hid("%s, size:%d\n", __func__, size);
 
@@ -714,34 +713,42 @@ static int logi_dj_raw_event(struct hid_device *hdev,
 	 * device (via hid_input_report() ) and return 1 so hid-core does not do
 	 * anything else with it.
 	 */
+
+	/* case 1) */
+	if (data[0] != REPORT_ID_DJ_SHORT)
+		return false;
+
 	if ((dj_report->device_index < DJ_DEVICE_INDEX_MIN) ||
 	    (dj_report->device_index > DJ_DEVICE_INDEX_MAX)) {
-		dev_err(&hdev->dev, "%s: invalid device index:%d\n",
+		/*
+		 * Device index is wrong, bail out.
+		 * This driver can ignore safely the receiver notifications,
+		 * so ignore those reports too.
+		 */
+		if (dj_report->device_index != DJ_RECEIVER_INDEX)
+			dev_err(&hdev->dev, "%s: invalid device index:%d\n",
 				__func__, dj_report->device_index);
 		return false;
 	}
 
 	spin_lock_irqsave(&djrcv_dev->lock, flags);
-	if (dj_report->report_id == REPORT_ID_DJ_SHORT) {
-		switch (dj_report->report_type) {
-		case REPORT_TYPE_NOTIF_DEVICE_PAIRED:
-		case REPORT_TYPE_NOTIF_DEVICE_UNPAIRED:
-			logi_dj_recv_queue_notification(djrcv_dev, dj_report);
-			break;
-		case REPORT_TYPE_NOTIF_CONNECTION_STATUS:
-			if (dj_report->report_params[CONNECTION_STATUS_PARAM_STATUS] ==
-			    STATUS_LINKLOSS) {
-				logi_dj_recv_forward_null_report(djrcv_dev, dj_report);
-			}
-			break;
-		default:
-			logi_dj_recv_forward_report(djrcv_dev, dj_report);
+	switch (dj_report->report_type) {
+	case REPORT_TYPE_NOTIF_DEVICE_PAIRED:
+	case REPORT_TYPE_NOTIF_DEVICE_UNPAIRED:
+		logi_dj_recv_queue_notification(djrcv_dev, dj_report);
+		break;
+	case REPORT_TYPE_NOTIF_CONNECTION_STATUS:
+		if (dj_report->report_params[CONNECTION_STATUS_PARAM_STATUS] ==
+		    STATUS_LINKLOSS) {
+			logi_dj_recv_forward_null_report(djrcv_dev, dj_report);
 		}
-		report_processed = true;
+		break;
+	default:
+		logi_dj_recv_forward_report(djrcv_dev, dj_report);
 	}
 	spin_unlock_irqrestore(&djrcv_dev->lock, flags);
 
-	return report_processed;
+	return true;
 }
 
 static int logi_dj_probe(struct hid_device *hdev,
diff --git a/drivers/hid/hid-logitech-dj.h b/drivers/hid/hid-logitech-dj.h
index 4a4000340ce1..daeb0aa4bee9 100644
--- a/drivers/hid/hid-logitech-dj.h
+++ b/drivers/hid/hid-logitech-dj.h
@@ -27,6 +27,7 @@
 
 #define DJ_MAX_PAIRED_DEVICES			6
 #define DJ_MAX_NUMBER_NOTIFICATIONS		8
+#define DJ_RECEIVER_INDEX			0
 #define DJ_DEVICE_INDEX_MIN 			1
 #define DJ_DEVICE_INDEX_MAX 			6
 
diff --git a/drivers/hid/hid-magicmouse.c b/drivers/hid/hid-magicmouse.c
index 3b43d1cfa936..991ba79cfc72 100644
--- a/drivers/hid/hid-magicmouse.c
+++ b/drivers/hid/hid-magicmouse.c
@@ -290,6 +290,11 @@ static int magicmouse_raw_event(struct hid_device *hdev,
 		if (size < 4 || ((size - 4) % 9) != 0)
 			return 0;
 		npoints = (size - 4) / 9;
+		if (npoints > 15) {
+			hid_warn(hdev, "invalid size value (%d) for TRACKPAD_REPORT_ID\n",
+					size);
+			return 0;
+		}
 		msc->ntouches = 0;
 		for (ii = 0; ii < npoints; ii++)
 			magicmouse_emit_touch(msc, ii, data + ii * 9 + 4);
@@ -307,6 +312,11 @@ static int magicmouse_raw_event(struct hid_device *hdev,
 		if (size < 6 || ((size - 6) % 8) != 0)
 			return 0;
 		npoints = (size - 6) / 8;
+		if (npoints > 15) {
+			hid_warn(hdev, "invalid size value (%d) for MOUSE_REPORT_ID\n",
+					size);
+			return 0;
+		}
 		msc->ntouches = 0;
 		for (ii = 0; ii < npoints; ii++)
 			magicmouse_emit_touch(msc, ii, data + ii * 8 + 6);
diff --git a/drivers/hid/hid-picolcd_core.c b/drivers/hid/hid-picolcd_core.c
index acbb021065ec..020df3c2e8b4 100644
--- a/drivers/hid/hid-picolcd_core.c
+++ b/drivers/hid/hid-picolcd_core.c
@@ -350,6 +350,12 @@ static int picolcd_raw_event(struct hid_device *hdev,
 	if (!data)
 		return 1;
 
+	if (size > 64) {
+		hid_warn(hdev, "invalid size value (%d) for picolcd raw event\n",
+				size);
+		return 0;
+	}
+
 	if (report->id == REPORT_KEY_STATE) {
 		if (data->input_keys)
 			ret = picolcd_raw_keypad(data, report, raw_data+1, size-1);
diff --git a/drivers/hwmon/ds1621.c b/drivers/hwmon/ds1621.c
index fc6f5d54e7f7..8890870309e4 100644
--- a/drivers/hwmon/ds1621.c
+++ b/drivers/hwmon/ds1621.c
@@ -309,6 +309,7 @@ static ssize_t set_convrate(struct device *dev, struct device_attribute *da,
 	data->conf |= (resol << DS1621_REG_CONFIG_RESOL_SHIFT);
 	i2c_smbus_write_byte_data(client, DS1621_REG_CONF, data->conf);
 	data->update_interval = ds1721_convrates[resol];
+	data->zbits = 7 - resol;
 	mutex_unlock(&data->update_lock);
 
 	return count;
diff --git a/drivers/i2c/busses/i2c-at91.c b/drivers/i2c/busses/i2c-at91.c
index c56be739006b..11e9c7f9bf9b 100644
--- a/drivers/i2c/busses/i2c-at91.c
+++ b/drivers/i2c/busses/i2c-at91.c
@@ -101,6 +101,7 @@ struct at91_twi_dev {
 	unsigned twi_cwgr_reg;
 	struct at91_twi_pdata *pdata;
 	bool use_dma;
+	bool recv_len_abort;
 	struct at91_twi_dma dma;
 };
 
@@ -267,12 +268,24 @@ static void at91_twi_read_next_byte(struct at91_twi_dev *dev)
 	*dev->buf = at91_twi_read(dev, AT91_TWI_RHR) & 0xff;
 	--dev->buf_len;
 
+	/* return if aborting, we only needed to read RHR to clear RXRDY*/
+	if (dev->recv_len_abort)
+		return;
+
 	/* handle I2C_SMBUS_BLOCK_DATA */
 	if (unlikely(dev->msg->flags & I2C_M_RECV_LEN)) {
-		dev->msg->flags &= ~I2C_M_RECV_LEN;
-		dev->buf_len += *dev->buf;
-		dev->msg->len = dev->buf_len + 1;
-		dev_dbg(dev->dev, "received block length %d\n", dev->buf_len);
+		/* ensure length byte is a valid value */
+		if (*dev->buf <= I2C_SMBUS_BLOCK_MAX && *dev->buf > 0) {
+			dev->msg->flags &= ~I2C_M_RECV_LEN;
+			dev->buf_len += *dev->buf;
+			dev->msg->len = dev->buf_len + 1;
+			dev_dbg(dev->dev, "received block length %d\n",
+					 dev->buf_len);
+		} else {
+			/* abort and send the stop by reading one more byte */
+			dev->recv_len_abort = true;
+			dev->buf_len = 1;
+		}
 	}
 
 	/* send stop if second but last byte has been read */
@@ -421,8 +434,8 @@ static int at91_do_twi_transfer(struct at91_twi_dev *dev)
 		}
 	}
 
-	ret = wait_for_completion_interruptible_timeout(&dev->cmd_complete,
-							dev->adapter.timeout);
+	ret = wait_for_completion_io_timeout(&dev->cmd_complete,
+					     dev->adapter.timeout);
 	if (ret == 0) {
 		dev_err(dev->dev, "controller timed out\n");
 		at91_init_twi_bus(dev);
@@ -444,6 +457,12 @@ static int at91_do_twi_transfer(struct at91_twi_dev *dev)
 		ret = -EIO;
 		goto error;
 	}
+	if (dev->recv_len_abort) {
+		dev_err(dev->dev, "invalid smbus block length recvd\n");
+		ret = -EPROTO;
+		goto error;
+	}
+
 	dev_dbg(dev->dev, "transfer complete\n");
 
 	return 0;
@@ -500,6 +519,7 @@ static int at91_twi_xfer(struct i2c_adapter *adap, struct i2c_msg *msg, int num)
 	dev->buf_len = m_start->len;
 	dev->buf = m_start->buf;
 	dev->msg = m_start;
+	dev->recv_len_abort = false;
 
 	ret = at91_do_twi_transfer(dev);
 
diff --git a/drivers/i2c/busses/i2c-ismt.c b/drivers/i2c/busses/i2c-ismt.c
index 8ce4f517fc56..6e932d140573 100644
--- a/drivers/i2c/busses/i2c-ismt.c
+++ b/drivers/i2c/busses/i2c-ismt.c
@@ -497,7 +497,7 @@ static int ismt_access(struct i2c_adapter *adap, u16 addr,
 			desc->wr_len_cmd = dma_size;
 			desc->control |= ISMT_DESC_BLK;
 			priv->dma_buffer[0] = command;
-			memcpy(&priv->dma_buffer[1], &data->block[1], dma_size);
+			memcpy(&priv->dma_buffer[1], &data->block[1], dma_size - 1);
 		} else {
 			/* Block Read */
 			dev_dbg(dev, "I2C_SMBUS_BLOCK_DATA:  READ\n");
@@ -525,7 +525,7 @@ static int ismt_access(struct i2c_adapter *adap, u16 addr,
 			desc->wr_len_cmd = dma_size;
 			desc->control |= ISMT_DESC_I2C;
 			priv->dma_buffer[0] = command;
-			memcpy(&priv->dma_buffer[1], &data->block[1], dma_size);
+			memcpy(&priv->dma_buffer[1], &data->block[1], dma_size - 1);
 		} else {
 			/* i2c Block Read */
 			dev_dbg(dev, "I2C_SMBUS_I2C_BLOCK_DATA:  READ\n");
diff --git a/drivers/i2c/busses/i2c-mv64xxx.c b/drivers/i2c/busses/i2c-mv64xxx.c
index d52d84937ad3..cf891752cc73 100644
--- a/drivers/i2c/busses/i2c-mv64xxx.c
+++ b/drivers/i2c/busses/i2c-mv64xxx.c
@@ -748,8 +748,7 @@ mv64xxx_of_config(struct mv64xxx_i2c_data *drv_data,
 	}
 	tclk = clk_get_rate(drv_data->clk);
 
-	rc = of_property_read_u32(np, "clock-frequency", &bus_freq);
-	if (rc)
+	if (of_property_read_u32(np, "clock-frequency", &bus_freq))
 		bus_freq = 100000; /* 100kHz by default */
 
 	if (!mv64xxx_find_baud_factors(bus_freq, tclk,
diff --git a/drivers/iio/accel/bma180.c b/drivers/iio/accel/bma180.c
index fe83d04784c8..6f039c300141 100644
--- a/drivers/iio/accel/bma180.c
+++ b/drivers/iio/accel/bma180.c
@@ -571,7 +571,7 @@ static int bma180_probe(struct i2c_client *client,
 	trig->ops = &bma180_trigger_ops;
 	iio_trigger_set_drvdata(trig, indio_dev);
 	data->trig = trig;
-	indio_dev->trig = trig;
+	indio_dev->trig = iio_trigger_get(trig);
 
 	ret = iio_trigger_register(trig);
 	if (ret)
diff --git a/drivers/iio/adc/ad_sigma_delta.c b/drivers/iio/adc/ad_sigma_delta.c
index 9a4e0e32a771..eb799a43aef0 100644
--- a/drivers/iio/adc/ad_sigma_delta.c
+++ b/drivers/iio/adc/ad_sigma_delta.c
@@ -472,7 +472,7 @@ static int ad_sd_probe_trigger(struct iio_dev *indio_dev)
 		goto error_free_irq;
 
 	/* select default trigger */
-	indio_dev->trig = sigma_delta->trig;
+	indio_dev->trig = iio_trigger_get(sigma_delta->trig);
 
 	return 0;
 
diff --git a/drivers/iio/common/hid-sensors/hid-sensor-trigger.c b/drivers/iio/common/hid-sensors/hid-sensor-trigger.c
index 7dcf83998e6f..1be235b01934 100644
--- a/drivers/iio/common/hid-sensors/hid-sensor-trigger.c
+++ b/drivers/iio/common/hid-sensors/hid-sensor-trigger.c
@@ -99,7 +99,8 @@ int hid_sensor_setup_trigger(struct iio_dev *indio_dev, const char *name,
 		dev_err(&indio_dev->dev, "Trigger Register Failed\n");
 		goto error_free_trig;
 	}
-	indio_dev->trig = attrb->trigger = trig;
+	attrb->trigger = trig;
+	indio_dev->trig = iio_trigger_get(trig);
 
 	return ret;
 
diff --git a/drivers/iio/common/st_sensors/st_sensors_trigger.c b/drivers/iio/common/st_sensors/st_sensors_trigger.c
index 8fc3a97eb266..8d8ca6f1e16a 100644
--- a/drivers/iio/common/st_sensors/st_sensors_trigger.c
+++ b/drivers/iio/common/st_sensors/st_sensors_trigger.c
@@ -49,7 +49,7 @@ int st_sensors_allocate_trigger(struct iio_dev *indio_dev,
 		dev_err(&indio_dev->dev, "failed to register iio trigger.\n");
 		goto iio_trigger_register_error;
 	}
-	indio_dev->trig = sdata->trig;
+	indio_dev->trig = iio_trigger_get(sdata->trig);
 
 	return 0;
 
diff --git a/drivers/iio/gyro/itg3200_buffer.c b/drivers/iio/gyro/itg3200_buffer.c
index e3b3c5084070..eef50e91f17c 100644
--- a/drivers/iio/gyro/itg3200_buffer.c
+++ b/drivers/iio/gyro/itg3200_buffer.c
@@ -132,7 +132,7 @@ int itg3200_probe_trigger(struct iio_dev *indio_dev)
 		goto error_free_irq;
 
 	/* select default trigger */
-	indio_dev->trig = st->trig;
+	indio_dev->trig = iio_trigger_get(st->trig);
 
 	return 0;
 
diff --git a/drivers/iio/imu/inv_mpu6050/inv_mpu_trigger.c b/drivers/iio/imu/inv_mpu6050/inv_mpu_trigger.c
index 03b9372c1212..926fccea8de0 100644
--- a/drivers/iio/imu/inv_mpu6050/inv_mpu_trigger.c
+++ b/drivers/iio/imu/inv_mpu6050/inv_mpu_trigger.c
@@ -135,7 +135,7 @@ int inv_mpu6050_probe_trigger(struct iio_dev *indio_dev)
 	ret = iio_trigger_register(st->trig);
 	if (ret)
 		goto error_free_irq;
-	indio_dev->trig = st->trig;
+	indio_dev->trig = iio_trigger_get(st->trig);
 
 	return 0;
 
diff --git a/drivers/iio/inkern.c b/drivers/iio/inkern.c
index 1e8e94d4db7d..4fc88e617acf 100644
--- a/drivers/iio/inkern.c
+++ b/drivers/iio/inkern.c
@@ -178,7 +178,7 @@ static struct iio_channel *of_iio_channel_get_by_name(struct device_node *np,
 			index = of_property_match_string(np, "io-channel-names",
 							 name);
 		chan = of_iio_channel_get(np, index);
-		if (!IS_ERR(chan))
+		if (!IS_ERR(chan) || PTR_ERR(chan) == -EPROBE_DEFER)
 			break;
 		else if (name && index >= 0) {
 			pr_err("ERROR: could not get IIO channel %s:%s(%i)\n",
diff --git a/drivers/iio/magnetometer/st_magn_core.c b/drivers/iio/magnetometer/st_magn_core.c
index 52bbcfa1e077..476aa132a192 100644
--- a/drivers/iio/magnetometer/st_magn_core.c
+++ b/drivers/iio/magnetometer/st_magn_core.c
@@ -42,7 +42,8 @@
 #define ST_MAGN_FS_AVL_5600MG			5600
 #define ST_MAGN_FS_AVL_8000MG			8000
 #define ST_MAGN_FS_AVL_8100MG			8100
-#define ST_MAGN_FS_AVL_10000MG			10000
+#define ST_MAGN_FS_AVL_12000MG			12000
+#define ST_MAGN_FS_AVL_16000MG			16000
 
 /* CUSTOM VALUES FOR SENSOR 1 */
 #define ST_MAGN_1_WAI_EXP			0x3c
@@ -69,20 +70,20 @@
 #define ST_MAGN_1_FS_AVL_4700_VAL		0x05
 #define ST_MAGN_1_FS_AVL_5600_VAL		0x06
 #define ST_MAGN_1_FS_AVL_8100_VAL		0x07
-#define ST_MAGN_1_FS_AVL_1300_GAIN_XY		1100
-#define ST_MAGN_1_FS_AVL_1900_GAIN_XY		855
-#define ST_MAGN_1_FS_AVL_2500_GAIN_XY		670
-#define ST_MAGN_1_FS_AVL_4000_GAIN_XY		450
-#define ST_MAGN_1_FS_AVL_4700_GAIN_XY		400
-#define ST_MAGN_1_FS_AVL_5600_GAIN_XY		330
-#define ST_MAGN_1_FS_AVL_8100_GAIN_XY		230
-#define ST_MAGN_1_FS_AVL_1300_GAIN_Z		980
-#define ST_MAGN_1_FS_AVL_1900_GAIN_Z		760
-#define ST_MAGN_1_FS_AVL_2500_GAIN_Z		600
-#define ST_MAGN_1_FS_AVL_4000_GAIN_Z		400
-#define ST_MAGN_1_FS_AVL_4700_GAIN_Z		355
-#define ST_MAGN_1_FS_AVL_5600_GAIN_Z		295
-#define ST_MAGN_1_FS_AVL_8100_GAIN_Z		205
+#define ST_MAGN_1_FS_AVL_1300_GAIN_XY		909
+#define ST_MAGN_1_FS_AVL_1900_GAIN_XY		1169
+#define ST_MAGN_1_FS_AVL_2500_GAIN_XY		1492
+#define ST_MAGN_1_FS_AVL_4000_GAIN_XY		2222
+#define ST_MAGN_1_FS_AVL_4700_GAIN_XY		2500
+#define ST_MAGN_1_FS_AVL_5600_GAIN_XY		3030
+#define ST_MAGN_1_FS_AVL_8100_GAIN_XY		4347
+#define ST_MAGN_1_FS_AVL_1300_GAIN_Z		1020
+#define ST_MAGN_1_FS_AVL_1900_GAIN_Z		1315
+#define ST_MAGN_1_FS_AVL_2500_GAIN_Z		1666
+#define ST_MAGN_1_FS_AVL_4000_GAIN_Z		2500
+#define ST_MAGN_1_FS_AVL_4700_GAIN_Z		2816
+#define ST_MAGN_1_FS_AVL_5600_GAIN_Z		3389
+#define ST_MAGN_1_FS_AVL_8100_GAIN_Z		4878
 #define ST_MAGN_1_MULTIREAD_BIT			false
 
 /* CUSTOM VALUES FOR SENSOR 2 */
@@ -105,10 +106,12 @@
 #define ST_MAGN_2_FS_MASK			0x60
 #define ST_MAGN_2_FS_AVL_4000_VAL		0x00
 #define ST_MAGN_2_FS_AVL_8000_VAL		0x01
-#define ST_MAGN_2_FS_AVL_10000_VAL		0x02
-#define ST_MAGN_2_FS_AVL_4000_GAIN		430
-#define ST_MAGN_2_FS_AVL_8000_GAIN		230
-#define ST_MAGN_2_FS_AVL_10000_GAIN		230
+#define ST_MAGN_2_FS_AVL_12000_VAL		0x02
+#define ST_MAGN_2_FS_AVL_16000_VAL		0x03
+#define ST_MAGN_2_FS_AVL_4000_GAIN		146
+#define ST_MAGN_2_FS_AVL_8000_GAIN		292
+#define ST_MAGN_2_FS_AVL_12000_GAIN		438
+#define ST_MAGN_2_FS_AVL_16000_GAIN		584
 #define ST_MAGN_2_MULTIREAD_BIT			false
 #define ST_MAGN_2_OUT_X_L_ADDR			0x28
 #define ST_MAGN_2_OUT_Y_L_ADDR			0x2a
@@ -266,9 +269,14 @@ static const struct st_sensors st_magn_sensors[] = {
 					.gain = ST_MAGN_2_FS_AVL_8000_GAIN,
 				},
 				[2] = {
-					.num = ST_MAGN_FS_AVL_10000MG,
-					.value = ST_MAGN_2_FS_AVL_10000_VAL,
-					.gain = ST_MAGN_2_FS_AVL_10000_GAIN,
+					.num = ST_MAGN_FS_AVL_12000MG,
+					.value = ST_MAGN_2_FS_AVL_12000_VAL,
+					.gain = ST_MAGN_2_FS_AVL_12000_GAIN,
+				},
+				[3] = {
+					.num = ST_MAGN_FS_AVL_16000MG,
+					.value = ST_MAGN_2_FS_AVL_16000_VAL,
+					.gain = ST_MAGN_2_FS_AVL_16000_GAIN,
 				},
 			},
 		},
diff --git a/drivers/infiniband/core/uverbs_marshall.c b/drivers/infiniband/core/uverbs_marshall.c
index e7bee46868d1..abd97247443e 100644
--- a/drivers/infiniband/core/uverbs_marshall.c
+++ b/drivers/infiniband/core/uverbs_marshall.c
@@ -140,5 +140,9 @@ void ib_copy_path_rec_from_user(struct ib_sa_path_rec *dst,
 	dst->packet_life_time	= src->packet_life_time;
 	dst->preference		= src->preference;
 	dst->packet_life_time_selector = src->packet_life_time_selector;
+
+	memset(dst->smac, 0, sizeof(dst->smac));
+	memset(dst->dmac, 0, sizeof(dst->dmac));
+	dst->vlan_id = 0xffff;
 }
 EXPORT_SYMBOL(ib_copy_path_rec_from_user);
diff --git a/drivers/infiniband/hw/mlx4/main.c b/drivers/infiniband/hw/mlx4/main.c
index f9c12e92fdd6..11f0606792bb 100644
--- a/drivers/infiniband/hw/mlx4/main.c
+++ b/drivers/infiniband/hw/mlx4/main.c
@@ -1622,6 +1622,7 @@ static void mlx4_ib_get_dev_addr(struct net_device *dev,
 	struct inet6_dev *in6_dev;
 	union ib_gid  *pgid;
 	struct inet6_ifaddr *ifp;
+	union ib_gid default_gid;
 #endif
 	union ib_gid gid;
 
@@ -1642,12 +1643,15 @@ static void mlx4_ib_get_dev_addr(struct net_device *dev,
 		in_dev_put(in_dev);
 	}
 #if IS_ENABLED(CONFIG_IPV6)
+	mlx4_make_default_gid(dev, &default_gid);
 	/* IPv6 gids */
 	in6_dev = in6_dev_get(dev);
 	if (in6_dev) {
 		read_lock_bh(&in6_dev->lock);
 		list_for_each_entry(ifp, &in6_dev->addr_list, if_list) {
 			pgid = (union ib_gid *)&ifp->addr;
+			if (!memcmp(pgid, &default_gid, sizeof(*pgid)))
+				continue;
 			update_gid_table(ibdev, port, pgid, 0, 0);
 		}
 		read_unlock_bh(&in6_dev->lock);
@@ -1723,31 +1727,34 @@ static void mlx4_ib_scan_netdevs(struct mlx4_ib_dev *ibdev)
 			port_state = (netif_running(curr_netdev) && netif_carrier_ok(curr_netdev)) ?
 						IB_PORT_ACTIVE : IB_PORT_DOWN;
 			mlx4_ib_set_default_gid(ibdev, curr_netdev, port);
-		} else {
-			reset_gid_table(ibdev, port);
-		}
-		/* if using bonding/team and a slave port is down, we don't the bond IP
-		 * based gids in the table since flows that select port by gid may get
-		 * the down port.
-		 */
-		if (curr_master && (port_state == IB_PORT_DOWN)) {
-			reset_gid_table(ibdev, port);
-			mlx4_ib_set_default_gid(ibdev, curr_netdev, port);
-		}
-		/* if bonding is used it is possible that we add it to masters
-		 * only after IP address is assigned to the net bonding
-		 * interface.
-		*/
-		if (curr_master && (old_master != curr_master)) {
-			reset_gid_table(ibdev, port);
-			mlx4_ib_set_default_gid(ibdev, curr_netdev, port);
-			mlx4_ib_get_dev_addr(curr_master, ibdev, port);
-		}
+			/* if using bonding/team and a slave port is down, we
+			 * don't the bond IP based gids in the table since
+			 * flows that select port by gid may get the down port.
+			 */
+			if (curr_master && (port_state == IB_PORT_DOWN)) {
+				reset_gid_table(ibdev, port);
+				mlx4_ib_set_default_gid(ibdev,
+							curr_netdev, port);
+			}
+			/* if bonding is used it is possible that we add it to
+			 * masters only after IP address is assigned to the
+			 * net bonding interface.
+			*/
+			if (curr_master && (old_master != curr_master)) {
+				reset_gid_table(ibdev, port);
+				mlx4_ib_set_default_gid(ibdev,
+							curr_netdev, port);
+				mlx4_ib_get_dev_addr(curr_master, ibdev, port);
+			}
 
-		if (!curr_master && (old_master != curr_master)) {
+			if (!curr_master && (old_master != curr_master)) {
+				reset_gid_table(ibdev, port);
+				mlx4_ib_set_default_gid(ibdev,
+							curr_netdev, port);
+				mlx4_ib_get_dev_addr(curr_netdev, ibdev, port);
+			}
+		} else {
 			reset_gid_table(ibdev, port);
-			mlx4_ib_set_default_gid(ibdev, curr_netdev, port);
-			mlx4_ib_get_dev_addr(curr_netdev, ibdev, port);
 		}
 	}
 
diff --git a/drivers/infiniband/hw/qib/qib_debugfs.c b/drivers/infiniband/hw/qib/qib_debugfs.c
index 799a0c3bffc4..6abd3ed3cd51 100644
--- a/drivers/infiniband/hw/qib/qib_debugfs.c
+++ b/drivers/infiniband/hw/qib/qib_debugfs.c
@@ -193,6 +193,7 @@ static void *_qp_stats_seq_start(struct seq_file *s, loff_t *pos)
 	struct qib_qp_iter *iter;
 	loff_t n = *pos;
 
+	rcu_read_lock();
 	iter = qib_qp_iter_init(s->private);
 	if (!iter)
 		return NULL;
@@ -224,7 +225,7 @@ static void *_qp_stats_seq_next(struct seq_file *s, void *iter_ptr,
 
 static void _qp_stats_seq_stop(struct seq_file *s, void *iter_ptr)
 {
-	/* nothing for now */
+	rcu_read_unlock();
 }
 
 static int _qp_stats_seq_show(struct seq_file *s, void *iter_ptr)
diff --git a/drivers/infiniband/hw/qib/qib_qp.c b/drivers/infiniband/hw/qib/qib_qp.c
index 0cad0c40d742..6a71b2b41b27 100644
--- a/drivers/infiniband/hw/qib/qib_qp.c
+++ b/drivers/infiniband/hw/qib/qib_qp.c
@@ -1324,7 +1324,6 @@ int qib_qp_iter_next(struct qib_qp_iter *iter)
 	struct qib_qp *pqp = iter->qp;
 	struct qib_qp *qp;
 
-	rcu_read_lock();
 	for (; n < dev->qp_table_size; n++) {
 		if (pqp)
 			qp = rcu_dereference(pqp->next);
@@ -1332,18 +1331,11 @@ int qib_qp_iter_next(struct qib_qp_iter *iter)
 			qp = rcu_dereference(dev->qp_table[n]);
 		pqp = qp;
 		if (qp) {
-			if (iter->qp)
-				atomic_dec(&iter->qp->refcount);
-			atomic_inc(&qp->refcount);
-			rcu_read_unlock();
 			iter->qp = qp;
 			iter->n = n;
 			return 0;
 		}
 	}
-	rcu_read_unlock();
-	if (iter->qp)
-		atomic_dec(&iter->qp->refcount);
 	return ret;
 }
 
diff --git a/drivers/infiniband/ulp/isert/ib_isert.c b/drivers/infiniband/ulp/isert/ib_isert.c
index 156205a81523..c5c194c2e0b6 100644
--- a/drivers/infiniband/ulp/isert/ib_isert.c
+++ b/drivers/infiniband/ulp/isert/ib_isert.c
@@ -511,7 +511,6 @@ isert_connect_request(struct rdma_cm_id *cma_id, struct rdma_cm_event *event)
 	init_completion(&isert_conn->conn_wait);
 	init_completion(&isert_conn->conn_wait_comp_err);
 	kref_init(&isert_conn->conn_kref);
-	kref_get(&isert_conn->conn_kref);
 	mutex_init(&isert_conn->conn_mutex);
 	spin_lock_init(&isert_conn->conn_lock);
 	INIT_LIST_HEAD(&isert_conn->conn_fr_pool);
@@ -663,7 +662,9 @@ isert_connect_release(struct isert_conn *isert_conn)
 static void
 isert_connected_handler(struct rdma_cm_id *cma_id)
 {
-	return;
+	struct isert_conn *isert_conn = cma_id->context;
+
+	kref_get(&isert_conn->conn_kref);
 }
 
 static void
@@ -715,7 +716,6 @@ isert_disconnect_work(struct work_struct *work)
 
 wake_up:
 	complete(&isert_conn->conn_wait);
-	isert_put_conn(isert_conn);
 }
 
 static void
@@ -2800,6 +2800,7 @@ static void isert_wait_conn(struct iscsi_conn *conn)
 	wait_for_completion(&isert_conn->conn_wait_comp_err);
 
 	wait_for_completion(&isert_conn->conn_wait);
+	isert_put_conn(isert_conn);
 }
 
 static void isert_free_conn(struct iscsi_conn *conn)
diff --git a/drivers/input/keyboard/atkbd.c b/drivers/input/keyboard/atkbd.c
index 2dd1d0dd4f7d..6f5d79569136 100644
--- a/drivers/input/keyboard/atkbd.c
+++ b/drivers/input/keyboard/atkbd.c
@@ -1791,14 +1791,6 @@ static const struct dmi_system_id atkbd_dmi_quirk_table[] __initconst = {
 	{
 		.matches = {
 			DMI_MATCH(DMI_SYS_VENDOR, "LG Electronics"),
-			DMI_MATCH(DMI_PRODUCT_NAME, "LW25-B7HV"),
-		},
-		.callback = atkbd_deactivate_fixup,
-	},
-	{
-		.matches = {
-			DMI_MATCH(DMI_SYS_VENDOR, "LG Electronics"),
-			DMI_MATCH(DMI_PRODUCT_NAME, "P1-J273B"),
 		},
 		.callback = atkbd_deactivate_fixup,
 	},
diff --git a/drivers/input/mouse/elantech.c b/drivers/input/mouse/elantech.c
index 233516aff595..0b75b5764f31 100644
--- a/drivers/input/mouse/elantech.c
+++ b/drivers/input/mouse/elantech.c
@@ -1253,6 +1253,13 @@ static bool elantech_is_signature_valid(const unsigned char *param)
 	if (param[1] == 0)
 		return true;
 
+	/*
+	 * Some models have a revision higher then 20. Meaning param[2] may
+	 * be 10 or 20, skip the rates check for these.
+	 */
+	if (param[0] == 0x46 && (param[1] & 0xef) == 0x0f && param[2] < 40)
+		return true;
+
 	for (i = 0; i < ARRAY_SIZE(rates); i++)
 		if (param[2] == rates[i])
 			return false;
diff --git a/drivers/input/mouse/synaptics.c b/drivers/input/mouse/synaptics.c
index ef9e0b8a9aa7..a50a2a7a43f7 100644
--- a/drivers/input/mouse/synaptics.c
+++ b/drivers/input/mouse/synaptics.c
@@ -626,10 +626,61 @@ static int synaptics_parse_hw_state(const unsigned char buf[],
 			 ((buf[0] & 0x04) >> 1) |
 			 ((buf[3] & 0x04) >> 2));
 
+		if ((SYN_CAP_ADV_GESTURE(priv->ext_cap_0c) ||
+			SYN_CAP_IMAGE_SENSOR(priv->ext_cap_0c)) &&
+		    hw->w == 2) {
+			synaptics_parse_agm(buf, priv, hw);
+			return 1;
+		}
+
+		hw->x = (((buf[3] & 0x10) << 8) |
+			 ((buf[1] & 0x0f) << 8) |
+			 buf[4]);
+		hw->y = (((buf[3] & 0x20) << 7) |
+			 ((buf[1] & 0xf0) << 4) |
+			 buf[5]);
+		hw->z = buf[2];
+
 		hw->left  = (buf[0] & 0x01) ? 1 : 0;
 		hw->right = (buf[0] & 0x02) ? 1 : 0;
 
-		if (SYN_CAP_CLICKPAD(priv->ext_cap_0c)) {
+		if (SYN_CAP_FORCEPAD(priv->ext_cap_0c)) {
+			/*
+			 * ForcePads, like Clickpads, use middle button
+			 * bits to report primary button clicks.
+			 * Unfortunately they report primary button not
+			 * only when user presses on the pad above certain
+			 * threshold, but also when there are more than one
+			 * finger on the touchpad, which interferes with
+			 * out multi-finger gestures.
+			 */
+			if (hw->z == 0) {
+				/* No contacts */
+				priv->press = priv->report_press = false;
+			} else if (hw->w >= 4 && ((buf[0] ^ buf[3]) & 0x01)) {
+				/*
+				 * Single-finger touch with pressure above
+				 * the threshold. If pressure stays long
+				 * enough, we'll start reporting primary
+				 * button. We rely on the device continuing
+				 * sending data even if finger does not
+				 * move.
+				 */
+				if  (!priv->press) {
+					priv->press_start = jiffies;
+					priv->press = true;
+				} else if (time_after(jiffies,
+						priv->press_start +
+							msecs_to_jiffies(50))) {
+					priv->report_press = true;
+				}
+			} else {
+				priv->press = false;
+			}
+
+			hw->left = priv->report_press;
+
+		} else if (SYN_CAP_CLICKPAD(priv->ext_cap_0c)) {
 			/*
 			 * Clickpad's button is transmitted as middle button,
 			 * however, since it is primary button, we will report
@@ -648,21 +699,6 @@ static int synaptics_parse_hw_state(const unsigned char buf[],
 			hw->down = ((buf[0] ^ buf[3]) & 0x02) ? 1 : 0;
 		}
 
-		if ((SYN_CAP_ADV_GESTURE(priv->ext_cap_0c) ||
-			SYN_CAP_IMAGE_SENSOR(priv->ext_cap_0c)) &&
-		    hw->w == 2) {
-			synaptics_parse_agm(buf, priv, hw);
-			return 1;
-		}
-
-		hw->x = (((buf[3] & 0x10) << 8) |
-			 ((buf[1] & 0x0f) << 8) |
-			 buf[4]);
-		hw->y = (((buf[3] & 0x20) << 7) |
-			 ((buf[1] & 0xf0) << 4) |
-			 buf[5]);
-		hw->z = buf[2];
-
 		if (SYN_CAP_MULTI_BUTTON_NO(priv->ext_cap) &&
 		    ((buf[0] ^ buf[3]) & 0x02)) {
 			switch (SYN_CAP_MULTI_BUTTON_NO(priv->ext_cap) & ~0x01) {
diff --git a/drivers/input/mouse/synaptics.h b/drivers/input/mouse/synaptics.h
index e594af0b264b..fb2e076738ae 100644
--- a/drivers/input/mouse/synaptics.h
+++ b/drivers/input/mouse/synaptics.h
@@ -78,6 +78,11 @@
  * 2	0x08	image sensor		image sensor tracks 5 fingers, but only
  *					reports 2.
  * 2	0x20	report min		query 0x0f gives min coord reported
+ * 2	0x80	forcepad		forcepad is a variant of clickpad that
+ *					does not have physical buttons but rather
+ *					uses pressure above certain threshold to
+ *					report primary clicks. Forcepads also have
+ *					clickpad bit set.
  */
 #define SYN_CAP_CLICKPAD(ex0c)		((ex0c) & 0x100000) /* 1-button ClickPad */
 #define SYN_CAP_CLICKPAD2BTN(ex0c)	((ex0c) & 0x000100) /* 2-button ClickPad */
@@ -86,6 +91,7 @@
 #define SYN_CAP_ADV_GESTURE(ex0c)	((ex0c) & 0x080000)
 #define SYN_CAP_REDUCED_FILTERING(ex0c)	((ex0c) & 0x000400)
 #define SYN_CAP_IMAGE_SENSOR(ex0c)	((ex0c) & 0x000800)
+#define SYN_CAP_FORCEPAD(ex0c)		((ex0c) & 0x008000)
 
 /* synaptics modes query bits */
 #define SYN_MODE_ABSOLUTE(m)		((m) & (1 << 7))
@@ -177,6 +183,11 @@ struct synaptics_data {
 	 */
 	struct synaptics_hw_state agm;
 	bool agm_pending;			/* new AGM packet received */
+
+	/* ForcePad handling */
+	unsigned long				press_start;
+	bool					press;
+	bool					report_press;
 };
 
 void synaptics_module_init(void);
diff --git a/drivers/input/serio/i8042-x86ia64io.h b/drivers/input/serio/i8042-x86ia64io.h
index 381b20d4c561..f1da362c3e65 100644
--- a/drivers/input/serio/i8042-x86ia64io.h
+++ b/drivers/input/serio/i8042-x86ia64io.h
@@ -458,6 +458,13 @@ static const struct dmi_system_id __initconst i8042_dmi_nomux_table[] = {
 			DMI_MATCH(DMI_PRODUCT_NAME, "HP Pavilion dv4 Notebook PC"),
 		},
 	},
+	{
+		/* Avatar AVIU-145A6 */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "Intel"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "IC4I"),
+		},
+	},
 	{ }
 };
 
@@ -601,6 +608,14 @@ static const struct dmi_system_id __initconst i8042_dmi_notimeout_table[] = {
 			DMI_MATCH(DMI_PRODUCT_NAME, "HP Pavilion dv4 Notebook PC"),
 		},
 	},
+	{
+		/* Fujitsu U574 laptop */
+		/* https://bugzilla.kernel.org/show_bug.cgi?id=69731 */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "FUJITSU"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "LIFEBOOK U574"),
+		},
+	},
 	{ }
 };
 
diff --git a/drivers/input/serio/serport.c b/drivers/input/serio/serport.c
index 0cb7ef59071b..69175b825346 100644
--- a/drivers/input/serio/serport.c
+++ b/drivers/input/serio/serport.c
@@ -21,6 +21,7 @@
 #include <linux/init.h>
 #include <linux/serio.h>
 #include <linux/tty.h>
+#include <linux/compat.h>
 
 MODULE_AUTHOR("Vojtech Pavlik <vojtech@ucw.cz>");
 MODULE_DESCRIPTION("Input device TTY line discipline");
@@ -198,28 +199,55 @@ static ssize_t serport_ldisc_read(struct tty_struct * tty, struct file * file, u
 	return 0;
 }
 
+static void serport_set_type(struct tty_struct *tty, unsigned long type)
+{
+	struct serport *serport = tty->disc_data;
+
+	serport->id.proto = type & 0x000000ff;
+	serport->id.id    = (type & 0x0000ff00) >> 8;
+	serport->id.extra = (type & 0x00ff0000) >> 16;
+}
+
 /*
  * serport_ldisc_ioctl() allows to set the port protocol, and device ID
  */
 
-static int serport_ldisc_ioctl(struct tty_struct * tty, struct file * file, unsigned int cmd, unsigned long arg)
+static int serport_ldisc_ioctl(struct tty_struct *tty, struct file *file,
+			       unsigned int cmd, unsigned long arg)
 {
-	struct serport *serport = (struct serport*) tty->disc_data;
-	unsigned long type;
-
 	if (cmd == SPIOCSTYPE) {
+		unsigned long type;
+
 		if (get_user(type, (unsigned long __user *) arg))
 			return -EFAULT;
 
-		serport->id.proto = type & 0x000000ff;
-		serport->id.id	  = (type & 0x0000ff00) >> 8;
-		serport->id.extra = (type & 0x00ff0000) >> 16;
+		serport_set_type(tty, type);
+		return 0;
+	}
+
+	return -EINVAL;
+}
+
+#ifdef CONFIG_COMPAT
+#define COMPAT_SPIOCSTYPE	_IOW('q', 0x01, compat_ulong_t)
+static long serport_ldisc_compat_ioctl(struct tty_struct *tty,
+				       struct file *file,
+				       unsigned int cmd, unsigned long arg)
+{
+	if (cmd == COMPAT_SPIOCSTYPE) {
+		void __user *uarg = compat_ptr(arg);
+		compat_ulong_t compat_type;
+
+		if (get_user(compat_type, (compat_ulong_t __user *)uarg))
+			return -EFAULT;
 
+		serport_set_type(tty, compat_type);
 		return 0;
 	}
 
 	return -EINVAL;
 }
+#endif
 
 static void serport_ldisc_write_wakeup(struct tty_struct * tty)
 {
@@ -243,6 +271,9 @@ static struct tty_ldisc_ops serport_ldisc = {
 	.close =	serport_ldisc_close,
 	.read =		serport_ldisc_read,
 	.ioctl =	serport_ldisc_ioctl,
+#ifdef CONFIG_COMPAT
+	.compat_ioctl =	serport_ldisc_compat_ioctl,
+#endif
 	.receive_buf =	serport_ldisc_receive,
 	.write_wakeup =	serport_ldisc_write_wakeup
 };
diff --git a/drivers/iommu/arm-smmu.c b/drivers/iommu/arm-smmu.c
index 1d9ab39af29f..2ecac467f78f 100644
--- a/drivers/iommu/arm-smmu.c
+++ b/drivers/iommu/arm-smmu.c
@@ -794,8 +794,11 @@ static void arm_smmu_init_context_bank(struct arm_smmu_domain *smmu_domain)
 	reg |= TTBCR_EAE |
 	      (TTBCR_SH_IS << TTBCR_SH0_SHIFT) |
 	      (TTBCR_RGN_WBWA << TTBCR_ORGN0_SHIFT) |
-	      (TTBCR_RGN_WBWA << TTBCR_IRGN0_SHIFT) |
-	      (TTBCR_SL0_LVL_1 << TTBCR_SL0_SHIFT);
+	      (TTBCR_RGN_WBWA << TTBCR_IRGN0_SHIFT);
+
+	if (!stage1)
+		reg |= (TTBCR_SL0_LVL_1 << TTBCR_SL0_SHIFT);
+
 	writel_relaxed(reg, cb_base + ARM_SMMU_CB_TTBCR);
 
 	/* MAIR0 (stage-1 only) */
diff --git a/drivers/md/dm-cache-target.c b/drivers/md/dm-cache-target.c
index 735e939a846d..2331543005b2 100644
--- a/drivers/md/dm-cache-target.c
+++ b/drivers/md/dm-cache-target.c
@@ -890,8 +890,8 @@ static void migration_success_pre_commit(struct dm_cache_migration *mg)
 	struct cache *cache = mg->cache;
 
 	if (mg->writeback) {
-		cell_defer(cache, mg->old_ocell, false);
 		clear_dirty(cache, mg->old_oblock, mg->cblock);
+		cell_defer(cache, mg->old_ocell, false);
 		cleanup_migration(mg);
 		return;
 
@@ -946,13 +946,13 @@ static void migration_success_post_commit(struct dm_cache_migration *mg)
 		}
 
 	} else {
+		clear_dirty(cache, mg->new_oblock, mg->cblock);
 		if (mg->requeue_holder)
 			cell_defer(cache, mg->new_ocell, true);
 		else {
 			bio_endio(mg->new_ocell->holder, 0);
 			cell_defer(cache, mg->new_ocell, false);
 		}
-		clear_dirty(cache, mg->new_oblock, mg->cblock);
 		cleanup_migration(mg);
 	}
 }
diff --git a/drivers/md/dm-crypt.c b/drivers/md/dm-crypt.c
index 53b213226c01..9533f835ce07 100644
--- a/drivers/md/dm-crypt.c
+++ b/drivers/md/dm-crypt.c
@@ -1681,6 +1681,7 @@ static int crypt_ctr(struct dm_target *ti, unsigned int argc, char **argv)
 	unsigned int key_size, opt_params;
 	unsigned long long tmpll;
 	int ret;
+	size_t iv_size_padding;
 	struct dm_arg_set as;
 	const char *opt_string;
 	char dummy;
@@ -1717,12 +1718,23 @@ static int crypt_ctr(struct dm_target *ti, unsigned int argc, char **argv)
 
 	cc->dmreq_start = sizeof(struct ablkcipher_request);
 	cc->dmreq_start += crypto_ablkcipher_reqsize(any_tfm(cc));
-	cc->dmreq_start = ALIGN(cc->dmreq_start, crypto_tfm_ctx_alignment());
-	cc->dmreq_start += crypto_ablkcipher_alignmask(any_tfm(cc)) &
-			   ~(crypto_tfm_ctx_alignment() - 1);
+	cc->dmreq_start = ALIGN(cc->dmreq_start, __alignof__(struct dm_crypt_request));
+
+	if (crypto_ablkcipher_alignmask(any_tfm(cc)) < CRYPTO_MINALIGN) {
+		/* Allocate the padding exactly */
+		iv_size_padding = -(cc->dmreq_start + sizeof(struct dm_crypt_request))
+				& crypto_ablkcipher_alignmask(any_tfm(cc));
+	} else {
+		/*
+		 * If the cipher requires greater alignment than kmalloc
+		 * alignment, we don't know the exact position of the
+		 * initialization vector. We must assume worst case.
+		 */
+		iv_size_padding = crypto_ablkcipher_alignmask(any_tfm(cc));
+	}
 
 	cc->req_pool = mempool_create_kmalloc_pool(MIN_IOS, cc->dmreq_start +
-			sizeof(struct dm_crypt_request) + cc->iv_size);
+			sizeof(struct dm_crypt_request) + iv_size_padding + cc->iv_size);
 	if (!cc->req_pool) {
 		ti->error = "Cannot allocate crypt request mempool";
 		goto bad;
diff --git a/drivers/md/raid1.c b/drivers/md/raid1.c
index d7690f86fdb9..55de4f6f7eaf 100644
--- a/drivers/md/raid1.c
+++ b/drivers/md/raid1.c
@@ -540,11 +540,7 @@ static int read_balance(struct r1conf *conf, struct r1bio *r1_bio, int *max_sect
 	has_nonrot_disk = 0;
 	choose_next_idle = 0;
 
-	if (conf->mddev->recovery_cp < MaxSector &&
-	    (this_sector + sectors >= conf->next_resync))
-		choose_first = 1;
-	else
-		choose_first = 0;
+	choose_first = (conf->mddev->recovery_cp < this_sector + sectors);
 
 	for (disk = 0 ; disk < conf->raid_disks * 2 ; disk++) {
 		sector_t dist;
@@ -831,7 +827,7 @@ static void flush_pending_writes(struct r1conf *conf)
  *    there is no normal IO happeing.  It must arrange to call
  *    lower_barrier when the particular background IO completes.
  */
-static void raise_barrier(struct r1conf *conf)
+static void raise_barrier(struct r1conf *conf, sector_t sector_nr)
 {
 	spin_lock_irq(&conf->resync_lock);
 
@@ -841,6 +837,7 @@ static void raise_barrier(struct r1conf *conf)
 
 	/* block any new IO from starting */
 	conf->barrier++;
+	conf->next_resync = sector_nr;
 
 	/* For these conditions we must wait:
 	 * A: while the array is in frozen state
@@ -849,14 +846,17 @@ static void raise_barrier(struct r1conf *conf)
 	 * C: next_resync + RESYNC_SECTORS > start_next_window, meaning
 	 *    next resync will reach to the window which normal bios are
 	 *    handling.
+	 * D: while there are any active requests in the current window.
 	 */
 	wait_event_lock_irq(conf->wait_barrier,
 			    !conf->array_frozen &&
 			    conf->barrier < RESYNC_DEPTH &&
+			    conf->current_window_requests == 0 &&
 			    (conf->start_next_window >=
 			     conf->next_resync + RESYNC_SECTORS),
 			    conf->resync_lock);
 
+	conf->nr_pending++;
 	spin_unlock_irq(&conf->resync_lock);
 }
 
@@ -866,6 +866,7 @@ static void lower_barrier(struct r1conf *conf)
 	BUG_ON(conf->barrier <= 0);
 	spin_lock_irqsave(&conf->resync_lock, flags);
 	conf->barrier--;
+	conf->nr_pending--;
 	spin_unlock_irqrestore(&conf->resync_lock, flags);
 	wake_up(&conf->wait_barrier);
 }
@@ -877,12 +878,10 @@ static bool need_to_wait_for_sync(struct r1conf *conf, struct bio *bio)
 	if (conf->array_frozen || !bio)
 		wait = true;
 	else if (conf->barrier && bio_data_dir(bio) == WRITE) {
-		if (conf->next_resync < RESYNC_WINDOW_SECTORS)
-			wait = true;
-		else if ((conf->next_resync - RESYNC_WINDOW_SECTORS
-				>= bio_end_sector(bio)) ||
-			 (conf->next_resync + NEXT_NORMALIO_DISTANCE
-				<= bio->bi_iter.bi_sector))
+		if ((conf->mddev->curr_resync_completed
+		     >= bio_end_sector(bio)) ||
+		    (conf->next_resync + NEXT_NORMALIO_DISTANCE
+		     <= bio->bi_iter.bi_sector))
 			wait = false;
 		else
 			wait = true;
@@ -919,8 +918,8 @@ static sector_t wait_barrier(struct r1conf *conf, struct bio *bio)
 	}
 
 	if (bio && bio_data_dir(bio) == WRITE) {
-		if (conf->next_resync + NEXT_NORMALIO_DISTANCE
-		    <= bio->bi_iter.bi_sector) {
+		if (bio->bi_iter.bi_sector >=
+		    conf->mddev->curr_resync_completed) {
 			if (conf->start_next_window == MaxSector)
 				conf->start_next_window =
 					conf->next_resync +
@@ -1186,6 +1185,7 @@ read_again:
 				   atomic_read(&bitmap->behind_writes) == 0);
 		}
 		r1_bio->read_disk = rdisk;
+		r1_bio->start_next_window = 0;
 
 		read_bio = bio_clone_mddev(bio, GFP_NOIO, mddev);
 		bio_trim(read_bio, r1_bio->sector - bio->bi_iter.bi_sector,
@@ -1548,8 +1548,13 @@ static void close_sync(struct r1conf *conf)
 	mempool_destroy(conf->r1buf_pool);
 	conf->r1buf_pool = NULL;
 
+	spin_lock_irq(&conf->resync_lock);
 	conf->next_resync = 0;
 	conf->start_next_window = MaxSector;
+	conf->current_window_requests +=
+		conf->next_window_requests;
+	conf->next_window_requests = 0;
+	spin_unlock_irq(&conf->resync_lock);
 }
 
 static int raid1_spare_active(struct mddev *mddev)
@@ -2150,7 +2155,7 @@ static void fix_read_error(struct r1conf *conf, int read_disk,
 			d--;
 			rdev = conf->mirrors[d].rdev;
 			if (rdev &&
-			    test_bit(In_sync, &rdev->flags))
+			    !test_bit(Faulty, &rdev->flags))
 				r1_sync_page_io(rdev, sect, s,
 						conf->tmppage, WRITE);
 		}
@@ -2162,7 +2167,7 @@ static void fix_read_error(struct r1conf *conf, int read_disk,
 			d--;
 			rdev = conf->mirrors[d].rdev;
 			if (rdev &&
-			    test_bit(In_sync, &rdev->flags)) {
+			    !test_bit(Faulty, &rdev->flags)) {
 				if (r1_sync_page_io(rdev, sect, s,
 						    conf->tmppage, READ)) {
 					atomic_add(s, &rdev->corrected_errors);
@@ -2541,9 +2546,8 @@ static sector_t sync_request(struct mddev *mddev, sector_t sector_nr, int *skipp
 
 	bitmap_cond_end_sync(mddev->bitmap, sector_nr);
 	r1_bio = mempool_alloc(conf->r1buf_pool, GFP_NOIO);
-	raise_barrier(conf);
 
-	conf->next_resync = sector_nr;
+	raise_barrier(conf, sector_nr);
 
 	rcu_read_lock();
 	/*
diff --git a/drivers/media/dvb-core/dvb-usb-ids.h b/drivers/media/dvb-core/dvb-usb-ids.h
index 80643ef9183f..fabe2fce9bc5 100644
--- a/drivers/media/dvb-core/dvb-usb-ids.h
+++ b/drivers/media/dvb-core/dvb-usb-ids.h
@@ -279,6 +279,8 @@
 #define USB_PID_PCTV_400E				0x020f
 #define USB_PID_PCTV_450E				0x0222
 #define USB_PID_PCTV_452E				0x021f
+#define USB_PID_PCTV_78E				0x025a
+#define USB_PID_PCTV_79E				0x0262
 #define USB_PID_REALTEK_RTL2831U			0x2831
 #define USB_PID_REALTEK_RTL2832U			0x2832
 #define USB_PID_TECHNOTREND_CONNECT_S2_3600		0x3007
diff --git a/drivers/media/i2c/adv7604.c b/drivers/media/i2c/adv7604.c
index 71c8570bd9ea..112394d138c9 100644
--- a/drivers/media/i2c/adv7604.c
+++ b/drivers/media/i2c/adv7604.c
@@ -1984,7 +1984,7 @@ static int adv7604_log_status(struct v4l2_subdev *sd)
 	v4l2_info(sd, "HDCP keys read: %s%s\n",
 			(hdmi_read(sd, 0x04) & 0x20) ? "yes" : "no",
 			(hdmi_read(sd, 0x04) & 0x10) ? "ERROR" : "");
-	if (!is_hdmi(sd)) {
+	if (is_hdmi(sd)) {
 		bool audio_pll_locked = hdmi_read(sd, 0x04) & 0x01;
 		bool audio_sample_packet_detect = hdmi_read(sd, 0x18) & 0x01;
 		bool audio_mute = io_read(sd, 0x65) & 0x40;
diff --git a/drivers/media/pci/cx18/cx18-driver.c b/drivers/media/pci/cx18/cx18-driver.c
index 716bdc57fac6..83f5074706f9 100644
--- a/drivers/media/pci/cx18/cx18-driver.c
+++ b/drivers/media/pci/cx18/cx18-driver.c
@@ -1091,6 +1091,7 @@ static int cx18_probe(struct pci_dev *pci_dev,
 		setup.addr = ADDR_UNSET;
 		setup.type = cx->options.tuner;
 		setup.mode_mask = T_ANALOG_TV;  /* matches TV tuners */
+		setup.config = NULL;
 		if (cx->options.radio > 0)
 			setup.mode_mask |= T_RADIO;
 		setup.tuner_callback = (setup.type == TUNER_XC2028) ?
diff --git a/drivers/media/usb/dvb-usb-v2/af9035.c b/drivers/media/usb/dvb-usb-v2/af9035.c
index 8ede8ea762e6..88228f735342 100644
--- a/drivers/media/usb/dvb-usb-v2/af9035.c
+++ b/drivers/media/usb/dvb-usb-v2/af9035.c
@@ -1541,6 +1541,10 @@ static const struct usb_device_id af9035_id_table[] = {
 		&af9035_props, "Leadtek WinFast DTV Dongle Dual", NULL) },
 	{ DVB_USB_DEVICE(USB_VID_HAUPPAUGE, 0xf900,
 		&af9035_props, "Hauppauge WinTV-MiniStick 2", NULL) },
+	{ DVB_USB_DEVICE(USB_VID_PCTV, USB_PID_PCTV_78E,
+		&af9035_props, "PCTV 78e", RC_MAP_IT913X_V1) },
+	{ DVB_USB_DEVICE(USB_VID_PCTV, USB_PID_PCTV_79E,
+		&af9035_props, "PCTV 79e", RC_MAP_IT913X_V2) },
 	{ }
 };
 MODULE_DEVICE_TABLE(usb, af9035_id_table);
diff --git a/drivers/net/ethernet/ibm/ibmveth.c b/drivers/net/ethernet/ibm/ibmveth.c
index 1fc8334fc181..55e3075492da 100644
--- a/drivers/net/ethernet/ibm/ibmveth.c
+++ b/drivers/net/ethernet/ibm/ibmveth.c
@@ -292,6 +292,18 @@ failure:
 	atomic_add(buffers_added, &(pool->available));
 }
 
+/*
+ * The final 8 bytes of the buffer list is a counter of frames dropped
+ * because there was not a buffer in the buffer list capable of holding
+ * the frame.
+ */
+static void ibmveth_update_rx_no_buffer(struct ibmveth_adapter *adapter)
+{
+	__be64 *p = adapter->buffer_list_addr + 4096 - 8;
+
+	adapter->rx_no_buffer = be64_to_cpup(p);
+}
+
 /* replenish routine */
 static void ibmveth_replenish_task(struct ibmveth_adapter *adapter)
 {
@@ -307,8 +319,7 @@ static void ibmveth_replenish_task(struct ibmveth_adapter *adapter)
 			ibmveth_replenish_buffer_pool(adapter, pool);
 	}
 
-	adapter->rx_no_buffer = *(u64 *)(((char*)adapter->buffer_list_addr) +
-						4096 - 8);
+	ibmveth_update_rx_no_buffer(adapter);
 }
 
 /* empty and free ana buffer pool - also used to do cleanup in error paths */
@@ -698,8 +709,7 @@ static int ibmveth_close(struct net_device *netdev)
 
 	free_irq(netdev->irq, netdev);
 
-	adapter->rx_no_buffer = *(u64 *)(((char *)adapter->buffer_list_addr) +
-						4096 - 8);
+	ibmveth_update_rx_no_buffer(adapter);
 
 	ibmveth_cleanup(adapter);
 
diff --git a/drivers/net/wireless/ath/carl9170/carl9170.h b/drivers/net/wireless/ath/carl9170/carl9170.h
index 8596aba34f96..237d0cda1bcb 100644
--- a/drivers/net/wireless/ath/carl9170/carl9170.h
+++ b/drivers/net/wireless/ath/carl9170/carl9170.h
@@ -256,6 +256,7 @@ struct ar9170 {
 	atomic_t rx_work_urbs;
 	atomic_t rx_pool_urbs;
 	kernel_ulong_t features;
+	bool usb_ep_cmd_is_bulk;
 
 	/* firmware settings */
 	struct completion fw_load_wait;
diff --git a/drivers/net/wireless/ath/carl9170/usb.c b/drivers/net/wireless/ath/carl9170/usb.c
index ca115f33746f..bc931f6f1f0f 100644
--- a/drivers/net/wireless/ath/carl9170/usb.c
+++ b/drivers/net/wireless/ath/carl9170/usb.c
@@ -621,9 +621,16 @@ int __carl9170_exec_cmd(struct ar9170 *ar, struct carl9170_cmd *cmd,
 		goto err_free;
 	}
 
-	usb_fill_int_urb(urb, ar->udev, usb_sndintpipe(ar->udev,
-		AR9170_USB_EP_CMD), cmd, cmd->hdr.len + 4,
-		carl9170_usb_cmd_complete, ar, 1);
+	if (ar->usb_ep_cmd_is_bulk)
+		usb_fill_bulk_urb(urb, ar->udev,
+				  usb_sndbulkpipe(ar->udev, AR9170_USB_EP_CMD),
+				  cmd, cmd->hdr.len + 4,
+				  carl9170_usb_cmd_complete, ar);
+	else
+		usb_fill_int_urb(urb, ar->udev,
+				 usb_sndintpipe(ar->udev, AR9170_USB_EP_CMD),
+				 cmd, cmd->hdr.len + 4,
+				 carl9170_usb_cmd_complete, ar, 1);
 
 	if (free_buf)
 		urb->transfer_flags |= URB_FREE_BUFFER;
@@ -1032,9 +1039,10 @@ static void carl9170_usb_firmware_step2(const struct firmware *fw,
 static int carl9170_usb_probe(struct usb_interface *intf,
 			      const struct usb_device_id *id)
 {
+	struct usb_endpoint_descriptor *ep;
 	struct ar9170 *ar;
 	struct usb_device *udev;
-	int err;
+	int i, err;
 
 	err = usb_reset_device(interface_to_usbdev(intf));
 	if (err)
@@ -1050,6 +1058,21 @@ static int carl9170_usb_probe(struct usb_interface *intf,
 	ar->intf = intf;
 	ar->features = id->driver_info;
 
+	/* We need to remember the type of endpoint 4 because it differs
+	 * between high- and full-speed configuration. The high-speed
+	 * configuration specifies it as interrupt and the full-speed
+	 * configuration as bulk endpoint. This information is required
+	 * later when sending urbs to that endpoint.
+	 */
+	for (i = 0; i < intf->cur_altsetting->desc.bNumEndpoints; ++i) {
+		ep = &intf->cur_altsetting->endpoint[i].desc;
+
+		if (usb_endpoint_num(ep) == AR9170_USB_EP_CMD &&
+		    usb_endpoint_dir_out(ep) &&
+		    usb_endpoint_type(ep) == USB_ENDPOINT_XFER_BULK)
+			ar->usb_ep_cmd_is_bulk = true;
+	}
+
 	usb_set_intfdata(intf, ar);
 	SET_IEEE80211_DEV(ar->hw, &intf->dev);
 
diff --git a/drivers/net/wireless/brcm80211/brcmfmac/fweh.c b/drivers/net/wireless/brcm80211/brcmfmac/fweh.c
index fad77dd2a3a5..3f9cb894d001 100644
--- a/drivers/net/wireless/brcm80211/brcmfmac/fweh.c
+++ b/drivers/net/wireless/brcm80211/brcmfmac/fweh.c
@@ -185,7 +185,13 @@ static void brcmf_fweh_handle_if_event(struct brcmf_pub *drvr,
 		  ifevent->action, ifevent->ifidx, ifevent->bssidx,
 		  ifevent->flags, ifevent->role);
 
-	if (ifevent->flags & BRCMF_E_IF_FLAG_NOIF) {
+	/* The P2P Device interface event must not be ignored
+	 * contrary to what firmware tells us. The only way to
+	 * distinguish the P2P Device is by looking at the ifidx
+	 * and bssidx received.
+	 */
+	if (!(ifevent->ifidx == 0 && ifevent->bssidx == 1) &&
+	    (ifevent->flags & BRCMF_E_IF_FLAG_NOIF)) {
 		brcmf_dbg(EVENT, "event can be ignored\n");
 		return;
 	}
@@ -210,12 +216,12 @@ static void brcmf_fweh_handle_if_event(struct brcmf_pub *drvr,
 				return;
 	}
 
-	if (ifevent->action == BRCMF_E_IF_CHANGE)
+	if (ifp && ifevent->action == BRCMF_E_IF_CHANGE)
 		brcmf_fws_reset_interface(ifp);
 
 	err = brcmf_fweh_call_event_handler(ifp, emsg->event_code, emsg, data);
 
-	if (ifevent->action == BRCMF_E_IF_DEL) {
+	if (ifp && ifevent->action == BRCMF_E_IF_DEL) {
 		brcmf_fws_del_interface(ifp);
 		brcmf_del_if(drvr, ifevent->bssidx);
 	}
diff --git a/drivers/net/wireless/brcm80211/brcmfmac/fweh.h b/drivers/net/wireless/brcm80211/brcmfmac/fweh.h
index 51b53a73d074..d26b47698f68 100644
--- a/drivers/net/wireless/brcm80211/brcmfmac/fweh.h
+++ b/drivers/net/wireless/brcm80211/brcmfmac/fweh.h
@@ -167,6 +167,8 @@ enum brcmf_fweh_event_code {
 #define BRCMF_E_IF_ROLE_STA			0
 #define BRCMF_E_IF_ROLE_AP			1
 #define BRCMF_E_IF_ROLE_WDS			2
+#define BRCMF_E_IF_ROLE_P2P_GO			3
+#define BRCMF_E_IF_ROLE_P2P_CLIENT		4
 
 /**
  * definitions for event packet validation.
diff --git a/drivers/net/wireless/iwlwifi/dvm/rxon.c b/drivers/net/wireless/iwlwifi/dvm/rxon.c
index c1e311341b74..503a81e58185 100644
--- a/drivers/net/wireless/iwlwifi/dvm/rxon.c
+++ b/drivers/net/wireless/iwlwifi/dvm/rxon.c
@@ -1068,6 +1068,13 @@ int iwlagn_commit_rxon(struct iwl_priv *priv, struct iwl_rxon_context *ctx)
 	/* recalculate basic rates */
 	iwl_calc_basic_rates(priv, ctx);
 
+	/*
+	 * force CTS-to-self frames protection if RTS-CTS is not preferred
+	 * one aggregation protection method
+	 */
+	if (!priv->hw_params.use_rts_for_aggregation)
+		ctx->staging.flags |= RXON_FLG_SELF_CTS_EN;
+
 	if ((ctx->vif && ctx->vif->bss_conf.use_short_slot) ||
 	    !(ctx->staging.flags & RXON_FLG_BAND_24G_MSK))
 		ctx->staging.flags |= RXON_FLG_SHORT_SLOT_MSK;
@@ -1473,6 +1480,11 @@ void iwlagn_bss_info_changed(struct ieee80211_hw *hw,
 	else
 		ctx->staging.flags &= ~RXON_FLG_TGG_PROTECT_MSK;
 
+	if (bss_conf->use_cts_prot)
+		ctx->staging.flags |= RXON_FLG_SELF_CTS_EN;
+	else
+		ctx->staging.flags &= ~RXON_FLG_SELF_CTS_EN;
+
 	memcpy(ctx->staging.bssid_addr, bss_conf->bssid, ETH_ALEN);
 
 	if (vif->type == NL80211_IFTYPE_AP ||
diff --git a/drivers/net/wireless/iwlwifi/iwl-config.h b/drivers/net/wireless/iwlwifi/iwl-config.h
index 1ced525157dc..b45d78f53f08 100644
--- a/drivers/net/wireless/iwlwifi/iwl-config.h
+++ b/drivers/net/wireless/iwlwifi/iwl-config.h
@@ -119,6 +119,8 @@ enum iwl_led_mode {
 #define IWL_LONG_WD_TIMEOUT	10000
 #define IWL_MAX_WD_TIMEOUT	120000
 
+#define IWL_DEFAULT_MAX_TX_POWER 22
+
 /* Antenna presence definitions */
 #define	ANT_NONE	0x0
 #define	ANT_A		BIT(0)
diff --git a/drivers/net/wireless/iwlwifi/iwl-nvm-parse.c b/drivers/net/wireless/iwlwifi/iwl-nvm-parse.c
index 725e954d8475..3c3eb7842c62 100644
--- a/drivers/net/wireless/iwlwifi/iwl-nvm-parse.c
+++ b/drivers/net/wireless/iwlwifi/iwl-nvm-parse.c
@@ -118,8 +118,6 @@ static const u8 iwl_nvm_channels[] = {
 #define LAST_2GHZ_HT_PLUS	9
 #define LAST_5GHZ_HT		161
 
-#define DEFAULT_MAX_TX_POWER 16
-
 /* rate data (static) */
 static struct ieee80211_rate iwl_cfg80211_rates[] = {
 	{ .bitrate = 1 * 10, .hw_value = 0, .hw_value_short = 0, },
@@ -242,7 +240,7 @@ static int iwl_init_channel_map(struct device *dev, const struct iwl_cfg *cfg,
 		 * Default value - highest tx power value.  max_power
 		 * is not used in mvm, and is used for backwards compatibility
 		 */
-		channel->max_power = DEFAULT_MAX_TX_POWER;
+		channel->max_power = IWL_DEFAULT_MAX_TX_POWER;
 		is_5ghz = channel->band == IEEE80211_BAND_5GHZ;
 		IWL_DEBUG_EEPROM(dev,
 				 "Ch. %d [%sGHz] %s%s%s%s%s%s(0x%02x %ddBm): Ad-Hoc %ssupported\n",
diff --git a/drivers/net/wireless/iwlwifi/mvm/fw-api.h b/drivers/net/wireless/iwlwifi/mvm/fw-api.h
index 989d7dbdca6c..d0a04779d734 100644
--- a/drivers/net/wireless/iwlwifi/mvm/fw-api.h
+++ b/drivers/net/wireless/iwlwifi/mvm/fw-api.h
@@ -1415,14 +1415,14 @@ enum iwl_sf_scenario {
 
 /**
  * Smart Fifo configuration command.
- * @state: smart fifo state, types listed in iwl_sf_sate.
+ * @state: smart fifo state, types listed in enum %iwl_sf_sate.
  * @watermark: Minimum allowed availabe free space in RXF for transient state.
  * @long_delay_timeouts: aging and idle timer values for each scenario
  * in long delay state.
  * @full_on_timeouts: timer values for each scenario in full on state.
  */
 struct iwl_sf_cfg_cmd {
-	enum iwl_sf_state state;
+	__le32 state;
 	__le32 watermark[SF_TRANSIENT_STATES_NUMBER];
 	__le32 long_delay_timeouts[SF_NUM_SCENARIO][SF_NUM_TIMEOUT_TYPES];
 	__le32 full_on_timeouts[SF_NUM_SCENARIO][SF_NUM_TIMEOUT_TYPES];
diff --git a/drivers/net/wireless/iwlwifi/mvm/sf.c b/drivers/net/wireless/iwlwifi/mvm/sf.c
index 88809b2d1654..dab8fd13857a 100644
--- a/drivers/net/wireless/iwlwifi/mvm/sf.c
+++ b/drivers/net/wireless/iwlwifi/mvm/sf.c
@@ -172,7 +172,7 @@ static int iwl_mvm_sf_config(struct iwl_mvm *mvm, u8 sta_id,
 			     enum iwl_sf_state new_state)
 {
 	struct iwl_sf_cfg_cmd sf_cmd = {
-		.state = new_state,
+		.state = cpu_to_le32(new_state),
 	};
 	struct ieee80211_sta *sta;
 	int ret = 0;
diff --git a/drivers/net/wireless/iwlwifi/mvm/tx.c b/drivers/net/wireless/iwlwifi/mvm/tx.c
index 76ee486039d7..2ca62af3f81b 100644
--- a/drivers/net/wireless/iwlwifi/mvm/tx.c
+++ b/drivers/net/wireless/iwlwifi/mvm/tx.c
@@ -173,10 +173,14 @@ static void iwl_mvm_set_tx_cmd_rate(struct iwl_mvm *mvm,
 
 	/*
 	 * for data packets, rate info comes from the table inside the fw. This
-	 * table is controlled by LINK_QUALITY commands
+	 * table is controlled by LINK_QUALITY commands. Exclude ctrl port
+	 * frames like EAPOLs which should be treated as mgmt frames. This
+	 * avoids them being sent initially in high rates which increases the
+	 * chances for completion of the 4-Way handshake.
 	 */
 
-	if (ieee80211_is_data(fc) && sta) {
+	if (ieee80211_is_data(fc) && sta &&
+	    !(info->control.flags & IEEE80211_TX_CTRL_PORT_CTRL_PROTO)) {
 		tx_cmd->initial_rate_index = 0;
 		tx_cmd->tx_flags |= cpu_to_le32(TX_CMD_FLG_STA_RATE);
 		return;
diff --git a/drivers/net/wireless/rtlwifi/rtl8192cu/sw.c b/drivers/net/wireless/rtlwifi/rtl8192cu/sw.c
index c61311084d7e..f58316769159 100644
--- a/drivers/net/wireless/rtlwifi/rtl8192cu/sw.c
+++ b/drivers/net/wireless/rtlwifi/rtl8192cu/sw.c
@@ -317,6 +317,7 @@ static struct usb_device_id rtl8192c_usb_ids[] = {
 	{RTL_USB_DEVICE(0x0bda, 0x5088, rtl92cu_hal_cfg)}, /*Thinkware-CC&C*/
 	{RTL_USB_DEVICE(0x0df6, 0x0052, rtl92cu_hal_cfg)}, /*Sitecom - Edimax*/
 	{RTL_USB_DEVICE(0x0df6, 0x005c, rtl92cu_hal_cfg)}, /*Sitecom - Edimax*/
+	{RTL_USB_DEVICE(0x0df6, 0x0070, rtl92cu_hal_cfg)}, /*Sitecom - 150N */
 	{RTL_USB_DEVICE(0x0df6, 0x0077, rtl92cu_hal_cfg)}, /*Sitecom-WLA2100V2*/
 	{RTL_USB_DEVICE(0x0eb0, 0x9071, rtl92cu_hal_cfg)}, /*NO Brand - Etop*/
 	{RTL_USB_DEVICE(0x4856, 0x0091, rtl92cu_hal_cfg)}, /*NetweeN - Feixun*/
diff --git a/drivers/nfc/microread/microread.c b/drivers/nfc/microread/microread.c
index f868333271aa..963a4a5dc88e 100644
--- a/drivers/nfc/microread/microread.c
+++ b/drivers/nfc/microread/microread.c
@@ -501,9 +501,13 @@ static void microread_target_discovered(struct nfc_hci_dev *hdev, u8 gate,
 		targets->sens_res =
 			 be16_to_cpu(*(u16 *)&skb->data[MICROREAD_EMCF_A_ATQA]);
 		targets->sel_res = skb->data[MICROREAD_EMCF_A_SAK];
-		memcpy(targets->nfcid1, &skb->data[MICROREAD_EMCF_A_UID],
-		       skb->data[MICROREAD_EMCF_A_LEN]);
 		targets->nfcid1_len = skb->data[MICROREAD_EMCF_A_LEN];
+		if (targets->nfcid1_len > sizeof(targets->nfcid1)) {
+			r = -EINVAL;
+			goto exit_free;
+		}
+		memcpy(targets->nfcid1, &skb->data[MICROREAD_EMCF_A_UID],
+		       targets->nfcid1_len);
 		break;
 	case MICROREAD_GATE_ID_MREAD_ISO_A_3:
 		targets->supported_protocols =
@@ -511,9 +515,13 @@ static void microread_target_discovered(struct nfc_hci_dev *hdev, u8 gate,
 		targets->sens_res =
 			 be16_to_cpu(*(u16 *)&skb->data[MICROREAD_EMCF_A3_ATQA]);
 		targets->sel_res = skb->data[MICROREAD_EMCF_A3_SAK];
-		memcpy(targets->nfcid1, &skb->data[MICROREAD_EMCF_A3_UID],
-		       skb->data[MICROREAD_EMCF_A3_LEN]);
 		targets->nfcid1_len = skb->data[MICROREAD_EMCF_A3_LEN];
+		if (targets->nfcid1_len > sizeof(targets->nfcid1)) {
+			r = -EINVAL;
+			goto exit_free;
+		}
+		memcpy(targets->nfcid1, &skb->data[MICROREAD_EMCF_A3_UID],
+		       targets->nfcid1_len);
 		break;
 	case MICROREAD_GATE_ID_MREAD_ISO_B:
 		targets->supported_protocols = NFC_PROTO_ISO14443_B_MASK;
diff --git a/drivers/of/irq.c b/drivers/of/irq.c
index ca0189308d72..48f20ff1add9 100644
--- a/drivers/of/irq.c
+++ b/drivers/of/irq.c
@@ -301,16 +301,17 @@ int of_irq_parse_one(struct device_node *device, int index, struct of_phandle_ar
 	/* Get the reg property (if any) */
 	addr = of_get_property(device, "reg", NULL);
 
+	/* Try the new-style interrupts-extended first */
+	res = of_parse_phandle_with_args(device, "interrupts-extended",
+					"#interrupt-cells", index, out_irq);
+	if (!res)
+		return of_irq_parse_raw(addr, out_irq);
+
 	/* Get the interrupts property */
 	intspec = of_get_property(device, "interrupts", &intlen);
-	if (intspec == NULL) {
-		/* Try the new-style interrupts-extended */
-		res = of_parse_phandle_with_args(device, "interrupts-extended",
-						"#interrupt-cells", index, out_irq);
-		if (res)
-			return -EINVAL;
-		return of_irq_parse_raw(addr, out_irq);
-	}
+	if (intspec == NULL)
+		return -EINVAL;
+
 	intlen /= sizeof(*intspec);
 
 	pr_debug(" intspec=%d intlen=%d\n", be32_to_cpup(intspec), intlen);
diff --git a/drivers/phy/phy-twl4030-usb.c b/drivers/phy/phy-twl4030-usb.c
index c3ace1db8136..aaac3594f83b 100644
--- a/drivers/phy/phy-twl4030-usb.c
+++ b/drivers/phy/phy-twl4030-usb.c
@@ -34,6 +34,7 @@
 #include <linux/delay.h>
 #include <linux/usb/otg.h>
 #include <linux/phy/phy.h>
+#include <linux/pm_runtime.h>
 #include <linux/usb/musb-omap.h>
 #include <linux/usb/ulpi.h>
 #include <linux/i2c/twl.h>
@@ -422,37 +423,55 @@ static void twl4030_phy_power(struct twl4030_usb *twl, int on)
 	}
 }
 
-static int twl4030_phy_power_off(struct phy *phy)
+static int twl4030_usb_runtime_suspend(struct device *dev)
 {
-	struct twl4030_usb *twl = phy_get_drvdata(phy);
+	struct twl4030_usb *twl = dev_get_drvdata(dev);
 
+	dev_dbg(twl->dev, "%s\n", __func__);
 	if (twl->asleep)
 		return 0;
 
 	twl4030_phy_power(twl, 0);
 	twl->asleep = 1;
-	dev_dbg(twl->dev, "%s\n", __func__);
+
 	return 0;
 }
 
-static void __twl4030_phy_power_on(struct twl4030_usb *twl)
+static int twl4030_usb_runtime_resume(struct device *dev)
 {
+	struct twl4030_usb *twl = dev_get_drvdata(dev);
+
+	dev_dbg(twl->dev, "%s\n", __func__);
+	if (!twl->asleep)
+		return 0;
+
 	twl4030_phy_power(twl, 1);
-	twl4030_i2c_access(twl, 1);
-	twl4030_usb_set_mode(twl, twl->usb_mode);
-	if (twl->usb_mode == T2_USB_MODE_ULPI)
-		twl4030_i2c_access(twl, 0);
+	twl->asleep = 0;
+
+	return 0;
+}
+
+static int twl4030_phy_power_off(struct phy *phy)
+{
+	struct twl4030_usb *twl = phy_get_drvdata(phy);
+
+	dev_dbg(twl->dev, "%s\n", __func__);
+	pm_runtime_mark_last_busy(twl->dev);
+	pm_runtime_put_autosuspend(twl->dev);
+
+	return 0;
 }
 
 static int twl4030_phy_power_on(struct phy *phy)
 {
 	struct twl4030_usb *twl = phy_get_drvdata(phy);
 
-	if (!twl->asleep)
-		return 0;
-	__twl4030_phy_power_on(twl);
-	twl->asleep = 0;
 	dev_dbg(twl->dev, "%s\n", __func__);
+	pm_runtime_get_sync(twl->dev);
+	twl4030_i2c_access(twl, 1);
+	twl4030_usb_set_mode(twl, twl->usb_mode);
+	if (twl->usb_mode == T2_USB_MODE_ULPI)
+		twl4030_i2c_access(twl, 0);
 
 	/*
 	 * XXX When VBUS gets driven after musb goes to A mode,
@@ -558,9 +577,27 @@ static irqreturn_t twl4030_usb_irq(int irq, void *_twl)
 		 * USB_LINK_VBUS state.  musb_hdrc won't care until it
 		 * starts to handle softconnect right.
 		 */
+		if ((status == OMAP_MUSB_VBUS_VALID) ||
+		    (status == OMAP_MUSB_ID_GROUND)) {
+			if (twl->asleep)
+				pm_runtime_get_sync(twl->dev);
+		} else {
+			if (!twl->asleep) {
+				pm_runtime_mark_last_busy(twl->dev);
+				pm_runtime_put_autosuspend(twl->dev);
+			}
+		}
 		omap_musb_mailbox(status);
 	}
-	sysfs_notify(&twl->dev->kobj, NULL, "vbus");
+
+	/* don't schedule during sleep - irq works right then */
+	if (status == OMAP_MUSB_ID_GROUND && !twl->asleep) {
+		cancel_delayed_work(&twl->id_workaround_work);
+		schedule_delayed_work(&twl->id_workaround_work, HZ);
+	}
+
+	if (irq)
+		sysfs_notify(&twl->dev->kobj, NULL, "vbus");
 
 	return IRQ_HANDLED;
 }
@@ -569,29 +606,8 @@ static void twl4030_id_workaround_work(struct work_struct *work)
 {
 	struct twl4030_usb *twl = container_of(work, struct twl4030_usb,
 		id_workaround_work.work);
-	enum omap_musb_vbus_id_status status;
-	bool status_changed = false;
-
-	status = twl4030_usb_linkstat(twl);
-
-	spin_lock_irq(&twl->lock);
-	if (status >= 0 && status != twl->linkstat) {
-		twl->linkstat = status;
-		status_changed = true;
-	}
-	spin_unlock_irq(&twl->lock);
-
-	if (status_changed) {
-		dev_dbg(twl->dev, "handle missing status change to %d\n",
-				status);
-		omap_musb_mailbox(status);
-	}
 
-	/* don't schedule during sleep - irq works right then */
-	if (status == OMAP_MUSB_ID_GROUND && !twl->asleep) {
-		cancel_delayed_work(&twl->id_workaround_work);
-		schedule_delayed_work(&twl->id_workaround_work, HZ);
-	}
+	twl4030_usb_irq(0, twl);
 }
 
 static int twl4030_phy_init(struct phy *phy)
@@ -599,22 +615,17 @@ static int twl4030_phy_init(struct phy *phy)
 	struct twl4030_usb *twl = phy_get_drvdata(phy);
 	enum omap_musb_vbus_id_status status;
 
-	/*
-	 * Start in sleep state, we'll get called through set_suspend()
-	 * callback when musb is runtime resumed and it's time to start.
-	 */
-	__twl4030_phy_power(twl, 0);
-	twl->asleep = 1;
-
+	pm_runtime_get_sync(twl->dev);
 	status = twl4030_usb_linkstat(twl);
 	twl->linkstat = status;
 
-	if (status == OMAP_MUSB_ID_GROUND || status == OMAP_MUSB_VBUS_VALID) {
+	if (status == OMAP_MUSB_ID_GROUND || status == OMAP_MUSB_VBUS_VALID)
 		omap_musb_mailbox(twl->linkstat);
-		twl4030_phy_power_on(phy);
-	}
 
 	sysfs_notify(&twl->dev->kobj, NULL, "vbus");
+	pm_runtime_mark_last_busy(twl->dev);
+	pm_runtime_put_autosuspend(twl->dev);
+
 	return 0;
 }
 
@@ -650,6 +661,11 @@ static const struct phy_ops ops = {
 	.owner		= THIS_MODULE,
 };
 
+static const struct dev_pm_ops twl4030_usb_pm_ops = {
+	SET_RUNTIME_PM_OPS(twl4030_usb_runtime_suspend,
+			   twl4030_usb_runtime_resume, NULL)
+};
+
 static int twl4030_usb_probe(struct platform_device *pdev)
 {
 	struct twl4030_usb_data *pdata = dev_get_platdata(&pdev->dev);
@@ -726,6 +742,11 @@ static int twl4030_usb_probe(struct platform_device *pdev)
 
 	ATOMIC_INIT_NOTIFIER_HEAD(&twl->phy.notifier);
 
+	pm_runtime_use_autosuspend(&pdev->dev);
+	pm_runtime_set_autosuspend_delay(&pdev->dev, 2000);
+	pm_runtime_enable(&pdev->dev);
+	pm_runtime_get_sync(&pdev->dev);
+
 	/* Our job is to use irqs and status from the power module
 	 * to keep the transceiver disabled when nothing's connected.
 	 *
@@ -744,6 +765,9 @@ static int twl4030_usb_probe(struct platform_device *pdev)
 		return status;
 	}
 
+	pm_runtime_mark_last_busy(&pdev->dev);
+	pm_runtime_put_autosuspend(twl->dev);
+
 	dev_info(&pdev->dev, "Initialized TWL4030 USB module\n");
 	return 0;
 }
@@ -753,6 +777,7 @@ static int twl4030_usb_remove(struct platform_device *pdev)
 	struct twl4030_usb *twl = platform_get_drvdata(pdev);
 	int val;
 
+	pm_runtime_get_sync(twl->dev);
 	cancel_delayed_work(&twl->id_workaround_work);
 	device_remove_file(twl->dev, &dev_attr_vbus);
 
@@ -772,9 +797,8 @@ static int twl4030_usb_remove(struct platform_device *pdev)
 
 	/* disable complete OTG block */
 	twl4030_usb_clear_bits(twl, POWER_CTRL, POWER_CTRL_OTG_ENAB);
-
-	if (!twl->asleep)
-		twl4030_phy_power(twl, 0);
+	pm_runtime_mark_last_busy(twl->dev);
+	pm_runtime_put(twl->dev);
 
 	return 0;
 }
@@ -792,6 +816,7 @@ static struct platform_driver twl4030_usb_driver = {
 	.remove		= twl4030_usb_remove,
 	.driver		= {
 		.name	= "twl4030_usb",
+		.pm	= &twl4030_usb_pm_ops,
 		.owner	= THIS_MODULE,
 		.of_match_table = of_match_ptr(twl4030_usb_id_table),
 	},
diff --git a/drivers/scsi/libiscsi.c b/drivers/scsi/libiscsi.c
index 40462415291e..454998669c2a 100644
--- a/drivers/scsi/libiscsi.c
+++ b/drivers/scsi/libiscsi.c
@@ -717,11 +717,21 @@ __iscsi_conn_send_pdu(struct iscsi_conn *conn, struct iscsi_hdr *hdr,
 			return NULL;
 		}
 
+		if (data_size > ISCSI_DEF_MAX_RECV_SEG_LEN) {
+			iscsi_conn_printk(KERN_ERR, conn, "Invalid buffer len of %u for login task. Max len is %u\n", data_size, ISCSI_DEF_MAX_RECV_SEG_LEN);
+			return NULL;
+		}
+
 		task = conn->login_task;
 	} else {
 		if (session->state != ISCSI_STATE_LOGGED_IN)
 			return NULL;
 
+		if (data_size != 0) {
+			iscsi_conn_printk(KERN_ERR, conn, "Can not send data buffer of len %u for op 0x%x\n", data_size, opcode);
+			return NULL;
+		}
+
 		BUG_ON(conn->c_stage == ISCSI_CONN_INITIAL_STAGE);
 		BUG_ON(conn->c_stage == ISCSI_CONN_STOPPED);
 
diff --git a/drivers/spi/spi-dw-pci.c b/drivers/spi/spi-dw-pci.c
index 3f3dc1226edf..e14960470d8d 100644
--- a/drivers/spi/spi-dw-pci.c
+++ b/drivers/spi/spi-dw-pci.c
@@ -62,6 +62,8 @@ static int spi_pci_probe(struct pci_dev *pdev,
 	if (ret)
 		return ret;
 
+	dws->regs = pcim_iomap_table(pdev)[pci_bar];
+
 	dws->bus_num = 0;
 	dws->num_cs = 4;
 	dws->irq = pdev->irq;
diff --git a/drivers/spi/spi-omap2-mcspi.c b/drivers/spi/spi-omap2-mcspi.c
index a64f1557c156..b0059e7552b0 100644
--- a/drivers/spi/spi-omap2-mcspi.c
+++ b/drivers/spi/spi-omap2-mcspi.c
@@ -321,7 +321,8 @@ static void omap2_mcspi_set_fifo(const struct spi_device *spi,
 disable_fifo:
 	if (t->rx_buf != NULL)
 		chconf &= ~OMAP2_MCSPI_CHCONF_FFER;
-	else
+
+	if (t->tx_buf != NULL)
 		chconf &= ~OMAP2_MCSPI_CHCONF_FFET;
 
 	mcspi_write_chconf0(spi, chconf);
diff --git a/drivers/staging/iio/meter/ade7758_trigger.c b/drivers/staging/iio/meter/ade7758_trigger.c
index 7a94ddd42f59..8c4f2896cd0d 100644
--- a/drivers/staging/iio/meter/ade7758_trigger.c
+++ b/drivers/staging/iio/meter/ade7758_trigger.c
@@ -85,7 +85,7 @@ int ade7758_probe_trigger(struct iio_dev *indio_dev)
 	ret = iio_trigger_register(st->trig);
 
 	/* select default trigger */
-	indio_dev->trig = st->trig;
+	indio_dev->trig = iio_trigger_get(st->trig);
 	if (ret)
 		goto error_free_irq;
 
diff --git a/drivers/staging/imx-drm/ipuv3-plane.c b/drivers/staging/imx-drm/ipuv3-plane.c
index 34b642a12f8b..c70f1734b274 100644
--- a/drivers/staging/imx-drm/ipuv3-plane.c
+++ b/drivers/staging/imx-drm/ipuv3-plane.c
@@ -277,7 +277,8 @@ static void ipu_plane_dpms(struct ipu_plane *ipu_plane, int mode)
 
 		ipu_idmac_put(ipu_plane->ipu_ch);
 		ipu_dmfc_put(ipu_plane->dmfc);
-		ipu_dp_put(ipu_plane->dp);
+		if (ipu_plane->dp)
+			ipu_dp_put(ipu_plane->dp);
 	}
 }
 
diff --git a/drivers/staging/lustre/lustre/Kconfig b/drivers/staging/lustre/lustre/Kconfig
index 209e4c7e6f8a..4f65ba1158bf 100644
--- a/drivers/staging/lustre/lustre/Kconfig
+++ b/drivers/staging/lustre/lustre/Kconfig
@@ -57,4 +57,5 @@ config LUSTRE_TRANSLATE_ERRNOS
 config LUSTRE_LLITE_LLOOP
 	tristate "Lustre virtual block device"
 	depends on LUSTRE_FS && BLOCK
+	depends on !PPC_64K_PAGES && !ARM64_64K_PAGES
 	default m
diff --git a/drivers/target/iscsi/iscsi_target.c b/drivers/target/iscsi/iscsi_target.c
index f329ad294fc0..104f29e6b290 100644
--- a/drivers/target/iscsi/iscsi_target.c
+++ b/drivers/target/iscsi/iscsi_target.c
@@ -4513,6 +4513,7 @@ static void iscsit_logout_post_handler_diffcid(
 {
 	struct iscsi_conn *l_conn;
 	struct iscsi_session *sess = conn->sess;
+	bool conn_found = false;
 
 	if (!sess)
 		return;
@@ -4521,12 +4522,13 @@ static void iscsit_logout_post_handler_diffcid(
 	list_for_each_entry(l_conn, &sess->sess_conn_list, conn_list) {
 		if (l_conn->cid == cid) {
 			iscsit_inc_conn_usage_count(l_conn);
+			conn_found = true;
 			break;
 		}
 	}
 	spin_unlock_bh(&sess->conn_lock);
 
-	if (!l_conn)
+	if (!conn_found)
 		return;
 
 	if (l_conn->sock)
diff --git a/drivers/target/iscsi/iscsi_target_parameters.c b/drivers/target/iscsi/iscsi_target_parameters.c
index 4d2e23fc76fd..43b7e6a616b8 100644
--- a/drivers/target/iscsi/iscsi_target_parameters.c
+++ b/drivers/target/iscsi/iscsi_target_parameters.c
@@ -601,7 +601,7 @@ int iscsi_copy_param_list(
 	param_list = kzalloc(sizeof(struct iscsi_param_list), GFP_KERNEL);
 	if (!param_list) {
 		pr_err("Unable to allocate memory for struct iscsi_param_list.\n");
-		goto err_out;
+		return -1;
 	}
 	INIT_LIST_HEAD(&param_list->param_list);
 	INIT_LIST_HEAD(&param_list->extra_response_list);
diff --git a/drivers/target/target_core_configfs.c b/drivers/target/target_core_configfs.c
index 483d324020a6..f30385385544 100644
--- a/drivers/target/target_core_configfs.c
+++ b/drivers/target/target_core_configfs.c
@@ -2359,7 +2359,7 @@ static ssize_t target_core_alua_tg_pt_gp_store_attr_alua_support_##_name(\
 		pr_err("Invalid value '%ld', must be '0' or '1'\n", tmp); \
 		return -EINVAL;						\
 	}								\
-	if (!tmp)							\
+	if (tmp)							\
 		t->_var |= _bit;					\
 	else								\
 		t->_var &= ~_bit;					\
diff --git a/drivers/tty/serial/8250/8250_dma.c b/drivers/tty/serial/8250/8250_dma.c
index ab9096dc3849..148ffe4c232f 100644
--- a/drivers/tty/serial/8250/8250_dma.c
+++ b/drivers/tty/serial/8250/8250_dma.c
@@ -192,21 +192,28 @@ int serial8250_request_dma(struct uart_8250_port *p)
 
 	dma->rx_buf = dma_alloc_coherent(dma->rxchan->device->dev, dma->rx_size,
 					&dma->rx_addr, GFP_KERNEL);
-	if (!dma->rx_buf) {
-		dma_release_channel(dma->rxchan);
-		dma_release_channel(dma->txchan);
-		return -ENOMEM;
-	}
+	if (!dma->rx_buf)
+		goto err;
 
 	/* TX buffer */
 	dma->tx_addr = dma_map_single(dma->txchan->device->dev,
 					p->port.state->xmit.buf,
 					UART_XMIT_SIZE,
 					DMA_TO_DEVICE);
+	if (dma_mapping_error(dma->txchan->device->dev, dma->tx_addr)) {
+		dma_free_coherent(dma->rxchan->device->dev, dma->rx_size,
+				  dma->rx_buf, dma->rx_addr);
+		goto err;
+	}
 
 	dev_dbg_ratelimited(p->port.dev, "got both dma channels\n");
 
 	return 0;
+err:
+	dma_release_channel(dma->rxchan);
+	dma_release_channel(dma->txchan);
+
+	return -ENOMEM;
 }
 EXPORT_SYMBOL_GPL(serial8250_request_dma);
 
diff --git a/drivers/usb/chipidea/ci_hdrc_msm.c b/drivers/usb/chipidea/ci_hdrc_msm.c
index 2d51d852b474..ca1123d415c5 100644
--- a/drivers/usb/chipidea/ci_hdrc_msm.c
+++ b/drivers/usb/chipidea/ci_hdrc_msm.c
@@ -20,13 +20,13 @@
 static void ci_hdrc_msm_notify_event(struct ci_hdrc *ci, unsigned event)
 {
 	struct device *dev = ci->gadget.dev.parent;
-	int val;
 
 	switch (event) {
 	case CI_HDRC_CONTROLLER_RESET_EVENT:
 		dev_dbg(dev, "CI_HDRC_CONTROLLER_RESET_EVENT received\n");
 		writel(0, USB_AHBBURST);
 		writel(0, USB_AHBMODE);
+		usb_phy_init(ci->transceiver);
 		break;
 	case CI_HDRC_CONTROLLER_STOPPED_EVENT:
 		dev_dbg(dev, "CI_HDRC_CONTROLLER_STOPPED_EVENT received\n");
@@ -34,10 +34,7 @@ static void ci_hdrc_msm_notify_event(struct ci_hdrc *ci, unsigned event)
 		 * Put the transceiver in non-driving mode. Otherwise host
 		 * may not detect soft-disconnection.
 		 */
-		val = usb_phy_io_read(ci->transceiver, ULPI_FUNC_CTRL);
-		val &= ~ULPI_FUNC_CTRL_OPMODE_MASK;
-		val |= ULPI_FUNC_CTRL_OPMODE_NONDRIVING;
-		usb_phy_io_write(ci->transceiver, val, ULPI_FUNC_CTRL);
+		usb_phy_notify_disconnect(ci->transceiver, USB_SPEED_UNKNOWN);
 		break;
 	default:
 		dev_dbg(dev, "unknown ci_hdrc event\n");
diff --git a/drivers/usb/core/hub.c b/drivers/usb/core/hub.c
index 6650df70bb35..263612ce1f62 100644
--- a/drivers/usb/core/hub.c
+++ b/drivers/usb/core/hub.c
@@ -4764,9 +4764,10 @@ static void hub_events(void)
 
 		hub = list_entry(tmp, struct usb_hub, event_list);
 		kref_get(&hub->kref);
+		hdev = hub->hdev;
+		usb_get_dev(hdev);
 		spin_unlock_irq(&hub_event_lock);
 
-		hdev = hub->hdev;
 		hub_dev = hub->intfdev;
 		intf = to_usb_interface(hub_dev);
 		dev_dbg(hub_dev, "state %d ports %d chg %04x evt %04x\n",
@@ -4979,6 +4980,7 @@ static void hub_events(void)
 		usb_autopm_put_interface(intf);
  loop_disconnected:
 		usb_unlock_device(hdev);
+		usb_put_dev(hdev);
 		kref_put(&hub->kref, hub_release);
 
 	} /* end while (1) */
diff --git a/drivers/usb/dwc3/core.c b/drivers/usb/dwc3/core.c
index a49217ae3533..f074755372a0 100644
--- a/drivers/usb/dwc3/core.c
+++ b/drivers/usb/dwc3/core.c
@@ -583,12 +583,6 @@ static int dwc3_remove(struct platform_device *pdev)
 {
 	struct dwc3	*dwc = platform_get_drvdata(pdev);
 
-	usb_phy_set_suspend(dwc->usb2_phy, 1);
-	usb_phy_set_suspend(dwc->usb3_phy, 1);
-
-	pm_runtime_put_sync(&pdev->dev);
-	pm_runtime_disable(&pdev->dev);
-
 	dwc3_debugfs_exit(dwc);
 
 	switch (dwc->dr_mode) {
@@ -609,8 +603,15 @@ static int dwc3_remove(struct platform_device *pdev)
 
 	dwc3_event_buffers_cleanup(dwc);
 	dwc3_free_event_buffers(dwc);
+
+	usb_phy_set_suspend(dwc->usb2_phy, 1);
+	usb_phy_set_suspend(dwc->usb3_phy, 1);
+
 	dwc3_core_exit(dwc);
 
+	pm_runtime_put_sync(&pdev->dev);
+	pm_runtime_disable(&pdev->dev);
+
 	return 0;
 }
 
diff --git a/drivers/usb/dwc3/dwc3-omap.c b/drivers/usb/dwc3/dwc3-omap.c
index b269dbd47fc4..2a6841c95b64 100644
--- a/drivers/usb/dwc3/dwc3-omap.c
+++ b/drivers/usb/dwc3/dwc3-omap.c
@@ -582,9 +582,9 @@ static int dwc3_omap_remove(struct platform_device *pdev)
 	if (omap->extcon_id_dev.edev)
 		extcon_unregister_interest(&omap->extcon_id_dev);
 	dwc3_omap_disable_irqs(omap);
+	device_for_each_child(&pdev->dev, NULL, dwc3_omap_remove_core);
 	pm_runtime_put_sync(&pdev->dev);
 	pm_runtime_disable(&pdev->dev);
-	device_for_each_child(&pdev->dev, NULL, dwc3_omap_remove_core);
 
 	return 0;
 }
diff --git a/drivers/usb/host/ehci-hcd.c b/drivers/usb/host/ehci-hcd.c
index 81cda09b47e3..488a30836c36 100644
--- a/drivers/usb/host/ehci-hcd.c
+++ b/drivers/usb/host/ehci-hcd.c
@@ -965,8 +965,6 @@ rescan:
 	}
 
 	qh->exception = 1;
-	if (ehci->rh_state < EHCI_RH_RUNNING)
-		qh->qh_state = QH_STATE_IDLE;
 	switch (qh->qh_state) {
 	case QH_STATE_LINKED:
 		WARN_ON(!list_empty(&qh->qtd_list));
diff --git a/drivers/usb/host/xhci-hub.c b/drivers/usb/host/xhci-hub.c
index 9992fbfec85f..93fe089cd51a 100644
--- a/drivers/usb/host/xhci-hub.c
+++ b/drivers/usb/host/xhci-hub.c
@@ -470,7 +470,8 @@ static void xhci_hub_report_usb2_link_state(u32 *status, u32 status_reg)
 }
 
 /* Updates Link Status for super Speed port */
-static void xhci_hub_report_usb3_link_state(u32 *status, u32 status_reg)
+static void xhci_hub_report_usb3_link_state(struct xhci_hcd *xhci,
+		u32 *status, u32 status_reg)
 {
 	u32 pls = status_reg & PORT_PLS_MASK;
 
@@ -509,7 +510,8 @@ static void xhci_hub_report_usb3_link_state(u32 *status, u32 status_reg)
 		 * in which sometimes the port enters compliance mode
 		 * caused by a delay on the host-device negotiation.
 		 */
-		if (pls == USB_SS_PORT_LS_COMP_MOD)
+		if ((xhci->quirks & XHCI_COMP_MODE_QUIRK) &&
+				(pls == USB_SS_PORT_LS_COMP_MOD))
 			pls |= USB_PORT_STAT_CONNECTION;
 	}
 
@@ -668,7 +670,7 @@ static u32 xhci_get_port_status(struct usb_hcd *hcd,
 	}
 	/* Update Port Link State */
 	if (hcd->speed == HCD_USB3) {
-		xhci_hub_report_usb3_link_state(&status, raw_port_status);
+		xhci_hub_report_usb3_link_state(xhci, &status, raw_port_status);
 		/*
 		 * Verify if all USB3 Ports Have entered U0 already.
 		 * Delete Compliance Mode Timer if so.
diff --git a/drivers/usb/host/xhci-mem.c b/drivers/usb/host/xhci-mem.c
index 4133a00461b1..9bce4f0e99be 100644
--- a/drivers/usb/host/xhci-mem.c
+++ b/drivers/usb/host/xhci-mem.c
@@ -1723,7 +1723,7 @@ void xhci_mem_cleanup(struct xhci_hcd *xhci)
 	}
 
 	num_ports = HCS_MAX_PORTS(xhci->hcs_params1);
-	for (i = 0; i < num_ports; i++) {
+	for (i = 0; i < num_ports && xhci->rh_bw; i++) {
 		struct xhci_interval_bw_table *bwt = &xhci->rh_bw[i].bw_table;
 		for (j = 0; j < XHCI_MAX_INTERVAL; j++) {
 			struct list_head *ep = &bwt->interval_bw[j].endpoints;
diff --git a/drivers/usb/host/xhci.c b/drivers/usb/host/xhci.c
index ab831048e8a4..82b563fc4fd6 100644
--- a/drivers/usb/host/xhci.c
+++ b/drivers/usb/host/xhci.c
@@ -3928,13 +3928,21 @@ static int __maybe_unused xhci_change_max_exit_latency(struct xhci_hcd *xhci,
 	int ret;
 
 	spin_lock_irqsave(&xhci->lock, flags);
-	if (max_exit_latency == xhci->devs[udev->slot_id]->current_mel) {
+
+	virt_dev = xhci->devs[udev->slot_id];
+
+	/*
+	 * virt_dev might not exists yet if xHC resumed from hibernate (S4) and
+	 * xHC was re-initialized. Exit latency will be set later after
+	 * hub_port_finish_reset() is done and xhci->devs[] are re-allocated
+	 */
+
+	if (!virt_dev || max_exit_latency == virt_dev->current_mel) {
 		spin_unlock_irqrestore(&xhci->lock, flags);
 		return 0;
 	}
 
 	/* Attempt to issue an Evaluate Context command to change the MEL. */
-	virt_dev = xhci->devs[udev->slot_id];
 	command = xhci->lpm_command;
 	ctrl_ctx = xhci_get_input_control_ctx(xhci, command->in_ctx);
 	if (!ctrl_ctx) {
diff --git a/drivers/usb/misc/sisusbvga/sisusb.c b/drivers/usb/misc/sisusbvga/sisusb.c
index de98906f786d..0aef801edbc1 100644
--- a/drivers/usb/misc/sisusbvga/sisusb.c
+++ b/drivers/usb/misc/sisusbvga/sisusb.c
@@ -3248,6 +3248,7 @@ static const struct usb_device_id sisusb_table[] = {
 	{ USB_DEVICE(0x0711, 0x0918) },
 	{ USB_DEVICE(0x0711, 0x0920) },
 	{ USB_DEVICE(0x0711, 0x0950) },
+	{ USB_DEVICE(0x0711, 0x5200) },
 	{ USB_DEVICE(0x182d, 0x021c) },
 	{ USB_DEVICE(0x182d, 0x0269) },
 	{ }
diff --git a/drivers/usb/phy/phy-tegra-usb.c b/drivers/usb/phy/phy-tegra-usb.c
index bbe4f8e6e8d7..8834b70c868c 100644
--- a/drivers/usb/phy/phy-tegra-usb.c
+++ b/drivers/usb/phy/phy-tegra-usb.c
@@ -881,8 +881,8 @@ static int utmi_phy_probe(struct tegra_usb_phy *tegra_phy,
 		return -ENOMEM;
 	}
 
-	tegra_phy->config = devm_kzalloc(&pdev->dev,
-		sizeof(*tegra_phy->config), GFP_KERNEL);
+	tegra_phy->config = devm_kzalloc(&pdev->dev, sizeof(*config),
+					 GFP_KERNEL);
 	if (!tegra_phy->config) {
 		dev_err(&pdev->dev,
 			"unable to allocate memory for USB UTMIP config\n");
diff --git a/drivers/usb/serial/ftdi_sio.c b/drivers/usb/serial/ftdi_sio.c
index 8b0f517abb6b..3614620e09e1 100644
--- a/drivers/usb/serial/ftdi_sio.c
+++ b/drivers/usb/serial/ftdi_sio.c
@@ -741,6 +741,7 @@ static const struct usb_device_id id_table_combined[] = {
 	{ USB_DEVICE(FTDI_VID, FTDI_NDI_AURORA_SCU_PID),
 		.driver_info = (kernel_ulong_t)&ftdi_NDI_device_quirk },
 	{ USB_DEVICE(TELLDUS_VID, TELLDUS_TELLSTICK_PID) },
+	{ USB_DEVICE(NOVITUS_VID, NOVITUS_BONO_E_PID) },
 	{ USB_DEVICE(RTSYSTEMS_VID, RTSYSTEMS_USB_S03_PID) },
 	{ USB_DEVICE(RTSYSTEMS_VID, RTSYSTEMS_USB_59_PID) },
 	{ USB_DEVICE(RTSYSTEMS_VID, RTSYSTEMS_USB_57A_PID) },
@@ -952,6 +953,8 @@ static const struct usb_device_id id_table_combined[] = {
 	{ USB_DEVICE(FTDI_VID, FTDI_EKEY_CONV_USB_PID) },
 	/* Infineon Devices */
 	{ USB_DEVICE_INTERFACE_NUMBER(INFINEON_VID, INFINEON_TRIBOARD_PID, 1) },
+	/* GE Healthcare devices */
+	{ USB_DEVICE(GE_HEALTHCARE_VID, GE_HEALTHCARE_NEMO_TRACKER_PID) },
 	{ }					/* Terminating entry */
 };
 
diff --git a/drivers/usb/serial/ftdi_sio_ids.h b/drivers/usb/serial/ftdi_sio_ids.h
index 70b0b1d88ae9..5937b2d242f2 100644
--- a/drivers/usb/serial/ftdi_sio_ids.h
+++ b/drivers/usb/serial/ftdi_sio_ids.h
@@ -837,6 +837,12 @@
 #define TELLDUS_TELLSTICK_PID		0x0C30	/* RF control dongle 433 MHz using FT232RL */
 
 /*
+ * NOVITUS printers
+ */
+#define NOVITUS_VID			0x1a28
+#define NOVITUS_BONO_E_PID		0x6010
+
+/*
  * RT Systems programming cables for various ham radios
  */
 #define RTSYSTEMS_VID		0x2100	/* Vendor ID */
@@ -1385,3 +1391,9 @@
  * ekey biometric systems GmbH (http://ekey.net/)
  */
 #define FTDI_EKEY_CONV_USB_PID		0xCB08	/* Converter USB */
+
+/*
+ * GE Healthcare devices
+ */
+#define GE_HEALTHCARE_VID		0x1901
+#define GE_HEALTHCARE_NEMO_TRACKER_PID	0x0015
diff --git a/drivers/usb/serial/option.c b/drivers/usb/serial/option.c
index 9da566a3f5c8..e47aabe0c760 100644
--- a/drivers/usb/serial/option.c
+++ b/drivers/usb/serial/option.c
@@ -275,8 +275,12 @@ static void option_instat_callback(struct urb *urb);
 #define ZTE_PRODUCT_MF622			0x0001
 #define ZTE_PRODUCT_MF628			0x0015
 #define ZTE_PRODUCT_MF626			0x0031
-#define ZTE_PRODUCT_MC2718			0xffe8
 #define ZTE_PRODUCT_AC2726			0xfff1
+#define ZTE_PRODUCT_CDMA_TECH			0xfffe
+#define ZTE_PRODUCT_AC8710T			0xffff
+#define ZTE_PRODUCT_MC2718			0xffe8
+#define ZTE_PRODUCT_AD3812			0xffeb
+#define ZTE_PRODUCT_MC2716			0xffed
 
 #define BENQ_VENDOR_ID				0x04a5
 #define BENQ_PRODUCT_H10			0x4068
@@ -494,6 +498,10 @@ static void option_instat_callback(struct urb *urb);
 #define INOVIA_VENDOR_ID			0x20a6
 #define INOVIA_SEW858				0x1105
 
+/* VIA Telecom */
+#define VIATELECOM_VENDOR_ID			0x15eb
+#define VIATELECOM_PRODUCT_CDS7			0x0001
+
 /* some devices interfaces need special handling due to a number of reasons */
 enum option_blacklist_reason {
 		OPTION_BLACKLIST_NONE = 0,
@@ -527,10 +535,18 @@ static const struct option_blacklist_info zte_k3765_z_blacklist = {
 	.reserved = BIT(4),
 };
 
+static const struct option_blacklist_info zte_ad3812_z_blacklist = {
+	.sendsetup = BIT(0) | BIT(1) | BIT(2),
+};
+
 static const struct option_blacklist_info zte_mc2718_z_blacklist = {
 	.sendsetup = BIT(1) | BIT(2) | BIT(3) | BIT(4),
 };
 
+static const struct option_blacklist_info zte_mc2716_z_blacklist = {
+	.sendsetup = BIT(1) | BIT(2) | BIT(3),
+};
+
 static const struct option_blacklist_info huawei_cdc12_blacklist = {
 	.reserved = BIT(1) | BIT(2),
 };
@@ -1070,6 +1086,7 @@ static const struct usb_device_id option_ids[] = {
 	{ USB_DEVICE_INTERFACE_CLASS(BANDRICH_VENDOR_ID, BANDRICH_PRODUCT_1012, 0xff) },
 	{ USB_DEVICE(KYOCERA_VENDOR_ID, KYOCERA_PRODUCT_KPC650) },
 	{ USB_DEVICE(KYOCERA_VENDOR_ID, KYOCERA_PRODUCT_KPC680) },
+	{ USB_DEVICE(QUALCOMM_VENDOR_ID, 0x6000)}, /* ZTE AC8700 */
 	{ USB_DEVICE(QUALCOMM_VENDOR_ID, 0x6613)}, /* Onda H600/ZTE MF330 */
 	{ USB_DEVICE(QUALCOMM_VENDOR_ID, 0x0023)}, /* ONYX 3G device */
 	{ USB_DEVICE(QUALCOMM_VENDOR_ID, 0x9000)}, /* SIMCom SIM5218 */
@@ -1544,13 +1561,18 @@ static const struct usb_device_id option_ids[] = {
 	{ USB_DEVICE_AND_INTERFACE_INFO(ZTE_VENDOR_ID, 0xff93, 0xff, 0xff, 0xff) },
 	{ USB_DEVICE_AND_INTERFACE_INFO(ZTE_VENDOR_ID, 0xff94, 0xff, 0xff, 0xff) },
 
-	/* NOTE: most ZTE CDMA devices should be driven by zte_ev, not option */
+	{ USB_DEVICE_AND_INTERFACE_INFO(ZTE_VENDOR_ID, ZTE_PRODUCT_CDMA_TECH, 0xff, 0xff, 0xff) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(ZTE_VENDOR_ID, ZTE_PRODUCT_AC2726, 0xff, 0xff, 0xff) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(ZTE_VENDOR_ID, ZTE_PRODUCT_AC8710T, 0xff, 0xff, 0xff) },
 	{ USB_DEVICE_AND_INTERFACE_INFO(ZTE_VENDOR_ID, ZTE_PRODUCT_MC2718, 0xff, 0xff, 0xff),
 	 .driver_info = (kernel_ulong_t)&zte_mc2718_z_blacklist },
+	{ USB_DEVICE_AND_INTERFACE_INFO(ZTE_VENDOR_ID, ZTE_PRODUCT_AD3812, 0xff, 0xff, 0xff),
+	 .driver_info = (kernel_ulong_t)&zte_ad3812_z_blacklist },
+	{ USB_DEVICE_AND_INTERFACE_INFO(ZTE_VENDOR_ID, ZTE_PRODUCT_MC2716, 0xff, 0xff, 0xff),
+	 .driver_info = (kernel_ulong_t)&zte_mc2716_z_blacklist },
 	{ USB_VENDOR_AND_INTERFACE_INFO(ZTE_VENDOR_ID, 0xff, 0x02, 0x01) },
 	{ USB_VENDOR_AND_INTERFACE_INFO(ZTE_VENDOR_ID, 0xff, 0x02, 0x05) },
 	{ USB_VENDOR_AND_INTERFACE_INFO(ZTE_VENDOR_ID, 0xff, 0x86, 0x10) },
-	{ USB_DEVICE_AND_INTERFACE_INFO(ZTE_VENDOR_ID, ZTE_PRODUCT_AC2726, 0xff, 0xff, 0xff) },
 
 	{ USB_DEVICE(BENQ_VENDOR_ID, BENQ_PRODUCT_H10) },
 	{ USB_DEVICE(DLINK_VENDOR_ID, DLINK_PRODUCT_DWM_652) },
@@ -1724,6 +1746,7 @@ static const struct usb_device_id option_ids[] = {
 	{ USB_DEVICE_AND_INTERFACE_INFO(0x07d1, 0x3e01, 0xff, 0xff, 0xff) }, /* D-Link DWM-152/C1 */
 	{ USB_DEVICE_AND_INTERFACE_INFO(0x07d1, 0x3e02, 0xff, 0xff, 0xff) }, /* D-Link DWM-156/C1 */
 	{ USB_DEVICE(INOVIA_VENDOR_ID, INOVIA_SEW858) },
+	{ USB_DEVICE(VIATELECOM_VENDOR_ID, VIATELECOM_PRODUCT_CDS7) },
 	{ } /* Terminating entry */
 };
 MODULE_DEVICE_TABLE(usb, option_ids);
diff --git a/drivers/usb/serial/pl2303.c b/drivers/usb/serial/pl2303.c
index b3d5a35c0d4b..e9bad928039f 100644
--- a/drivers/usb/serial/pl2303.c
+++ b/drivers/usb/serial/pl2303.c
@@ -45,6 +45,7 @@ static const struct usb_device_id id_table[] = {
 	{ USB_DEVICE(PL2303_VENDOR_ID, PL2303_PRODUCT_ID_GPRS) },
 	{ USB_DEVICE(PL2303_VENDOR_ID, PL2303_PRODUCT_ID_HCR331) },
 	{ USB_DEVICE(PL2303_VENDOR_ID, PL2303_PRODUCT_ID_MOTOROLA) },
+	{ USB_DEVICE(PL2303_VENDOR_ID, PL2303_PRODUCT_ID_ZTEK) },
 	{ USB_DEVICE(IODATA_VENDOR_ID, IODATA_PRODUCT_ID) },
 	{ USB_DEVICE(IODATA_VENDOR_ID, IODATA_PRODUCT_ID_RSAQ5) },
 	{ USB_DEVICE(ATEN_VENDOR_ID, ATEN_PRODUCT_ID) },
diff --git a/drivers/usb/serial/pl2303.h b/drivers/usb/serial/pl2303.h
index 42bc082896ac..71fd9da1d6e7 100644
--- a/drivers/usb/serial/pl2303.h
+++ b/drivers/usb/serial/pl2303.h
@@ -22,6 +22,7 @@
 #define PL2303_PRODUCT_ID_GPRS		0x0609
 #define PL2303_PRODUCT_ID_HCR331	0x331a
 #define PL2303_PRODUCT_ID_MOTOROLA	0x0307
+#define PL2303_PRODUCT_ID_ZTEK		0xe1f1
 
 #define ATEN_VENDOR_ID		0x0557
 #define ATEN_VENDOR_ID2		0x0547
diff --git a/drivers/usb/serial/sierra.c b/drivers/usb/serial/sierra.c
index 37480348e39b..74a9375a9bb5 100644
--- a/drivers/usb/serial/sierra.c
+++ b/drivers/usb/serial/sierra.c
@@ -282,14 +282,19 @@ static const struct usb_device_id id_table[] = {
 	/* Sierra Wireless HSPA Non-Composite Device */
 	{ USB_DEVICE_AND_INTERFACE_INFO(0x1199, 0x6892, 0xFF, 0xFF, 0xFF)},
 	{ USB_DEVICE(0x1199, 0x6893) },	/* Sierra Wireless Device */
-	{ USB_DEVICE(0x1199, 0x68A3), 	/* Sierra Wireless Direct IP modems */
+	/* Sierra Wireless Direct IP modems */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x1199, 0x68A3, 0xFF, 0xFF, 0xFF),
+	  .driver_info = (kernel_ulong_t)&direct_ip_interface_blacklist
+	},
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x1199, 0x68AA, 0xFF, 0xFF, 0xFF),
 	  .driver_info = (kernel_ulong_t)&direct_ip_interface_blacklist
 	},
 	/* AT&T Direct IP LTE modems */
 	{ USB_DEVICE_AND_INTERFACE_INFO(0x0F3D, 0x68AA, 0xFF, 0xFF, 0xFF),
 	  .driver_info = (kernel_ulong_t)&direct_ip_interface_blacklist
 	},
-	{ USB_DEVICE(0x0f3d, 0x68A3), 	/* Airprime/Sierra Wireless Direct IP modems */
+	/* Airprime/Sierra Wireless Direct IP modems */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x0F3D, 0x68A3, 0xFF, 0xFF, 0xFF),
 	  .driver_info = (kernel_ulong_t)&direct_ip_interface_blacklist
 	},
 
diff --git a/drivers/usb/serial/usb-serial.c b/drivers/usb/serial/usb-serial.c
index b169b0f9b3a2..9a08e18e09b9 100644
--- a/drivers/usb/serial/usb-serial.c
+++ b/drivers/usb/serial/usb-serial.c
@@ -764,29 +764,39 @@ static int usb_serial_probe(struct usb_interface *interface,
 		if (usb_endpoint_is_bulk_in(endpoint)) {
 			/* we found a bulk in endpoint */
 			dev_dbg(ddev, "found bulk in on endpoint %d\n", i);
-			bulk_in_endpoint[num_bulk_in] = endpoint;
-			++num_bulk_in;
+			if (num_bulk_in < MAX_NUM_PORTS) {
+				bulk_in_endpoint[num_bulk_in] = endpoint;
+				++num_bulk_in;
+			}
 		}
 
 		if (usb_endpoint_is_bulk_out(endpoint)) {
 			/* we found a bulk out endpoint */
 			dev_dbg(ddev, "found bulk out on endpoint %d\n", i);
-			bulk_out_endpoint[num_bulk_out] = endpoint;
-			++num_bulk_out;
+			if (num_bulk_out < MAX_NUM_PORTS) {
+				bulk_out_endpoint[num_bulk_out] = endpoint;
+				++num_bulk_out;
+			}
 		}
 
 		if (usb_endpoint_is_int_in(endpoint)) {
 			/* we found a interrupt in endpoint */
 			dev_dbg(ddev, "found interrupt in on endpoint %d\n", i);
-			interrupt_in_endpoint[num_interrupt_in] = endpoint;
-			++num_interrupt_in;
+			if (num_interrupt_in < MAX_NUM_PORTS) {
+				interrupt_in_endpoint[num_interrupt_in] =
+						endpoint;
+				++num_interrupt_in;
+			}
 		}
 
 		if (usb_endpoint_is_int_out(endpoint)) {
 			/* we found an interrupt out endpoint */
 			dev_dbg(ddev, "found interrupt out on endpoint %d\n", i);
-			interrupt_out_endpoint[num_interrupt_out] = endpoint;
-			++num_interrupt_out;
+			if (num_interrupt_out < MAX_NUM_PORTS) {
+				interrupt_out_endpoint[num_interrupt_out] =
+						endpoint;
+				++num_interrupt_out;
+			}
 		}
 	}
 
@@ -809,8 +819,10 @@ static int usb_serial_probe(struct usb_interface *interface,
 				if (usb_endpoint_is_int_in(endpoint)) {
 					/* we found a interrupt in endpoint */
 					dev_dbg(ddev, "found interrupt in for Prolific device on separate interface\n");
-					interrupt_in_endpoint[num_interrupt_in] = endpoint;
-					++num_interrupt_in;
+					if (num_interrupt_in < MAX_NUM_PORTS) {
+						interrupt_in_endpoint[num_interrupt_in] = endpoint;
+						++num_interrupt_in;
+					}
 				}
 			}
 		}
@@ -850,6 +862,11 @@ static int usb_serial_probe(struct usb_interface *interface,
 			num_ports = type->num_ports;
 	}
 
+	if (num_ports > MAX_NUM_PORTS) {
+		dev_warn(ddev, "too many ports requested: %d\n", num_ports);
+		num_ports = MAX_NUM_PORTS;
+	}
+
 	serial->num_ports = num_ports;
 	serial->num_bulk_in = num_bulk_in;
 	serial->num_bulk_out = num_bulk_out;
diff --git a/drivers/usb/serial/zte_ev.c b/drivers/usb/serial/zte_ev.c
index e40ab739c4a6..c9bb107d5e5c 100644
--- a/drivers/usb/serial/zte_ev.c
+++ b/drivers/usb/serial/zte_ev.c
@@ -272,28 +272,16 @@ static void zte_ev_usb_serial_close(struct usb_serial_port *port)
 }
 
 static const struct usb_device_id id_table[] = {
-	/* AC8710, AC8710T */
-	{ USB_DEVICE_AND_INTERFACE_INFO(0x19d2, 0xffff, 0xff, 0xff, 0xff) },
-	 /* AC8700 */
-	{ USB_DEVICE_AND_INTERFACE_INFO(0x19d2, 0xfffe, 0xff, 0xff, 0xff) },
-	/* MG880 */
-	{ USB_DEVICE(0x19d2, 0xfffd) },
-	{ USB_DEVICE(0x19d2, 0xfffc) },
-	{ USB_DEVICE(0x19d2, 0xfffb) },
-	/* AC8710_V3 */
+	{ USB_DEVICE(0x19d2, 0xffec) },
+	{ USB_DEVICE(0x19d2, 0xffee) },
 	{ USB_DEVICE(0x19d2, 0xfff6) },
 	{ USB_DEVICE(0x19d2, 0xfff7) },
 	{ USB_DEVICE(0x19d2, 0xfff8) },
 	{ USB_DEVICE(0x19d2, 0xfff9) },
-	{ USB_DEVICE(0x19d2, 0xffee) },
-	/* AC2716, MC2716 */
-	{ USB_DEVICE_AND_INTERFACE_INFO(0x19d2, 0xffed, 0xff, 0xff, 0xff) },
-	/* AD3812 */
-	{ USB_DEVICE_AND_INTERFACE_INFO(0x19d2, 0xffeb, 0xff, 0xff, 0xff) },
-	{ USB_DEVICE(0x19d2, 0xffec) },
-	{ USB_DEVICE(0x05C6, 0x3197) },
-	{ USB_DEVICE(0x05C6, 0x6000) },
-	{ USB_DEVICE(0x05C6, 0x9008) },
+	{ USB_DEVICE(0x19d2, 0xfffb) },
+	{ USB_DEVICE(0x19d2, 0xfffc) },
+	/* MG880 */
+	{ USB_DEVICE(0x19d2, 0xfffd) },
 	{ },
 };
 MODULE_DEVICE_TABLE(usb, id_table);
diff --git a/drivers/usb/storage/unusual_devs.h b/drivers/usb/storage/unusual_devs.h
index 042c83b01046..7f625306ea80 100644
--- a/drivers/usb/storage/unusual_devs.h
+++ b/drivers/usb/storage/unusual_devs.h
@@ -101,6 +101,12 @@ UNUSUAL_DEV(  0x03f0, 0x4002, 0x0001, 0x0001,
 		"PhotoSmart R707",
 		USB_SC_DEVICE, USB_PR_DEVICE, NULL, US_FL_FIX_CAPACITY),
 
+UNUSUAL_DEV(  0x03f3, 0x0001, 0x0000, 0x9999,
+		"Adaptec",
+		"USBConnect 2000",
+		USB_SC_DEVICE, USB_PR_DEVICE, usb_stor_euscsi_init,
+		US_FL_SCM_MULT_TARG ),
+
 /* Reported by Sebastian Kapfer <sebastian_kapfer@gmx.net>
  * and Olaf Hering <olh@suse.de> (different bcd's, same vendor/product)
  * for USB floppies that need the SINGLE_LUN enforcement.
@@ -741,6 +747,12 @@ UNUSUAL_DEV(  0x059b, 0x0001, 0x0100, 0x0100,
 		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
 		US_FL_SINGLE_LUN ),
 
+UNUSUAL_DEV(  0x059b, 0x0040, 0x0100, 0x0100,
+		"Iomega",
+		"Jaz USB Adapter",
+		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
+		US_FL_SINGLE_LUN ),
+
 /* Reported by <Hendryk.Pfeiffer@gmx.de> */
 UNUSUAL_DEV(  0x059f, 0x0643, 0x0000, 0x0000,
 		"LaCie",
@@ -1113,6 +1125,18 @@ UNUSUAL_DEV(  0x0851, 0x1543, 0x0200, 0x0200,
 		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
 		US_FL_NOT_LOCKABLE),
 
+UNUSUAL_DEV(  0x085a, 0x0026, 0x0100, 0x0133,
+		"Xircom",
+		"PortGear USB-SCSI (Mac USB Dock)",
+		USB_SC_DEVICE, USB_PR_DEVICE, usb_stor_euscsi_init,
+		US_FL_SCM_MULT_TARG ),
+
+UNUSUAL_DEV(  0x085a, 0x0028, 0x0100, 0x0133,
+		"Xircom",
+		"PortGear USB to SCSI Converter",
+		USB_SC_DEVICE, USB_PR_DEVICE, usb_stor_euscsi_init,
+		US_FL_SCM_MULT_TARG ),
+
 /* Submitted by Jan De Luyck <lkml@kcore.org> */
 UNUSUAL_DEV(  0x08bd, 0x1100, 0x0000, 0x0000,
 		"CITIZEN",
@@ -1945,6 +1969,14 @@ UNUSUAL_DEV(  0x152d, 0x2329, 0x0100, 0x0100,
 		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
 		US_FL_IGNORE_RESIDUE | US_FL_SANE_SENSE ),
 
+/* Entrega Technologies U1-SC25 (later Xircom PortGear PGSCSI)
+ * and Mac USB Dock USB-SCSI */
+UNUSUAL_DEV(  0x1645, 0x0007, 0x0100, 0x0133,
+		"Entrega Technologies",
+		"USB to SCSI Converter",
+		USB_SC_DEVICE, USB_PR_DEVICE, usb_stor_euscsi_init,
+		US_FL_SCM_MULT_TARG ),
+
 /* Reported by Robert Schedel <r.schedel@yahoo.de>
  * Note: this is a 'super top' device like the above 14cd/6600 device */
 UNUSUAL_DEV(  0x1652, 0x6600, 0x0201, 0x0201,
@@ -1967,6 +1999,12 @@ UNUSUAL_DEV(  0x177f, 0x0400, 0x0000, 0x0000,
 		USB_SC_DEVICE, USB_PR_DEVICE, NULL,
 		US_FL_BULK_IGNORE_TAG | US_FL_MAX_SECTORS_64 ),
 
+UNUSUAL_DEV(  0x1822, 0x0001, 0x0000, 0x9999,
+		"Ariston Technologies",
+		"iConnect USB to SCSI adapter",
+		USB_SC_DEVICE, USB_PR_DEVICE, usb_stor_euscsi_init,
+		US_FL_SCM_MULT_TARG ),
+
 /* Reported by Hans de Goede <hdegoede@redhat.com>
  * These Appotech controllers are found in Picture Frames, they provide a
  * (buggy) emulation of a cdrom drive which contains the windows software
diff --git a/drivers/uwb/lc-dev.c b/drivers/uwb/lc-dev.c
index 80079b8fed15..d0303f0dbe15 100644
--- a/drivers/uwb/lc-dev.c
+++ b/drivers/uwb/lc-dev.c
@@ -431,16 +431,19 @@ void uwbd_dev_onair(struct uwb_rc *rc, struct uwb_beca_e *bce)
 	uwb_dev->mac_addr = *bce->mac_addr;
 	uwb_dev->dev_addr = bce->dev_addr;
 	dev_set_name(&uwb_dev->dev, "%s", macbuf);
+
+	/* plug the beacon cache */
+	bce->uwb_dev = uwb_dev;
+	uwb_dev->bce = bce;
+	uwb_bce_get(bce);		/* released in uwb_dev_sys_release() */
+
 	result = uwb_dev_add(uwb_dev, &rc->uwb_dev.dev, rc);
 	if (result < 0) {
 		dev_err(dev, "new device %s: cannot instantiate device\n",
 			macbuf);
 		goto error_dev_add;
 	}
-	/* plug the beacon cache */
-	bce->uwb_dev = uwb_dev;
-	uwb_dev->bce = bce;
-	uwb_bce_get(bce);		/* released in uwb_dev_sys_release() */
+
 	dev_info(dev, "uwb device (mac %s dev %s) connected to %s %s\n",
 		 macbuf, devbuf, rc->uwb_dev.dev.parent->bus->name,
 		 dev_name(rc->uwb_dev.dev.parent));
@@ -448,6 +451,8 @@ void uwbd_dev_onair(struct uwb_rc *rc, struct uwb_beca_e *bce)
 	return;
 
 error_dev_add:
+	bce->uwb_dev = NULL;
+	uwb_bce_put(bce);
 	kfree(uwb_dev);
 	return;
 }
diff --git a/drivers/xen/manage.c b/drivers/xen/manage.c
index 624e8dc24532..602913d7ae03 100644
--- a/drivers/xen/manage.c
+++ b/drivers/xen/manage.c
@@ -111,16 +111,11 @@ static void do_suspend(void)
 
 	shutting_down = SHUTDOWN_SUSPEND;
 
-#ifdef CONFIG_PREEMPT
-	/* If the kernel is preemptible, we need to freeze all the processes
-	   to prevent them from being in the middle of a pagetable update
-	   during suspend. */
 	err = freeze_processes();
 	if (err) {
 		pr_err("%s: freeze failed %d\n", __func__, err);
 		goto out;
 	}
-#endif
 
 	err = dpm_suspend_start(PMSG_FREEZE);
 	if (err) {
@@ -169,10 +164,8 @@ out_resume:
 	dpm_resume_end(si.cancelled ? PMSG_THAW : PMSG_RESTORE);
 
 out_thaw:
-#ifdef CONFIG_PREEMPT
 	thaw_processes();
 out:
-#endif
 	shutting_down = SHUTDOWN_INVALID;
 }
 #endif	/* CONFIG_HIBERNATE_CALLBACKS */
diff --git a/fs/aio.c b/fs/aio.c
index 6d68e01dc7ca..f45ddaa4fffa 100644
--- a/fs/aio.c
+++ b/fs/aio.c
@@ -141,6 +141,7 @@ struct kioctx {
 
 	struct {
 		unsigned	tail;
+		unsigned	completed_events;
 		spinlock_t	completion_lock;
 	} ____cacheline_aligned_in_smp;
 
@@ -796,6 +797,9 @@ void exit_aio(struct mm_struct *mm)
 	unsigned i = 0;
 
 	while (1) {
+		struct completion requests_done =
+			COMPLETION_INITIALIZER_ONSTACK(requests_done);
+
 		rcu_read_lock();
 		table = rcu_dereference(mm->ioctx_table);
 
@@ -823,7 +827,10 @@ void exit_aio(struct mm_struct *mm)
 		 */
 		ctx->mmap_size = 0;
 
-		kill_ioctx(mm, ctx, NULL);
+		kill_ioctx(mm, ctx, &requests_done);
+
+		/* Wait until all IO for the context are done. */
+		wait_for_completion(&requests_done);
 	}
 }
 
@@ -880,6 +887,68 @@ out:
 	return ret;
 }
 
+/* refill_reqs_available
+ *	Updates the reqs_available reference counts used for tracking the
+ *	number of free slots in the completion ring.  This can be called
+ *	from aio_complete() (to optimistically update reqs_available) or
+ *	from aio_get_req() (the we're out of events case).  It must be
+ *	called holding ctx->completion_lock.
+ */
+static void refill_reqs_available(struct kioctx *ctx, unsigned head,
+                                  unsigned tail)
+{
+	unsigned events_in_ring, completed;
+
+	/* Clamp head since userland can write to it. */
+	head %= ctx->nr_events;
+	if (head <= tail)
+		events_in_ring = tail - head;
+	else
+		events_in_ring = ctx->nr_events - (head - tail);
+
+	completed = ctx->completed_events;
+	if (events_in_ring < completed)
+		completed -= events_in_ring;
+	else
+		completed = 0;
+
+	if (!completed)
+		return;
+
+	ctx->completed_events -= completed;
+	put_reqs_available(ctx, completed);
+}
+
+/* user_refill_reqs_available
+ *	Called to refill reqs_available when aio_get_req() encounters an
+ *	out of space in the completion ring.
+ */
+static void user_refill_reqs_available(struct kioctx *ctx)
+{
+	spin_lock_irq(&ctx->completion_lock);
+	if (ctx->completed_events) {
+		struct aio_ring *ring;
+		unsigned head;
+
+		/* Access of ring->head may race with aio_read_events_ring()
+		 * here, but that's okay since whether we read the old version
+		 * or the new version, and either will be valid.  The important
+		 * part is that head cannot pass tail since we prevent
+		 * aio_complete() from updating tail by holding
+		 * ctx->completion_lock.  Even if head is invalid, the check
+		 * against ctx->completed_events below will make sure we do the
+		 * safe/right thing.
+		 */
+		ring = kmap_atomic(ctx->ring_pages[0]);
+		head = ring->head;
+		kunmap_atomic(ring);
+
+		refill_reqs_available(ctx, head, ctx->tail);
+	}
+
+	spin_unlock_irq(&ctx->completion_lock);
+}
+
 /* aio_get_req
  *	Allocate a slot for an aio request.
  * Returns NULL if no requests are free.
@@ -888,8 +957,11 @@ static inline struct kiocb *aio_get_req(struct kioctx *ctx)
 {
 	struct kiocb *req;
 
-	if (!get_reqs_available(ctx))
-		return NULL;
+	if (!get_reqs_available(ctx)) {
+		user_refill_reqs_available(ctx);
+		if (!get_reqs_available(ctx))
+			return NULL;
+	}
 
 	req = kmem_cache_alloc(kiocb_cachep, GFP_KERNEL|__GFP_ZERO);
 	if (unlikely(!req))
@@ -948,8 +1020,8 @@ void aio_complete(struct kiocb *iocb, long res, long res2)
 	struct kioctx	*ctx = iocb->ki_ctx;
 	struct aio_ring	*ring;
 	struct io_event	*ev_page, *event;
+	unsigned tail, pos, head;
 	unsigned long	flags;
-	unsigned tail, pos;
 
 	/*
 	 * Special case handling for sync iocbs:
@@ -1010,10 +1082,14 @@ void aio_complete(struct kiocb *iocb, long res, long res2)
 	ctx->tail = tail;
 
 	ring = kmap_atomic(ctx->ring_pages[0]);
+	head = ring->head;
 	ring->tail = tail;
 	kunmap_atomic(ring);
 	flush_dcache_page(ctx->ring_pages[0]);
 
+	ctx->completed_events++;
+	if (ctx->completed_events > 1)
+		refill_reqs_available(ctx, head, tail);
 	spin_unlock_irqrestore(&ctx->completion_lock, flags);
 
 	pr_debug("added to ring %p at [%u]\n", iocb, tail);
@@ -1028,7 +1104,6 @@ void aio_complete(struct kiocb *iocb, long res, long res2)
 
 	/* everything turned out well, dispose of the aiocb. */
 	kiocb_free(iocb);
-	put_reqs_available(ctx, 1);
 
 	/*
 	 * We have to order our ring_info tail store above and test
@@ -1065,6 +1140,12 @@ static long aio_read_events_ring(struct kioctx *ctx,
 	tail = ring->tail;
 	kunmap_atomic(ring);
 
+	/*
+	 * Ensure that once we've read the current tail pointer, that
+	 * we also see the events that were stored up to the tail.
+	 */
+	smp_rmb();
+
 	pr_debug("h%u t%u m%u\n", head, tail, ctx->nr_events);
 
 	if (head == tail)
diff --git a/fs/buffer.c b/fs/buffer.c
index 27265a8b43c1..71e2d0ed8530 100644
--- a/fs/buffer.c
+++ b/fs/buffer.c
@@ -1029,7 +1029,8 @@ grow_dev_page(struct block_device *bdev, sector_t block,
 		bh = page_buffers(page);
 		if (bh->b_size == size) {
 			end_block = init_page_buffers(page, bdev,
-						index << sizebits, size);
+						(sector_t)index << sizebits,
+						size);
 			goto done;
 		}
 		if (!try_to_free_buffers(page))
@@ -1050,7 +1051,8 @@ grow_dev_page(struct block_device *bdev, sector_t block,
 	 */
 	spin_lock(&inode->i_mapping->private_lock);
 	link_dev_buffers(page, bh);
-	end_block = init_page_buffers(page, bdev, index << sizebits, size);
+	end_block = init_page_buffers(page, bdev, (sector_t)index << sizebits,
+			size);
 	spin_unlock(&inode->i_mapping->private_lock);
 done:
 	ret = (block < end_block) ? 1 : -ENXIO;
diff --git a/fs/cifs/link.c b/fs/cifs/link.c
index 68559fd557fb..a5c2812ead68 100644
--- a/fs/cifs/link.c
+++ b/fs/cifs/link.c
@@ -213,8 +213,12 @@ create_mf_symlink(const unsigned int xid, struct cifs_tcon *tcon,
 	if (rc)
 		goto out;
 
-	rc = tcon->ses->server->ops->create_mf_symlink(xid, tcon, cifs_sb,
-					fromName, buf, &bytes_written);
+	if (tcon->ses->server->ops->create_mf_symlink)
+		rc = tcon->ses->server->ops->create_mf_symlink(xid, tcon,
+					cifs_sb, fromName, buf, &bytes_written);
+	else
+		rc = -EOPNOTSUPP;
+
 	if (rc)
 		goto out;
 
diff --git a/fs/eventpoll.c b/fs/eventpoll.c
index ead00467282d..f50d79eb52db 100644
--- a/fs/eventpoll.c
+++ b/fs/eventpoll.c
@@ -1852,7 +1852,8 @@ SYSCALL_DEFINE4(epoll_ctl, int, epfd, int, op, int, fd,
 		goto error_tgt_fput;
 
 	/* Check if EPOLLWAKEUP is allowed */
-	ep_take_care_of_epollwakeup(&epds);
+	if (ep_op_has_event(op))
+		ep_take_care_of_epollwakeup(&epds);
 
 	/*
 	 * We have to check that the file structure underneath the file descriptor
diff --git a/fs/gfs2/inode.c b/fs/gfs2/inode.c
index 5c524180c98e..bc643b97423c 100644
--- a/fs/gfs2/inode.c
+++ b/fs/gfs2/inode.c
@@ -606,8 +606,10 @@ static int gfs2_create_inode(struct inode *dir, struct dentry *dentry,
 	if (!IS_ERR(inode)) {
 		d = d_splice_alias(inode, dentry);
 		error = PTR_ERR(d);
-		if (IS_ERR(d))
+		if (IS_ERR(d)) {
+			inode = ERR_CAST(d);
 			goto fail_gunlock;
+		}
 		error = 0;
 		if (file) {
 			if (S_ISREG(inode->i_mode)) {
@@ -823,7 +825,6 @@ static struct dentry *__gfs2_lookup(struct inode *dir, struct dentry *dentry,
 
 	d = d_splice_alias(inode, dentry);
 	if (IS_ERR(d)) {
-		iput(inode);
 		gfs2_glock_dq_uninit(&gh);
 		return d;
 	}
diff --git a/fs/lockd/svc.c b/fs/lockd/svc.c
index 6bf06a07f3e0..223e1cb14345 100644
--- a/fs/lockd/svc.c
+++ b/fs/lockd/svc.c
@@ -253,13 +253,11 @@ static int lockd_up_net(struct svc_serv *serv, struct net *net)
 
 	error = make_socks(serv, net);
 	if (error < 0)
-		goto err_socks;
+		goto err_bind;
 	set_grace_period(net);
 	dprintk("lockd_up_net: per-net data created; net=%p\n", net);
 	return 0;
 
-err_socks:
-	svc_rpcb_cleanup(serv, net);
 err_bind:
 	ln->nlmsvc_users--;
 	return error;
diff --git a/fs/namei.c b/fs/namei.c
index d5a4faeb39a5..dd2f2c5bda55 100644
--- a/fs/namei.c
+++ b/fs/namei.c
@@ -642,24 +642,22 @@ static int complete_walk(struct nameidata *nd)
 
 static __always_inline void set_root(struct nameidata *nd)
 {
-	if (!nd->root.mnt)
-		get_fs_root(current->fs, &nd->root);
+	get_fs_root(current->fs, &nd->root);
 }
 
 static int link_path_walk(const char *, struct nameidata *);
 
-static __always_inline void set_root_rcu(struct nameidata *nd)
+static __always_inline unsigned set_root_rcu(struct nameidata *nd)
 {
-	if (!nd->root.mnt) {
-		struct fs_struct *fs = current->fs;
-		unsigned seq;
+	struct fs_struct *fs = current->fs;
+	unsigned seq, res;
 
-		do {
-			seq = read_seqcount_begin(&fs->seq);
-			nd->root = fs->root;
-			nd->seq = __read_seqcount_begin(&nd->root.dentry->d_seq);
-		} while (read_seqcount_retry(&fs->seq, seq));
-	}
+	do {
+		seq = read_seqcount_begin(&fs->seq);
+		nd->root = fs->root;
+		res = __read_seqcount_begin(&nd->root.dentry->d_seq);
+	} while (read_seqcount_retry(&fs->seq, seq));
+	return res;
 }
 
 static void path_put_conditional(struct path *path, struct nameidata *nd)
@@ -859,7 +857,8 @@ follow_link(struct path *link, struct nameidata *nd, void **p)
 			return PTR_ERR(s);
 		}
 		if (*s == '/') {
-			set_root(nd);
+			if (!nd->root.mnt)
+				set_root(nd);
 			path_put(&nd->path);
 			nd->path = nd->root;
 			path_get(&nd->root);
@@ -1132,7 +1131,8 @@ static bool __follow_mount_rcu(struct nameidata *nd, struct path *path,
 
 static int follow_dotdot_rcu(struct nameidata *nd)
 {
-	set_root_rcu(nd);
+	if (!nd->root.mnt)
+		set_root_rcu(nd);
 
 	while (1) {
 		if (nd->path.dentry == nd->root.dentry &&
@@ -1244,7 +1244,8 @@ static void follow_mount(struct path *path)
 
 static void follow_dotdot(struct nameidata *nd)
 {
-	set_root(nd);
+	if (!nd->root.mnt)
+		set_root(nd);
 
 	while(1) {
 		struct dentry *old = nd->path.dentry;
@@ -1842,7 +1843,7 @@ static int path_init(int dfd, const char *name, unsigned int flags,
 	if (*name=='/') {
 		if (flags & LOOKUP_RCU) {
 			rcu_read_lock();
-			set_root_rcu(nd);
+			nd->seq = set_root_rcu(nd);
 		} else {
 			set_root(nd);
 			path_get(&nd->root);
diff --git a/fs/nfs/nfs4client.c b/fs/nfs/nfs4client.c
index 0e46d3d1b6cc..1abe4f55dea2 100644
--- a/fs/nfs/nfs4client.c
+++ b/fs/nfs/nfs4client.c
@@ -482,6 +482,16 @@ int nfs40_walk_client_list(struct nfs_client *new,
 
 	spin_lock(&nn->nfs_client_lock);
 	list_for_each_entry(pos, &nn->nfs_client_list, cl_share_link) {
+
+		if (pos->rpc_ops != new->rpc_ops)
+			continue;
+
+		if (pos->cl_proto != new->cl_proto)
+			continue;
+
+		if (pos->cl_minorversion != new->cl_minorversion)
+			continue;
+
 		/* If "pos" isn't marked ready, we can't trust the
 		 * remaining fields in "pos" */
 		if (pos->cl_cons_state > NFS_CS_READY) {
@@ -501,15 +511,6 @@ int nfs40_walk_client_list(struct nfs_client *new,
 		if (pos->cl_cons_state != NFS_CS_READY)
 			continue;
 
-		if (pos->rpc_ops != new->rpc_ops)
-			continue;
-
-		if (pos->cl_proto != new->cl_proto)
-			continue;
-
-		if (pos->cl_minorversion != new->cl_minorversion)
-			continue;
-
 		if (pos->cl_clientid != new->cl_clientid)
 			continue;
 
@@ -615,6 +616,16 @@ int nfs41_walk_client_list(struct nfs_client *new,
 
 	spin_lock(&nn->nfs_client_lock);
 	list_for_each_entry(pos, &nn->nfs_client_list, cl_share_link) {
+
+		if (pos->rpc_ops != new->rpc_ops)
+			continue;
+
+		if (pos->cl_proto != new->cl_proto)
+			continue;
+
+		if (pos->cl_minorversion != new->cl_minorversion)
+			continue;
+
 		/* If "pos" isn't marked ready, we can't trust the
 		 * remaining fields in "pos", especially the client
 		 * ID and serverowner fields.  Wait for CREATE_SESSION
@@ -640,15 +651,6 @@ int nfs41_walk_client_list(struct nfs_client *new,
 		if (pos->cl_cons_state != NFS_CS_READY)
 			continue;
 
-		if (pos->rpc_ops != new->rpc_ops)
-			continue;
-
-		if (pos->cl_proto != new->cl_proto)
-			continue;
-
-		if (pos->cl_minorversion != new->cl_minorversion)
-			continue;
-
 		if (!nfs4_match_clientids(pos, new))
 			continue;
 
diff --git a/fs/nfs/nfs4proc.c b/fs/nfs/nfs4proc.c
index 17f91a72840b..2e9662ea5451 100644
--- a/fs/nfs/nfs4proc.c
+++ b/fs/nfs/nfs4proc.c
@@ -2558,23 +2558,23 @@ static void nfs4_close_prepare(struct rpc_task *task, void *data)
 	is_rdwr = test_bit(NFS_O_RDWR_STATE, &state->flags);
 	is_rdonly = test_bit(NFS_O_RDONLY_STATE, &state->flags);
 	is_wronly = test_bit(NFS_O_WRONLY_STATE, &state->flags);
-	/* Calculate the current open share mode */
-	calldata->arg.fmode = 0;
-	if (is_rdonly || is_rdwr)
-		calldata->arg.fmode |= FMODE_READ;
-	if (is_wronly || is_rdwr)
-		calldata->arg.fmode |= FMODE_WRITE;
 	/* Calculate the change in open mode */
+	calldata->arg.fmode = 0;
 	if (state->n_rdwr == 0) {
-		if (state->n_rdonly == 0) {
-			call_close |= is_rdonly || is_rdwr;
-			calldata->arg.fmode &= ~FMODE_READ;
-		}
-		if (state->n_wronly == 0) {
-			call_close |= is_wronly || is_rdwr;
-			calldata->arg.fmode &= ~FMODE_WRITE;
-		}
-	}
+		if (state->n_rdonly == 0)
+			call_close |= is_rdonly;
+		else if (is_rdonly)
+			calldata->arg.fmode |= FMODE_READ;
+		if (state->n_wronly == 0)
+			call_close |= is_wronly;
+		else if (is_wronly)
+			calldata->arg.fmode |= FMODE_WRITE;
+	} else if (is_rdwr)
+		calldata->arg.fmode |= FMODE_READ|FMODE_WRITE;
+
+	if (calldata->arg.fmode == 0)
+		call_close |= is_rdwr;
+
 	if (!nfs4_valid_open_stateid(state))
 		call_close = 0;
 	spin_unlock(&state->owner->so_lock);
diff --git a/fs/nilfs2/inode.c b/fs/nilfs2/inode.c
index 7e350c562e0e..1e0bbae06ee7 100644
--- a/fs/nilfs2/inode.c
+++ b/fs/nilfs2/inode.c
@@ -24,6 +24,7 @@
 #include <linux/buffer_head.h>
 #include <linux/gfp.h>
 #include <linux/mpage.h>
+#include <linux/pagemap.h>
 #include <linux/writeback.h>
 #include <linux/aio.h>
 #include "nilfs.h"
@@ -219,10 +220,10 @@ static int nilfs_writepage(struct page *page, struct writeback_control *wbc)
 
 static int nilfs_set_page_dirty(struct page *page)
 {
+	struct inode *inode = page->mapping->host;
 	int ret = __set_page_dirty_nobuffers(page);
 
 	if (page_has_buffers(page)) {
-		struct inode *inode = page->mapping->host;
 		unsigned nr_dirty = 0;
 		struct buffer_head *bh, *head;
 
@@ -245,6 +246,10 @@ static int nilfs_set_page_dirty(struct page *page)
 
 		if (nr_dirty)
 			nilfs_set_file_dirty(inode, nr_dirty);
+	} else if (ret) {
+		unsigned nr_dirty = 1 << (PAGE_CACHE_SHIFT - inode->i_blkbits);
+
+		nilfs_set_file_dirty(inode, nr_dirty);
 	}
 	return ret;
 }
diff --git a/fs/notify/fdinfo.c b/fs/notify/fdinfo.c
index 238a5930cb3c..9d7e2b9659cb 100644
--- a/fs/notify/fdinfo.c
+++ b/fs/notify/fdinfo.c
@@ -42,7 +42,7 @@ static int show_mark_fhandle(struct seq_file *m, struct inode *inode)
 {
 	struct {
 		struct file_handle handle;
-		u8 pad[64];
+		u8 pad[MAX_HANDLE_SZ];
 	} f;
 	int size, ret, i;
 
@@ -50,7 +50,7 @@ static int show_mark_fhandle(struct seq_file *m, struct inode *inode)
 	size = f.handle.handle_bytes >> 2;
 
 	ret = exportfs_encode_inode_fh(inode, (struct fid *)f.handle.f_handle, &size, 0);
-	if ((ret == 255) || (ret == -ENOSPC)) {
+	if ((ret == FILEID_INVALID) || (ret < 0)) {
 		WARN_ONCE(1, "Can't encode file handler for inotify: %d\n", ret);
 		return 0;
 	}
diff --git a/fs/ocfs2/dlm/dlmmaster.c b/fs/ocfs2/dlm/dlmmaster.c
index af3f7aa73e13..1be3398c96f6 100644
--- a/fs/ocfs2/dlm/dlmmaster.c
+++ b/fs/ocfs2/dlm/dlmmaster.c
@@ -650,12 +650,9 @@ void dlm_lockres_clear_refmap_bit(struct dlm_ctxt *dlm,
 	clear_bit(bit, res->refmap);
 }
 
-
-void dlm_lockres_grab_inflight_ref(struct dlm_ctxt *dlm,
+static void __dlm_lockres_grab_inflight_ref(struct dlm_ctxt *dlm,
 				   struct dlm_lock_resource *res)
 {
-	assert_spin_locked(&res->spinlock);
-
 	res->inflight_locks++;
 
 	mlog(0, "%s: res %.*s, inflight++: now %u, %ps()\n", dlm->name,
@@ -663,6 +660,13 @@ void dlm_lockres_grab_inflight_ref(struct dlm_ctxt *dlm,
 	     __builtin_return_address(0));
 }
 
+void dlm_lockres_grab_inflight_ref(struct dlm_ctxt *dlm,
+				   struct dlm_lock_resource *res)
+{
+	assert_spin_locked(&res->spinlock);
+	__dlm_lockres_grab_inflight_ref(dlm, res);
+}
+
 void dlm_lockres_drop_inflight_ref(struct dlm_ctxt *dlm,
 				   struct dlm_lock_resource *res)
 {
@@ -852,10 +856,8 @@ lookup:
 	/* finally add the lockres to its hash bucket */
 	__dlm_insert_lockres(dlm, res);
 
-	/* Grab inflight ref to pin the resource */
-	spin_lock(&res->spinlock);
-	dlm_lockres_grab_inflight_ref(dlm, res);
-	spin_unlock(&res->spinlock);
+	/* since this lockres is new it doesn't not require the spinlock */
+	__dlm_lockres_grab_inflight_ref(dlm, res);
 
 	/* get an extra ref on the mle in case this is a BLOCK
 	 * if so, the creator of the BLOCK may try to put the last
diff --git a/include/acpi/acpi_bus.h b/include/acpi/acpi_bus.h
index e9c4f190ffae..ac46782c10d3 100644
--- a/include/acpi/acpi_bus.h
+++ b/include/acpi/acpi_bus.h
@@ -118,6 +118,7 @@ struct acpi_device;
 struct acpi_hotplug_profile {
 	struct kobject kobj;
 	int (*scan_dependent)(struct acpi_device *adev);
+	void (*notify_online)(struct acpi_device *adev);
 	bool enabled:1;
 	bool demand_offline:1;
 };
diff --git a/include/linux/iio/trigger.h b/include/linux/iio/trigger.h
index 369cf2cd5144..68f46cd5d514 100644
--- a/include/linux/iio/trigger.h
+++ b/include/linux/iio/trigger.h
@@ -84,10 +84,12 @@ static inline void iio_trigger_put(struct iio_trigger *trig)
 	put_device(&trig->dev);
 }
 
-static inline void iio_trigger_get(struct iio_trigger *trig)
+static inline struct iio_trigger *iio_trigger_get(struct iio_trigger *trig)
 {
 	get_device(&trig->dev);
 	__module_get(trig->ops->owner);
+
+	return trig;
 }
 
 /**
diff --git a/include/linux/seqlock.h b/include/linux/seqlock.h
index 535f158977b9..8cf350325dc6 100644
--- a/include/linux/seqlock.h
+++ b/include/linux/seqlock.h
@@ -164,8 +164,6 @@ static inline unsigned read_seqcount_begin(const seqcount_t *s)
 static inline unsigned raw_seqcount_begin(const seqcount_t *s)
 {
 	unsigned ret = ACCESS_ONCE(s->sequence);
-
-	seqcount_lockdep_reader_access(s);
 	smp_rmb();
 	return ret & ~1;
 }
diff --git a/include/linux/vga_switcheroo.h b/include/linux/vga_switcheroo.h
index 502073a53dd3..b483abd34493 100644
--- a/include/linux/vga_switcheroo.h
+++ b/include/linux/vga_switcheroo.h
@@ -64,6 +64,7 @@ int vga_switcheroo_get_client_state(struct pci_dev *dev);
 void vga_switcheroo_set_dynamic_switch(struct pci_dev *pdev, enum vga_switcheroo_state dynamic);
 
 int vga_switcheroo_init_domain_pm_ops(struct device *dev, struct dev_pm_domain *domain);
+void vga_switcheroo_fini_domain_pm_ops(struct device *dev);
 int vga_switcheroo_init_domain_pm_optimus_hdmi_audio(struct device *dev, struct dev_pm_domain *domain);
 #else
 
@@ -82,6 +83,7 @@ static inline int vga_switcheroo_get_client_state(struct pci_dev *dev) { return
 static inline void vga_switcheroo_set_dynamic_switch(struct pci_dev *pdev, enum vga_switcheroo_state dynamic) {}
 
 static inline int vga_switcheroo_init_domain_pm_ops(struct device *dev, struct dev_pm_domain *domain) { return -EINVAL; }
+static inline void vga_switcheroo_fini_domain_pm_ops(struct device *dev) {}
 static inline int vga_switcheroo_init_domain_pm_optimus_hdmi_audio(struct device *dev, struct dev_pm_domain *domain) { return -EINVAL; }
 
 #endif
diff --git a/include/linux/workqueue.h b/include/linux/workqueue.h
index 704f4f652d0a..6c62cfa25f1a 100644
--- a/include/linux/workqueue.h
+++ b/include/linux/workqueue.h
@@ -452,7 +452,7 @@ __alloc_workqueue_key(const char *fmt, unsigned int flags, int max_active,
 	alloc_workqueue("%s", WQ_FREEZABLE | WQ_UNBOUND | WQ_MEM_RECLAIM, \
 			1, (name))
 #define create_singlethread_workqueue(name)				\
-	alloc_workqueue("%s", WQ_UNBOUND | WQ_MEM_RECLAIM, 1, (name))
+	alloc_ordered_workqueue("%s", WQ_MEM_RECLAIM, name)
 
 extern void destroy_workqueue(struct workqueue_struct *wq);
 
diff --git a/include/net/regulatory.h b/include/net/regulatory.h
index b07cdc9fa454..f103f30122a1 100644
--- a/include/net/regulatory.h
+++ b/include/net/regulatory.h
@@ -160,7 +160,7 @@ struct ieee80211_reg_rule {
 struct ieee80211_regdomain {
 	struct rcu_head rcu_head;
 	u32 n_reg_rules;
-	char alpha2[2];
+	char alpha2[3];
 	enum nl80211_dfs_regions dfs_region;
 	struct ieee80211_reg_rule reg_rules[];
 };
diff --git a/include/uapi/linux/usb/functionfs.h b/include/uapi/linux/usb/functionfs.h
index 29e9c7aa9c66..f279394aafb0 100644
--- a/include/uapi/linux/usb/functionfs.h
+++ b/include/uapi/linux/usb/functionfs.h
@@ -27,24 +27,18 @@ struct usb_endpoint_descriptor_no_audio {
 	__u8  bInterval;
 } __attribute__((packed));
 
-/* Legacy format, deprecated as of 3.14. */
-struct usb_functionfs_descs_head {
-	__le32 magic;
-	__le32 length;
-	__le32 fs_count;
-	__le32 hs_count;
-} __attribute__((packed, deprecated));
 
 /*
  * All numbers must be in little endian order.
  */
 
+/* Legacy format, deprecated as of 3.14. */
 struct usb_functionfs_descs_head {
 	__le32 magic;
 	__le32 length;
 	__le32 fs_count;
 	__le32 hs_count;
-} __attribute__((packed));
+} __attribute__((packed, deprecated));
 
 /*
  * Descriptors format:
diff --git a/include/uapi/linux/xattr.h b/include/uapi/linux/xattr.h
index c38355c1f3c9..1590c49cae57 100644
--- a/include/uapi/linux/xattr.h
+++ b/include/uapi/linux/xattr.h
@@ -13,7 +13,7 @@
 #ifndef _UAPI_LINUX_XATTR_H
 #define _UAPI_LINUX_XATTR_H
 
-#ifdef __UAPI_DEF_XATTR
+#if __UAPI_DEF_XATTR
 #define __USE_KERNEL_XATTR_DEFS
 
 #define XATTR_CREATE	0x1	/* set value, fail if attr already exists */
diff --git a/kernel/cgroup.c b/kernel/cgroup.c
index 0c753ddd223b..550e2050d778 100644
--- a/kernel/cgroup.c
+++ b/kernel/cgroup.c
@@ -3663,7 +3663,6 @@ static int pidlist_array_load(struct cgroup *cgrp, enum cgroup_filetype type,
 
 	l = cgroup_pidlist_find_create(cgrp, type);
 	if (!l) {
-		mutex_unlock(&cgrp->pidlist_mutex);
 		pidlist_free(array);
 		return -ENOMEM;
 	}
diff --git a/kernel/events/core.c b/kernel/events/core.c
index f774e9365a03..3a140ca37777 100644
--- a/kernel/events/core.c
+++ b/kernel/events/core.c
@@ -1516,6 +1516,11 @@ retry:
 	 */
 	if (ctx->is_active) {
 		raw_spin_unlock_irq(&ctx->lock);
+		/*
+		 * Reload the task pointer, it might have been changed by
+		 * a concurrent perf_event_context_sched_out().
+		 */
+		task = ctx->task;
 		goto retry;
 	}
 
@@ -1957,6 +1962,11 @@ retry:
 	 */
 	if (ctx->is_active) {
 		raw_spin_unlock_irq(&ctx->lock);
+		/*
+		 * Reload the task pointer, it might have been changed by
+		 * a concurrent perf_event_context_sched_out().
+		 */
+		task = ctx->task;
 		goto retry;
 	}
 
diff --git a/kernel/futex.c b/kernel/futex.c
index e3087afb7429..0b0dc02aabce 100644
--- a/kernel/futex.c
+++ b/kernel/futex.c
@@ -2614,6 +2614,7 @@ static int futex_wait_requeue_pi(u32 __user *uaddr, unsigned int flags,
 	 * shared futexes. We need to compare the keys:
 	 */
 	if (match_futex(&q.key, &key2)) {
+		queue_unlock(hb);
 		ret = -EINVAL;
 		goto out_put_keys;
 	}
diff --git a/kernel/kcmp.c b/kernel/kcmp.c
index e30ac0fe61c3..0aa69ea1d8fd 100644
--- a/kernel/kcmp.c
+++ b/kernel/kcmp.c
@@ -44,11 +44,12 @@ static long kptr_obfuscate(long v, int type)
  */
 static int kcmp_ptr(void *v1, void *v2, enum kcmp_type type)
 {
-	long ret;
+	long t1, t2;
 
-	ret = kptr_obfuscate((long)v1, type) - kptr_obfuscate((long)v2, type);
+	t1 = kptr_obfuscate((long)v1, type);
+	t2 = kptr_obfuscate((long)v2, type);
 
-	return (ret < 0) | ((ret > 0) << 1);
+	return (t1 < t2) | ((t1 > t2) << 1);
 }
 
 /* The caller must have pinned the task */
diff --git a/kernel/power/main.c b/kernel/power/main.c
index 1d1bf630e6e9..3ae41cdd804a 100644
--- a/kernel/power/main.c
+++ b/kernel/power/main.c
@@ -293,12 +293,12 @@ static ssize_t state_show(struct kobject *kobj, struct kobj_attribute *attr,
 {
 	char *s = buf;
 #ifdef CONFIG_SUSPEND
-	int i;
+	suspend_state_t i;
+
+	for (i = PM_SUSPEND_MIN; i < PM_SUSPEND_MAX; i++)
+		if (pm_states[i].state)
+			s += sprintf(s,"%s ", pm_states[i].label);
 
-	for (i = 0; i < PM_SUSPEND_MAX; i++) {
-		if (pm_states[i] && valid_state(i))
-			s += sprintf(s,"%s ", pm_states[i]);
-	}
 #endif
 #ifdef CONFIG_HIBERNATION
 	s += sprintf(s, "%s\n", "disk");
@@ -314,7 +314,7 @@ static suspend_state_t decode_state(const char *buf, size_t n)
 {
 #ifdef CONFIG_SUSPEND
 	suspend_state_t state = PM_SUSPEND_MIN;
-	const char * const *s;
+	struct pm_sleep_state *s;
 #endif
 	char *p;
 	int len;
@@ -328,8 +328,9 @@ static suspend_state_t decode_state(const char *buf, size_t n)
 
 #ifdef CONFIG_SUSPEND
 	for (s = &pm_states[state]; state < PM_SUSPEND_MAX; s++, state++)
-		if (*s && len == strlen(*s) && !strncmp(buf, *s, len))
-			return state;
+		if (s->state && len == strlen(s->label)
+		    && !strncmp(buf, s->label, len))
+			return s->state;
 #endif
 
 	return PM_SUSPEND_ON;
@@ -447,8 +448,8 @@ static ssize_t autosleep_show(struct kobject *kobj,
 
 #ifdef CONFIG_SUSPEND
 	if (state < PM_SUSPEND_MAX)
-		return sprintf(buf, "%s\n", valid_state(state) ?
-						pm_states[state] : "error");
+		return sprintf(buf, "%s\n", pm_states[state].state ?
+					pm_states[state].label : "error");
 #endif
 #ifdef CONFIG_HIBERNATION
 	return sprintf(buf, "disk\n");
diff --git a/kernel/power/power.h b/kernel/power/power.h
index 7d4b7ffb3c1d..f770cad3666c 100644
--- a/kernel/power/power.h
+++ b/kernel/power/power.h
@@ -175,17 +175,20 @@ extern void swsusp_show_speed(struct timeval *, struct timeval *,
 				unsigned int, char *);
 
 #ifdef CONFIG_SUSPEND
+struct pm_sleep_state {
+	const char *label;
+	suspend_state_t state;
+};
+
 /* kernel/power/suspend.c */
-extern const char *const pm_states[];
+extern struct pm_sleep_state pm_states[];
 
-extern bool valid_state(suspend_state_t state);
 extern int suspend_devices_and_enter(suspend_state_t state);
 #else /* !CONFIG_SUSPEND */
 static inline int suspend_devices_and_enter(suspend_state_t state)
 {
 	return -ENOSYS;
 }
-static inline bool valid_state(suspend_state_t state) { return false; }
 #endif /* !CONFIG_SUSPEND */
 
 #ifdef CONFIG_PM_TEST_SUSPEND
diff --git a/kernel/power/suspend.c b/kernel/power/suspend.c
index 62ee437b5c7e..5455d5c3c149 100644
--- a/kernel/power/suspend.c
+++ b/kernel/power/suspend.c
@@ -29,10 +29,10 @@
 
 #include "power.h"
 
-const char *const pm_states[PM_SUSPEND_MAX] = {
-	[PM_SUSPEND_FREEZE]	= "freeze",
-	[PM_SUSPEND_STANDBY]	= "standby",
-	[PM_SUSPEND_MEM]	= "mem",
+struct pm_sleep_state pm_states[PM_SUSPEND_MAX] = {
+	[PM_SUSPEND_FREEZE] = { .label = "freeze", .state = PM_SUSPEND_FREEZE },
+	[PM_SUSPEND_STANDBY] = { .label = "standby", },
+	[PM_SUSPEND_MEM] = { .label = "mem", },
 };
 
 static const struct platform_suspend_ops *suspend_ops;
@@ -62,42 +62,34 @@ void freeze_wake(void)
 }
 EXPORT_SYMBOL_GPL(freeze_wake);
 
+static bool valid_state(suspend_state_t state)
+{
+	/*
+	 * PM_SUSPEND_STANDBY and PM_SUSPEND_MEM states need low level
+	 * support and need to be valid to the low level
+	 * implementation, no valid callback implies that none are valid.
+	 */
+	return suspend_ops && suspend_ops->valid && suspend_ops->valid(state);
+}
+
 /**
  * suspend_set_ops - Set the global suspend method table.
  * @ops: Suspend operations to use.
  */
 void suspend_set_ops(const struct platform_suspend_ops *ops)
 {
+	suspend_state_t i;
+
 	lock_system_sleep();
+
 	suspend_ops = ops;
+	for (i = PM_SUSPEND_STANDBY; i <= PM_SUSPEND_MEM; i++)
+		pm_states[i].state = valid_state(i) ? i : 0;
+
 	unlock_system_sleep();
 }
 EXPORT_SYMBOL_GPL(suspend_set_ops);
 
-bool valid_state(suspend_state_t state)
-{
-	if (state == PM_SUSPEND_FREEZE) {
-#ifdef CONFIG_PM_DEBUG
-		if (pm_test_level != TEST_NONE &&
-		    pm_test_level != TEST_FREEZER &&
-		    pm_test_level != TEST_DEVICES &&
-		    pm_test_level != TEST_PLATFORM) {
-			printk(KERN_WARNING "Unsupported pm_test mode for "
-					"freeze state, please choose "
-					"none/freezer/devices/platform.\n");
-			return false;
-		}
-#endif
-			return true;
-	}
-	/*
-	 * PM_SUSPEND_STANDBY and PM_SUSPEND_MEMORY states need lowlevel
-	 * support and need to be valid to the lowlevel
-	 * implementation, no valid callback implies that none are valid.
-	 */
-	return suspend_ops && suspend_ops->valid && suspend_ops->valid(state);
-}
-
 /**
  * suspend_valid_only_mem - Generic memory-only valid callback.
  *
@@ -324,9 +316,17 @@ static int enter_state(suspend_state_t state)
 {
 	int error;
 
-	if (!valid_state(state))
-		return -ENODEV;
-
+	if (state == PM_SUSPEND_FREEZE) {
+#ifdef CONFIG_PM_DEBUG
+		if (pm_test_level != TEST_NONE && pm_test_level <= TEST_CPUS) {
+			pr_warning("PM: Unsupported test mode for freeze state,"
+				   "please choose none/freezer/devices/platform.\n");
+			return -EAGAIN;
+		}
+#endif
+	} else if (!valid_state(state)) {
+		return -EINVAL;
+	}
 	if (!mutex_trylock(&pm_mutex))
 		return -EBUSY;
 
@@ -337,7 +337,7 @@ static int enter_state(suspend_state_t state)
 	sys_sync();
 	printk("done.\n");
 
-	pr_debug("PM: Preparing system for %s sleep\n", pm_states[state]);
+	pr_debug("PM: Preparing system for %s sleep\n", pm_states[state].label);
 	error = suspend_prepare(state);
 	if (error)
 		goto Unlock;
@@ -345,7 +345,7 @@ static int enter_state(suspend_state_t state)
 	if (suspend_test(TEST_FREEZER))
 		goto Finish;
 
-	pr_debug("PM: Entering %s sleep\n", pm_states[state]);
+	pr_debug("PM: Entering %s sleep\n", pm_states[state].label);
 	pm_restrict_gfp_mask();
 	error = suspend_devices_and_enter(state);
 	pm_restore_gfp_mask();
diff --git a/kernel/power/suspend_test.c b/kernel/power/suspend_test.c
index 9b2a1d58558d..269b097e78ea 100644
--- a/kernel/power/suspend_test.c
+++ b/kernel/power/suspend_test.c
@@ -92,13 +92,13 @@ static void __init test_wakealarm(struct rtc_device *rtc, suspend_state_t state)
 	}
 
 	if (state == PM_SUSPEND_MEM) {
-		printk(info_test, pm_states[state]);
+		printk(info_test, pm_states[state].label);
 		status = pm_suspend(state);
 		if (status == -ENODEV)
 			state = PM_SUSPEND_STANDBY;
 	}
 	if (state == PM_SUSPEND_STANDBY) {
-		printk(info_test, pm_states[state]);
+		printk(info_test, pm_states[state].label);
 		status = pm_suspend(state);
 	}
 	if (status < 0)
@@ -136,18 +136,16 @@ static char warn_bad_state[] __initdata =
 
 static int __init setup_test_suspend(char *value)
 {
-	unsigned i;
+	suspend_state_t i;
 
 	/* "=mem" ==> "mem" */
 	value++;
-	for (i = 0; i < PM_SUSPEND_MAX; i++) {
-		if (!pm_states[i])
-			continue;
-		if (strcmp(pm_states[i], value) != 0)
-			continue;
-		test_state = (__force suspend_state_t) i;
-		return 0;
-	}
+	for (i = PM_SUSPEND_MIN; i < PM_SUSPEND_MAX; i++)
+		if (!strcmp(pm_states[i].label, value)) {
+			test_state = pm_states[i].state;
+			return 0;
+		}
+
 	printk(warn_bad_state, value);
 	return 0;
 }
@@ -164,8 +162,8 @@ static int __init test_suspend(void)
 	/* PM is initialized by now; is that state testable? */
 	if (test_state == PM_SUSPEND_ON)
 		goto done;
-	if (!valid_state(test_state)) {
-		printk(warn_bad_state, pm_states[test_state]);
+	if (!pm_states[test_state].state) {
+		printk(warn_bad_state, pm_states[test_state].label);
 		goto done;
 	}
 
diff --git a/kernel/time/alarmtimer.c b/kernel/time/alarmtimer.c
index fe75444ae7ec..cd45a0727a16 100644
--- a/kernel/time/alarmtimer.c
+++ b/kernel/time/alarmtimer.c
@@ -464,18 +464,26 @@ static enum alarmtimer_type clock2alarm(clockid_t clockid)
 static enum alarmtimer_restart alarm_handle_timer(struct alarm *alarm,
 							ktime_t now)
 {
+	unsigned long flags;
 	struct k_itimer *ptr = container_of(alarm, struct k_itimer,
 						it.alarm.alarmtimer);
-	if (posix_timer_event(ptr, 0) != 0)
-		ptr->it_overrun++;
+	enum alarmtimer_restart result = ALARMTIMER_NORESTART;
+
+	spin_lock_irqsave(&ptr->it_lock, flags);
+	if ((ptr->it_sigev_notify & ~SIGEV_THREAD_ID) != SIGEV_NONE) {
+		if (posix_timer_event(ptr, 0) != 0)
+			ptr->it_overrun++;
+	}
 
 	/* Re-add periodic timers */
 	if (ptr->it.alarm.interval.tv64) {
 		ptr->it_overrun += alarm_forward(alarm, now,
 						ptr->it.alarm.interval);
-		return ALARMTIMER_RESTART;
+		result = ALARMTIMER_RESTART;
 	}
-	return ALARMTIMER_NORESTART;
+	spin_unlock_irqrestore(&ptr->it_lock, flags);
+
+	return result;
 }
 
 /**
@@ -541,18 +549,22 @@ static int alarm_timer_create(struct k_itimer *new_timer)
  * @new_timer: k_itimer pointer
  * @cur_setting: itimerspec data to fill
  *
- * Copies the itimerspec data out from the k_itimer
+ * Copies out the current itimerspec data
  */
 static void alarm_timer_get(struct k_itimer *timr,
 				struct itimerspec *cur_setting)
 {
-	memset(cur_setting, 0, sizeof(struct itimerspec));
+	ktime_t relative_expiry_time =
+		alarm_expires_remaining(&(timr->it.alarm.alarmtimer));
+
+	if (ktime_to_ns(relative_expiry_time) > 0) {
+		cur_setting->it_value = ktime_to_timespec(relative_expiry_time);
+	} else {
+		cur_setting->it_value.tv_sec = 0;
+		cur_setting->it_value.tv_nsec = 0;
+	}
 
-	cur_setting->it_interval =
-			ktime_to_timespec(timr->it.alarm.interval);
-	cur_setting->it_value =
-		ktime_to_timespec(timr->it.alarm.alarmtimer.node.expires);
-	return;
+	cur_setting->it_interval = ktime_to_timespec(timr->it.alarm.interval);
 }
 
 /**
diff --git a/kernel/trace/ring_buffer.c b/kernel/trace/ring_buffer.c
index a53f1bbc546b..773aba836e81 100644
--- a/kernel/trace/ring_buffer.c
+++ b/kernel/trace/ring_buffer.c
@@ -626,8 +626,22 @@ int ring_buffer_poll_wait(struct ring_buffer *buffer, int cpu,
 		work = &cpu_buffer->irq_work;
 	}
 
-	work->waiters_pending = true;
 	poll_wait(filp, &work->waiters, poll_table);
+	work->waiters_pending = true;
+	/*
+	 * There's a tight race between setting the waiters_pending and
+	 * checking if the ring buffer is empty.  Once the waiters_pending bit
+	 * is set, the next event will wake the task up, but we can get stuck
+	 * if there's only a single event in.
+	 *
+	 * FIXME: Ideally, we need a memory barrier on the writer side as well,
+	 * but adding a memory barrier to all events will cause too much of a
+	 * performance hit in the fast path.  We only need a memory barrier when
+	 * the buffer goes from empty to having content.  But as this race is
+	 * extremely small, and it's not a problem if another event comes in, we
+	 * will fix it later.
+	 */
+	smp_mb();
 
 	if ((cpu == RING_BUFFER_ALL_CPUS && !ring_buffer_empty(buffer)) ||
 	    (cpu != RING_BUFFER_ALL_CPUS && !ring_buffer_empty_cpu(buffer, cpu)))
diff --git a/mm/memblock.c b/mm/memblock.c
index 39a31e7f0045..0739dc1b4095 100644
--- a/mm/memblock.c
+++ b/mm/memblock.c
@@ -183,8 +183,7 @@ phys_addr_t __init_memblock memblock_find_in_range_node(phys_addr_t size,
 					phys_addr_t align, phys_addr_t start,
 					phys_addr_t end, int nid)
 {
-	int ret;
-	phys_addr_t kernel_end;
+	phys_addr_t kernel_end, ret;
 
 	/* pump up @end */
 	if (end == MEMBLOCK_ALLOC_ACCESSIBLE)
diff --git a/mm/memory.c b/mm/memory.c
index 2121d8b8db56..492e36f27f43 100644
--- a/mm/memory.c
+++ b/mm/memory.c
@@ -1120,7 +1120,7 @@ again:
 						addr) != page->index) {
 				pte_t ptfile = pgoff_to_pte(page->index);
 				if (pte_soft_dirty(ptent))
-					pte_file_mksoft_dirty(ptfile);
+					ptfile = pte_file_mksoft_dirty(ptfile);
 				set_pte_at(mm, addr, pte, ptfile);
 			}
 			if (PageAnon(page))
diff --git a/mm/percpu-vm.c b/mm/percpu-vm.c
index 3707c71ae4cd..51108165f829 100644
--- a/mm/percpu-vm.c
+++ b/mm/percpu-vm.c
@@ -108,7 +108,7 @@ static int pcpu_alloc_pages(struct pcpu_chunk *chunk,
 			    int page_start, int page_end)
 {
 	const gfp_t gfp = GFP_KERNEL | __GFP_HIGHMEM | __GFP_COLD;
-	unsigned int cpu;
+	unsigned int cpu, tcpu;
 	int i;
 
 	for_each_possible_cpu(cpu) {
@@ -116,14 +116,23 @@ static int pcpu_alloc_pages(struct pcpu_chunk *chunk,
 			struct page **pagep = &pages[pcpu_page_idx(cpu, i)];
 
 			*pagep = alloc_pages_node(cpu_to_node(cpu), gfp, 0);
-			if (!*pagep) {
-				pcpu_free_pages(chunk, pages, populated,
-						page_start, page_end);
-				return -ENOMEM;
-			}
+			if (!*pagep)
+				goto err;
 		}
 	}
 	return 0;
+
+err:
+	while (--i >= page_start)
+		__free_page(pages[pcpu_page_idx(cpu, i)]);
+
+	for_each_possible_cpu(tcpu) {
+		if (tcpu == cpu)
+			break;
+		for (i = page_start; i < page_end; i++)
+			__free_page(pages[pcpu_page_idx(tcpu, i)]);
+	}
+	return -ENOMEM;
 }
 
 /**
@@ -263,6 +272,7 @@ err:
 		__pcpu_unmap_pages(pcpu_chunk_addr(chunk, tcpu, page_start),
 				   page_end - page_start);
 	}
+	pcpu_post_unmap_tlb_flush(chunk, page_start, page_end);
 	return err;
 }
 
diff --git a/mm/percpu.c b/mm/percpu.c
index a2a54a85f691..8cd4308471c3 100644
--- a/mm/percpu.c
+++ b/mm/percpu.c
@@ -1917,6 +1917,8 @@ void __init setup_per_cpu_areas(void)
 
 	if (pcpu_setup_first_chunk(ai, fc) < 0)
 		panic("Failed to initialize percpu areas.");
+
+	pcpu_free_alloc_info(ai);
 }
 
 #endif	/* CONFIG_SMP */
diff --git a/mm/shmem.c b/mm/shmem.c
index ff85863587ee..f0d698ba7d0f 100644
--- a/mm/shmem.c
+++ b/mm/shmem.c
@@ -2143,8 +2143,10 @@ static int shmem_rename(struct inode *old_dir, struct dentry *old_dentry, struct
 
 	if (new_dentry->d_inode) {
 		(void) shmem_unlink(new_dir, new_dentry);
-		if (they_are_dirs)
+		if (they_are_dirs) {
+			drop_nlink(new_dentry->d_inode);
 			drop_nlink(old_dir);
+		}
 	} else if (they_are_dirs) {
 		drop_nlink(old_dir);
 		inc_nlink(new_dir);
diff --git a/mm/slab.c b/mm/slab.c
index 6dd8d5f3a3ac..ea854eb2388c 100644
--- a/mm/slab.c
+++ b/mm/slab.c
@@ -2189,7 +2189,8 @@ static int __init_refok setup_cpu_cache(struct kmem_cache *cachep, gfp_t gfp)
 int
 __kmem_cache_create (struct kmem_cache *cachep, unsigned long flags)
 {
-	size_t left_over, freelist_size, ralign;
+	size_t left_over, freelist_size;
+	size_t ralign = BYTES_PER_WORD;
 	gfp_t gfp;
 	int err;
 	size_t size = cachep->size;
@@ -2222,14 +2223,6 @@ __kmem_cache_create (struct kmem_cache *cachep, unsigned long flags)
 		size &= ~(BYTES_PER_WORD - 1);
 	}
 
-	/*
-	 * Redzoning and user store require word alignment or possibly larger.
-	 * Note this will be overridden by architecture or caller mandated
-	 * alignment if either is greater than BYTES_PER_WORD.
-	 */
-	if (flags & SLAB_STORE_USER)
-		ralign = BYTES_PER_WORD;
-
 	if (flags & SLAB_RED_ZONE) {
 		ralign = REDZONE_ALIGN;
 		/* If redzoning, ensure that the second redzone is suitably
diff --git a/net/mac80211/mlme.c b/net/mac80211/mlme.c
index e6a84cb1a5e4..189eef014c4f 100644
--- a/net/mac80211/mlme.c
+++ b/net/mac80211/mlme.c
@@ -4240,8 +4240,7 @@ int ieee80211_mgd_assoc(struct ieee80211_sub_if_data *sdata,
 	rcu_read_unlock();
 
 	if (bss->wmm_used && bss->uapsd_supported &&
-	    (sdata->local->hw.flags & IEEE80211_HW_SUPPORTS_UAPSD) &&
-	    sdata->wmm_acm != 0xff) {
+	    (sdata->local->hw.flags & IEEE80211_HW_SUPPORTS_UAPSD)) {
 		assoc_data->uapsd = true;
 		ifmgd->flags |= IEEE80211_STA_UAPSD_ENABLED;
 	} else {
diff --git a/net/netfilter/ipvs/ip_vs_conn.c b/net/netfilter/ipvs/ip_vs_conn.c
index a8eb0a89326a..610e19c0e13f 100644
--- a/net/netfilter/ipvs/ip_vs_conn.c
+++ b/net/netfilter/ipvs/ip_vs_conn.c
@@ -797,7 +797,6 @@ static void ip_vs_conn_expire(unsigned long data)
 			ip_vs_control_del(cp);
 
 		if (cp->flags & IP_VS_CONN_F_NFCT) {
-			ip_vs_conn_drop_conntrack(cp);
 			/* Do not access conntracks during subsys cleanup
 			 * because nf_conntrack_find_get can not be used after
 			 * conntrack cleanup for the net.
diff --git a/net/netfilter/ipvs/ip_vs_core.c b/net/netfilter/ipvs/ip_vs_core.c
index 3d2d2c8108ca..27d3f40de3cd 100644
--- a/net/netfilter/ipvs/ip_vs_core.c
+++ b/net/netfilter/ipvs/ip_vs_core.c
@@ -1906,7 +1906,7 @@ static struct nf_hook_ops ip_vs_ops[] __read_mostly = {
 	{
 		.hook		= ip_vs_local_reply6,
 		.owner		= THIS_MODULE,
-		.pf		= NFPROTO_IPV4,
+		.pf		= NFPROTO_IPV6,
 		.hooknum	= NF_INET_LOCAL_OUT,
 		.priority	= NF_IP6_PRI_NAT_DST + 1,
 	},
diff --git a/net/netfilter/ipvs/ip_vs_xmit.c b/net/netfilter/ipvs/ip_vs_xmit.c
index 7f0e1cf2d7e8..1692e7534759 100644
--- a/net/netfilter/ipvs/ip_vs_xmit.c
+++ b/net/netfilter/ipvs/ip_vs_xmit.c
@@ -967,8 +967,8 @@ ip_vs_tunnel_xmit_v6(struct sk_buff *skb, struct ip_vs_conn *cp,
 	iph->nexthdr		=	IPPROTO_IPV6;
 	iph->payload_len	=	old_iph->payload_len;
 	be16_add_cpu(&iph->payload_len, sizeof(*old_iph));
-	iph->priority		=	old_iph->priority;
 	memset(&iph->flow_lbl, 0, sizeof(iph->flow_lbl));
+	ipv6_change_dsfield(iph, 0, ipv6_get_dsfield(old_iph));
 	iph->daddr = cp->daddr.in6;
 	iph->saddr = saddr;
 	iph->hop_limit		=	old_iph->hop_limit;
diff --git a/net/netfilter/xt_cgroup.c b/net/netfilter/xt_cgroup.c
index 9a8e77e7f8d4..ef5c75a5b200 100644
--- a/net/netfilter/xt_cgroup.c
+++ b/net/netfilter/xt_cgroup.c
@@ -31,7 +31,7 @@ static int cgroup_mt_check(const struct xt_mtchk_param *par)
 	if (info->invert & ~1)
 		return -EINVAL;
 
-	return info->id ? 0 : -EINVAL;
+	return 0;
 }
 
 static bool
diff --git a/net/netfilter/xt_hashlimit.c b/net/netfilter/xt_hashlimit.c
index a3910fc2122b..47dc6836830a 100644
--- a/net/netfilter/xt_hashlimit.c
+++ b/net/netfilter/xt_hashlimit.c
@@ -104,7 +104,7 @@ struct xt_hashlimit_htable {
 	spinlock_t lock;		/* lock for list_head */
 	u_int32_t rnd;			/* random seed for hash */
 	unsigned int count;		/* number entries in table */
-	struct timer_list timer;	/* timer for gc */
+	struct delayed_work gc_work;
 
 	/* seq_file stuff */
 	struct proc_dir_entry *pde;
@@ -213,7 +213,7 @@ dsthash_free(struct xt_hashlimit_htable *ht, struct dsthash_ent *ent)
 	call_rcu_bh(&ent->rcu, dsthash_free_rcu);
 	ht->count--;
 }
-static void htable_gc(unsigned long htlong);
+static void htable_gc(struct work_struct *work);
 
 static int htable_create(struct net *net, struct xt_hashlimit_mtinfo1 *minfo,
 			 u_int8_t family)
@@ -273,9 +273,9 @@ static int htable_create(struct net *net, struct xt_hashlimit_mtinfo1 *minfo,
 	}
 	hinfo->net = net;
 
-	setup_timer(&hinfo->timer, htable_gc, (unsigned long)hinfo);
-	hinfo->timer.expires = jiffies + msecs_to_jiffies(hinfo->cfg.gc_interval);
-	add_timer(&hinfo->timer);
+	INIT_DEFERRABLE_WORK(&hinfo->gc_work, htable_gc);
+	queue_delayed_work(system_power_efficient_wq, &hinfo->gc_work,
+			   msecs_to_jiffies(hinfo->cfg.gc_interval));
 
 	hlist_add_head(&hinfo->node, &hashlimit_net->htables);
 
@@ -300,29 +300,30 @@ static void htable_selective_cleanup(struct xt_hashlimit_htable *ht,
 {
 	unsigned int i;
 
-	/* lock hash table and iterate over it */
-	spin_lock_bh(&ht->lock);
 	for (i = 0; i < ht->cfg.size; i++) {
 		struct dsthash_ent *dh;
 		struct hlist_node *n;
+
+		spin_lock_bh(&ht->lock);
 		hlist_for_each_entry_safe(dh, n, &ht->hash[i], node) {
 			if ((*select)(ht, dh))
 				dsthash_free(ht, dh);
 		}
+		spin_unlock_bh(&ht->lock);
+		cond_resched();
 	}
-	spin_unlock_bh(&ht->lock);
 }
 
-/* hash table garbage collector, run by timer */
-static void htable_gc(unsigned long htlong)
+static void htable_gc(struct work_struct *work)
 {
-	struct xt_hashlimit_htable *ht = (struct xt_hashlimit_htable *)htlong;
+	struct xt_hashlimit_htable *ht;
+
+	ht = container_of(work, struct xt_hashlimit_htable, gc_work.work);
 
 	htable_selective_cleanup(ht, select_gc);
 
-	/* re-add the timer accordingly */
-	ht->timer.expires = jiffies + msecs_to_jiffies(ht->cfg.gc_interval);
-	add_timer(&ht->timer);
+	queue_delayed_work(system_power_efficient_wq,
+			   &ht->gc_work, msecs_to_jiffies(ht->cfg.gc_interval));
 }
 
 static void htable_remove_proc_entry(struct xt_hashlimit_htable *hinfo)
@@ -341,7 +342,7 @@ static void htable_remove_proc_entry(struct xt_hashlimit_htable *hinfo)
 
 static void htable_destroy(struct xt_hashlimit_htable *hinfo)
 {
-	del_timer_sync(&hinfo->timer);
+	cancel_delayed_work_sync(&hinfo->gc_work);
 	htable_remove_proc_entry(hinfo);
 	htable_selective_cleanup(hinfo, select_all);
 	kfree(hinfo->name);
diff --git a/net/wireless/nl80211.c b/net/wireless/nl80211.c
index e6283464a8e6..df33156ecd2d 100644
--- a/net/wireless/nl80211.c
+++ b/net/wireless/nl80211.c
@@ -6796,6 +6796,9 @@ void __cfg80211_send_event_skb(struct sk_buff *skb, gfp_t gfp)
 	struct nlattr *data = ((void **)skb->cb)[2];
 	enum nl80211_multicast_groups mcgrp = NL80211_MCGRP_TESTMODE;
 
+	/* clear CB data for netlink core to own from now on */
+	memset(skb->cb, 0, sizeof(skb->cb));
+
 	nla_nest_end(skb, data);
 	genlmsg_end(skb, hdr);
 
@@ -9075,6 +9078,9 @@ int cfg80211_vendor_cmd_reply(struct sk_buff *skb)
 	void *hdr = ((void **)skb->cb)[1];
 	struct nlattr *data = ((void **)skb->cb)[2];
 
+	/* clear CB data for netlink core to own from now on */
+	memset(skb->cb, 0, sizeof(skb->cb));
+
 	if (WARN_ON(!rdev->cur_cmd_info)) {
 		kfree_skb(skb);
 		return -EINVAL;
diff --git a/sound/core/info.c b/sound/core/info.c
index e79baa11b60e..08070e1eefeb 100644
--- a/sound/core/info.c
+++ b/sound/core/info.c
@@ -679,7 +679,7 @@ int snd_info_card_free(struct snd_card *card)
  * snd_info_get_line - read one line from the procfs buffer
  * @buffer: the procfs buffer
  * @line: the buffer to store
- * @len: the max. buffer size - 1
+ * @len: the max. buffer size
  *
  * Reads one line from the buffer and stores the string.
  *
@@ -699,7 +699,7 @@ int snd_info_get_line(struct snd_info_buffer *buffer, char *line, int len)
 			buffer->stop = 1;
 		if (c == '\n')
 			break;
-		if (len) {
+		if (len > 1) {
 			len--;
 			*line++ = c;
 		}
diff --git a/sound/core/pcm_lib.c b/sound/core/pcm_lib.c
index a2104671f51d..e1ef106c8a6f 100644
--- a/sound/core/pcm_lib.c
+++ b/sound/core/pcm_lib.c
@@ -1783,14 +1783,16 @@ static int snd_pcm_lib_ioctl_fifo_size(struct snd_pcm_substream *substream,
 {
 	struct snd_pcm_hw_params *params = arg;
 	snd_pcm_format_t format;
-	int channels, width;
+	int channels;
+	ssize_t frame_size;
 
 	params->fifo_size = substream->runtime->hw.fifo_size;
 	if (!(substream->runtime->hw.info & SNDRV_PCM_INFO_FIFO_IN_FRAMES)) {
 		format = params_format(params);
 		channels = params_channels(params);
-		width = snd_pcm_format_physical_width(format);
-		params->fifo_size /= width * channels;
+		frame_size = snd_pcm_format_size(format, channels);
+		if (frame_size > 0)
+			params->fifo_size /= (unsigned)frame_size;
 	}
 	return 0;
 }
diff --git a/sound/pci/hda/patch_conexant.c b/sound/pci/hda/patch_conexant.c
index bcf91bea3317..ffc19464b978 100644
--- a/sound/pci/hda/patch_conexant.c
+++ b/sound/pci/hda/patch_conexant.c
@@ -3237,6 +3237,7 @@ enum {
 	CXT_FIXUP_HEADPHONE_MIC_PIN,
 	CXT_FIXUP_HEADPHONE_MIC,
 	CXT_FIXUP_GPIO1,
+	CXT_FIXUP_ASPIRE_DMIC,
 	CXT_FIXUP_THINKPAD_ACPI,
 };
 
@@ -3397,6 +3398,12 @@ static const struct hda_fixup cxt_fixups[] = {
 			{ }
 		},
 	},
+	[CXT_FIXUP_ASPIRE_DMIC] = {
+		.type = HDA_FIXUP_FUNC,
+		.v.func = cxt_fixup_stereo_dmic,
+		.chained = true,
+		.chain_id = CXT_FIXUP_GPIO1,
+	},
 	[CXT_FIXUP_THINKPAD_ACPI] = {
 		.type = HDA_FIXUP_FUNC,
 		.v.func = hda_fixup_thinkpad_acpi,
@@ -3410,7 +3417,7 @@ static const struct snd_pci_quirk cxt5051_fixups[] = {
 
 static const struct snd_pci_quirk cxt5066_fixups[] = {
 	SND_PCI_QUIRK(0x1025, 0x0543, "Acer Aspire One 522", CXT_FIXUP_STEREO_DMIC),
-	SND_PCI_QUIRK(0x1025, 0x054c, "Acer Aspire 3830TG", CXT_FIXUP_GPIO1),
+	SND_PCI_QUIRK(0x1025, 0x054c, "Acer Aspire 3830TG", CXT_FIXUP_ASPIRE_DMIC),
 	SND_PCI_QUIRK(0x1043, 0x138d, "Asus", CXT_FIXUP_HEADPHONE_MIC_PIN),
 	SND_PCI_QUIRK(0x17aa, 0x20f2, "Lenovo T400", CXT_PINCFG_LENOVO_TP410),
 	SND_PCI_QUIRK(0x17aa, 0x215e, "Lenovo T410", CXT_PINCFG_LENOVO_TP410),
diff --git a/sound/pci/hda/patch_realtek.c b/sound/pci/hda/patch_realtek.c
index b35dbe25a6e3..5d0058bd6259 100644
--- a/sound/pci/hda/patch_realtek.c
+++ b/sound/pci/hda/patch_realtek.c
@@ -327,6 +327,7 @@ static void alc_auto_init_amp(struct hda_codec *codec, int type)
 		case 0x10ec0885:
 		case 0x10ec0887:
 		/*case 0x10ec0889:*/ /* this causes an SPDIF problem */
+		case 0x10ec0900:
 			alc889_coef_init(codec);
 			break;
 		case 0x10ec0888:
@@ -2330,6 +2331,7 @@ static int patch_alc882(struct hda_codec *codec)
 	switch (codec->vendor_id) {
 	case 0x10ec0882:
 	case 0x10ec0885:
+	case 0x10ec0900:
 		break;
 	default:
 		/* ALC883 and variants */
diff --git a/sound/pci/hda/patch_sigmatel.c b/sound/pci/hda/patch_sigmatel.c
index 978df990f27c..15270a2e71cc 100644
--- a/sound/pci/hda/patch_sigmatel.c
+++ b/sound/pci/hda/patch_sigmatel.c
@@ -559,8 +559,8 @@ static void stac_init_power_map(struct hda_codec *codec)
 		if (snd_hda_jack_tbl_get(codec, nid))
 			continue;
 		if (def_conf == AC_JACK_PORT_COMPLEX &&
-		    !(spec->vref_mute_led_nid == nid ||
-		      is_jack_detectable(codec, nid))) {
+		    spec->vref_mute_led_nid != nid &&
+		    is_jack_detectable(codec, nid)) {
 			snd_hda_jack_detect_enable_callback(codec, nid,
 							    STAC_PWR_EVENT,
 							    jack_update_power);
@@ -4212,11 +4212,18 @@ static int stac_parse_auto_config(struct hda_codec *codec)
 			return err;
 	}
 
-	stac_init_power_map(codec);
-
 	return 0;
 }
 
+static int stac_build_controls(struct hda_codec *codec)
+{
+	int err = snd_hda_gen_build_controls(codec);
+
+	if (err < 0)
+		return err;
+	stac_init_power_map(codec);
+	return 0;
+}
 
 static int stac_init(struct hda_codec *codec)
 {
@@ -4328,7 +4335,7 @@ static int stac_suspend(struct hda_codec *codec)
 #endif /* CONFIG_PM */
 
 static const struct hda_codec_ops stac_patch_ops = {
-	.build_controls = snd_hda_gen_build_controls,
+	.build_controls = stac_build_controls,
 	.build_pcms = snd_hda_gen_build_pcms,
 	.init = stac_init,
 	.free = stac_free,
diff --git a/sound/soc/davinci/davinci-mcasp.c b/sound/soc/davinci/davinci-mcasp.c
index 670afa29e30d..7350ebbae642 100644
--- a/sound/soc/davinci/davinci-mcasp.c
+++ b/sound/soc/davinci/davinci-mcasp.c
@@ -418,8 +418,17 @@ static int davinci_config_channel_size(struct davinci_mcasp *mcasp,
 {
 	u32 fmt;
 	u32 tx_rotate = (word_length / 4) & 0x7;
-	u32 rx_rotate = (32 - word_length) / 4;
 	u32 mask = (1ULL << word_length) - 1;
+	/*
+	 * For captured data we should not rotate, inversion and masking is
+	 * enoguh to get the data to the right position:
+	 * Format	  data from bus		after reverse (XRBUF)
+	 * S16_LE:	|LSB|MSB|xxx|xxx|	|xxx|xxx|MSB|LSB|
+	 * S24_3LE:	|LSB|DAT|MSB|xxx|	|xxx|MSB|DAT|LSB|
+	 * S24_LE:	|LSB|DAT|MSB|xxx|	|xxx|MSB|DAT|LSB|
+	 * S32_LE:	|LSB|DAT|DAT|MSB|	|MSB|DAT|DAT|LSB|
+	 */
+	u32 rx_rotate = 0;
 
 	/*
 	 * if s BCLK-to-LRCLK ratio has been configured via the set_clkdiv()
