# -*- coding: utf-8; mode: tcl; tab-width: 4; indent-tabs-mode: nil; c-basic-offset: 4 -*- vim:fenc=utf-8:ft=tcl:et:sw=4:ts=4:sts=4

PortSystem          1.0
PortGroup           cmake 1.1
PortGroup           github 1.0

github.setup        inilabs libcaer 2.4.0
# Change github.tarball_from to 'releases' or 'archive' next update
github.tarball_from tarball
categories          devel
license             BSD
maintainers         {@ierofant gmail.com:aw.kornilov} openmaintainer

description         Minimal C library to access, configure and get/send AER data
long_description    Minimal C library to access, configure and get/send AER data from sensors \
                    or to/from neuromorphic processors. Supported devices are the Dynamic Vision Sensor (DVS), \
                    all the DAVIS cameras, and the Dynap-se neuromorphic processor.

depends_build-append \
                    port:pkgconfig

depends_lib-append  path:lib/pkgconfig/libusb-1.0.pc:libusb

checksums           rmd160  67b5c16b8da39a193249dcdd055d90a9930cd9e4 \
                    sha256  431b606934b40de498a7d0f50876745b92b95d64b5ea81da0a52d055a2b89cd7

compiler.cxx_standard   2011

compiler.blacklist-append \
                    {clang < 602}
