diff --git a/src/Registers.hpp b/src/Registers.hpp
index 36653ef..ad8b906 100644
--- a/src/Registers.hpp
+++ b/src/Registers.hpp
@@ -486,7 +486,6 @@ public:
   uint64_t  getIP() const         { return _registers.__srr0; }
   void      setIP(uint32_t value) { _registers.__srr0 = value; }
 
-private:
   struct ppc_thread_state_t {
     unsigned int __srr0; /* Instruction address register (PC) */
     unsigned int __srr1; /* Machine state register (supervisor) */
@@ -537,6 +536,7 @@ private:
     unsigned int __fpscr;     /* floating point status register */
   };
 
+private:
   ppc_thread_state_t _registers;
   ppc_float_state_t  _floatRegisters;
   v128               _vectorRegisters[32]; // offset 424
@@ -1052,7 +1052,6 @@ public:
   uint64_t  getFP() const         { return _registers.__fp; }
   void      setFP(uint64_t value) { _registers.__fp = value; }
 
-private:
   struct GPRs {
     uint64_t __x[29]; // x0-x28
     uint64_t __fp;    // Frame pointer x29
@@ -1062,6 +1061,7 @@ private:
     uint64_t padding; // 16-byte align
   };
 
+private:
   GPRs    _registers;
   double  _vectorHalfRegisters[32];
   // Currently only the lower double in 128-bit vectore registers
