# -*- coding: utf-8; mode: tcl; tab-width: 4; indent-tabs-mode: nil; c-basic-offset: 4 -*- vim:fenc=utf-8:ft=tcl:et:sw=4:ts=4:sts=4

PortSystem              1.0

name                    libdivecomputer

# please, when updating libdivecomputer, check whether subsurface still builds against the new version
version                 0.4.1
epoch                   1
categories              devel
platforms               darwin
license                 LGPL-2.1
maintainers             nomaintainer

description             Libdivecomputer is a cross-platform and open source \
                        library for communication with dive computers from \
                        various manufacturers.
long_description        {*}${description} Supported devices include devices \
                        manufactured by Suunto, Uwatec, Reefnet, Oceanic, \
                        Aeris, Sherwood, Hollis, Genesis, Tusa, Mares, \
                        Heinrichs Weikamp, Cressi, Zeagle, Mares and Atomic \
                        Aquatics.

homepage                http://www.divesoftware.org/libdc/
master_sites            http://www.divesoftware.org/libdc/releases/

checksums               rmd160 63b5d8eeb36c58a3736f5daddb12ec2fab85542e \
                        sha256 7d64032d2e5cd4d6315ebb7ed5bcccc9399166d40228ae2e96e435749b950a0a

depends_lib             port:gconf \
                        path:lib/pkgconfig/gtk+-2.0.pc:gtk2 \
                        path:lib/pkgconfig/libusb-1.0.pc:libusb

use_autoreconf          yes

