#! /bin/bash
# FS QA Test No. btrfs/020
#
# btrfs device replace test on RO fs
#
# Regression test for commit:
# bbb651e Btrfs: don't allow the replace procedure on read only filesystems
#
#-----------------------------------------------------------------------
# Copyright (c) 2013 Red Hat, Inc.  All Rights Reserved.
#
# This program is free software; you can redistribute it and/or
# modify it under the terms of the GNU General Public License as
# published by the Free Software Foundation.
#
# This program is distributed in the hope that it would be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program; if not, write the Free Software Foundation,
# Inc.,  51 Franklin St, Fifth Floor, Boston, MA  02110-1301  USA
#
#-----------------------------------------------------------------------
#

seq=`basename $0`
seqres=$RESULT_DIR/$seq
echo "QA output created by $seq"

here=`pwd`
tmp=/tmp/$$

status=1	# failure is the default!

_cleanup()
{
	cd /
	rm -f $tmp.*
	$UMOUNT_PROG $loop_mnt
	_destroy_loop_device $loop_dev1
	losetup -d $loop_dev2 >/dev/null 2>&1
	_destroy_loop_device $loop_dev3
	rm -rf $loop_mnt
	rm -f $fs_img1 $fs_img2 $fs_img3
}

trap "_cleanup ; exit \$status" 0 1 2 3 15

# get standard environment, filters and checks
. ./common/rc
. ./common/filter

# real QA test starts here
_supported_fs btrfs
_supported_os Linux
_require_test

rm -f $seqres.full
echo "Silence is golden"

loop_mnt=$TEST_DIR/$seq.$$.mnt
fs_img1=$TEST_DIR/$seq.$$.img1
fs_img2=$TEST_DIR/$seq.$$.img2
fs_img3=$TEST_DIR/$seq.$$.img3
mkdir $loop_mnt
$XFS_IO_PROG -f -c "truncate 256m" $fs_img1 >>$seqres.full 2>&1
$XFS_IO_PROG -f -c "truncate 256m" $fs_img2 >>$seqres.full 2>&1
$XFS_IO_PROG -f -c "truncate 256m" $fs_img3 >>$seqres.full 2>&1

loop_dev1=`_create_loop_device $fs_img1`
loop_dev2=`_create_loop_device $fs_img2`
loop_dev3=`_create_loop_device $fs_img3`

_mkfs_dev -m raid1 -d raid1 $loop_dev1 $loop_dev2 >>$seqres.full 2>&1
_mount -o ro $loop_dev1 $loop_mnt

$BTRFS_UTIL_PROG replace start -B 2 $loop_dev3 $loop_mnt >>$seqres.full 2>&1 && \
_fail "FAIL: Device replaced on RO btrfs"

status=0
exit
