From fc926d1d75ffe9da12e856320e2ad0eb02a28ca2 Mon Sep 17 00:00:00 2001
From: Martin Blumenstingl <martin.blumenstingl@googlemail.com>
Date: Tue, 31 Dec 2024 20:42:06 +0100
Subject: [PATCH 14/50] FROMGIT(6.16): dt-bindings: iio: adc:
 amlogic,meson-saradc: Add GXLX SoC compatible

Add a compatible string for the GXLX SoC. It's very similar to GXL but
has three additional bits in MESON_SAR_ADC_REG12 for the three MPLL
clocks.

Signed-off-by: Martin Blumenstingl <martin.blumenstingl@googlemail.com>
---
 .../devicetree/bindings/iio/adc/amlogic,meson-saradc.yaml        | 1 +
 1 file changed, 1 insertion(+)

diff --git a/Documentation/devicetree/bindings/iio/adc/amlogic,meson-saradc.yaml b/Documentation/devicetree/bindings/iio/adc/amlogic,meson-saradc.yaml
index b0962a4583ac..bb9825e7346d 100644
--- a/Documentation/devicetree/bindings/iio/adc/amlogic,meson-saradc.yaml
+++ b/Documentation/devicetree/bindings/iio/adc/amlogic,meson-saradc.yaml
@@ -23,6 +23,7 @@ properties:
               - amlogic,meson8m2-saradc
               - amlogic,meson-gxbb-saradc
               - amlogic,meson-gxl-saradc
+              - amlogic,meson-gxlx-saradc
               - amlogic,meson-gxm-saradc
               - amlogic,meson-axg-saradc
               - amlogic,meson-g12a-saradc
-- 
2.34.1

